(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "GND")
	(net 2 "/DCDC/5V")
	(net 3 "Net-(U1-VUSB)")
	(net 4 "/DCDC/V_Var")
	(net 5 "Net-(D1-A)")
	(net 6 "Net-(D2-A)")
	(net 7 "Net-(D3-A)")
	(net 8 "Net-(D4-A)")
	(net 9 "Net-(D5-A)")
	(net 10 "Net-(D6-A)")
	(net 11 "Net-(D7-A)")
	(net 12 "Net-(D8-A)")
	(net 13 "Net-(D9-K)")
	(net 14 "Net-(D10-K)")
	(net 15 "Net-(D11-K)")
	(net 16 "Net-(J1-Shield)")
	(net 17 "/Output/SCK")
	(net 18 "/Output/MOSI")
	(net 19 "/Output/CS")
	(net 20 "/Output/MISO")
	(net 21 "Net-(L1-Pad1)")
	(net 22 "/uC/!RES")
	(net 23 "/DCDC/SDA")
	(net 24 "/DCDC/SCL")
	(net 25 "Net-(U3-XTAL32K1{slash}PF0)")
	(net 26 "Net-(U3-XTAL32K2{slash}PF1)")
	(net 27 "Net-(U3-PF2)")
	(net 28 "Net-(U3-PF3)")
	(net 29 "Net-(U3-PF4)")
	(net 30 "Net-(U3-PF5)")
	(net 31 "Net-(U3-PD0)")
	(net 32 "Net-(U3-PD1)")
	(net 33 "unconnected-(U1-GP3-Pad8)")
	(net 34 "unconnected-(U1-SDA-Pad9)")
	(net 35 "unconnected-(U1-GP2-Pad7)")
	(net 36 "/uC/RX_D")
	(net 37 "unconnected-(U1-GP0-Pad2)")
	(net 38 "unconnected-(U1-SCL-Pad10)")
	(net 39 "/uC/TX_D")
	(net 40 "unconnected-(U1-GP1-Pad3)")
	(net 41 "unconnected-(U3-PD3-Pad13)")
	(net 42 "unconnected-(U3-PD6-Pad16)")
	(net 43 "unconnected-(U3-VREFA{slash}PD7-Pad17)")
	(net 44 "unconnected-(U3-PD2-Pad12)")
	(net 45 "unconnected-(U3-PC2-Pad8)")
	(net 46 "/DCDC/EN")
	(net 47 "unconnected-(U3-PD5-Pad15)")
	(net 48 "unconnected-(U3-PD4-Pad14)")
	(net 49 "unconnected-(U3-PC3-Pad9)")
	(net 50 "Net-(U2-UPDI)")
	(net 51 "Net-(U4-SENSE{slash}ADJ)")
	(net 52 "Net-(J2-Pin_4)")
	(net 53 "Net-(J2-Pin_2)")
	(net 54 "Net-(J2-Pin_5)")
	(net 55 "Net-(J2-Pin_3)")
	(net 56 "unconnected-(U1-~{RST}-Pad4)")
	(footprint "Connector_IDC:IDC-Header_2x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 154.29 96.04 180)
		(descr "Through hole IDC box header, 2x03, 2.54mm pitch, DIN 41651 / IEC 60603-13, double rows, https://docs.google.com/spreadsheets/d/16SsEcesNF15N3Lb4niX7dcUr-NY5_MFPQhobNuNppn4/edit#gid=0")
		(tags "Through hole vertical IDC box header THT 2x03 2.54mm double row")
		(property "Reference" "J2"
			(at 1.27 -6.1 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x06_Socket"
			(at 1.27 11.18 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_IDC:IDC-Header_2x03_P2.54mm_Vertical"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x06, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Output")
		(sheetfile "Out.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 1.27 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole roundrect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(roundrect_rratio 0.147059)
			(net 4 "/DCDC/V_Var")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 2.54 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 53 "Net-(J2-Pin_2)")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 55 "Net-(J2-Pin_3)")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at 2.54 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 52 "Net-(J2-Pin_4)")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 54 "Net-(J2-Pin_5)")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" thru_hole circle
			(at 2.54 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_IDC.3dshapes/IDC-Header_2x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:TSOT-23-5"
		(layer "F.Cu")
		(at 114.55 103.75 90)
		(descr "TSOT, 5 Pin (https://www.jedec.org/sites/default/files/docs/MO-193D.pdf variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSOT TO_SOT_SMD")
		(property "Reference" "U4"
			(at 0 -2.4 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "AP7330-W5-7"
			(at 0 2.4 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:TSOT-23-5"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/ADP7142.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "200mA, Low Noise, CMOS Low Dropout Regulator, Positive, Adjustable, TSOT-23-5"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSOT?23*")
		(sheetname "DCDC")
		(sheetfile "DCDC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/DCDC/5V")
			(pinfunction "VIN")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 46 "/DCDC/EN")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 51 "Net-(U4-SENSE{slash}ADJ)")
			(pinfunction "SENSE/ADJ")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 1.1375 -0.95 90)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "/DCDC/V_Var")
			(pinfunction "VOUT")
			(pintype "power_out")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/TSOT-23-5.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-363_SC-70-6"
		(layer "F.Cu")
		(at 119.25 103.75 90)
		(descr "SOT-363, SC-70-6")
		(tags "SOT-363 SC-70-6")
		(property "Reference" "U6"
			(at 0 -2.25 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MCP4018-xxxxLT"
			(at 0 2 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-363_SC-70-6"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/22147a.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Low-Cost 128-Step Volatile I2C Digital Potentiometer, SC-70-6"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*SC?70*")
		(sheetname "DCDC")
		(sheetfile "DCDC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 -0.65 90)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/DCDC/5V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -0.95 0 90)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -0.95 0.65 90)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 24 "/DCDC/SCL")
			(pinfunction "SCL")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at 0.95 0.65 90)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "/DCDC/SDA")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at 0.95 0 90)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 51 "Net-(U4-SENSE{slash}ADJ)")
			(pinfunction "W")
			(pintype "passive")
		)
		(pad "6" smd roundrect
			(at 0.95 -0.65 90)
			(size 0.65 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "/DCDC/V_Var")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-363_SC-70-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 145.75 87.5)
		(descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "diode handsolder")
		(property "Reference" "C8"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Output")
		(sheetfile "Out.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 4 "/DCDC/V_Var")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 125.75 85 -90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D5"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1V2"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "uC")
		(sheetfile "UC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "Net-(D5-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:CP_Elec_6.3x7.7"
		(layer "F.Cu")
		(at 107 103.75 180)
		(descr "SMD capacitor, aluminum electrolytic, Nichicon, 6.3x7.7mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C5"
			(at 0 -4.35 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C"
			(at 0 4.35 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:CP_Elec_6.3x7.7"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "DCDC")
		(sheetfile "DCDC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.7 0 180)
			(size 3.5 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.15625)
			(net 4 "/DCDC/V_Var")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.7 0 180)
			(size 3.5 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.15625)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_6.3x7.7.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 129.25 85 -90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D4"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "1V8"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "uC")
		(sheetfile "UC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "Net-(D4-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 139.75 89 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R6"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "uC")
		(sheetfile "UC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 25 "Net-(U3-XTAL32K1{slash}PF0)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 5 "Net-(D1-A)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
		(layer "F.Cu")
		(at 107.5 90.5 90)
		(descr "SOIC, 14 Pin (JEDEC MS-012AB, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_14.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U1"
			(at 0 -5.28 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MCP2221AxSL"
			(at 0 5.28 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_SO:SOIC-14_3.9x8.7mm_P1.27mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/20005565B.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "USB to I2C/UART Protocol Converter with GPIO, SOIC-14"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*3.9x8.7mm*P1.27mm*")
		(sheetname "USB_IN")
		(sheetfile "USB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -3.81 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/DCDC/5V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -2.475 -2.54 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 37 "unconnected-(U1-GP0-Pad2)")
			(pinfunction "GP0")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -2.475 -1.27 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 40 "unconnected-(U1-GP1-Pad3)")
			(pinfunction "GP1")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -2.475 0 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 56 "unconnected-(U1-~{RST}-Pad4)")
			(pinfunction "~{RST}")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -2.475 1.27 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 39 "/uC/TX_D")
			(pinfunction "URx")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at -2.475 2.54 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "/uC/RX_D")
			(pinfunction "UTx")
			(pintype "output")
		)
		(pad "7" smd roundrect
			(at -2.475 3.81 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 35 "unconnected-(U1-GP2-Pad7)")
			(pinfunction "GP2")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 2.475 3.81 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "unconnected-(U1-GP3-Pad8)")
			(pinfunction "GP3")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at 2.475 2.54 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 34 "unconnected-(U1-SDA-Pad9)")
			(pinfunction "SDA")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at 2.475 1.27 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 38 "unconnected-(U1-SCL-Pad10)")
			(pinfunction "SCL")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at 2.475 0 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(U1-VUSB)")
			(pinfunction "VUSB")
			(pintype "passive")
		)
		(pad "12" smd roundrect
			(at 2.475 -1.27 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "Net-(D11-K)")
			(pinfunction "D-")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at 2.475 -2.54 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "Net-(D10-K)")
			(pinfunction "D+")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at 2.475 -3.81 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-14_3.9x8.7mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 145.75 99.5)
		(descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "diode handsolder")
		(property "Reference" "C10"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Output")
		(sheetfile "Out.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 4 "/DCDC/V_Var")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 132.5 105.75 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R3"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "DCDC")
		(sheetfile "DCDC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 4 "/DCDC/V_Var")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-6"
		(layer "F.Cu")
		(at 144.5 96.5)
		(descr "SOT, 6 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U8"
			(at 0 -2.4 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SN74LVC1T45DBV"
			(at 0 2.4 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74lvc1t45.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Single-Bit Dual-Supply Bus Transceiver With Configurable Voltage Translation and 3-State Outputs, SOT-23-6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "Output")
		(sheetfile "Out.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/DCDC/5V")
			(pinfunction "VCCA")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 17 "/Output/SCK")
			(pinfunction "A")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 52 "Net-(J2-Pin_4)")
			(pinfunction "B")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at 1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/DCDC/5V")
			(pinfunction "DIR")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "/DCDC/V_Var")
			(pinfunction "VCCB")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 145.75 93.5)
		(descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "diode handsolder")
		(property "Reference" "C9"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Output")
		(sheetfile "Out.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 4 "/DCDC/V_Var")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0402_1005Metric"
		(layer "F.Cu")
		(at 105 85.25 90)
		(descr "Diode SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D10"
			(at 0 -1 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ESD321DPYR"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Diode_SMD:D_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/esd5z2.5t1-d.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "ESD Protection Diode, SOD-523"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D?SOD?523*")
		(sheetname "USB_IN")
		(sheetfile "USB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 90)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "Net-(D10-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.485 0 90)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 136.25 85 -90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D2"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "3V3"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "uC")
		(sheetfile "UC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 129.25 89 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R9"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "uC")
		(sheetfile "UC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 28 "Net-(U3-PF3)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 8 "Net-(D4-A)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 136.25 96.75 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R12"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "uC")
		(sheetfile "UC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 31 "Net-(U3-PD0)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 11 "Net-(D7-A)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 139.75 85 -90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D1"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "5V"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "uC")
		(sheetfile "UC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 136.25 89 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R7"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "uC")
		(sheetfile "UC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 26 "Net-(U3-XTAL32K2{slash}PF1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 6 "Net-(D2-A)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 125.75 89 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R10"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "uC")
		(sheetfile "UC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 29 "Net-(U3-PF4)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 9 "Net-(D5-A)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 121 97.75 90)
		(descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "diode handsolder")
		(property "Reference" "C4"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C"
			(at 0 1.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "uC")
		(sheetfile "UC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.025 0 90)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.025 0 90)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 2 "/DCDC/5V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 110 97.75 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0 -1.68 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1u"
			(at 0 1.68 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "USB_IN")
		(sheetfile "USB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/DCDC/5V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0402_1005Metric"
		(layer "F.Cu")
		(at 106.25 85.25 90)
		(descr "Diode SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D11"
			(at 0 -1.17 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ESD321DPYR"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Diode_SMD:D_0402_1005Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/esd5z2.5t1-d.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "ESD Protection Diode, SOD-523"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D?SOD?523*")
		(sheetname "USB_IN")
		(sheetfile "USB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 90)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "Net-(D11-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.485 0 90)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 122.25 85 -90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D6"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Enabled"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "uC")
		(sheetfile "UC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "Net-(D6-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 124 106.5 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R5"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "uC")
		(sheetfile "UC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 2 "/DCDC/5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 24 "/DCDC/SCL")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 108 84.5 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 -1.68 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1u"
			(at 0 1.68 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "USB_IN")
		(sheetfile "USB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(U1-VUSB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 121 93.25 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R2"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "uC")
		(sheetfile "UC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 2 "/DCDC/5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 22 "/uC/!RES")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 145.5 105.5)
		(descr "Diode SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "diode handsolder")
		(property "Reference" "C11"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Diode_SMD:D_0805_2012Metric_Pad1.15x1.40mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Output")
		(sheetfile "Out.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 4 "/DCDC/V_Var")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.025 0)
			(size 1.15 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 132.75 89 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R8"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "uC")
		(sheetfile "UC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 27 "Net-(U3-PF2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 7 "Net-(D3-A)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_USB:USB_B_Lumberg_2411_02_Horizontal"
		(layer "F.Cu")
		(at 100.2875 94.75 180)
		(descr "USB 2.0 receptacle type B, horizontal version, through-hole, https://downloads.lumberg.com/datenblaetter/en/2411_02.pdf")
		(tags "USB B receptacle horizontal through-hole")
		(property "Reference" "J1"
			(at 7.5 -7.65 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USB-B1HSW6"
			(at 7.05 10.45 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Connector_USB:USB_B_Lumberg_2411_02_Horizontal"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "USB Type B connector"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "USB*")
		(sheetname "USB_IN")
		(sheetfile "USB.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 7.5 1.25 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 13 "Net-(D9-K)")
			(pinfunction "VBUS")
			(pintype "power_out")
		)
		(pad "2" thru_hole circle
			(at 0 2.5 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 15 "Net-(D11-K)")
			(pinfunction "D-")
			(pintype "bidirectional")
		)
		(pad "3" thru_hole circle
			(at 2 2.5 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 14 "Net-(D10-K)")
			(pinfunction "D+")
			(pintype "bidirectional")
		)
		(pad "4" thru_hole circle
			(at 2 0 270)
			(size 1.6 1.6)
			(drill 0.95)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_out")
		)
		(pad "5" thru_hole circle
			(at 4.86 -4.75 270)
			(size 4 4)
			(drill 2.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(J1-Shield)")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 4.86 7.25 270)
			(size 4 4)
			(drill 2.3)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "Net-(J1-Shield)")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_USB.3dshapes/USB_B_Lumberg_2411_02_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_QFP:TQFP-32_7x7mm_P0.8mm"
		(layer "F.Cu")
		(at 127.75 97.5 90)
		(descr "32-Lead Plastic Thin Quad Flatpack (PT) - 7x7x1.0 mm Body, 2.00 mm [TQFP] (see Microchip Packaging Specification 00000049BS.pdf)")
		(tags "QFP 0.8")
		(property "Reference" "U3"
			(at 0 -6.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "AVR16EA32x-xPT"
			(at 18.35 18.32 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_QFP:TQFP-32_7x7mm_P0.8mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://ww1.microchip.com/downloads/en/DeviceDoc/AVR128DA28-32-48-64-DataSheet-DS40002183B.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "24MHz, 128kB Flash, 16kB SRAM, EEPROM with Touch Sensing, TQFP-32"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TQFP*7x7mm*P0.8mm*")
		(sheetname "uC")
		(sheetfile "UC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -4.25 -2.8 90)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "/DCDC/SCL")
			(pinfunction "PA3")
			(pintype "bidirectional")
		)
		(pad "2" smd rect
			(at -4.25 -2 90)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "/Output/MOSI")
			(pinfunction "PA4")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at -4.25 -1.2 90)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "/Output/MISO")
			(pinfunction "PA5")
			(pintype "bidirectional")
		)
		(pad "4" smd rect
			(at -4.25 -0.4 90)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "/Output/SCK")
			(pinfunction "PA6")
			(pintype "bidirectional")
		)
		(pad "5" smd rect
			(at -4.25 0.4 90)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "/Output/CS")
			(pinfunction "PA7")
			(pintype "bidirectional")
		)
		(pad "6" smd rect
			(at -4.25 1.2 90)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "/DCDC/V_Var")
			(pinfunction "PC0")
			(pintype "bidirectional")
		)
		(pad "7" smd rect
			(at -4.25 2 90)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "/DCDC/EN")
			(pinfunction "PC1")
			(pintype "bidirectional")
		)
		(pad "8" smd rect
			(at -4.25 2.8 90)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 45 "unconnected-(U3-PC2-Pad8)")
			(pinfunction "PC2")
			(pintype "bidirectional")
		)
		(pad "9" smd rect
			(at -2.8 4.25 180)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 49 "unconnected-(U3-PC3-Pad9)")
			(pinfunction "PC3")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at -2 4.25 180)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "Net-(U3-PD0)")
			(pinfunction "PD0")
			(pintype "bidirectional")
		)
		(pad "11" smd rect
			(at -1.2 4.25 180)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "Net-(U3-PD1)")
			(pinfunction "PD1")
			(pintype "bidirectional")
		)
		(pad "12" smd rect
			(at -0.4 4.25 180)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "unconnected-(U3-PD2-Pad12)")
			(pinfunction "PD2")
			(pintype "bidirectional")
		)
		(pad "13" smd rect
			(at 0.4 4.25 180)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 41 "unconnected-(U3-PD3-Pad13)")
			(pinfunction "PD3")
			(pintype "bidirectional")
		)
		(pad "14" smd rect
			(at 1.2 4.25 180)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 48 "unconnected-(U3-PD4-Pad14)")
			(pinfunction "PD4")
			(pintype "bidirectional")
		)
		(pad "15" smd rect
			(at 2 4.25 180)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "unconnected-(U3-PD5-Pad15)")
			(pinfunction "PD5")
			(pintype "bidirectional")
		)
		(pad "16" smd rect
			(at 2.8 4.25 180)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "unconnected-(U3-PD6-Pad16)")
			(pinfunction "PD6")
			(pintype "bidirectional")
		)
		(pad "17" smd rect
			(at 4.25 2.8 90)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 43 "unconnected-(U3-VREFA{slash}PD7-Pad17)")
			(pinfunction "VREFA/PD7")
			(pintype "bidirectional")
		)
		(pad "18" smd rect
			(at 4.25 2 90)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "/DCDC/5V")
			(pinfunction "AVDD")
			(pintype "power_in")
		)
		(pad "19" smd rect
			(at 4.25 1.2 90)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "20" smd rect
			(at 4.25 0.4 90)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "Net-(U3-XTAL32K1{slash}PF0)")
			(pinfunction "XTAL32K1/PF0")
			(pintype "bidirectional")
		)
		(pad "21" smd rect
			(at 4.25 -0.4 90)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "Net-(U3-XTAL32K2{slash}PF1)")
			(pinfunction "XTAL32K2/PF1")
			(pintype "bidirectional")
		)
		(pad "22" smd rect
			(at 4.25 -1.2 90)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "Net-(U3-PF2)")
			(pinfunction "PF2")
			(pintype "bidirectional")
		)
		(pad "23" smd rect
			(at 4.25 -2 90)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "Net-(U3-PF3)")
			(pinfunction "PF3")
			(pintype "bidirectional")
		)
		(pad "24" smd rect
			(at 4.25 -2.8 90)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "Net-(U3-PF4)")
			(pinfunction "PF4")
			(pintype "bidirectional")
		)
		(pad "25" smd rect
			(at 2.8 -4.25 180)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "Net-(U3-PF5)")
			(pinfunction "PF5")
			(pintype "bidirectional")
		)
		(pad "26" smd rect
			(at 2 -4.25 180)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "/uC/!RES")
			(pinfunction "~{RESET}/PF6")
			(pintype "bidirectional")
		)
		(pad "27" smd rect
			(at 1.2 -4.25 180)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "Net-(U2-UPDI)")
			(pinfunction "UPDI")
			(pintype "input")
		)
		(pad "28" smd rect
			(at 0.4 -4.25 180)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "/DCDC/5V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "29" smd rect
			(at -0.4 -4.25 180)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "30" smd rect
			(at -1.2 -4.25 180)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "/uC/TX_D")
			(pinfunction "PA0")
			(pintype "bidirectional")
		)
		(pad "31" smd rect
			(at -2 -4.25 180)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "/uC/RX_D")
			(pinfunction "PA1")
			(pintype "bidirectional")
		)
		(pad "32" smd rect
			(at -2.8 -4.25 180)
			(size 1.6 0.55)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "/DCDC/SDA")
			(pinfunction "PA2")
			(pintype "bidirectional")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_QFP.3dshapes/TQFP-32_7x7mm_P0.8mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 139.75 96.75 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R13"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "uC")
		(sheetfile "UC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 32 "Net-(U3-PD1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 12 "Net-(D8-A)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-6"
		(layer "F.Cu")
		(at 144.5 102.5)
		(descr "SOT, 6 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U5"
			(at 0 -2.4 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SN74LVC1T45DBV"
			(at 0 2.4 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74lvc1t45.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Single-Bit Dual-Supply Bus Transceiver With Configurable Voltage Translation and 3-State Outputs, SOT-23-6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "Output")
		(sheetfile "Out.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/DCDC/5V")
			(pinfunction "VCCA")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "/Output/MOSI")
			(pinfunction "A")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 53 "Net-(J2-Pin_2)")
			(pinfunction "B")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at 1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/DCDC/5V")
			(pinfunction "DIR")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "/DCDC/V_Var")
			(pinfunction "VCCB")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 127.5 105.75 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at 0 -1.68 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1u"
			(at 0 1.68 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "DCDC")
		(sheetfile "DCDC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/DCDC/5V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 104.5 97.75 -90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R1"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "R"
			(at 0 1.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "USB_IN")
		(sheetfile "USB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 13 "Net-(D9-K)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 270)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 21 "Net-(L1-Pad1)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "F.Cu")
		(at 130 105.75 90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 0 -1.68 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1u"
			(at 0 1.68 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:C_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "DCDC")
		(sheetfile "DCDC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 90)
			(size 1 1.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "/DCDC/V_Var")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-6"
		(layer "F.Cu")
		(at 144.5 84.49)
		(descr "SOT, 6 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U9"
			(at 0 -2.4 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SN74LVC1T45DBV"
			(at 0 2.4 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74lvc1t45.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Single-Bit Dual-Supply Bus Transceiver With Configurable Voltage Translation and 3-State Outputs, SOT-23-6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "Output")
		(sheetfile "Out.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/DCDC/5V")
			(pinfunction "VCCA")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 19 "/Output/CS")
			(pinfunction "A")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 54 "Net-(J2-Pin_5)")
			(pinfunction "B")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at 1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/DCDC/5V")
			(pinfunction "DIR")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "/DCDC/V_Var")
			(pinfunction "VCCB")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-6"
		(layer "F.Cu")
		(at 144.5 90.55)
		(descr "SOT, 6 Pin (https://www.jedec.org/sites/default/files/docs/Mo-178c.PDF variant AB), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U7"
			(at 0 -2.4 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SN74LVC1T45DBV"
			(at 0 2.4 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23-6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://www.ti.com/lit/ds/symlink/sn74lvc1t45.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Single-Bit Dual-Supply Bus Transceiver With Configurable Voltage Translation and 3-State Outputs, SOT-23-6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "Output")
		(sheetfile "Out.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/DCDC/5V")
			(pinfunction "VCCA")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 20 "/Output/MISO")
			(pinfunction "A")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 55 "Net-(J2-Pin_3)")
			(pinfunction "B")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at 1.1375 0)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "DIR")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at 1.1375 -0.95)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "/DCDC/V_Var")
			(pinfunction "VCCB")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:CP_Elec_6.3x7.7"
		(layer "F.Cu")
		(at 116 96 -90)
		(descr "SMD capacitor, aluminum electrolytic, Nichicon, 6.3x7.7mm")
		(tags "capacitor electrolytic")
		(property "Reference" "C1"
			(at 0 -4.35 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "C"
			(at 0 4.35 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Capacitor_SMD:CP_Elec_6.3x7.7"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Polarized capacitor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "CP_*")
		(sheetname "USB_IN")
		(sheetfile "USB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.7 0 270)
			(size 3.5 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.15625)
			(net 2 "/DCDC/5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 2.7 0 270)
			(size 3.5 1.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.15625)
			(net 1 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/CP_Elec_6.3x7.7.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 139.75 100.75 90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D8"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Failure"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "uC")
		(sheetfile "UC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "Net-(D8-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 136.25 100.75 90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D7"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Busy"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "uC")
		(sheetfile "UC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 90)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "Net-(D7-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
		(layer "F.Cu")
		(at 100.25 83.5 180)
		(descr "SMD Solder Jumper, 1x1.5mm, rounded Pads, 0.3mm gap, open")
		(tags "solder jumper open")
		(property "Reference" "JP1"
			(at 0 -1.8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Jumper_2_Open"
			(at 0 1.9 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Jumper:SolderJumper-2_P1.3mm_Open_RoundedPad1.0x1.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Jumper, 2-pole, open"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jumper* TestPoint*2Pads* TestPoint*Bridge*")
		(sheetname "USB_IN")
		(sheetfile "USB.kicad_sch")
		(zone_connect 1)
		(attr exclude_from_pos_files)
		(pad "1" smd custom
			(at -0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 1 "GND")
			(pinfunction "A")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0.5 0.75) (xy 0 0.75) (xy 0 -0.75) (xy 0.5 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(pad "2" smd custom
			(at 0.65 0 180)
			(size 1 0.5)
			(layers "F.Cu" "F.Mask")
			(net 16 "Net-(J1-Shield)")
			(pinfunction "B")
			(pintype "passive")
			(zone_connect 2)
			(thermal_bridge_angle 45)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_circle
					(center 0 0.25)
					(end 0.5 0.25)
					(width 0)
					(fill yes)
				)
				(gr_circle
					(center 0 -0.25)
					(end 0.5 -0.25)
					(width 0)
					(fill yes)
				)
				(gr_poly
					(pts
						(xy 0 0.75) (xy -0.5 0.75) (xy -0.5 -0.75) (xy 0 -0.75)
					)
					(width 0)
					(fill yes)
				)
			)
		)
	)
	(footprint "Diode_SMD:D_0402_1005Metric"
		(layer "F.Cu")
		(at 102.75 97.75 -90)
		(descr "Diode SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "diode")
		(property "Reference" "D9"
			(at 0 -1.17 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ESD441DPLR"
			(at 0 1.17 -90)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:D_0402_1005Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.onsemi.com/pdf/datasheet/esd5z2.5t1-d.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "ESD Protection Diode, SOD-523"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D?SOD?523*")
		(sheetname "USB_IN")
		(sheetfile "USB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 270)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "Net-(D9-K)")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.485 0 270)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 122.25 89 90)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R11"
			(at 0 -1.65 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.65 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "uC")
		(sheetfile "UC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 30 "Net-(U3-PF5)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 90)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 10 "Net-(D6-A)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
		(layer "F.Cu")
		(at 124 104.5 180)
		(descr "Resistor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor handsolder")
		(property "Reference" "R4"
			(at 0 -1.65 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.65 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "uC")
		(sheetfile "UC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 2 "/DCDC/5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1 0 180)
			(size 1.2 1.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.208333)
			(net 23 "/DCDC/SDA")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0805_2012Metric"
		(layer "F.Cu")
		(at 107.25 97.75 90)
		(descr "Inductor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 80, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L1"
			(at 0 -1.55 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "L"
			(at 0 1.55 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "Inductor_SMD:L_0805_2012Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "USB_IN")
		(sheetfile "USB.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.0625 0 90)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 21 "Net-(L1-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.0625 0 90)
			(size 0.875 1.2)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "/DCDC/5V")
			(pinfunction "2")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 132.75 85 -90)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D3"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "LED_SMD:LED_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "2V5"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "uC")
		(sheetfile "UC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "GND")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "Net-(D3-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "W_PROG_Footprints:TC2030_6Pin_Hooked"
		(layer "F.Cu")
		(at 116.25 86.75)
		(property "Reference" "U2"
			(at 0 -5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "~"
			(at 0 5 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" "W_PROG_Footprints:TC2030_6Pin_Hooked"
			(at 0 -4.5 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 -4.5 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 -4.5 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "uC")
		(sheetfile "UC.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 6.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -2.54 -2.54)
			(size 0.8 0.8)
			(drill 2.375)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -2.54 0)
			(size 0.8 0.8)
			(drill 1)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -2.54 2.54)
			(size 0.8 0.8)
			(drill 2.375)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0.635 -2.54)
			(size 0.8 0.8)
			(drill 2.375)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 0.635 2.54)
			(size 0.8 0.8)
			(drill 2.375)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2.54 -1.016)
			(size 0.8 0.8)
			(drill 1)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2.54 1.016)
			(size 0.8 0.8)
			(drill 1)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "1" smd circle
			(at -1.27 0.635)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "Net-(U2-UPDI)")
			(pinfunction "UPDI")
			(pintype "input")
		)
		(pad "2" smd circle
			(at -1.27 -0.635)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "/DCDC/5V")
			(pinfunction "VDD")
			(pintype "input")
		)
		(pad "3" smd circle
			(at 0 0.635)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "/uC/RX_D")
			(pinfunction "RX_Target")
			(pintype "input")
		)
		(pad "4" smd circle
			(at 0 -0.635)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "/uC/!RES")
			(pinfunction "!Reset")
			(pintype "input")
		)
		(pad "5" smd circle
			(at 1.27 0.635)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "/uC/TX_D")
			(pinfunction "TX_Target")
			(pintype "input")
		)
		(pad "6" smd circle
			(at 1.27 -0.635)
			(size 0.8 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "GND")
			(pinfunction "GND")
			(pintype "input")
		)
	)
	(gr_rect
		(start 90 78.5)
		(end 160 108.5)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_text "USB-SPI Interface\nYUKARI V1\n2025 hackaday.io/voltweasel"
		(at 148.25 94.5 0)
		(layer "B.SilkS")
	)
	(gr_text "EN"
		(at 122.25 83 270)
		(layer "F.SilkS")
	)
	(gr_text "FAIL"
		(at 139.75 106.75 270)
		(layer "F.SilkS")
	)
	(gr_text "2,5"
		(at 132.75 83.515 270)
		(layer "F.SilkS")
	)
	(gr_text "1,8"
		(at 129.25 83.515 270)
		(layer "F.SilkS")
	)
	(gr_text "3,3"
		(at 136.25 83.515 270)
		(layer "F.SilkS")
	)
	(gr_text "1,2"
		(at 125.75 83.515 270)
		(layer "F.SilkS")
	)
	(gr_text "5,0"
		(at 139.75 83.515 270)
		(layer "F.SilkS")
	)
	(gr_text "BUSY"
		(at 136.25 108 270)
		(layer "F.SilkS")
	)
	(zone
		(net 1)
		(net_name "GND")
		(layers "F&B.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.25)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.25)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 160 78.5) (xy 160 108.5) (xy 90 108.5) (xy 90 78.5)
			)
		)
	)
)
