(kicad_sch (version 20230121) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "MCU_Module:Arduino_Nano_v3.x" (in_bom yes) (on_board yes)
      (property "Reference" "A" (at -10.16 23.495 0))
      (property "Value" "Arduino_Nano_v3.x" (at 5.08 -24.13 0))
      (property "Footprint" "Module:Arduino_Nano" (at 0 0 0))
      (property "Datasheet" "http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf" (at 0 0 0))
      (property "ki_keywords" "Arduino nano microcontroller module USB" (at 0 0 0))
      (property "ki_description" "Arduino Nano v3.x" (at 0 0 0))
      (property "ki_fp_filters" "Arduino*Nano*" (at 0 0 0))
      (symbol "Arduino_Nano_v3.x_0_1"
        (rectangle (start -10.16 22.86) (end 10.16 -22.86)
          (fill (type background))
        )
      )
      (symbol "Arduino_Nano_v3.x_1_1"
        (pin bidirectional line (at -12.7 12.7 0) (length 2.54)
          (name "D1/TX")
          (number "1")
        )
        (pin bidirectional line (at -12.7 -2.54 0) (length 2.54)
          (name "D7")
          (number "10")
        )
        (pin bidirectional line (at -12.7 -5.08 0) (length 2.54)
          (name "D8")
          (number "11")
        )
        (pin bidirectional line (at -12.7 -7.62 0) (length 2.54)
          (name "D9")
          (number "12")
        )
        (pin bidirectional line (at -12.7 -10.16 0) (length 2.54)
          (name "D10")
          (number "13")
        )
        (pin bidirectional line (at -12.7 -12.7 0) (length 2.54)
          (name "D11")
          (number "14")
        )
        (pin bidirectional line (at -12.7 -15.24 0) (length 2.54)
          (name "D12")
          (number "15")
        )
        (pin bidirectional line (at -12.7 -17.78 0) (length 2.54)
          (name "D13")
          (number "16")
        )
        (pin power_out line (at 2.54 25.4 270) (length 2.54)
          (name "3V3")
          (number "17")
        )
        (pin input line (at 12.7 5.08 180) (length 2.54)
          (name "AREF")
          (number "18")
        )
        (pin bidirectional line (at 12.7 0 180) (length 2.54)
          (name "A0")
          (number "19")
        )
        (pin bidirectional line (at -12.7 15.24 0) (length 2.54)
          (name "D0/RX")
          (number "2")
        )
        (pin bidirectional line (at 12.7 -2.54 180) (length 2.54)
          (name "A1")
          (number "20")
        )
        (pin bidirectional line (at 12.7 -5.08 180) (length 2.54)
          (name "A2")
          (number "21")
        )
        (pin bidirectional line (at 12.7 -7.62 180) (length 2.54)
          (name "A3")
          (number "22")
        )
        (pin bidirectional line (at 12.7 -10.16 180) (length 2.54)
          (name "A4")
          (number "23")
        )
        (pin bidirectional line (at 12.7 -12.7 180) (length 2.54)
          (name "A5")
          (number "24")
        )
        (pin bidirectional line (at 12.7 -15.24 180) (length 2.54)
          (name "A6")
          (number "25")
        )
        (pin bidirectional line (at 12.7 -17.78 180) (length 2.54)
          (name "A7")
          (number "26")
        )
        (pin power_out line (at 5.08 25.4 270) (length 2.54)
          (name "+5V")
          (number "27")
        )
        (pin input line (at 12.7 15.24 180) (length 2.54)
          (name "~{RESET}")
          (number "28")
        )
        (pin power_in line (at 2.54 -25.4 90) (length 2.54)
          (name "GND")
          (number "29")
        )
        (pin input line (at 12.7 12.7 180) (length 2.54)
          (name "~{RESET}")
          (number "3")
        )
        (pin power_in line (at -2.54 25.4 270) (length 2.54)
          (name "VIN")
          (number "30")
        )
        (pin power_in line (at 0 -25.4 90) (length 2.54)
          (name "GND")
          (number "4")
        )
        (pin bidirectional line (at -12.7 10.16 0) (length 2.54)
          (name "D2")
          (number "5")
        )
        (pin bidirectional line (at -12.7 7.62 0) (length 2.54)
          (name "D3")
          (number "6")
        )
        (pin bidirectional line (at -12.7 5.08 0) (length 2.54)
          (name "D4")
          (number "7")
        )
        (pin bidirectional line (at -12.7 2.54 0) (length 2.54)
          (name "D5")
          (number "8")
        )
        (pin bidirectional line (at -12.7 0 0) (length 2.54)
          (name "D6")
          (number "9")
        )
      )
    )
    (symbol "Motor:Motor_Servo" (pin_names (offset 0.0254)) (in_bom yes) (on_board yes)
      (property "Reference" "M" (at -5.08 4.445 0))
      (property "Value" "Motor_Servo" (at -5.08 -4.064 0))
      (property "Footprint" "" (at 0 -4.826 0))
      (property "Datasheet" "http://forums.parallax.com/uploads/attachments/46831/74481.png" (at 0 -4.826 0))
      (property "ki_keywords" "Servo Motor" (at 0 0 0))
      (property "ki_description" "Servo Motor (Futaba, HiTec, JR connector)" (at 0 0 0))
      (property "ki_fp_filters" "PinHeader*P2.54mm*" (at 0 0 0))
      (symbol "Motor_Servo_0_1"
        (polyline
          (pts
            (xy 2.413 -1.778)
            (xy 2.032 -1.778)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.413 -1.778)
            (xy 2.286 -1.397)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.413 1.778)
            (xy 1.905 1.778)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.413 1.778)
            (xy 2.286 1.397)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 6.35 4.445)
            (xy 2.54 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 7.62 3.175)
            (xy 4.191 -1.016)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 5.08 3.556)
            (xy -5.08 3.556)
            (xy -5.08 -3.556)
            (xy 6.35 -3.556)
            (xy 6.35 1.524)
          )
          (fill (type none))
        )
        (arc (start 2.413 1.778) (mid 1.2406 0) (end 2.413 -1.778)
          (fill (type none))
        )
        (circle (center 3.175 0) (radius 0.1778)
          (fill (type none))
        )
        (circle (center 3.175 0) (radius 1.4224)
          (fill (type none))
        )
        (circle (center 5.969 2.794) (radius 0.127)
          (fill (type none))
        )
        (circle (center 6.477 3.302) (radius 0.127)
          (fill (type none))
        )
        (circle (center 6.985 3.81) (radius 0.127)
          (fill (type none))
        )
        (arc (start 7.62 3.175) (mid 7.4485 4.2735) (end 6.35 4.445)
          (fill (type none))
        )
      )
      (symbol "Motor_Servo_1_1"
        (pin passive line (at -7.62 2.54 0) (length 2.54)
          (name "PWM")
          (number "1")
        )
        (pin passive line (at -7.62 0 0) (length 2.54)
          (name "+")
          (number "2")
        )
        (pin passive line (at -7.62 -2.54 0) (length 2.54)
          (name "-")
          (number "3")
        )
      )
    )
    (symbol "custom:ESC" (in_bom yes) (on_board yes)
      (property "Reference" "ESC" (at 2.54 0 0))
      (property "Value" "" (at 0 0 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (symbol "ESC_0_1"
        (rectangle (start -10.16 5.08) (end 10.16 -5.08)
          (fill (type none))
        )
      )
      (symbol "ESC_1_1"
        (pin input line (at -2.54 -7.62 90) (length 2.54)
          (name "GND")
          (number "")
        )
        (pin output line (at 12.7 2.54 180) (length 2.54)
          (name "Out1")
          (number "")
        )
        (pin output line (at 12.7 0 180) (length 2.54)
          (name "Out2")
          (number "")
        )
        (pin output line (at 12.7 -2.54 180) (length 2.54)
          (name "Out3")
          (number "")
        )
        (pin input line (at -2.54 7.62 270) (length 2.54)
          (name "VCC")
          (number "")
        )
        (pin input line (at -12.7 2.54 0) (length 2.54)
          (name "Data")
          (number "1")
        )
        (pin input line (at -12.7 0 0) (length 2.54)
          (name "+5V")
          (number "2")
        )
        (pin input line (at -12.7 -2.54 0) (length 2.54)
          (name "GND")
          (number "3")
        )
      )
    )
    (symbol "custom:GPS_NEO-7M" (in_bom yes) (on_board yes)
      (property "Reference" "GPS" (at 0 0 0))
      (property "Value" "" (at 0 0 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (symbol "GPS_NEO-7M_0_1"
        (rectangle (start -6.35 5.08) (end 6.35 -5.08)
          (fill (type none))
        )
      )
      (symbol "GPS_NEO-7M_1_1"
        (pin input line (at -8.89 -2.54 0) (length 2.54)
          (name "GND")
          (number "1")
        )
        (pin output line (at 8.89 2.54 180) (length 2.54)
          (name "TX")
          (number "2")
        )
        (pin input line (at 8.89 -2.54 180) (length 2.54)
          (name "RX")
          (number "3")
        )
        (pin input line (at -8.89 2.54 0) (length 2.54)
          (name "+3.3V")
          (number "4")
        )
      )
    )
    (symbol "custom:GY-271_compass" (in_bom yes) (on_board yes)
      (property "Reference" "U" (at 0 0 0))
      (property "Value" "" (at 0 0 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (symbol "GY-271_compass_0_1"
        (rectangle (start -6.35 6.35) (end 6.35 -6.35)
          (fill (type none))
        )
      )
      (symbol "GY-271_compass_1_1"
        (pin input line (at -8.89 5.08 0) (length 2.54)
          (name "VCC")
          (number "1")
        )
        (pin input line (at -8.89 2.54 0) (length 2.54)
          (name "GND")
          (number "2")
        )
        (pin input line (at -8.89 0 0) (length 2.54)
          (name "SCL")
          (number "3")
        )
        (pin output line (at -8.89 -2.54 0) (length 2.54)
          (name "SDA")
          (number "4")
        )
        (pin output line (at -8.89 -5.08 0) (length 2.54)
          (name "DRDY")
          (number "5")
        )
      )
    )
    (symbol "custom:Pressure_Sensor" (in_bom yes) (on_board yes)
      (property "Reference" "PressureSensor" (at 0 -2.54 0))
      (property "Value" "" (at 0 0 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (symbol "Pressure_Sensor_0_1"
        (rectangle (start -7.62 2.54) (end 7.62 -7.62)
          (fill (type none))
        )
      )
      (symbol "Pressure_Sensor_1_1"
        (pin output line (at 10.16 -5.08 180) (length 2.54)
          (name "Data")
          (number "1")
        )
        (pin input line (at -10.16 0 0) (length 2.54)
          (name "+5v")
          (number "2")
        )
        (pin input line (at -10.16 -5.08 0) (length 2.54)
          (name "GND")
          (number "3")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (at 0 -6.35 0))
      (property "Value" "GND" (at 0 -3.81 0))
      (property "Footprint" "" (at 0 0 0))
      (property "Datasheet" "" (at 0 0 0))
      (property "ki_keywords" "global power" (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
  )
  (no_connect (at 76.2 71.12))
  (no_connect (at 93.98 48.26))
  (no_connect (at 76.2 81.28))
  (no_connect (at 76.2 91.44))
  (no_connect (at 76.2 88.9))
  (no_connect (at 76.2 83.82))
  (no_connect (at 101.6 68.58))
  (no_connect (at 101.6 88.9))
  (no_connect (at 76.2 73.66))
  (no_connect (at 101.6 78.74))
  (no_connect (at 101.6 91.44))
  (no_connect (at 76.2 76.2))
  (no_connect (at 101.6 86.36))
  (no_connect (at 76.2 78.74))
  (no_connect (at 134.62 86.36))
  (no_connect (at 149.86 93.98))
  (no_connect (at 163.83 81.28))
  (no_connect (at 101.6 60.96))
  (no_connect (at 76.2 86.36))
  (no_connect (at 149.86 96.52))
  (no_connect (at 101.6 58.42))
  (no_connect (at 149.86 91.44))
  (wire (pts (xy 111.76 110.49) (xy 111.76 76.2)))
  (wire (pts (xy 118.11 76.2) (xy 118.11 81.28)))
  (wire (pts (xy 54.61 86.36) (xy 54.61 110.49)))
  (wire (pts (xy 60.96 58.42) (xy 76.2 58.42)))
  (wire (pts (xy 163.83 78.74) (xy 121.92 78.74)))
  (wire (pts (xy 111.76 76.2) (xy 101.6 76.2)))
  (wire (pts (xy 72.39 63.5) (xy 76.2 63.5)))
  (wire (pts (xy 114.3 106.68) (xy 72.39 106.68)))
  (wire (pts (xy 91.44 44.45) (xy 36.83 44.45)))
  (wire (pts (xy 91.44 48.26) (xy 91.44 44.45)))
  (wire (pts (xy 125.73 29.21) (xy 137.16 29.21)))
  (wire (pts (xy 114.3 91.44) (xy 114.3 106.68)))
  (wire (pts (xy 54.61 110.49) (xy 111.76 110.49)))
  (wire (pts (xy 124.46 91.44) (xy 114.3 91.44)))
  (wire (pts (xy 72.39 106.68) (xy 72.39 68.58)))
  (wire (pts (xy 101.6 29.21) (xy 72.39 29.21)))
  (wire (pts (xy 36.83 44.45) (xy 36.83 55.88)))
  (wire (pts (xy 54.61 60.96) (xy 76.2 60.96)))
  (wire (pts (xy 72.39 68.58) (xy 76.2 68.58)))
  (wire (pts (xy 121.92 83.82) (xy 101.6 83.82)))
  (wire (pts (xy 153.67 73.66) (xy 101.6 73.66)))
  (wire (pts (xy 54.61 55.88) (xy 60.96 55.88)))
  (wire (pts (xy 163.83 76.2) (xy 118.11 76.2)))
  (wire (pts (xy 118.11 81.28) (xy 101.6 81.28)))
  (wire (pts (xy 69.85 66.04) (xy 69.85 25.4)))
  (wire (pts (xy 76.2 66.04) (xy 69.85 66.04)))
  (wire (pts (xy 125.73 25.4) (xy 125.73 29.21)))
  (wire (pts (xy 69.85 25.4) (xy 125.73 25.4)))
  (wire (pts (xy 72.39 29.21) (xy 72.39 63.5)))
  (wire (pts (xy 121.92 78.74) (xy 121.92 83.82)))
  (wire (pts (xy 153.67 60.96) (xy 153.67 73.66)))
  (wire (pts (xy 60.96 55.88) (xy 60.96 58.42)))
  (global_label "+5V" (shape input) (at 137.16 31.75 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 130.3043 31.75 0))
  )
  (global_label "+5V" (shape input) (at 124.46 93.98 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 117.6043 93.98 0))
  )
  (global_label "+5V" (shape input) (at 101.6 31.75 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 94.7443 31.75 0))
  )
  (global_label "+5V" (shape input) (at 133.35 55.88 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 126.4943 55.88 0))
  )
  (global_label "+5V" (shape input) (at 34.29 81.28 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 27.4343 81.28 0))
  )
  (global_label "+5V" (shape input) (at 86.36 48.26 90) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 86.36 41.4043 90))
  )
  (global_label "+5V" (shape input) (at 163.83 71.12 180) (fields_autoplaced)
    (property "Intersheetrefs" "${INTERSHEET_REFS}" (at 156.9743 71.12 0))
  )
  (symbol (lib_id "custom:ESC") (at 137.16 93.98 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "ESC1" (at 136.8141 86.36 0))
    (property "Value" "~" (at 137.16 93.98 0))
    (property "Footprint" "custom:ESC" (at 137.16 93.98 0))
    (property "Datasheet" "" (at 137.16 93.98 0))
    (pin "3")
    (pin "")
    (pin "1")
    (pin "")
    (pin "")
    (pin "")
    (pin "")
    (pin "2")
    (instances
      (project "schematic"
        (path
          (reference "ESC1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Motor:Motor_Servo") (at 109.22 31.75 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "M1" (at 118.11 30.0466 0))
    (property "Value" "Ballast" (at 118.11 32.5866 0))
    (property "Footprint" "custom:ESC" (at 109.22 36.576 0))
    (property "Datasheet" "http://forums.parallax.com/uploads/attachments/46831/74481.png" (at 109.22 36.576 0))
    (pin "2")
    (pin "1")
    (pin "3")
    (instances
      (project "schematic"
        (path
          (reference "M1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 34.29 86.36 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR09" (at 34.29 92.71 0))
    (property "Value" "GND" (at 34.29 91.44 0))
    (property "Footprint" "" (at 34.29 86.36 0))
    (property "Datasheet" "" (at 34.29 86.36 0))
    (pin "1")
    (instances
      (project "schematic"
        (path
          (reference "#PWR09") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 137.16 34.29 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR07" (at 137.16 40.64 0))
    (property "Value" "GND" (at 137.16 39.37 0))
    (property "Footprint" "" (at 137.16 34.29 0))
    (property "Datasheet" "" (at 137.16 34.29 0))
    (pin "1")
    (instances
      (project "schematic"
        (path
          (reference "#PWR07") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 134.62 101.6 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR04" (at 134.62 107.95 0))
    (property "Value" "GND" (at 134.62 106.68 0))
    (property "Footprint" "" (at 134.62 101.6 0))
    (property "Datasheet" "" (at 134.62 101.6 0))
    (pin "1")
    (instances
      (project "schematic"
        (path
          (reference "#PWR04") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 88.9 99.06 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR01" (at 88.9 105.41 0))
    (property "Value" "GND" (at 88.9 104.14 0))
    (property "Footprint" "" (at 88.9 99.06 0))
    (property "Datasheet" "" (at 88.9 99.06 0))
    (pin "1")
    (instances
      (project "schematic"
        (path
          (reference "#PWR01") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 91.44 99.06 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR08" (at 91.44 105.41 0))
    (property "Value" "GND" (at 91.44 104.14 0))
    (property "Footprint" "" (at 91.44 99.06 0))
    (property "Datasheet" "" (at 91.44 99.06 0))
    (pin "1")
    (instances
      (project "schematic"
        (path
          (reference "#PWR08") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "MCU_Module:Arduino_Nano_v3.x") (at 88.9 73.66 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "A1" (at 93.6341 99.06 0))
    (property "Value" "Arduino_Nano_v3.x" (at 93.6341 101.6 0))
    (property "Footprint" "Module:Arduino_Nano" (at 88.9 73.66 0))
    (property "Datasheet" "http://www.mouser.com/pdfdocs/Gravitech_Arduino_Nano3_0.pdf" (at 88.9 73.66 0))
    (pin "17")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "5")
    (pin "22")
    (pin "11")
    (pin "12")
    (pin "7")
    (pin "8")
    (pin "14")
    (pin "6")
    (pin "27")
    (pin "3")
    (pin "21")
    (pin "20")
    (pin "2")
    (pin "15")
    (pin "19")
    (pin "18")
    (pin "4")
    (pin "26")
    (pin "30")
    (pin "29")
    (pin "28")
    (pin "13")
    (pin "9")
    (pin "10")
    (pin "1")
    (pin "16")
    (instances
      (project "schematic"
        (path
          (reference "A1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 101.6 34.29 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR06" (at 101.6 40.64 0))
    (property "Value" "GND" (at 101.6 39.37 0))
    (property "Footprint" "" (at 101.6 34.29 0))
    (property "Datasheet" "" (at 101.6 34.29 0))
    (pin "1")
    (instances
      (project "schematic"
        (path
          (reference "#PWR06") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "custom:Pressure_Sensor") (at 143.51 55.88 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "PressureSensor1" (at 143.51 50.8 0))
    (property "Value" "~" (at 143.51 55.88 0))
    (property "Footprint" "custom:ESC" (at 143.51 55.88 0))
    (property "Datasheet" "" (at 143.51 55.88 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (instances
      (project "schematic"
        (path
          (reference "PressureSensor1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 124.46 96.52 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR02" (at 124.46 102.87 0))
    (property "Value" "GND" (at 124.46 101.6 0))
    (property "Footprint" "" (at 124.46 96.52 0))
    (property "Datasheet" "" (at 124.46 96.52 0))
    (pin "1")
    (instances
      (project "schematic"
        (path
          (reference "#PWR02") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 133.35 60.96 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR03" (at 133.35 67.31 0))
    (property "Value" "GND" (at 133.35 66.04 0))
    (property "Footprint" "" (at 133.35 60.96 0))
    (property "Datasheet" "" (at 133.35 60.96 0))
    (pin "1")
    (instances
      (project "schematic"
        (path
          (reference "#PWR03") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "Motor:Motor_Servo") (at 144.78 31.75 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "M2" (at 153.67 30.0466 0))
    (property "Value" "Rudder" (at 153.67 32.5866 0))
    (property "Footprint" "custom:ESC" (at 144.78 36.576 0))
    (property "Datasheet" "http://forums.parallax.com/uploads/attachments/46831/74481.png" (at 144.78 36.576 0))
    (pin "2")
    (pin "1")
    (pin "3")
    (instances
      (project "schematic"
        (path
          (reference "M2") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "custom:GPS_NEO-7M") (at 45.72 58.42 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "GPS1" (at 45.72 50.8 0))
    (property "Value" "~" (at 45.72 58.42 0))
    (property "Footprint" "custom:GPS" (at 45.72 58.42 0))
    (property "Datasheet" "" (at 45.72 58.42 0))
    (pin "1")
    (pin "3")
    (pin "2")
    (pin "4")
    (instances
      (project "schematic"
        (path
          (reference "GPS1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 36.83 60.96 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR05" (at 36.83 67.31 0))
    (property "Value" "GND" (at 36.83 66.04 0))
    (property "Footprint" "" (at 36.83 60.96 0))
    (property "Datasheet" "" (at 36.83 60.96 0))
    (pin "1")
    (instances
      (project "schematic"
        (path
          (reference "#PWR05") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "power:GND") (at 163.83 73.66 270) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "#PWR010" (at 157.48 73.66 0))
    (property "Value" "GND" (at 160.02 73.66 90))
    (property "Footprint" "" (at 163.83 73.66 0))
    (property "Datasheet" "" (at 163.83 73.66 0))
    (pin "1")
    (instances
      (project "schematic"
        (path
          (reference "#PWR010") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "custom:GY-271_compass") (at 172.72 76.2 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "U1" (at 180.34 76.2 0))
    (property "Value" "~" (at 172.72 76.2 0))
    (property "Footprint" "custom:compass" (at 172.72 76.2 0))
    (property "Datasheet" "" (at 172.72 76.2 0))
    (pin "1")
    (pin "4")
    (pin "2")
    (pin "3")
    (pin "5")
    (instances
      (project "schematic"
        (path
          (reference "U1") (unit 1)
        )
      )
    )
  )
  (symbol (lib_id "custom:Pressure_Sensor") (at 44.45 81.28 0) (unit 1)
    (in_bom yes) (on_board yes) (dnp no) (fields_autoplaced)
    (property "Reference" "Transducer1" (at 44.45 76.2 0))
    (property "Value" "~" (at 44.45 81.28 0))
    (property "Footprint" "custom:ESC" (at 44.45 81.28 0))
    (property "Datasheet" "" (at 44.45 81.28 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (instances
      (project "schematic"
        (path
          (reference "Transducer1") (unit 1)
        )
      )
    )
  )
  (sheet_instances
    (path (page "1"))
  )
)
