(kicad_sch (version 20211123) (generator eeschema)
  (paper "A4")
  (lib_symbols
    (symbol "74xx:74HC14" (pin_names (offset 1.016)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 0 1.27 0))
      (property "Value" "74HC14" (id 1) (at 0 -1.27 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "http://www.ti.com/lit/gpn/sn74HC14" (id 3) (at 0 0 0))
      (property "ki_locked" "" (id 4) (at 0 0 0))
      (property "ki_keywords" "HCMOS not inverter" (id 5) (at 0 0 0))
      (property "ki_description" "Hex inverter schmitt trigger" (id 6) (at 0 0 0))
      (property "ki_fp_filters" "DIP*W7.62mm*" (id 7) (at 0 0 0))
      (symbol "74HC14_1_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "1")
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "2")
        )
      )
      (symbol "74HC14_1_1"
        (polyline
          (pts
            (xy -1.905 -1.27)
            (xy -1.905 1.27)
            (xy -0.635 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -1.27)
            (xy -0.635 -1.27)
            (xy -0.635 1.27)
            (xy 0 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "74HC14_2_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "3")
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "4")
        )
      )
      (symbol "74HC14_2_1"
        (polyline
          (pts
            (xy -1.905 -1.27)
            (xy -1.905 1.27)
            (xy -0.635 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -1.27)
            (xy -0.635 -1.27)
            (xy -0.635 1.27)
            (xy 0 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "74HC14_3_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "5")
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "6")
        )
      )
      (symbol "74HC14_3_1"
        (polyline
          (pts
            (xy -1.905 -1.27)
            (xy -1.905 1.27)
            (xy -0.635 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -1.27)
            (xy -0.635 -1.27)
            (xy -0.635 1.27)
            (xy 0 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "74HC14_4_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "8")
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "9")
        )
      )
      (symbol "74HC14_4_1"
        (polyline
          (pts
            (xy -1.905 -1.27)
            (xy -1.905 1.27)
            (xy -0.635 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -1.27)
            (xy -0.635 -1.27)
            (xy -0.635 1.27)
            (xy 0 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "74HC14_5_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "10")
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "11")
        )
      )
      (symbol "74HC14_5_1"
        (polyline
          (pts
            (xy -1.905 -1.27)
            (xy -1.905 1.27)
            (xy -0.635 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -1.27)
            (xy -0.635 -1.27)
            (xy -0.635 1.27)
            (xy 0 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "74HC14_6_0"
        (polyline
          (pts
            (xy -3.81 3.81)
            (xy -3.81 -3.81)
            (xy 3.81 0)
            (xy -3.81 3.81)
          )
          (fill (type background))
        )
        (pin output inverted (at 7.62 0 180) (length 3.81)
          (name "~")
          (number "12")
        )
        (pin input line (at -7.62 0 0) (length 3.81)
          (name "~")
          (number "13")
        )
      )
      (symbol "74HC14_6_1"
        (polyline
          (pts
            (xy -1.905 -1.27)
            (xy -1.905 1.27)
            (xy -0.635 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.54 -1.27)
            (xy -0.635 -1.27)
            (xy -0.635 1.27)
            (xy 0 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "74HC14_7_0"
        (pin power_in line (at 0 12.7 270) (length 5.08)
          (name "VCC")
          (number "14")
        )
        (pin power_in line (at 0 -12.7 90) (length 5.08)
          (name "GND")
          (number "7")
        )
      )
      (symbol "74HC14_7_1"
        (rectangle (start -5.08 7.62) (end 5.08 -7.62)
          (fill (type background))
        )
      )
    )
    (symbol "Amplifier_Operational:MCP6002-xP" (pin_names (offset 0.127)) (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at 0 5.08 0))
      (property "Value" "MCP6002-xP" (id 1) (at 0 -5.08 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21733j.pdf" (id 3) (at 0 0 0))
      (property "ki_locked" "" (id 4) (at 0 0 0))
      (property "ki_keywords" "dual opamp" (id 5) (at 0 0 0))
      (property "ki_description" "1MHz, Low-Power Op Amp, DIP-8" (id 6) (at 0 0 0))
      (property "ki_fp_filters" "SOIC*3.9x4.9mm*P1.27mm* DIP*W7.62mm* TO*99* OnSemi*Micro8* TSSOP*3x3mm*P0.65mm* TSSOP*4.4x3mm*P0.65mm* MSOP*3x3mm*P0.65mm* SSOP*3.9x4.9mm*P0.635mm* LFCSP*2x2mm*P0.5mm* *SIP* SOIC*5.3x6.2mm*P1.27mm*" (id 7) (at 0 0 0))
      (symbol "MCP6002-xP_1_1"
        (polyline
          (pts
            (xy -5.08 5.08)
            (xy 5.08 0)
            (xy -5.08 -5.08)
            (xy -5.08 5.08)
          )
          (fill (type background))
        )
        (pin output line (at 7.62 0 180) (length 2.54)
          (name "~")
          (number "1")
        )
        (pin input line (at -7.62 -2.54 0) (length 2.54)
          (name "-")
          (number "2")
        )
        (pin input line (at -7.62 2.54 0) (length 2.54)
          (name "+")
          (number "3")
        )
      )
      (symbol "MCP6002-xP_2_1"
        (polyline
          (pts
            (xy -5.08 5.08)
            (xy 5.08 0)
            (xy -5.08 -5.08)
            (xy -5.08 5.08)
          )
          (fill (type background))
        )
        (pin input line (at -7.62 2.54 0) (length 2.54)
          (name "+")
          (number "5")
        )
        (pin input line (at -7.62 -2.54 0) (length 2.54)
          (name "-")
          (number "6")
        )
        (pin output line (at 7.62 0 180) (length 2.54)
          (name "~")
          (number "7")
        )
      )
      (symbol "MCP6002-xP_3_1"
        (pin power_in line (at -2.54 -7.62 90) (length 3.81)
          (name "V-")
          (number "4")
        )
        (pin power_in line (at -2.54 7.62 270) (length 3.81)
          (name "V+")
          (number "8")
        )
      )
    )
    (symbol "Device:C" (pin_numbers hide) (pin_names (offset 0.254)) (in_bom yes) (on_board yes)
      (property "Reference" "C" (id 0) (at 0.635 2.54 0))
      (property "Value" "C" (id 1) (at 0.635 -2.54 0))
      (property "Footprint" "" (id 2) (at 0.9652 -3.81 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "cap capacitor" (id 4) (at 0 0 0))
      (property "ki_description" "Unpolarized capacitor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "C_*" (id 6) (at 0 0 0))
      (symbol "C_0_1"
        (polyline
          (pts
            (xy -2.032 -0.762)
            (xy 2.032 -0.762)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -2.032 0.762)
            (xy 2.032 0.762)
          )
          (fill (type none))
        )
      )
      (symbol "C_1_1"
        (pin passive line (at 0 3.81 270) (length 2.794)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 2.794)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:LED" (pin_numbers hide) (pin_names (offset 1.016) hide) (in_bom yes) (on_board yes)
      (property "Reference" "D" (id 0) (at 0 2.54 0))
      (property "Value" "LED" (id 1) (at 0 -2.54 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "LED diode" (id 4) (at 0 0 0))
      (property "ki_description" "Light emitting diode" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "LED* LED_SMD:* LED_THT:*" (id 6) (at 0 0 0))
      (symbol "LED_0_1"
        (polyline
          (pts
            (xy -1.27 -1.27)
            (xy -1.27 1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.27 0)
            (xy 1.27 0)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 1.27 -1.27)
            (xy 1.27 1.27)
            (xy -1.27 0)
            (xy 1.27 -1.27)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -3.048 -0.762)
            (xy -4.572 -2.286)
            (xy -3.81 -2.286)
            (xy -4.572 -2.286)
            (xy -4.572 -1.524)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy -1.778 -0.762)
            (xy -3.302 -2.286)
            (xy -2.54 -2.286)
            (xy -3.302 -2.286)
            (xy -3.302 -1.524)
          )
          (fill (type none))
        )
      )
      (symbol "LED_1_1"
        (pin passive line (at -3.81 0 0) (length 2.54)
          (name "K")
          (number "1")
        )
        (pin passive line (at 3.81 0 180) (length 2.54)
          (name "A")
          (number "2")
        )
      )
    )
    (symbol "Device:R" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 2.032 0 90))
      (property "Value" "R" (id 1) (at 0 0 90))
      (property "Footprint" "" (id 2) (at -1.778 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R res resistor" (id 4) (at 0 0 0))
      (property "ki_description" "Resistor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
      )
      (symbol "R_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "Device:R_Variable" (pin_numbers hide) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "R" (id 0) (at 2.54 -2.54 90))
      (property "Value" "R_Variable" (id 1) (at -2.54 -1.27 90))
      (property "Footprint" "" (id 2) (at -1.778 0 90))
      (property "Datasheet" "~" (id 3) (at 0 0 0))
      (property "ki_keywords" "R res resistor variable potentiometer rheostat" (id 4) (at 0 0 0))
      (property "ki_description" "Variable resistor" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "R_*" (id 6) (at 0 0 0))
      (symbol "R_Variable_0_1"
        (rectangle (start -1.016 -2.54) (end 1.016 2.54)
          (fill (type none))
        )
        (polyline
          (pts
            (xy 2.54 1.524)
            (xy 2.54 2.54)
            (xy 1.524 2.54)
            (xy 2.54 2.54)
            (xy -2.032 -2.032)
          )
          (fill (type none))
        )
      )
      (symbol "R_Variable_1_1"
        (pin passive line (at 0 3.81 270) (length 1.27)
          (name "~")
          (number "1")
        )
        (pin passive line (at 0 -3.81 90) (length 1.27)
          (name "~")
          (number "2")
        )
      )
    )
    (symbol "MCU_ST_STM32F4:STM32F411CEUx" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -15.24 36.83 0))
      (property "Value" "STM32F411CEUx" (id 1) (at 7.62 36.83 0))
      (property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm" (id 2) (at -15.24 -38.1 0))
      (property "Datasheet" "http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/DM00115249.pdf" (id 3) (at 0 0 0))
      (property "ki_keywords" "ARM Cortex-M4 STM32F4 STM32F411" (id 4) (at 0 0 0))
      (property "ki_description" "ARM Cortex-M4 MCU, 512KB flash, 128KB RAM, 100MHz, 1.7-3.6V, 36 GPIO, UFQFPN-48" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "QFN*1EP*7x7mm*P0.5mm*" (id 6) (at 0 0 0))
      (symbol "STM32F411CEUx_0_1"
        (rectangle (start -15.24 -38.1) (end 12.7 35.56)
          (fill (type background))
        )
      )
      (symbol "STM32F411CEUx_1_1"
        (pin power_in line (at -5.08 38.1 270) (length 2.54)
          (name "VBAT")
          (number "1")
        )
        (pin bidirectional line (at 15.24 2.54 180) (length 2.54)
          (name "PA0")
          (number "10")
        )
        (pin bidirectional line (at 15.24 0 180) (length 2.54)
          (name "PA1")
          (number "11")
        )
        (pin bidirectional line (at 15.24 -2.54 180) (length 2.54)
          (name "PA2")
          (number "12")
        )
        (pin bidirectional line (at 15.24 -5.08 180) (length 2.54)
          (name "PA3")
          (number "13")
        )
        (pin bidirectional line (at 15.24 -7.62 180) (length 2.54)
          (name "PA4")
          (number "14")
        )
        (pin bidirectional line (at 15.24 -10.16 180) (length 2.54)
          (name "PA5")
          (number "15")
        )
        (pin bidirectional line (at 15.24 -12.7 180) (length 2.54)
          (name "PA6")
          (number "16")
        )
        (pin bidirectional line (at 15.24 -15.24 180) (length 2.54)
          (name "PA7")
          (number "17")
        )
        (pin bidirectional line (at -17.78 0 0) (length 2.54)
          (name "PB0")
          (number "18")
        )
        (pin bidirectional line (at -17.78 -2.54 0) (length 2.54)
          (name "PB1")
          (number "19")
        )
        (pin bidirectional line (at -17.78 10.16 0) (length 2.54)
          (name "PC13")
          (number "2")
        )
        (pin bidirectional line (at -17.78 -5.08 0) (length 2.54)
          (name "PB2")
          (number "20")
        )
        (pin bidirectional line (at -17.78 -25.4 0) (length 2.54)
          (name "PB10")
          (number "21")
        )
        (pin power_in line (at -17.78 22.86 0) (length 2.54)
          (name "VCAP1")
          (number "22")
        )
        (pin power_in line (at -5.08 -40.64 90) (length 2.54)
          (name "VSS")
          (number "23")
        )
        (pin power_in line (at -2.54 38.1 270) (length 2.54)
          (name "VDD")
          (number "24")
        )
        (pin bidirectional line (at -17.78 -27.94 0) (length 2.54)
          (name "PB12")
          (number "25")
        )
        (pin bidirectional line (at -17.78 -30.48 0) (length 2.54)
          (name "PB13")
          (number "26")
        )
        (pin bidirectional line (at -17.78 -33.02 0) (length 2.54)
          (name "PB14")
          (number "27")
        )
        (pin bidirectional line (at -17.78 -35.56 0) (length 2.54)
          (name "PB15")
          (number "28")
        )
        (pin bidirectional line (at 15.24 -17.78 180) (length 2.54)
          (name "PA8")
          (number "29")
        )
        (pin bidirectional line (at -17.78 7.62 0) (length 2.54)
          (name "PC14")
          (number "3")
        )
        (pin bidirectional line (at 15.24 -20.32 180) (length 2.54)
          (name "PA9")
          (number "30")
        )
        (pin bidirectional line (at 15.24 -22.86 180) (length 2.54)
          (name "PA10")
          (number "31")
        )
        (pin bidirectional line (at 15.24 -25.4 180) (length 2.54)
          (name "PA11")
          (number "32")
        )
        (pin bidirectional line (at 15.24 -27.94 180) (length 2.54)
          (name "PA12")
          (number "33")
        )
        (pin bidirectional line (at 15.24 -30.48 180) (length 2.54)
          (name "PA13")
          (number "34")
        )
        (pin power_in line (at -2.54 -40.64 90) (length 2.54)
          (name "VSS")
          (number "35")
        )
        (pin power_in line (at 0 38.1 270) (length 2.54)
          (name "VDD")
          (number "36")
        )
        (pin bidirectional line (at 15.24 -33.02 180) (length 2.54)
          (name "PA14")
          (number "37")
        )
        (pin bidirectional line (at 15.24 -35.56 180) (length 2.54)
          (name "PA15")
          (number "38")
        )
        (pin bidirectional line (at -17.78 -7.62 0) (length 2.54)
          (name "PB3")
          (number "39")
        )
        (pin bidirectional line (at -17.78 5.08 0) (length 2.54)
          (name "PC15")
          (number "4")
        )
        (pin bidirectional line (at -17.78 -10.16 0) (length 2.54)
          (name "PB4")
          (number "40")
        )
        (pin bidirectional line (at -17.78 -12.7 0) (length 2.54)
          (name "PB5")
          (number "41")
        )
        (pin bidirectional line (at -17.78 -15.24 0) (length 2.54)
          (name "PB6")
          (number "42")
        )
        (pin bidirectional line (at -17.78 -17.78 0) (length 2.54)
          (name "PB7")
          (number "43")
        )
        (pin input line (at -17.78 27.94 0) (length 2.54)
          (name "BOOT0")
          (number "44")
        )
        (pin bidirectional line (at -17.78 -20.32 0) (length 2.54)
          (name "PB8")
          (number "45")
        )
        (pin bidirectional line (at -17.78 -22.86 0) (length 2.54)
          (name "PB9")
          (number "46")
        )
        (pin power_in line (at 0 -40.64 90) (length 2.54)
          (name "VSS")
          (number "47")
        )
        (pin power_in line (at 2.54 38.1 270) (length 2.54)
          (name "VDD")
          (number "48")
        )
        (pin power_in line (at 2.54 -40.64 90) (length 2.54)
          (name "VSS")
          (number "49")
        )
        (pin input line (at -17.78 17.78 0) (length 2.54)
          (name "PH0")
          (number "5")
        )
        (pin input line (at -17.78 15.24 0) (length 2.54)
          (name "PH1")
          (number "6")
        )
        (pin input line (at -17.78 33.02 0) (length 2.54)
          (name "NRST")
          (number "7")
        )
        (pin power_in line (at 5.08 -40.64 90) (length 2.54)
          (name "VSSA")
          (number "8")
        )
        (pin power_in line (at 5.08 38.1 270) (length 2.54)
          (name "VDDA")
          (number "9")
        )
      )
    )
    (symbol "Timer:NE555P" (in_bom yes) (on_board yes)
      (property "Reference" "U" (id 0) (at -10.16 8.89 0))
      (property "Value" "NE555P" (id 1) (at 2.54 8.89 0))
      (property "Footprint" "Package_DIP:DIP-8_W7.62mm" (id 2) (at 16.51 -10.16 0))
      (property "Datasheet" "http://www.ti.com/lit/ds/symlink/ne555.pdf" (id 3) (at 21.59 -10.16 0))
      (property "ki_keywords" "single timer 555" (id 4) (at 0 0 0))
      (property "ki_description" "Precision Timers, 555 compatible,  PDIP-8" (id 5) (at 0 0 0))
      (property "ki_fp_filters" "DIP*W7.62mm*" (id 6) (at 0 0 0))
      (symbol "NE555P_0_0"
        (pin power_in line (at 0 -10.16 90) (length 2.54)
          (name "GND")
          (number "1")
        )
        (pin power_in line (at 0 10.16 270) (length 2.54)
          (name "VCC")
          (number "8")
        )
      )
      (symbol "NE555P_0_1"
        (rectangle (start -8.89 -7.62) (end 8.89 7.62)
          (fill (type background))
        )
        (rectangle (start -8.89 -7.62) (end 8.89 7.62)
          (fill (type background))
        )
      )
      (symbol "NE555P_1_1"
        (pin input line (at -12.7 5.08 0) (length 3.81)
          (name "TR")
          (number "2")
        )
        (pin output line (at 12.7 5.08 180) (length 3.81)
          (name "Q")
          (number "3")
        )
        (pin input inverted (at -12.7 -5.08 0) (length 3.81)
          (name "R")
          (number "4")
        )
        (pin input line (at -12.7 0 0) (length 3.81)
          (name "CV")
          (number "5")
        )
        (pin input line (at 12.7 -5.08 180) (length 3.81)
          (name "THR")
          (number "6")
        )
        (pin input line (at 12.7 0 180) (length 3.81)
          (name "DIS")
          (number "7")
        )
      )
    )
    (symbol "power:+5V" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -3.81 0))
      (property "Value" "+5V" (id 1) (at 0 3.556 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "global power" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"+5V\"" (id 5) (at 0 0 0))
      (symbol "+5V_0_1"
        (polyline
          (pts
            (xy -0.762 1.27)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 0)
            (xy 0 2.54)
          )
          (fill (type none))
        )
        (polyline
          (pts
            (xy 0 2.54)
            (xy 0.762 1.27)
          )
          (fill (type none))
        )
      )
      (symbol "+5V_1_1"
        (pin power_in line (at 0 0 90) (length 0) hide
          (name "+5V")
          (number "1")
        )
      )
    )
    (symbol "power:GND" (power) (pin_names (offset 0)) (in_bom yes) (on_board yes)
      (property "Reference" "#PWR" (id 0) (at 0 -6.35 0))
      (property "Value" "GND" (id 1) (at 0 -3.81 0))
      (property "Footprint" "" (id 2) (at 0 0 0))
      (property "Datasheet" "" (id 3) (at 0 0 0))
      (property "ki_keywords" "global power" (id 4) (at 0 0 0))
      (property "ki_description" "Power symbol creates a global label with name \"GND\" , ground" (id 5) (at 0 0 0))
      (symbol "GND_0_1"
        (polyline
          (pts
            (xy 0 0)
            (xy 0 -1.27)
            (xy 1.27 -1.27)
            (xy 0 -2.54)
            (xy -1.27 -1.27)
            (xy 0 -1.27)
          )
          (fill (type none))
        )
      )
      (symbol "GND_1_1"
        (pin power_in line (at 0 0 270) (length 0) hide
          (name "GND")
          (number "1")
        )
      )
    )
  )
  (junction (at 81.28 80.01) (diameter 0) (color 0 0 0 0))
  (junction (at 107.95 57.15) (diameter 0) (color 0 0 0 0))
  (junction (at 157.48 67.31) (diameter 0) (color 0 0 0 0))
  (junction (at 55.88 54.61) (diameter 0) (color 0 0 0 0))
  (junction (at 245.11 54.61) (diameter 0) (color 0 0 0 0))
  (junction (at 149.86 62.23) (diameter 0) (color 0 0 0 0))
  (junction (at 69.85 54.61) (diameter 0) (color 0 0 0 0))
  (junction (at 107.95 80.01) (diameter 0) (color 0 0 0 0))
  (junction (at 134.62 80.01) (diameter 0) (color 0 0 0 0))
  (junction (at 134.62 29.21) (diameter 0) (color 0 0 0 0))
  (junction (at 104.14 57.15) (diameter 0) (color 0 0 0 0))
  (junction (at 185.42 52.07) (diameter 0) (color 0 0 0 0))
  (junction (at 118.11 29.21) (diameter 0) (color 0 0 0 0))
  (junction (at 69.85 80.01) (diameter 0) (color 0 0 0 0))
  (junction (at 55.88 58.42) (diameter 0) (color 0 0 0 0))
  (junction (at 157.48 80.01) (diameter 0) (color 0 0 0 0))
  (junction (at 157.48 57.15) (diameter 0) (color 0 0 0 0))
  (junction (at 81.28 54.61) (diameter 0) (color 0 0 0 0))
  (junction (at 149.86 29.21) (diameter 0) (color 0 0 0 0))
  (junction (at 177.8 80.01) (diameter 0) (color 0 0 0 0))
  (junction (at 204.47 60.96) (diameter 0) (color 0 0 0 0))
  (junction (at 187.96 52.07) (diameter 0) (color 0 0 0 0))
  (no_connect (at 290.83 20.32))
  (wire (pts (xy 43.18 48.26) (xy 55.88 48.26)))
  (wire (pts (xy 204.47 69.85) (xy 204.47 71.12)))
  (wire (pts (xy 157.48 57.15) (xy 157.48 58.42)))
  (wire (pts (xy 243.84 60.96) (xy 245.11 60.96)))
  (wire (pts (xy 107.95 57.15) (xy 121.92 57.15)))
  (wire (pts (xy 227.33 80.01) (xy 259.08 80.01)))
  (wire (pts (xy 107.95 80.01) (xy 81.28 80.01)))
  (wire (pts (xy 31.75 105.41) (xy 95.25 105.41)))
  (wire (pts (xy 52.07 58.42) (xy 55.88 58.42)))
  (wire (pts (xy 149.86 29.21) (xy 134.62 29.21)))
  (wire (pts (xy 69.85 54.61) (xy 69.85 57.15)))
  (wire (pts (xy 157.48 29.21) (xy 157.48 34.29)))
  (wire (pts (xy 123.19 153.67) (xy 123.19 143.51)))
  (wire (pts (xy 55.88 68.58) (xy 55.88 80.01)))
  (wire (pts (xy 204.47 60.96) (xy 204.47 62.23)))
  (wire (pts (xy 134.62 29.21) (xy 118.11 29.21)))
  (wire (pts (xy 157.48 50.8) (xy 157.48 57.15)))
  (wire (pts (xy 227.33 60.96) (xy 227.33 80.01)))
  (wire (pts (xy 55.88 54.61) (xy 59.69 54.61)))
  (wire (pts (xy 55.88 54.61) (xy 55.88 58.42)))
  (wire (pts (xy 184.15 52.07) (xy 185.42 52.07)))
  (wire (pts (xy 69.85 52.07) (xy 69.85 54.61)))
  (wire (pts (xy 245.11 54.61) (xy 245.11 60.96)))
  (wire (pts (xy 27.94 48.26) (xy 35.56 48.26)))
  (wire (pts (xy 69.85 54.61) (xy 81.28 54.61)))
  (wire (pts (xy 95.25 110.49) (xy 95.25 105.41)))
  (wire (pts (xy 104.14 64.77) (xy 88.9 64.77)))
  (wire (pts (xy 134.62 67.31) (xy 134.62 80.01)))
  (wire (pts (xy 121.92 52.07) (xy 120.65 52.07)))
  (wire (pts (xy 228.6 60.96) (xy 228.6 74.93)))
  (wire (pts (xy 245.11 46.99) (xy 245.11 54.61)))
  (wire (pts (xy 203.2 60.96) (xy 204.47 60.96)))
  (wire (pts (xy 107.95 72.39) (xy 107.95 80.01)))
  (wire (pts (xy 204.47 78.74) (xy 204.47 80.01)))
  (wire (pts (xy 120.65 52.07) (xy 120.65 44.45)))
  (wire (pts (xy 104.14 57.15) (xy 104.14 64.77)))
  (wire (pts (xy 120.65 44.45) (xy 149.86 44.45)))
  (wire (pts (xy 214.63 46.99) (xy 214.63 151.13)))
  (wire (pts (xy 81.28 54.61) (xy 88.9 54.61)))
  (wire (pts (xy 118.11 29.21) (xy 118.11 34.29)))
  (wire (pts (xy 217.17 153.67) (xy 123.19 153.67)))
  (wire (pts (xy 185.42 52.07) (xy 187.96 52.07)))
  (wire (pts (xy 157.48 66.04) (xy 157.48 67.31)))
  (wire (pts (xy 157.48 67.31) (xy 157.48 68.58)))
  (wire (pts (xy 157.48 41.91) (xy 157.48 43.18)))
  (wire (pts (xy 203.2 46.99) (xy 214.63 46.99)))
  (wire (pts (xy 134.62 80.01) (xy 107.95 80.01)))
  (wire (pts (xy 104.14 57.15) (xy 107.95 57.15)))
  (wire (pts (xy 147.32 57.15) (xy 157.48 57.15)))
  (wire (pts (xy 69.85 80.01) (xy 81.28 80.01)))
  (wire (pts (xy 107.95 64.77) (xy 107.95 57.15)))
  (wire (pts (xy 228.6 74.93) (xy 259.08 74.93)))
  (wire (pts (xy 149.86 67.31) (xy 157.48 67.31)))
  (wire (pts (xy 55.88 80.01) (xy 69.85 80.01)))
  (wire (pts (xy 31.75 58.42) (xy 35.56 58.42)))
  (wire (pts (xy 187.96 52.07) (xy 187.96 60.96)))
  (wire (pts (xy 134.62 29.21) (xy 134.62 46.99)))
  (wire (pts (xy 81.28 54.61) (xy 81.28 63.5)))
  (wire (pts (xy 217.17 46.99) (xy 217.17 153.67)))
  (wire (pts (xy 177.8 80.01) (xy 204.47 80.01)))
  (wire (pts (xy 243.84 46.99) (xy 245.11 46.99)))
  (wire (pts (xy 67.31 54.61) (xy 69.85 54.61)))
  (wire (pts (xy 69.85 44.45) (xy 69.85 29.21)))
  (wire (pts (xy 107.95 147.32) (xy 27.94 147.32)))
  (wire (pts (xy 214.63 151.13) (xy 125.73 151.13)))
  (wire (pts (xy 125.73 151.13) (xy 125.73 143.51)))
  (wire (pts (xy 204.47 60.96) (xy 227.33 60.96)))
  (wire (pts (xy 147.32 52.07) (xy 170.18 52.07)))
  (wire (pts (xy 149.86 62.23) (xy 147.32 62.23)))
  (wire (pts (xy 121.92 62.23) (xy 118.11 62.23)))
  (wire (pts (xy 228.6 46.99) (xy 217.17 46.99)))
  (wire (pts (xy 69.85 29.21) (xy 118.11 29.21)))
  (wire (pts (xy 157.48 80.01) (xy 177.8 80.01)))
  (wire (pts (xy 69.85 64.77) (xy 69.85 80.01)))
  (wire (pts (xy 31.75 105.41) (xy 31.75 58.42)))
  (wire (pts (xy 55.88 48.26) (xy 55.88 54.61)))
  (wire (pts (xy 55.88 58.42) (xy 55.88 60.96)))
  (wire (pts (xy 157.48 29.21) (xy 149.86 29.21)))
  (wire (pts (xy 149.86 62.23) (xy 149.86 67.31)))
  (wire (pts (xy 118.11 41.91) (xy 118.11 62.23)))
  (wire (pts (xy 107.95 143.51) (xy 107.95 147.32)))
  (wire (pts (xy 260.35 54.61) (xy 262.89 54.61)))
  (wire (pts (xy 81.28 71.12) (xy 81.28 80.01)))
  (wire (pts (xy 157.48 80.01) (xy 157.48 76.2)))
  (wire (pts (xy 134.62 80.01) (xy 157.48 80.01)))
  (wire (pts (xy 88.9 64.77) (xy 88.9 59.69)))
  (wire (pts (xy 27.94 147.32) (xy 27.94 48.26)))
  (wire (pts (xy 43.18 58.42) (xy 44.45 58.42)))
  (wire (pts (xy 187.96 46.99) (xy 187.96 52.07)))
  (wire (pts (xy 149.86 44.45) (xy 149.86 62.23)))
  (global_label "GPS PPS" (shape input) (at 262.89 54.61 0) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 273.7698 54.5306 0))
  )
  (global_label "555 PPS Out" (shape output) (at 259.08 80.01 0) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 274.0117 79.9306 0))
  )
  (global_label "GPS PPS Out" (shape output) (at 259.08 74.93 0) (fields_autoplaced)
    (property "Intersheet References" "${INTERSHEET_REFS}" (id 0) (at 274.1326 74.8506 0))
  )
  (symbol (lib_id "Device:R") (at 69.85 48.26 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R?" (id 0) (at 72.39 46.9899 0))
    (property "Value" "10k" (id 1) (at 72.39 49.5299 0))
    (property "Footprint" "" (id 2) (at 68.072 48.26 90))
    (property "Datasheet" "~" (id 3) (at 69.85 48.26 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 204.47 74.93 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R?" (id 0) (at 207.01 73.6599 0))
    (property "Value" "220" (id 1) (at 207.01 76.1999 0))
    (property "Footprint" "" (id 2) (at 202.692 74.93 90))
    (property "Datasheet" "~" (id 3) (at 204.47 74.93 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 157.48 38.1 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R?" (id 0) (at 160.02 36.8299 0))
    (property "Value" "1k" (id 1) (at 160.02 39.3699 0))
    (property "Footprint" "" (id 2) (at 155.702 38.1 90))
    (property "Datasheet" "~" (id 3) (at 157.48 38.1 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 48.26 58.42 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "C?" (id 0) (at 48.26 50.8 90))
    (property "Value" "1uf" (id 1) (at 48.26 53.34 90))
    (property "Footprint" "" (id 2) (at 52.07 57.4548 0))
    (property "Datasheet" "~" (id 3) (at 48.26 58.42 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "74xx:74HC14") (at 252.73 54.61 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U?" (id 0) (at 252.73 63.5 0))
    (property "Value" "74AC14" (id 1) (at 252.73 60.96 0))
    (property "Footprint" "" (id 2) (at 252.73 54.61 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74HC14" (id 3) (at 252.73 54.61 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "MCU_ST_STM32F4:STM32F411CEUx") (at 128.27 128.27 270) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U?" (id 0) (at 81.28 139.1795 90))
    (property "Value" "STM32F411CEUx" (id 1) (at 81.28 136.6395 90))
    (property "Footprint" "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm" (id 2) (at 90.17 113.03 0))
    (property "Datasheet" "http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/DM00115249.pdf" (id 3) (at 128.27 128.27 0))
    (pin "1")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "15")
    (pin "16")
    (pin "17")
    (pin "18")
    (pin "19")
    (pin "2")
    (pin "20")
    (pin "21")
    (pin "22")
    (pin "23")
    (pin "24")
    (pin "25")
    (pin "26")
    (pin "27")
    (pin "28")
    (pin "29")
    (pin "3")
    (pin "30")
    (pin "31")
    (pin "32")
    (pin "33")
    (pin "34")
    (pin "35")
    (pin "36")
    (pin "37")
    (pin "38")
    (pin "39")
    (pin "4")
    (pin "40")
    (pin "41")
    (pin "42")
    (pin "43")
    (pin "44")
    (pin "45")
    (pin "46")
    (pin "47")
    (pin "48")
    (pin "49")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "8")
    (pin "9")
  )
  (symbol (lib_id "74xx:74HC14") (at 236.22 60.96 180) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "U?" (id 0) (at 236.22 69.85 0))
    (property "Value" "74AC14" (id 1) (at 236.22 67.31 0))
    (property "Footprint" "" (id 2) (at 236.22 60.96 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74HC14" (id 3) (at 236.22 60.96 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "74xx:74HC14") (at 177.8 52.07 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U?" (id 0) (at 177.8 43.18 0))
    (property "Value" "74AC14" (id 1) (at 177.8 45.72 0))
    (property "Footprint" "" (id 2) (at 177.8 52.07 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74HC14" (id 3) (at 177.8 52.07 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "Device:R_Variable") (at 157.48 46.99 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R?" (id 0) (at 161.29 45.7199 0))
    (property "Value" "10k" (id 1) (at 161.29 48.2599 0))
    (property "Footprint" "" (id 2) (at 155.702 46.99 90))
    (property "Datasheet" "~" (id 3) (at 157.48 46.99 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 63.5 54.61 90) (unit 1)
    (in_bom yes) (on_board yes)
    (property "Reference" "R?" (id 0) (at 63.5 48.26 90))
    (property "Value" "10k" (id 1) (at 63.5 50.8 90))
    (property "Footprint" "" (id 2) (at 63.5 56.388 90))
    (property "Datasheet" "~" (id 3) (at 63.5 54.61 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 118.11 38.1 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R?" (id 0) (at 120.65 36.8299 0))
    (property "Value" "10k" (id 1) (at 120.65 39.3699 0))
    (property "Footprint" "" (id 2) (at 116.332 38.1 90))
    (property "Datasheet" "~" (id 3) (at 118.11 38.1 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "74xx:74HC14") (at 195.58 60.96 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U?" (id 0) (at 195.58 52.07 0))
    (property "Value" "74AC14" (id 1) (at 195.58 54.61 0))
    (property "Footprint" "" (id 2) (at 195.58 60.96 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74HC14" (id 3) (at 195.58 60.96 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "Device:C") (at 107.95 68.58 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "C?" (id 0) (at 111.76 67.3099 0))
    (property "Value" "100uf" (id 1) (at 111.76 69.8499 0))
    (property "Footprint" "" (id 2) (at 108.9152 72.39 0))
    (property "Datasheet" "~" (id 3) (at 107.95 68.58 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 81.28 67.31 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "C?" (id 0) (at 85.09 66.0399 0))
    (property "Value" "100uf" (id 1) (at 85.09 68.5799 0))
    (property "Footprint" "" (id 2) (at 82.2452 71.12 0))
    (property "Datasheet" "~" (id 3) (at 81.28 67.31 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "power:GND") (at 177.8 80.01 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR?" (id 0) (at 177.8 86.36 0))
    (property "Value" "GND" (id 1) (at 177.8 85.09 0))
    (property "Footprint" "" (id 2) (at 177.8 80.01 0))
    (property "Datasheet" "" (id 3) (at 177.8 80.01 0))
    (pin "1")
  )
  (symbol (lib_id "Device:LED") (at 204.47 66.04 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "D?" (id 0) (at 208.28 66.3574 90))
    (property "Value" "LED" (id 1) (at 208.28 68.8974 90))
    (property "Footprint" "" (id 2) (at 204.47 66.04 0))
    (property "Datasheet" "~" (id 3) (at 204.47 66.04 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 157.48 62.23 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R?" (id 0) (at 160.02 60.9599 0))
    (property "Value" "10k" (id 1) (at 160.02 63.4999 0))
    (property "Footprint" "" (id 2) (at 155.702 62.23 90))
    (property "Datasheet" "~" (id 3) (at 157.48 62.23 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Amplifier_Operational:MCP6002-xP") (at 96.52 57.15 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U?" (id 0) (at 96.52 46.99 0))
    (property "Value" "MCP6002" (id 1) (at 96.52 49.53 0))
    (property "Footprint" "" (id 2) (at 96.52 57.15 0))
    (property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/21733j.pdf" (id 3) (at 96.52 57.15 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "5")
    (pin "6")
    (pin "7")
    (pin "4")
    (pin "8")
  )
  (symbol (lib_id "Timer:NE555P") (at 134.62 57.15 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U?" (id 0) (at 136.6394 44.45 0))
    (property "Value" "NE555P" (id 1) (at 136.6394 46.99 0))
    (property "Footprint" "Package_DIP:DIP-8_W7.62mm" (id 2) (at 151.13 67.31 0))
    (property "Datasheet" "http://www.ti.com/lit/ds/symlink/ne555.pdf" (id 3) (at 156.21 67.31 0))
    (pin "1")
    (pin "8")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "7")
  )
  (symbol (lib_id "power:+5V") (at 149.86 29.21 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "#PWR?" (id 0) (at 149.86 33.02 0))
    (property "Value" "+5V" (id 1) (at 149.86 24.13 0))
    (property "Footprint" "" (id 2) (at 149.86 29.21 0))
    (property "Datasheet" "" (id 3) (at 149.86 29.21 0))
    (pin "1")
  )
  (symbol (lib_id "74xx:74HC14") (at 195.58 46.99 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U?" (id 0) (at 195.58 38.1 0))
    (property "Value" "74AC14" (id 1) (at 195.58 40.64 0))
    (property "Footprint" "" (id 2) (at 195.58 46.99 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74HC14" (id 3) (at 195.58 46.99 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (symbol (lib_id "Device:R") (at 39.37 48.26 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R?" (id 0) (at 39.37 41.91 90))
    (property "Value" "1k" (id 1) (at 39.37 44.45 90))
    (property "Footprint" "" (id 2) (at 39.37 50.038 90))
    (property "Datasheet" "~" (id 3) (at 39.37 48.26 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 69.85 60.96 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R?" (id 0) (at 72.39 59.6899 0))
    (property "Value" "100k" (id 1) (at 72.39 62.2299 0))
    (property "Footprint" "" (id 2) (at 68.072 60.96 90))
    (property "Datasheet" "~" (id 3) (at 69.85 60.96 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:R") (at 39.37 58.42 90) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "R?" (id 0) (at 39.37 52.07 90))
    (property "Value" "1k" (id 1) (at 39.37 54.61 90))
    (property "Footprint" "" (id 2) (at 39.37 60.198 90))
    (property "Datasheet" "~" (id 3) (at 39.37 58.42 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 157.48 72.39 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "C?" (id 0) (at 161.29 71.1199 0))
    (property "Value" "47uf" (id 1) (at 161.29 73.6599 0))
    (property "Footprint" "" (id 2) (at 158.4452 76.2 0))
    (property "Datasheet" "~" (id 3) (at 157.48 72.39 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "Device:C") (at 55.88 64.77 0) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "C?" (id 0) (at 59.69 63.4999 0))
    (property "Value" "10uf" (id 1) (at 59.69 66.0399 0))
    (property "Footprint" "" (id 2) (at 56.8452 68.58 0))
    (property "Datasheet" "~" (id 3) (at 55.88 64.77 0))
    (pin "1")
    (pin "2")
  )
  (symbol (lib_id "74xx:74HC14") (at 236.22 46.99 180) (unit 1)
    (in_bom yes) (on_board yes) (fields_autoplaced)
    (property "Reference" "U?" (id 0) (at 236.22 38.1 0))
    (property "Value" "74AC14" (id 1) (at 236.22 40.64 0))
    (property "Footprint" "" (id 2) (at 236.22 46.99 0))
    (property "Datasheet" "http://www.ti.com/lit/gpn/sn74HC14" (id 3) (at 236.22 46.99 0))
    (pin "1")
    (pin "2")
    (pin "3")
    (pin "4")
    (pin "5")
    (pin "6")
    (pin "8")
    (pin "9")
    (pin "10")
    (pin "11")
    (pin "12")
    (pin "13")
    (pin "14")
    (pin "7")
  )
  (sheet_instances
    (path (page "1"))
  )
  (symbol_instances
    (path
      (reference "#PWR?") (unit 1) (value "GND") (footprint "")
    )
    (path
      (reference "#PWR?") (unit 1) (value "+5V") (footprint "")
    )
    (path
      (reference "C?") (unit 1) (value "1uf") (footprint "")
    )
    (path
      (reference "C?") (unit 1) (value "100uf") (footprint "")
    )
    (path
      (reference "C?") (unit 1) (value "100uf") (footprint "")
    )
    (path
      (reference "C?") (unit 1) (value "47uf") (footprint "")
    )
    (path
      (reference "C?") (unit 1) (value "10uf") (footprint "")
    )
    (path
      (reference "D?") (unit 1) (value "LED") (footprint "")
    )
    (path
      (reference "R?") (unit 1) (value "10k") (footprint "")
    )
    (path
      (reference "R?") (unit 1) (value "220") (footprint "")
    )
    (path
      (reference "R?") (unit 1) (value "1k") (footprint "")
    )
    (path
      (reference "R?") (unit 1) (value "10k") (footprint "")
    )
    (path
      (reference "R?") (unit 1) (value "10k") (footprint "")
    )
    (path
      (reference "R?") (unit 1) (value "10k") (footprint "")
    )
    (path
      (reference "R?") (unit 1) (value "10k") (footprint "")
    )
    (path
      (reference "R?") (unit 1) (value "1k") (footprint "")
    )
    (path
      (reference "R?") (unit 1) (value "100k") (footprint "")
    )
    (path
      (reference "R?") (unit 1) (value "1k") (footprint "")
    )
    (path
      (reference "U?") (unit 1) (value "74AC14") (footprint "")
    )
    (path
      (reference "U?") (unit 1) (value "STM32F411CEUx") (footprint "Package_DFN_QFN:QFN-48-1EP_7x7mm_P0.5mm_EP5.6x5.6mm")
    )
    (path
      (reference "U?") (unit 1) (value "74AC14") (footprint "")
    )
    (path
      (reference "U?") (unit 1) (value "74AC14") (footprint "")
    )
    (path
      (reference "U?") (unit 1) (value "74AC14") (footprint "")
    )
    (path
      (reference "U?") (unit 1) (value "MCP6002") (footprint "")
    )
    (path
      (reference "U?") (unit 1) (value "NE555P") (footprint "Package_DIP:DIP-8_W7.62mm")
    )
    (path
      (reference "U?") (unit 1) (value "74AC14") (footprint "")
    )
    (path
      (reference "U?") (unit 1) (value "74AC14") (footprint "")
    )
  )
)
