(kicad_pcb
	(version 20240108)
	(generator "pcbnew")
	(generator_version "8.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(1 "In1.Cu" signal)
		(2 "In2.Cu" signal)
		(31 "B.Cu" signal)
		(32 "B.Adhes" user "B.Adhesive")
		(33 "F.Adhes" user "F.Adhesive")
		(34 "B.Paste" user)
		(35 "F.Paste" user)
		(36 "B.SilkS" user "B.Silkscreen")
		(37 "F.SilkS" user "F.Silkscreen")
		(38 "B.Mask" user)
		(39 "F.Mask" user)
		(40 "Dwgs.User" user "User.Drawings")
		(41 "Cmts.User" user "User.Comments")
		(42 "Eco1.User" user "User.Eco1")
		(43 "Eco2.User" user "User.Eco2")
		(44 "Edge.Cuts" user)
		(45 "Margin" user)
		(46 "B.CrtYd" user "B.Courtyard")
		(47 "F.CrtYd" user "F.Courtyard")
		(48 "B.Fab" user)
		(49 "F.Fab" user)
		(50 "User.1" user)
		(51 "User.2" user)
		(52 "User.3" user)
		(53 "User.4" user)
		(54 "User.5" user)
		(55 "User.6" user)
		(56 "User.7" user)
		(57 "User.8" user)
		(58 "User.9" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In1.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 2"
				(type "core")
				(thickness 1.24)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "In2.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 3"
				(type "prepreg")
				(thickness 0.1)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(grid_origin 100 50)
		(pcbplotparams
			(layerselection 0x00010fc_ffffffff)
			(plot_on_all_layers_selection 0x0000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(viasonmask no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plotreference yes)
			(plotvalue yes)
			(plotfptext yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "/home/justinas/JPL.mp3/0.1.3.a/JPL.mp3/cad/eda/gerbers0.1.3.a/")
		)
	)
	(net 0 "")
	(net 1 "Net-(BOOT1-A)")
	(net 2 "GND")
	(net 3 "Net-(BT1-+)")
	(net 4 "+3.3V")
	(net 5 "AUDIO_LEFT")
	(net 6 "AUDIO_RIGHT")
	(net 7 "Net-(U4-LDOO)")
	(net 8 "BAT_SENSE")
	(net 9 "Net-(RST1-B)")
	(net 10 "+5V")
	(net 11 "Net-(U4-CAPP)")
	(net 12 "Net-(U4-CAPM)")
	(net 13 "Net-(U4-VNEG)")
	(net 14 "Net-(D1-A)")
	(net 15 "Net-(D2-A)")
	(net 16 "SW2")
	(net 17 "SW4")
	(net 18 "ENCA")
	(net 19 "SW3")
	(net 20 "SW5")
	(net 21 "ENCB")
	(net 22 "SW1")
	(net 23 "SD_CMD")
	(net 24 "SD_D0")
	(net 25 "Net-(J1-DAT1)")
	(net 26 "Net-(J1-DAT3{slash}CD)")
	(net 27 "SD_CLK")
	(net 28 "Net-(J1-DAT2)")
	(net 29 "Net-(J2-CC2)")
	(net 30 "USB_D+")
	(net 31 "Net-(J2-CC1)")
	(net 32 "USB_D-")
	(net 33 "unconnected-(J2-SBU2-PadB8)")
	(net 34 "unconnected-(J2-SBU1-PadA8)")
	(net 35 "TFT_DC")
	(net 36 "TFT_RST")
	(net 37 "unconnected-(J4-Pin_7-Pad7)")
	(net 38 "Net-(J4-Pin_10)")
	(net 39 "TFT_CS")
	(net 40 "TFT_SDA")
	(net 41 "Net-(J4-Pin_11)")
	(net 42 "TFT_SCLK")
	(net 43 "UART_RX")
	(net 44 "UART_TX")
	(net 45 "Net-(Q1-G)")
	(net 46 "CHG")
	(net 47 "BACKLIGHT")
	(net 48 "Net-(U4-OUTL)")
	(net 49 "Net-(U4-OUTR)")
	(net 50 "HOLD")
	(net 51 "VOL_UP")
	(net 52 "VOL_DOWN")
	(net 53 "S_B")
	(net 54 "unconnected-(U1-GPIO15{slash}U0RTS{slash}ADC2_CH4{slash}XTAL_32K_P-Pad8)")
	(net 55 "unconnected-(U1-GPIO17{slash}U1TXD{slash}ADC2_CH6-Pad10)")
	(net 56 "unconnected-(U1-GPIO18{slash}U1RXD{slash}ADC2_CH7{slash}CLK_OUT3-Pad11)")
	(net 57 "DAC_MCLK")
	(net 58 "I2S_SCLK")
	(net 59 "unconnected-(U1-GPIO13{slash}TOUCH13{slash}ADC2_CH2{slash}FSPIQ{slash}FSPIIO7{slash}SUBSPIQ-Pad21)")
	(net 60 "I2S_LRCLK")
	(net 61 "S_A")
	(net 62 "I2S_SD")
	(footprint "Connector_Audio:Jack_3.5mm_KoreanHropartsElec_PJ-320D-4A_Horizontal"
		(layer "F.Cu")
		(at 108.75 57.8 -90)
		(descr "Korean Hroparts Elec PJ-320D-4A (https://datasheet.lcsc.com/lcsc/1810121716_Korean-Hroparts-Elec-PJ-320D-4A_C95562.pdf)")
		(tags "smt female jack horizontal")
		(property "Reference" "J5"
			(at 0 -6 -90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "AudioJack3"
			(at 0 6 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Audio:Jack_3.5mm_KoreanHropartsElec_PJ-320D-4A_Horizontal"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Jack*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -4.75 0 270)
			(size 1.6 1.6)
			(drill 1.6)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2.25 0 270)
			(size 1.6 1.6)
			(drill 1.6)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "R1" smd rect
			(at -0.15 -3.25 270)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 6 "AUDIO_RIGHT")
		)
		(pad "R2" smd rect
			(at -3.15 -3.25 270)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "S" smd rect
			(at 4.95 3.25 270)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "T" smd rect
			(at 3.85 -3.25 270)
			(size 1.2 2.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 5 "AUDIO_LEFT")
			(pintype "passive")
		)
		(model "/home/justinas/Downloads/pj320/PJ320D/PJ320D.STEP"
			(offset
				(xyz -1.2 0 -11.6)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 133.75 85.25 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R14"
			(at -3 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10K"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 23 "SD_CMD")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 119.7 80.1875 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R11"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10K"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 47 "BACKLIGHT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 134.5 80.025 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R17"
			(at 2.275 -1.43 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10K"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Net-(BOOT1-A)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 113 102.5 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C14"
			(at -2.725 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7 uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 110.8875 80.625 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C20"
			(at 2.75 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 116.95 80.4375 -90)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q2"
			(at 1.5 -1 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "BSS138"
			(at 0 2.4 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BSS138-D.PDF"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 47 "BACKLIGHT")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 270)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 41 "Net-(J4-Pin_11)")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 130.75 85.25 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R15"
			(at 2 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10K"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 24 "SD_D0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3.3V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "RF_Module:ESP32-S3-WROOM-1"
		(layer "F.Cu")
		(at 125.65 62.96)
		(descr "2.4 GHz Wi-Fi and Bluetooth module  https://www.espressif.com/sites/default/files/documentation/esp32-s3-wroom-1_wroom-1u_datasheet_en.pdf")
		(tags "2.4 GHz Wi-Fi and Bluetooth module")
		(property "Reference" "U1"
			(at -10.5 11.4 90)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ESP32-S3-WROOM-1"
			(at 0 14.6 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "RF_Module:ESP32-S3-WROOM-1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-s3-wroom-1_wroom-1u_datasheet_en.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "Antenna"
			(at -0.05 -9.44 0)
			(layer "Cmts.User")
		)
		(fp_text user "${REFERENCE}"
			(at 0 -0.6 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "" smd rect
			(at -2.9 1.06)
			(size 0.9 0.9)
			(layers "F.Paste")
		)
		(pad "" smd rect
			(at -2.9 2.46 270)
			(size 0.9 0.9)
			(layers "F.Paste")
		)
		(pad "" smd rect
			(at -2.9 3.86)
			(size 0.9 0.9)
			(layers "F.Paste")
		)
		(pad "" smd rect
			(at -1.5 1.06 270)
			(size 0.9 0.9)
			(layers "F.Paste")
		)
		(pad "" smd rect
			(at -1.5 2.46 270)
			(size 0.9 0.9)
			(layers "F.Paste")
		)
		(pad "" smd rect
			(at -1.5 3.86 270)
			(size 0.9 0.9)
			(layers "F.Paste")
		)
		(pad "" smd rect
			(at -0.1 1.06 270)
			(size 0.9 0.9)
			(layers "F.Paste")
		)
		(pad "" smd rect
			(at -0.1 2.46 270)
			(size 0.9 0.9)
			(layers "F.Paste")
		)
		(pad "" smd rect
			(at -0.1 3.86 270)
			(size 0.9 0.9)
			(layers "F.Paste")
		)
		(pad "1" smd rect
			(at -8.75 -5.26)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at -8.75 -3.99)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "+3.3V")
			(pinfunction "3V3")
			(pintype "power_in")
		)
		(pad "3" smd rect
			(at -8.75 -2.72)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "Net-(RST1-B)")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "4" smd rect
			(at -8.75 -1.45)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 57 "DAC_MCLK")
			(pinfunction "GPIO4/TOUCH4/ADC1_CH3")
			(pintype "bidirectional")
		)
		(pad "5" smd rect
			(at -8.75 -0.18)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 60 "I2S_LRCLK")
			(pinfunction "GPIO5/TOUCH5/ADC1_CH4")
			(pintype "bidirectional")
		)
		(pad "6" smd rect
			(at -8.75 1.09)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 62 "I2S_SD")
			(pinfunction "GPIO6/TOUCH6/ADC1_CH5")
			(pintype "bidirectional")
		)
		(pad "7" smd rect
			(at -8.75 2.36)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 58 "I2S_SCLK")
			(pinfunction "GPIO7/TOUCH7/ADC1_CH6")
			(pintype "bidirectional")
		)
		(pad "8" smd rect
			(at -8.75 3.63)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 54 "unconnected-(U1-GPIO15{slash}U0RTS{slash}ADC2_CH4{slash}XTAL_32K_P-Pad8)")
			(pinfunction "GPIO15/U0RTS/ADC2_CH4/XTAL_32K_P")
			(pintype "bidirectional+no_connect")
		)
		(pad "9" smd rect
			(at -8.75 4.9)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "HOLD")
			(pinfunction "GPIO16/U0CTS/ADC2_CH5/XTAL_32K_N")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at -8.75 6.17)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 55 "unconnected-(U1-GPIO17{slash}U1TXD{slash}ADC2_CH6-Pad10)")
			(pinfunction "GPIO17/U1TXD/ADC2_CH6")
			(pintype "bidirectional")
		)
		(pad "11" smd rect
			(at -8.75 7.44)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 56 "unconnected-(U1-GPIO18{slash}U1RXD{slash}ADC2_CH7{slash}CLK_OUT3-Pad11)")
			(pinfunction "GPIO18/U1RXD/ADC2_CH7/CLK_OUT3")
			(pintype "bidirectional")
		)
		(pad "12" smd rect
			(at -8.75 8.71)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 46 "CHG")
			(pinfunction "GPIO8/TOUCH8/ADC1_CH7/SUBSPICS1")
			(pintype "bidirectional")
		)
		(pad "13" smd rect
			(at -8.75 9.98)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "USB_D-")
			(pinfunction "GPIO19/U1RTS/ADC2_CH8/CLK_OUT2/USB_D-")
			(pintype "bidirectional")
		)
		(pad "14" smd rect
			(at -8.75 11.25 180)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "USB_D+")
			(pinfunction "GPIO20/U1CTS/ADC2_CH9/CLK_OUT1/USB_D+")
			(pintype "bidirectional")
		)
		(pad "15" smd rect
			(at -6.985 12.5 270)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 36 "TFT_RST")
			(pinfunction "GPIO3/TOUCH3/ADC1_CH2")
			(pintype "bidirectional")
		)
		(pad "16" smd rect
			(at -5.715 12.5 270)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 61 "S_A")
			(pinfunction "GPIO46")
			(pintype "bidirectional")
		)
		(pad "17" smd rect
			(at -4.445 12.5 270)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 47 "BACKLIGHT")
			(pinfunction "GPIO9/TOUCH9/ADC1_CH8/FSPIHD/SUBSPIHD")
			(pintype "bidirectional")
		)
		(pad "18" smd rect
			(at -3.175 12.5 270)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 8 "BAT_SENSE")
			(pinfunction "GPIO10/TOUCH10/ADC1_CH9/FSPICS0/FSPIIO4/SUBSPICS0")
			(pintype "bidirectional")
		)
		(pad "19" smd rect
			(at -1.905 12.5 270)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 40 "TFT_SDA")
			(pinfunction "GPIO11/TOUCH11/ADC2_CH0/FSPID/FSPIIO5/SUBSPID")
			(pintype "bidirectional")
		)
		(pad "20" smd rect
			(at -0.635 12.5 270)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 42 "TFT_SCLK")
			(pinfunction "GPIO12/TOUCH12/ADC2_CH1/FSPICLK/FSPIIO6/SUBSPICLK")
			(pintype "bidirectional")
		)
		(pad "21" smd rect
			(at 0.635 12.5 270)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 59 "unconnected-(U1-GPIO13{slash}TOUCH13{slash}ADC2_CH2{slash}FSPIQ{slash}FSPIIO7{slash}SUBSPIQ-Pad21)")
			(pinfunction "GPIO13/TOUCH13/ADC2_CH2/FSPIQ/FSPIIO7/SUBSPIQ")
			(pintype "bidirectional+no_connect")
		)
		(pad "22" smd rect
			(at 1.905 12.5 270)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 35 "TFT_DC")
			(pinfunction "GPIO14/TOUCH14/ADC2_CH3/FSPIWP/FSPIDQS/SUBSPIWP")
			(pintype "bidirectional")
		)
		(pad "23" smd rect
			(at 3.175 12.5 270)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 39 "TFT_CS")
			(pinfunction "GPIO21")
			(pintype "bidirectional")
		)
		(pad "24" smd rect
			(at 4.445 12.5 270)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 52 "VOL_DOWN")
			(pinfunction "GPIO47/SPICLK_P/SUBSPICLK_P_DIFF")
			(pintype "bidirectional")
		)
		(pad "25" smd rect
			(at 5.715 12.5 270)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 51 "VOL_UP")
			(pinfunction "GPIO48/SPICLK_N/SUBSPICLK_N_DIFF")
			(pintype "bidirectional")
		)
		(pad "26" smd rect
			(at 6.985 12.5 270)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 53 "S_B")
			(pinfunction "GPIO45")
			(pintype "bidirectional")
		)
		(pad "27" smd rect
			(at 8.75 11.25)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "Net-(BOOT1-A)")
			(pinfunction "GPIO0/BOOT")
			(pintype "bidirectional")
		)
		(pad "28" smd rect
			(at 8.75 9.98)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "SD_CMD")
			(pinfunction "SPIIO6/GPIO35/FSPID/SUBSPID")
			(pintype "bidirectional")
		)
		(pad "29" smd rect
			(at 8.75 8.71)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "SD_CLK")
			(pinfunction "SPIIO7/GPIO36/FSPICLK/SUBSPICLK")
			(pintype "bidirectional")
		)
		(pad "30" smd rect
			(at 8.75 7.44)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "SD_D0")
			(pinfunction "SPIDQS/GPIO37/FSPIQ/SUBSPIQ")
			(pintype "bidirectional")
		)
		(pad "31" smd rect
			(at 8.75 6.17)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 22 "SW1")
			(pinfunction "GPIO38/FSPIWP/SUBSPIWP")
			(pintype "bidirectional")
		)
		(pad "32" smd rect
			(at 8.75 4.9)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 16 "SW2")
			(pinfunction "MTCK/GPIO39/CLK_OUT3/SUBSPICS1")
			(pintype "bidirectional")
		)
		(pad "33" smd rect
			(at 8.75 3.63)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 19 "SW3")
			(pinfunction "MTDO/GPIO40/CLK_OUT2")
			(pintype "bidirectional")
		)
		(pad "34" smd rect
			(at 8.75 2.36)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 17 "SW4")
			(pinfunction "MTDI/GPIO41/CLK_OUT1")
			(pintype "bidirectional")
		)
		(pad "35" smd rect
			(at 8.75 1.09)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 20 "SW5")
			(pinfunction "MTMS/GPIO42")
			(pintype "bidirectional")
		)
		(pad "36" smd rect
			(at 8.75 -0.18)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 43 "UART_RX")
			(pinfunction "U0RXD/GPIO44/CLK_OUT2")
			(pintype "bidirectional")
		)
		(pad "37" smd rect
			(at 8.75 -1.45)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 44 "UART_TX")
			(pinfunction "U0TXD/GPIO43/CLK_OUT1")
			(pintype "bidirectional")
		)
		(pad "38" smd rect
			(at 8.75 -2.72)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 18 "ENCA")
			(pinfunction "GPIO2/TOUCH2/ADC1_CH1")
			(pintype "bidirectional")
		)
		(pad "39" smd rect
			(at 8.75 -3.99)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 21 "ENCB")
			(pinfunction "GPIO1/TOUCH1/ADC1_CH0")
			(pintype "bidirectional")
		)
		(pad "40" smd rect
			(at 8.75 -5.26)
			(size 1.5 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "41" thru_hole circle
			(at -2.9 1.76 90)
			(size 0.6 0.6)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "41" thru_hole circle
			(at -2.9 3.16)
			(size 0.6 0.6)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "41" thru_hole circle
			(at -2.2 1.06)
			(size 0.6 0.6)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "41" thru_hole circle
			(at -2.2 2.46)
			(size 0.6 0.6)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "41" thru_hole circle
			(at -2.2 3.86)
			(size 0.6 0.6)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "41" thru_hole circle
			(at -1.5 1.76)
			(size 0.6 0.6)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "41" smd rect
			(at -1.5 2.46 270)
			(size 3.9 3.9)
			(layers "F.Cu" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "41" thru_hole circle
			(at -1.5 3.16)
			(size 0.6 0.6)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "41" thru_hole circle
			(at -0.8 1.06)
			(size 0.6 0.6)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "41" thru_hole circle
			(at -0.8 2.46)
			(size 0.6 0.6)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "41" thru_hole circle
			(at -0.8 3.86)
			(size 0.6 0.6)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "41" thru_hole circle
			(at -0.1 1.76)
			(size 0.6 0.6)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(zone_connect 2)
		)
		(pad "41" thru_hole circle
			(at -0.1 3.16)
			(size 0.6 0.6)
			(drill 0.2)
			(property pad_prop_heatsink)
			(layers "*.Cu" "F.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
			(zone_connect 2)
		)
		(model "${KICAD8_3DMODEL_DIR}/RF_Module.3dshapes/ESP32-S3-WROOM-1.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "F.Cu")
		(at 104.5625 94.45 180)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q1"
			(at 2.5625 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "BSS138"
			(at 0 2.4 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.onsemi.com/pub/Collateral/BSS138-D.PDF"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 -0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 45 "Net-(Q1-G)")
			(pinfunction "G")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 0.95 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 46 "CHG")
			(pinfunction "S")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 180)
			(size 1.475 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "D")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D2.0mm"
		(layer "F.Cu")
		(at 116 136)
		(descr "SMD pad as test Point, diameter 2.0mm")
		(tags "test point SMD pad")
		(property "Reference" "COMA"
			(at 0.1 2 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint_Pad_D2.0mm"
			(at 0 2.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D2.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 119.5 138.5 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 2.5 0.25 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "5.1K"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 31 "Net-(J2-CC1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_Card:microSD_HC_Molex_104031-0811"
		(layer "F.Cu")
		(at 131.9125 94.5 -90)
		(descr "1.10mm Pitch microSD Memory Card Connector, Surface Mount, Push-Pull Type, 1.42mm Height, with Detect Switch (https://www.molex.com/pdm_docs/sd/1040310811_sd.pdf)")
		(tags "microSD SD molex")
		(property "Reference" "J1"
			(at 0 -7.18 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Micro_SD_Card"
			(at 0 7.39 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_Card:microSD_HC_Molex_104031-0811"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "http://katalog.we-online.de/em/datasheet/693072010801.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "microSD*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -3.105 -5.45 270)
			(size 0.85 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 28 "Net-(J1-DAT2)")
			(pinfunction "DAT2")
			(pintype "bidirectional")
		)
		(pad "2" smd rect
			(at -2.005 -5.45 270)
			(size 0.85 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 26 "Net-(J1-DAT3{slash}CD)")
			(pinfunction "DAT3/CD")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at -0.905 -5.45 270)
			(size 0.85 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 23 "SD_CMD")
			(pinfunction "CMD")
			(pintype "input")
		)
		(pad "4" smd rect
			(at 0.195 -5.45 270)
			(size 0.85 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 4 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "5" smd rect
			(at 1.295 -5.45 270)
			(size 0.85 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 27 "SD_CLK")
			(pinfunction "CLK")
			(pintype "input")
		)
		(pad "6" smd rect
			(at 2.395 -5.45 270)
			(size 0.85 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "7" smd rect
			(at 3.495 -5.45 270)
			(size 0.85 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 24 "SD_D0")
			(pinfunction "DAT0")
			(pintype "bidirectional")
		)
		(pad "8" smd rect
			(at 4.545 -5.45 270)
			(size 0.75 1.1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 25 "Net-(J1-DAT1)")
			(pinfunction "DAT1")
			(pintype "bidirectional")
		)
		(pad "9" smd rect
			(at -5.74 0.7 270)
			(size 1.2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at -5.74 4.4 270)
			(size 1.2 1)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "11" smd rect
			(at -5.565 -5.325 270)
			(size 1.55 1.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "11" smd rect
			(at -2.24 5.375 270)
			(size 1.9 1.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
		)
		(pad "11" smd rect
			(at 3.73 5.375 270)
			(size 1.9 1.35)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "11" smd rect
			(at 5.755 -5.1 270)
			(size 1.17 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_Card.3dshapes/microSD_HC_Hirose_DM3D-SF.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 -180)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_Push_1P1T-MP_NO_Horizontal_Alps_SKRTLAE010"
		(layer "F.Cu")
		(at 138.25 79.5 90)
		(descr "Side push button (https://www.alps.com/prod/info/E/PDF/Tact/SurfaceMount/SKRT/SKRT.pdf)")
		(tags "push horizontal SPST 1P1T")
		(property "Reference" "SW2"
			(at -3.5 0.25 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_Push"
			(at 0 2.9 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Button_Switch_SMD:SW_Push_1P1T-MP_NO_Horizontal_Alps_SKRTLAE010"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -2.125 0 90)
			(size 0.9 0.9)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2.125 0 90)
			(size 0.9 0.9)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd roundrect
			(at -1.225 -0.9 90)
			(size 0.75 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" smd roundrect
			(at 1.225 -0.9 90)
			(size 0.75 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0 -0.9 90)
			(size 0.6 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 52 "VOL_DOWN")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -1.85 1.05 90)
			(size 1.3 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
		)
		(pad "MP" smd roundrect
			(at 1.85 1.05 90)
			(size 1.3 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
		)
		(model "/home/justinas/Downloads/alps/SKRTLAE010/SKRTLA.STEP"
			(offset
				(xyz 0 -1 1.7)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_1210_3225Metric"
		(layer "F.Cu")
		(at 119.525 107)
		(descr "Capacitor SMD 1210 (3225 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0 -2.3 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "47uF"
			(at 0 2.3 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_1210_3225Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.475 0)
			(size 1.15 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 4 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.475 0)
			(size 1.15 2.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.217391)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_1210_3225Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-323"
		(layer "F.Cu")
		(at 130.75 146.25 -90)
		(descr "SOD-323")
		(tags "SOD-323")
		(property "Reference" "D2"
			(at 0 -1.85 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1N5819WS"
			(at 0.1 1.9 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:D_SOD-323"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/2204281430_Guangdong-Hottech-1N5819WS_C191023.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*SOD?323*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.85 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.05 0 270)
			(size 0.6 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+5V")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.05 0 270)
			(size 0.6 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D2.0mm"
		(layer "F.Cu")
		(at 120 112)
		(descr "SMD pad as test Point, diameter 2.0mm")
		(tags "test point SMD pad")
		(property "Reference" "COMB"
			(at 0 1.9 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint_Pad_D2.0mm"
			(at 0 2.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D2.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 102 137.92)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "J6"
			(at 0 -2.33 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_01x03_Pin"
			(at 0 7.41 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x03, script generated"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 43 "UART_RX")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 44 "UART_TX")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_SPST_B3U-1000P"
		(layer "F.Cu")
		(at 126.5 80.25 90)
		(descr "Ultra-small-sized Tactile Switch with High Contact Reliability, Top-actuated Model, without Ground Terminal, without Boss")
		(tags "Tactile Switch")
		(property "Reference" "RST1"
			(at 0 -2.5 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_SPST"
			(at 0 2.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Button_Switch_SMD:SW_SPST_B3U-1000P"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0 90)
			(size 0.9 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0 90)
			(size 0.9 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 9 "Net-(RST1-B)")
			(pinfunction "B")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_SPST_B3U-1000P"
		(layer "F.Cu")
		(at 130 80.25 -90)
		(descr "Ultra-small-sized Tactile Switch with High Contact Reliability, Top-actuated Model, without Ground Terminal, without Boss")
		(tags "Tactile Switch")
		(property "Reference" "BOOT1"
			(at -0.25 -2.25 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "BOOT"
			(at 0 2.5 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Button_Switch_SMD:SW_SPST_B3U-1000P"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0 270)
			(size 0.9 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 1 "Net-(BOOT1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0 270)
			(size 0.9 1.7)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "B")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D2.0mm"
		(layer "F.Cu")
		(at 121 129)
		(descr "SMD pad as test Point, diameter 2.0mm")
		(tags "test point SMD pad")
		(property "Reference" "SW1"
			(at 0.1 1.9 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint_Pad_D2.0mm"
			(at 0 2.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D2.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D2.0mm"
		(layer "F.Cu")
		(at 129 123)
		(descr "SMD pad as test Point, diameter 2.0mm")
		(tags "test point SMD pad")
		(property "Reference" "ENCA"
			(at 0.1 2.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint_Pad_D2.0mm"
			(at 0 2.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D2.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D2.0mm"
		(layer "F.Cu")
		(at 105.5 127)
		(descr "SMD pad as test Point, diameter 2.0mm")
		(tags "test point SMD pad")
		(property "Reference" "SW5"
			(at 0 1.9 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint_Pad_D2.0mm"
			(at 0 2.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D2.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 135.25 85.25 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at -2.5 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10K"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 26 "Net-(J1-DAT3{slash}CD)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 111.5 72.5 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C15"
			(at -2 0 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ".1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 121 138.5 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R2"
			(at 2.5 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "5.1K"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 29 "Net-(J2-CC2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 113 92 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at 0 1.5 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10 nF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "BAT_SENSE")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_Push_1P1T-MP_NO_Horizontal_Alps_SKRTLAE010"
		(layer "F.Cu")
		(at 138.25 73.75 90)
		(descr "Side push button (https://www.alps.com/prod/info/E/PDF/Tact/SurfaceMount/SKRT/SKRT.pdf)")
		(tags "push horizontal SPST 1P1T")
		(property "Reference" "SW1"
			(at 3.75 -0.25 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_Push"
			(at 0 2.9 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Button_Switch_SMD:SW_Push_1P1T-MP_NO_Horizontal_Alps_SKRTLAE010"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -2.125 0 90)
			(size 0.9 0.9)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2.125 0 90)
			(size 0.9 0.9)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd roundrect
			(at -1.225 -0.9 90)
			(size 0.75 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" smd roundrect
			(at 1.225 -0.9 90)
			(size 0.75 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0 -0.9 90)
			(size 0.6 1.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 51 "VOL_UP")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "MP" smd roundrect
			(at -1.85 1.05 90)
			(size 1.3 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
		)
		(pad "MP" smd roundrect
			(at 1.85 1.05 90)
			(size 1.3 0.9)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
		)
		(model "/home/justinas/Downloads/alps/SKRTLAE010/SKRTLA.STEP"
			(offset
				(xyz 0 -1 1.7)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D2.0mm"
		(layer "F.Cu")
		(at 137 134.5)
		(descr "SMD pad as test Point, diameter 2.0mm")
		(tags "test point SMD pad")
		(property "Reference" "SW3"
			(at 0 2.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint_Pad_D2.0mm"
			(at 0 2.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D2.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 108.5 95.5)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R13"
			(at 2.325 1 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10K"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 45 "Net-(Q1-G)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3.3V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 114.4 51.6 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at 2.475 -0.01 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
		(layer "F.Cu")
		(at 105.3875 74.625)
		(descr "TSSOP, 20 Pin (JEDEC MO-153 Var AC https://www.jedec.org/document_search?search_api_views_fulltext=MO-153), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "TSSOP SO")
		(property "Reference" "U4"
			(at -0.5 0.25 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "PCM5102A"
			(at 0 4.2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.ti.com/lit/ds/symlink/pcm5102a.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TSSOP*4.4x6.5mm*P0.65mm*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.8625 -2.925)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3.3V")
			(pinfunction "CPVDD")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -2.8625 -2.275)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "Net-(U4-CAPP)")
			(pinfunction "CAPP")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -2.8625 -1.625)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "CPGND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -2.8625 -0.975)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "Net-(U4-CAPM)")
			(pinfunction "CAPM")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at -2.8625 -0.325)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "Net-(U4-VNEG)")
			(pinfunction "VNEG")
			(pintype "passive")
		)
		(pad "6" smd roundrect
			(at -2.8625 0.325)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 48 "Net-(U4-OUTL)")
			(pinfunction "OUTL")
			(pintype "output")
		)
		(pad "7" smd roundrect
			(at -2.8625 0.975)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 49 "Net-(U4-OUTR)")
			(pinfunction "OUTR")
			(pintype "output")
		)
		(pad "8" smd roundrect
			(at -2.8625 1.625)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3.3V")
			(pinfunction "AVDD")
			(pintype "power_in")
		)
		(pad "9" smd roundrect
			(at -2.8625 2.275)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "AGND")
			(pintype "power_in")
		)
		(pad "10" smd roundrect
			(at -2.8625 2.925)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "DEMP")
			(pintype "input")
		)
		(pad "11" smd roundrect
			(at 2.8625 2.925)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "FLT")
			(pintype "input")
		)
		(pad "12" smd roundrect
			(at 2.8625 2.275)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "SCK")
			(pintype "input")
		)
		(pad "13" smd roundrect
			(at 2.8625 1.625)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 58 "I2S_SCLK")
			(pinfunction "BCK")
			(pintype "input")
		)
		(pad "14" smd roundrect
			(at 2.8625 0.975)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 62 "I2S_SD")
			(pinfunction "DIN")
			(pintype "input")
		)
		(pad "15" smd roundrect
			(at 2.8625 0.325)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 60 "I2S_LRCLK")
			(pinfunction "LRCK")
			(pintype "input")
		)
		(pad "16" smd roundrect
			(at 2.8625 -0.325)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "FMT")
			(pintype "input")
		)
		(pad "17" smd roundrect
			(at 2.8625 -0.975)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3.3V")
			(pinfunction "XSMT")
			(pintype "input")
		)
		(pad "18" smd roundrect
			(at 2.8625 -1.625)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "Net-(U4-LDOO)")
			(pinfunction "LDOO")
			(pintype "passive")
		)
		(pad "19" smd roundrect
			(at 2.8625 -2.275)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "DGND")
			(pintype "power_in")
		)
		(pad "20" smd roundrect
			(at 2.8625 -2.925)
			(size 1.475 0.4)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3.3V")
			(pinfunction "DVDD")
			(pintype "power_in")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/TSSOP-20_4.4x6.5mm_P0.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 108.5 93.5)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R10"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10K"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 46 "CHG")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3.3V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 113 72.5 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C23"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 114 65.75 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R18"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10K"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "Net-(RST1-B)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
		(layer "F.Cu")
		(at 119.5 96.5)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal with elongated pad for handsoldering. (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor handsolder")
		(property "Reference" "C1"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ".47uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric_Pad1.08x0.95mm_HandSolder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(BT1-+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.8625 0)
			(size 1.075 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 112.49 65.75 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R19"
			(at -0.25 1.24 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10K"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "Net-(RST1-B)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 114.5 92 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at 2.745 -0.02 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100K"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "BAT_SENSE")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 114 68.75 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C12"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "Net-(RST1-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "ANORotaryEncoder:ANO Rotary Encoder"
		(layer "F.Cu")
		(at 120 128)
		(property "Reference" "Enc1"
			(at 0 -0.5 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "~"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Footprint" "ANORotaryEncoder:ANO Rotary Encoder"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -10.606602 -10.606602 315)
			(size 4 4)
			(drill 4)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -10.606602 10.606602 315)
			(size 4 4)
			(drill 4)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -3.181981 3.181981 315)
			(size 1.6 1.6)
			(drill 1.6)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 3.181981 -3.181981 315)
			(size 1.6 1.6)
			(drill 1.6)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 10.606602 -10.606602 315)
			(size 4 4)
			(drill 4)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 10.606602 10.606602 315)
			(size 4 4)
			(drill 4)
			(layers "F&B.Cu" "*.Mask")
		)
		(pad "A" thru_hole circle
			(at 6.547809 -6.547809 315)
			(size 2.54 2.54)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 18 "ENCA")
			(pinfunction "A")
			(pintype "output")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
		)
		(pad "B" thru_hole circle
			(at 6.547809 6.547809 315)
			(size 2.54 2.54)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 21 "ENCB")
			(pinfunction "B")
			(pintype "output")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
		)
		(pad "COM_A" thru_hole circle
			(at -6.547809 6.547809 315)
			(size 2.54 2.54)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "COM_A")
			(pintype "power_in")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
		)
		(pad "COM_B" thru_hole circle
			(at -3.252691 -16.079608 315)
			(size 2.54 2.54)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "COM_B")
			(pintype "power_in")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
		)
		(pad "S1" thru_hole circle
			(at -1.110158 -1.110158 315)
			(size 2.54 2.54)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 22 "SW1")
			(pinfunction "S1")
			(pintype "output")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
		)
		(pad "S2" thru_hole circle
			(at 7.74989 -15.103801 315)
			(size 2.54 2.54)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 16 "SW2")
			(pinfunction "S2")
			(pintype "output")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
		)
		(pad "S3" thru_hole circle
			(at 16.150319 3.606245 315)
			(size 2.54 2.54)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 19 "SW3")
			(pinfunction "S3")
			(pintype "output")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
		)
		(pad "S4" thru_hole circle
			(at -7.74989 15.103801 315)
			(size 2.54 2.54)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 17 "SW4")
			(pinfunction "S4")
			(pintype "output")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
		)
		(pad "S5" thru_hole circle
			(at -16.150319 -3.606245 315)
			(size 2.54 2.54)
			(drill 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 20 "SW5")
			(pinfunction "S5")
			(pintype "output")
			(solder_mask_margin 0.0508)
			(thermal_bridge_angle 0)
		)
		(model "/home/justinas/JPL.mp3/ANORotaryEncoder.step"
			(offset
				(xyz 0 0 -1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Symbol:OSHW-Logo2_7.3x6mm_SilkScreen"
		(layer "F.Cu")
		(at 135 105)
		(descr "Open Source Hardware Symbol")
		(tags "Logo Symbol OSHW")
		(property "Reference" "REF**"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "OSHW-Logo2_7.3x6mm_SilkScreen"
			(at 0.75 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 105.75 80.5 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C18"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "Net-(U4-VNEG)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 109.3875 80.625 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C21"
			(at -2.75 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ".1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3.3V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 132.25 85.25 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R16"
			(at 2.75 0 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10K"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 27 "SD_CLK")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3.3V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
		(layer "F.Cu")
		(at 109 101 90)
		(descr "SOIC, 8 Pin (JEDEC MS-012AA, https://www.analog.com/media/en/package-pcb-resources/package/pkg_pdf/soic_narrow-r/r_8.pdf), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO")
		(property "Reference" "U2"
			(at -6 0.5 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MAX1811"
			(at 0 3.4 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_SO:SOIC-8_3.9x4.9mm_P1.27mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://datasheets.maximintegrated.com/en/ds/MAX1811.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOIC*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -2.475 -1.905 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+5V")
			(pinfunction "SELV")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -2.475 -0.635 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+5V")
			(pinfunction "SELI")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -2.475 0.635 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "4" smd roundrect
			(at -2.475 1.905 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+5V")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at 2.475 1.905 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(BT1-+)")
			(pinfunction "BATT")
			(pintype "power_out")
		)
		(pad "6" smd roundrect
			(at 2.475 0.635 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "7" smd roundrect
			(at 2.475 -0.635 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+5V")
			(pinfunction "EN")
			(pintype "input")
		)
		(pad "8" smd roundrect
			(at 2.475 -1.905 90)
			(size 1.95 0.6)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 45 "Net-(Q1-G)")
			(pinfunction "~{CHG}")
			(pintype "open_collector")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_3.9x4.9mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 114.5 95 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R6"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100K"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(BT1-+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "BAT_SENSE")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 102.6375 80.5 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C19"
			(at 2.725 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ".1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3.3V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 112.5 68.75 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C13"
			(at 0 1.25 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "Net-(RST1-B)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 133 80.025 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at 0 -3 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Net-(BOOT1-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_SPDT_PCM12"
		(layer "F.Cu")
		(at 101.97 63.65 -90)
		(descr "Ultraminiature Surface Mount Slide Switch, right-angle, https://www.ckswitches.com/media/1424/pcm.pdf")
		(property "Reference" "SL2"
			(at 0 -3.2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "HOLD"
			(at 0 4.25 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Button_Switch_SMD:SW_SPDT_PCM12"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -3.2 90)
			(layer "F.Fab")
		)
		(pad "" smd rect
			(at -3.65 -0.78 270)
			(size 1 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "" smd rect
			(at -3.65 1.43 270)
			(size 1 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "" np_thru_hole circle
			(at -1.5 0.33 270)
			(size 0.9 0.9)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 1.5 0.33 270)
			(size 0.9 0.9)
			(drill 0.9)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" smd rect
			(at 3.65 -0.78 270)
			(size 1 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "" smd rect
			(at 3.65 1.43 270)
			(size 1 0.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(pad "1" smd rect
			(at -2.25 -1.43 270)
			(size 0.7 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 50 "HOLD")
			(pinfunction "A")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.75 -1.43 270)
			(size 0.7 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "B")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 2.25 -1.43 270)
			(size 0.7 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
		)
		(model "${KICAD8_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPDT_PCM12.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 113 75.5 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C16"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "Net-(U4-LDOO)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D2.0mm"
		(layer "F.Cu")
		(at 109.5 144)
		(descr "SMD pad as test Point, diameter 2.0mm")
		(tags "test point SMD pad")
		(property "Reference" "SW4"
			(at -0.1 2.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint_Pad_D2.0mm"
			(at 0 2.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D2.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 118.25 91.25 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R12"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 38 "Net-(J4-Pin_10)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 129.25 85.25 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at 2 -0.75 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10K"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "Net-(J1-DAT1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3.3V")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 106.25 65.75 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2nF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "AUDIO_LEFT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 109.25 65.75)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 2.525 0.25 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2nF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "AUDIO_RIGHT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
		(layer "F.Cu")
		(at 119.5 101.3)
		(descr "module CMS SOT223 4 pins")
		(tags "CMS SOT")
		(property "Reference" "U5"
			(at 3 -3.8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LT1963AxST-3.3"
			(at 0 4.5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Package_TO_SOT_SMD:SOT-223-3_TabPin2"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.analog.com/media/en/technical-documentation/data-sheets/1963aff.pdf"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "3.3V, 1.5A, Low Noise, Fast Transient Response LDO Regulator, SOT-223"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT*223*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.15 -2.3)
			(size 2 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(BT1-+)")
			(pinfunction "IN")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -3.15 0)
			(size 2 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at 3.15 0)
			(size 2 3.8)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -3.15 2.3)
			(size 2 1.5)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3.3V")
			(pinfunction "OUT")
			(pintype "power_out")
		)
		(model "${KICAD8_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-223.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 113 99.5 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2 uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(BT1-+)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D2.0mm"
		(layer "F.Cu")
		(at 126.5 137.5)
		(descr "SMD pad as test Point, diameter 2.0mm")
		(tags "test point SMD pad")
		(property "Reference" "ENCB"
			(at 0.1 2.2 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint_Pad_D2.0mm"
			(at 0 2.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D2.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D2.0mm"
		(layer "F.Cu")
		(at 125 114)
		(descr "SMD pad as test Point, diameter 2.0mm")
		(tags "test point SMD pad")
		(property "Reference" "SW2"
			(at 0.2 2 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint_Pad_D2.0mm"
			(at 0 2.05 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_Pad_D2.0mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 0 -2 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 2 2)
			(layers "F.Cu" "F.Mask")
		)
	)
	(footprint "TestPoint:TestPoint_2Pads_Pitch2.54mm_Drill0.8mm"
		(layer "F.Cu")
		(at 133.5 142.5)
		(descr "Test point with 2 pins, pitch 2.54mm, drill diameter 0.8mm")
		(tags "CONN DEV")
		(property "Reference" "BAT"
			(at 1.3 -1.75 0)
			(layer "F.SilkS")
		)
		(property "Value" "TestPoint_2Pads_Pitch2.54mm_Drill0.8mm"
			(at 1.27 2 0)
			(layer "F.Fab")
		)
		(property "Footprint" "TestPoint:TestPoint_2Pads_Pitch2.54mm_Drill0.8mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(attr exclude_from_pos_files exclude_from_bom)
		(fp_text user "${REFERENCE}"
			(at 1.3 -2 0)
			(layer "F.Fab")
		)
		(pad "" thru_hole circle
			(at 0 0)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 3 "Net-(BT1-+)")
		)
		(pad "2" thru_hole circle
			(at 2.54 0)
			(size 1.4 1.4)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
		)
	)
	(footprint "Diode_SMD:D_SOD-323"
		(layer "F.Cu")
		(at 123.5 138.25 -90)
		(descr "SOD-323")
		(tags "SOD-323")
		(property "Reference" "D1"
			(at 0 -1.85 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1N5819WS"
			(at 0.1 1.9 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Diode_SMD:D_SOD-323"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/lcsc/2204281430_Guangdong-Hottech-1N5819WS_C191023.pdf"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*SOD?323*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.85 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.05 0 270)
			(size 0.6 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "+5V")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.05 0 270)
			(size 0.6 0.45)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-323.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 136.75 85.25 -90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R9"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10K"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 270)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 28 "Net-(J1-DAT2)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 108.5 68.025 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R5"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "470"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 49 "Net-(U4-OUTR)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "AUDIO_RIGHT")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_USB:USB_C_Receptacle_G-Switch_GT-USB-7010ASV"
		(layer "F.Cu")
		(at 120 147)
		(descr "USB Type C, right-angle, SMT, https://datasheet.lcsc.com/lcsc/2204071530_G-Switch-GT-USB-7010ASV_C2988369.pdf")
		(tags "USB C Type-C Receptacle SMD")
		(property "Reference" "J2"
			(at 0 -5.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USB_C"
			(at 0 5 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Connector_USB:USB_C_Receptacle_G-Switch_GT-USB-7010ASV"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "https://www.usb.org/sites/default/files/documents/usb_type-c.zip"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "USB*C*Receptacle*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -2.89 -2.605)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2.89 -2.605)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
		)
		(pad "A1" smd rect
			(at -3.2 -3.725)
			(size 0.6 1.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "A4" smd rect
			(at -2.4 -3.725)
			(size 0.6 1.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "Net-(D1-A)")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "A5" smd rect
			(at -1.25 -3.725)
			(size 0.3 1.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 31 "Net-(J2-CC1)")
			(pinfunction "CC1")
			(pintype "bidirectional")
		)
		(pad "A6" smd rect
			(at -0.25 -3.725)
			(size 0.3 1.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "USB_D+")
			(pinfunction "D+")
			(pintype "bidirectional")
		)
		(pad "A7" smd rect
			(at 0.25 -3.725)
			(size 0.3 1.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "USB_D-")
			(pinfunction "D-")
			(pintype "bidirectional")
		)
		(pad "A8" smd rect
			(at 1.25 -3.725)
			(size 0.3 1.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 34 "unconnected-(J2-SBU1-PadA8)")
			(pinfunction "SBU1")
			(pintype "bidirectional+no_connect")
		)
		(pad "A9" smd rect
			(at 2.4 -3.725)
			(size 0.6 1.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "Net-(D1-A)")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "A12" smd rect
			(at 3.2 -3.725)
			(size 0.6 1.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "B1" smd rect
			(at 3.2 -3.725)
			(size 0.6 1.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "B4" smd rect
			(at 2.4 -3.725)
			(size 0.6 1.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "Net-(D1-A)")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "B5" smd rect
			(at 1.75 -3.725)
			(size 0.3 1.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 29 "Net-(J2-CC2)")
			(pinfunction "CC2")
			(pintype "bidirectional")
		)
		(pad "B6" smd rect
			(at 0.75 -3.725)
			(size 0.3 1.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 30 "USB_D+")
			(pinfunction "D+")
			(pintype "bidirectional")
		)
		(pad "B7" smd rect
			(at -0.75 -3.725)
			(size 0.3 1.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 32 "USB_D-")
			(pinfunction "D-")
			(pintype "bidirectional")
		)
		(pad "B8" smd rect
			(at -1.75 -3.725)
			(size 0.3 1.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 33 "unconnected-(J2-SBU2-PadB8)")
			(pinfunction "SBU2")
			(pintype "bidirectional+no_connect")
		)
		(pad "B9" smd rect
			(at -2.4 -3.725)
			(size 0.6 1.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 14 "Net-(D1-A)")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "B12" smd rect
			(at -3.2 -3.725)
			(size 0.6 1.24)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(net 2 "GND")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at -4.32 -3.125)
			(size 1 2.1)
			(drill oval 0.6 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at -4.32 1.075)
			(size 1 1.8)
			(drill oval 0.6 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at 4.32 -3.125)
			(size 1 2.1)
			(drill oval 0.6 1.7)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at 4.32 1.075)
			(size 1 1.8)
			(drill oval 0.6 1.4)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "GND")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_GCT_USB4105-xx-A_16P_TopMnt_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 102.8875 69.625)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C17"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "Net-(U4-CAPP)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "Net-(U4-CAPM)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 102.6375 82)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 0 1.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0603_1608Metric"
		(layer "F.Cu")
		(at 107 68.025 90)
		(descr "Resistor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at 0.125 1.5875 -90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "470"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Resistor_SMD:R_0603_1608Metric"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 48 "Net-(U4-OUTL)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.825 0 90)
			(size 0.8 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "AUDIO_LEFT")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 114.4 53.1 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at 0 -2.5 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ".1uF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 111.5 75.5 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 2.75 -0.25 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" ".1uF"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Footprint" "Capacitor_SMD:C_0603_1608Metric"
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 -90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Paste" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "Net-(U4-LDOO)")
			(pintype "passive")
		)
		(model "${KICAD8_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_FFC-FPC:TE_1-1734839-2_1x12-1MP_P0.5mm_Horizontal"
		(layer "B.Cu")
		(at 119.9 90 180)
		(descr "TE FPC connector, 12 top-side contacts, 0.5mm pitch, SMT, https://www.te.com/commerce/DocumentDelivery/DDEController?Action=showdoc&DocId=Customer+Drawing%7F1734839%7FC%7Fpdf%7FEnglish%7FENG_CD_1734839_C_C_1734839.pdf%7F4-1734839-0")
		(tags "te fpc 1734839")
		(property "Reference" "J4"
			(at 0 3.1 0)
			(layer "B.SilkS")
		)
		(property "Value" "Conn_01x12"
			(at 0 -3.25 0)
			(layer "Dwgs.User")
		)
		(property "Footprint" "Connector_FFC-FPC:TE_1-1734839-2_1x12-1MP_P0.5mm_Horizontal"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "Root")
		(sheetfile "JPL.mp3.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -1.55 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -2.75 1.35 180)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "GND")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2.25 1.35 180)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 39 "TFT_CS")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.75 1.35 180)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 35 "TFT_DC")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.25 1.35 180)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 42 "TFT_SCLK")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -0.75 1.35 180)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 40 "TFT_SDA")
			(pinfunction "Pin_5")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -0.25 1.35 180)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 36 "TFT_RST")
			(pinfunction "Pin_6")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.25 1.35 180)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 37 "unconnected-(J4-Pin_7-Pad7)")
			(pinfunction "Pin_7")
			(pintype "passive+no_connect")
		)
		(pad "8" smd rect
			(at 0.75 1.35 180)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 4 "+3.3V")
			(pinfunction "Pin_8")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 1.25 1.35 180)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 4 "+3.3V")
			(pinfunction "Pin_9")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 1.75 1.35 180)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 38 "Net-(J4-Pin_10)")
			(pinfunction "Pin_10")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at 2.25 1.35 180)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 41 "Net-(J4-Pin_11)")
			(pinfunction "Pin_11")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at 2.75 1.35 180)
			(size 0.3 1.1)
			(layers "B.Cu" "B.Paste" "B.Mask")
			(net 2 "GND")
			(pinfunction "Pin_12")
			(pintype "passive")
		)
		(pad "MP" smd rect
			(at -4.42 -0.35 180)
			(size 2.3 3.1)
			(layers "B.Cu" "B.Paste" "B.Mask")
		)
		(pad "MP" smd rect
			(at 4.42 -0.35 180)
			(size 2.3 3.1)
			(layers "B.Cu" "B.Paste" "B.Mask")
		)
		(model "${KICAD8_3DMODEL_DIR}/Connector_FFC-FPC.3dshapes/TE_1-1734839-2_1x12-1MP_P0.5mm_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "/home/justinas/Downloads/TEfpc/c-1-1734592-2-c-3d.stp"
			(offset
				(xyz 0 -3.5 1)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 0 0)
			)
		)
	)
	(footprint "footprints:JPL"
		(layer "B.Cu")
		(at 132.75 58.8 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Footprint" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
	)
	(gr_arc
		(start 140 147.5)
		(mid 139.267767 149.267767)
		(end 137.5 150)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 137.5 52.5)
		(end 136.5 52.5)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 102.5 52.5)
		(end 103.5 52.5)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 100 52.5)
		(mid 100.732233 50.732233)
		(end 102.5 50)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 137.5 147.5)
		(end 138.5 147.5)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 102.5 150)
		(mid 100.732233 149.267767)
		(end 100 147.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 100 147.5)
		(end 100 52.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 140 52.5)
		(end 140 147.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 102.5 50)
		(end 137.5 50)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 137.5 150)
		(end 102.5 150)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 102.5 147.5)
		(end 101.5 147.5)
		(fill none)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 137.5 50)
		(mid 139.267767 50.732233)
		(end 140 52.5)
		(layer "Edge.Cuts")
	)
	(gr_text "GND"
		(at 104.75 143 0)
		(layer "F.SilkS")
	)
	(gr_text "BOOT"
		(at 128.25 83.75 0)
		(layer "F.SilkS")
	)
	(gr_text "RX"
		(at 104.75 138 0)
		(layer "F.SilkS")
	)
	(gr_text "JPL.mp3\n0.1.3.A\n1/2025"
		(at 134.9 112.6 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "TX"
		(at 104.75 140.5 0)
		(layer "F.SilkS")
	)
	(gr_text "+ -"
		(at 133 145.25 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "RST"
		(at 125.25 83.75 0)
		(layer "F.SilkS")
	)
	(dimension
		(type aligned)
		(layer "Cmts.User")
		(pts
			(xy 102 140.445) (xy 100 140.43)
		)
		(height 0.804923)
		(gr_text "2.0001 mm"
			(at 101.014662 138.482632 -0.4297102894)
			(layer "Cmts.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Cmts.User")
		(pts
			(xy 130 80.25) (xy 140 80.3)
		)
		(height 3.162586)
		(gr_text "10.0001 mm"
			(at 134.989937 82.28756 359.7135235)
			(layer "Cmts.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Cmts.User")
		(pts
			(xy 102 140.445) (xy 102 150)
		)
		(height 2.5)
		(gr_text "9.5550 mm"
			(at 98.35 145.2225 90)
			(layer "Cmts.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Cmts.User")
		(pts
			(xy 126.5 80.25) (xy 140 80.3)
		)
		(height 4.998663)
		(gr_text "13.5001 mm"
			(at 133.235746 84.123637 359.7877944)
			(layer "Cmts.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(dimension
		(type aligned)
		(layer "Cmts.User")
		(pts
			(xy 126.5 80.25) (xy 126.6 50)
		)
		(height 17.122721)
		(gr_text "30.2502 mm"
			(at 142.522633 65.177802 89.81059315)
			(layer "Cmts.User")
		)
		(format
			(prefix "")
			(suffix "")
			(units 3)
			(units_format 1)
			(precision 4)
		)
		(style
			(thickness 0.1)
			(arrow_length 1.27)
			(text_position_mode 0)
			(extension_height 0.58642)
			(extension_offset 0.5) keep_text_aligned)
	)
	(zone
		(net 0)
		(net_name "")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks allowed)
			(vias allowed)
			(pads allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 2)
			(island_area_min 5)
		)
		(polygon
			(pts
				(xy 104 78) (xy 103.75 78.75) (xy 108.25 81.25) (xy 108.75 80.5) (xy 105 77) (xy 104 77)
			)
		)
	)
	(zone
		(net 2)
		(net_name "GND")
		(layers "F.Cu" "In1.Cu" "In2.Cu")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 2)
			(island_area_min 5)
		)
		(polygon
			(pts
				(xy 96.5 45.25) (xy 144.75 44.75) (xy 144.5 153.5) (xy 95.75 154.25)
			)
		)
	)
	(zone
		(net 0)
		(net_name "")
		(layers "F.Cu" "In1.Cu" "In2.Cu" "B.Cu" "Cmts.User")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(keepout
			(tracks not_allowed)
			(vias not_allowed)
			(pads not_allowed)
			(copperpour not_allowed)
			(footprints allowed)
		)
		(fill
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 116.4 50) (xy 134.9 50) (xy 134.9 56.2) (xy 116.4 56.2)
			)
		)
	)
	(zone
		(net 4)
		(net_name "+3.3V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 94 43) (xy 146.25 43.25) (xy 147.75 156) (xy 93 156.25)
			)
		)
	)
)
