(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "Gerbers/")
		)
	)
	(net 0 "")
	(net 1 "Earth")
	(net 2 "Net-(AE1-A)")
	(net 3 "Net-(DD1-XC2)")
	(net 4 "Net-(DD1-XC1)")
	(net 5 "Net-(DD1-DVDD)")
	(net 6 "3.3V")
	(net 7 "VDD_PA")
	(net 8 "Net-(C7-Pad1)")
	(net 9 "Net-(DA1-TXRX)")
	(net 10 "Net-(DA1-ANT)")
	(net 11 "Net-(C16-Pad1)")
	(net 12 "Net-(DD3-DVDD_1)")
	(net 13 "Net-(DD3-ADC_AVDD)")
	(net 14 "Net-(DD3-XOUT)")
	(net 15 "Net-(DD3-XIN)")
	(net 16 "VCC-5V")
	(net 17 "Net-(D1-A)")
	(net 18 "Net-(D2-A)")
	(net 19 "Net-(D3-A)")
	(net 20 "unconnected-(DA1-N{slash}C_4-Pad15)")
	(net 21 "unconnected-(DA1-DNC-Pad13)")
	(net 22 "Net-(DA1-TXEN)")
	(net 23 "unconnected-(DA1-N{slash}C_1-Pad1)")
	(net 24 "unconnected-(DA1-VDD_1-Pad14)")
	(net 25 "Net-(DA1-RXEN)")
	(net 26 "unconnected-(DA1-N{slash}C_2-Pad7)")
	(net 27 "unconnected-(DA1-N{slash}C_3-Pad12)")
	(net 28 "SPI_MOSI")
	(net 29 "NRF_CE")
	(net 30 "NRF_CS")
	(net 31 "SPI_SCK")
	(net 32 "SPI_MISO")
	(net 33 "Net-(DD1-ANT1)")
	(net 34 "NRF_IRQ")
	(net 35 "Net-(DD1-ANT2)")
	(net 36 "Net-(DD1-IREF)")
	(net 37 "QSPI_SD0")
	(net 38 "QSPI_SD1")
	(net 39 "QSPI_SD3")
	(net 40 "QSPI_SS")
	(net 41 "QSPI_SD2")
	(net 42 "unconnected-(DD2-EP-Pad9)")
	(net 43 "QSPI_SCLK")
	(net 44 "Net-(DD3-SWCLK)")
	(net 45 "unconnected-(DD3-GPIO34-Pad43)")
	(net 46 "unconnected-(DD3-GPIO43_ADC3-Pad54)")
	(net 47 "unconnected-(DD3-GPIO38-Pad47)")
	(net 48 "Net-(DD3-SWDIO)")
	(net 49 "LED1")
	(net 50 "Net-(DD3-VREG_LX)")
	(net 51 "unconnected-(DD3-GPIO44_ADC4-Pad55)")
	(net 52 "unconnected-(DD3-GPIO46_ADC6-Pad57)")
	(net 53 "unconnected-(DD3-GPIO41_ADC1-Pad52)")
	(net 54 "unconnected-(DD3-GPIO36-Pad45)")
	(net 55 "unconnected-(DD3-GPIO42_ADC2-Pad53)")
	(net 56 "unconnected-(DD3-GPIO33-Pad42)")
	(net 57 "unconnected-(DD3-GPIO39-Pad48)")
	(net 58 "unconnected-(DD3-GPIO0-Pad77)")
	(net 59 "RUN")
	(net 60 "unconnected-(DD3-GPIO45_ADC5-Pad56)")
	(net 61 "unconnected-(DD3-GPIO37-Pad46)")
	(net 62 "LED2")
	(net 63 "unconnected-(DD3-GPIO47_ADC7-Pad58)")
	(net 64 "unconnected-(DD3-GPIO1-Pad78)")
	(net 65 "USB_R+")
	(net 66 "unconnected-(DD3-GPIO2-Pad79)")
	(net 67 "unconnected-(DD3-GPIO35-Pad44)")
	(net 68 "USB_R-")
	(net 69 "unconnected-(DD3-GPIO40_ADC0-Pad49)")
	(net 70 "unconnected-(DD4-FB-Pad2)")
	(net 71 "unconnected-(DD4-NC-Pad5)")
	(net 72 "Net-(R10-Pad2)")
	(net 73 "Net-(R11-Pad2)")
	(net 74 "USB_ESD+")
	(net 75 "USB_ESD-")
	(net 76 "USB_Conn+")
	(net 77 "USB_Conn-")
	(net 78 "Net-(DD3-GPIO19)")
	(net 79 "Net-(DD3-GPIO21)")
	(net 80 "unconnected-(DD3-GPIO5-Pad2)")
	(net 81 "unconnected-(DD3-GPIO9-Pad7)")
	(net 82 "unconnected-(DD3-GPIO7-Pad4)")
	(net 83 "unconnected-(DD3-GPIO13-Pad12)")
	(net 84 "Net-(DD3-GPIO20)")
	(net 85 "unconnected-(DD3-GPIO14-Pad13)")
	(net 86 "unconnected-(DD3-GPIO8-Pad6)")
	(net 87 "Net-(DD3-GPIO22)")
	(net 88 "unconnected-(DD3-GPIO11-Pad9)")
	(net 89 "unconnected-(DD3-GPIO6-Pad3)")
	(net 90 "Net-(DD3-GPIO23)")
	(net 91 "unconnected-(DD3-GPIO16-Pad16)")
	(net 92 "unconnected-(DD3-GPIO12-Pad11)")
	(net 93 "unconnected-(DD3-GPIO10-Pad8)")
	(net 94 "unconnected-(DD3-GPIO15-Pad14)")
	(net 95 "unconnected-(DD3-GPIO4-Pad1)")
	(net 96 "unconnected-(DD3-GPIO3-Pad80)")
	(net 97 "Net-(DD3-GPIO25)")
	(net 98 "Net-(DD3-GPIO24)")
	(net 99 "Net-(DD3-GPIO26)")
	(footprint "PCM_Resistor_SMD_AKL:R_0201_0603Metric"
		(layer "F.Cu")
		(at 199.2 119.7 -90)
		(descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R11"
			(at 0 -1.1176 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1K"
			(at 0 1.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.4 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 40 "QSPI_SS")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 73 "Net-(R11-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 214.6 122.6)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP6"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 98 "Net-(DD3-GPIO24)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 200.2 121.4 -90)
		(property "Reference" "G***"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 206 122.1 -90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C25"
			(at 0 -1.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10nF"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "Net-(DD3-DVDD_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-6"
		(layer "F.Cu")
		(at 195.823301 114.145001 180)
		(descr "SOT, 6 Pin (JEDEC MO-178 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U1"
			(at 0 -2.4 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "USBLC6-2SC6"
			(at 0 2.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/usblc6-2.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Very low capacitance ESD protection diode, 2 data-line, SOT-23-6"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 74 "USB_ESD+")
			(pinfunction "I/O1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "USB_ESD-")
			(pinfunction "I/O2")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 77 "USB_Conn-")
			(pinfunction "I/O2")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at 1.1375 0 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "VCC-5V")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "6" smd roundrect
			(at 1.1375 -0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 76 "USB_Conn+")
			(pinfunction "I/O1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0201_0603Metric"
		(layer "F.Cu")
		(at 199.559428 110.062728 180)
		(descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R10"
			(at 0 -1.1176 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1K"
			(at 0 1.05 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.4 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 59 "RUN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 72 "Net-(R10-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 218 111.4)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C45"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7uF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 220.526466 119.399399 180)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1nF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_SPST_PTS810"
		(layer "F.Cu")
		(at 196 110.5)
		(descr "C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, http://www.ckswitches.com/media/1476/pts810.pdf")
		(tags "SPST Button Switch")
		(property "Reference" "SW1"
			(at 0 -2.6 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "KMR221GLFS"
			(at 0 2.6 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Earth")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" smd rect
			(at 2.075 -1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Earth")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "Net-(R10-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.075 1.075)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "Net-(R10-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_PTS810.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 223.8 114 90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at 0 -1.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1.5pF"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.680001 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345001 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345001 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.319999 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "Net-(C7-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.319999 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "Net-(DA1-TXRX)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 192.3 112.98 180)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C43"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7uF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "VCC-5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0201_0603Metric"
		(layer "F.Cu")
		(at 199.183612 114.490734 180)
		(descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R13"
			(at 0 -1.1176 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "27R"
			(at 0 1.05 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.4 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 65 "USB_R+")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 74 "USB_ESD+")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 220.52 120.1 180)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "33nF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 5 "Net-(DD1-DVDD)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 193 118.7 180)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C19"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7uF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0201_0603Metric"
		(layer "F.Cu")
		(at 224.504005 115.420045 90)
		(descr "Inductor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L3"
			(at 0 -1.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.7nH"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "Net-(DD1-ANT1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "VDD_PA")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 213.2 112.4 -90)
		(property "Reference" "G***"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0201_0603Metric"
		(layer "F.Cu")
		(at 227.78 113.6)
		(descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R7"
			(at 0 -1.1176 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "20K"
			(at 0 1.05 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.4 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "Net-(DA1-RXEN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0402_1005Metric"
		(layer "F.Cu")
		(at 219.8 109.815 -90)
		(descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D3"
			(at 0 -1.17 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED 0402"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 270)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.485 0 270)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 19 "Net-(D3-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 206.5 109.3 90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C21"
			(at 0 -1.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7uF"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "Net-(DD3-DVDD_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 220.9 114.9 -90)
		(property "Reference" "G***"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 201.3 109.3 90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C30"
			(at 0 -1.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 218.6 115.1 90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C29"
			(at 0 -1.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "22pF"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "Net-(DD3-XOUT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 214.9 119.8)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP7"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 97 "Net-(DD3-GPIO25)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm"
		(layer "F.Cu")
		(at 229 118.9 90)
		(descr "SMD3225/4, Crystal, 3.2x2.5mm package, SMD, generated with kicad-footprint-generator make_crystal.py, http://www.txccrystal.com/images/pdf/7m-accuracy.pdf")
		(property "Reference" "Y1"
			(at 0 -2.45 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "16MHz"
			(at 0 2.45 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Four pin crystal, GND on pins 2 and 4"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Crystal*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1 0.85 90)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 3 "Net-(DD1-XC2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.1 0.85 90)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "Earth")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.1 -0.85 90)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 4 "Net-(DD1-XC1)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -1.1 -0.85 90)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "Earth")
			(pinfunction "4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 225.562722 115.061326)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7pF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "VDD_PA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0201_0603Metric"
		(layer "F.Cu")
		(at 221.5 111.515 90)
		(descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R3"
			(at 0 -1.1176 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1K"
			(at 0 1.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.4 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 62 "LED2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 17 "Net-(D1-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 202 109.3 90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C33"
			(at 0 -1.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7uF"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 223.2 110.7 180)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C14"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "220pF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 214.9 118.4)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP8"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 99 "Net-(DD3-GPIO26)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 211.4 122.6)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP2"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 84 "Net-(DD3-GPIO20)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 225.562722 115.761326)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.2nF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "VDD_PA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 216 122.6 90)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP10"
			(at 0 -1.448 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 90)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0 90)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 44 "Net-(DD3-SWCLK)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 207.2 109.3 90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C28"
			(at 0 -1.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "BCT2057ELTAJ:BCT2057ELTAJ"
		(layer "F.Cu")
		(at 216.2 110 90)
		(property "Reference" "DD4"
			(at -0.069875 -2.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "BCT2057ELT33"
			(at -0.069875 2.247 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://item.szlcsc.com/datasheet/BCT2057ELTAJ-TR/3451387.html"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Output Type:Adjustable Voltage - Supply:5.5V Output Voltage:800mV~5V Output Voltage:800mV~5V Output Current:1A Power Supply Rejection Ratio (PSRR):65dB@(1kHz) Voltage Dropout:350mV@(1A) standby current:100uA Features:Over Current Protection；Enable；Over Te"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part" "BCT2057ELTAJ-TR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "BROADCHIP(广芯电子)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier Part" "C2990820"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "LCSC"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC Part Name" "1A, 低 dropout 线性稳压器"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(pad "0" smd rect
			(at 0.0005 0 90)
			(size 1.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Earth")
			(pinfunction "EP")
			(pintype "unspecified")
		)
		(pad "1" smd rect
			(at -0.65 1 90)
			(size 0.35 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "3.3V")
			(pinfunction "OUT")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 0.0005 1 90)
			(size 0.35 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 70 "unconnected-(DD4-FB-Pad2)")
			(pinfunction "FB")
			(pintype "unspecified+no_connect")
		)
		(pad "3" smd rect
			(at 0.65 1 90)
			(size 0.35 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Earth")
			(pinfunction "GND")
			(pintype "unspecified")
		)
		(pad "4" smd rect
			(at 0.65 -1 90)
			(size 0.35 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "VCC-5V")
			(pinfunction "EN")
			(pintype "unspecified")
		)
		(pad "5" smd rect
			(at 0 -1 90)
			(size 0.35 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 71 "unconnected-(DD4-NC-Pad5)")
			(pinfunction "NC")
			(pintype "unspecified")
		)
		(pad "6" smd rect
			(at -0.65 -1 90)
			(size 0.35 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "VCC-5V")
			(pinfunction "IN")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/DFN-6-1EP_2x2mm_P0.65mm_EP1x1.6mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -90)
			)
		)
	)
	(footprint "LED_SMD:LED_0402_1005Metric"
		(layer "F.Cu")
		(at 220.8 109.815 -90)
		(descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D2"
			(at 0 -1.17 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED 0402"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 270)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.485 0 270)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 192.62 111.88 90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C41"
			(at 0 -1.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "VCC-5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0201_0603Metric"
		(layer "F.Cu")
		(at 226.38 113.6)
		(descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R6"
			(at 0 -1.1176 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1K"
			(at 0 1.05 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.4 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 29 "NRF_CE")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 25 "Net-(DA1-RXEN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 230.41768 112.044984)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C16"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1.5pF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "Net-(C16-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 230.42113 110.590132)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C18"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1.5pF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "Net-(C16-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 228.9 116.4)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "22pF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "Net-(DD1-XC1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 213.7 121.5)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP5"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 90 "Net-(DD3-GPIO23)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0201_0603Metric"
		(layer "F.Cu")
		(at 220.8 111.515 90)
		(descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R4"
			(at 0 -1.1176 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1K"
			(at 0 1.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.4 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 49 "LED1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 18 "Net-(D2-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0201_0603Metric"
		(layer "F.Cu")
		(at 230.42 111.3)
		(descr "Inductor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L5"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.4nH"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "Net-(C16-Pad1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "Net-(AE1-A)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 217.9 120 -90)
		(property "Reference" "G***"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 231.5 111.62 -90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C20"
			(at 0 -1.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1.5pF"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "Net-(AE1-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 218.6 116.8 -90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C36"
			(at 0 -1.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "22pF"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "Net-(DD3-XIN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_SPST_PTS810"
		(layer "F.Cu")
		(at 196 121.1 180)
		(descr "C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, http://www.ckswitches.com/media/1476/pts810.pdf")
		(tags "SPST Button Switch")
		(property "Reference" "SW2"
			(at 0 -2.6 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "KMR221GLFS"
			(at 0 2.6 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.075 -1.075 180)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Earth")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" smd rect
			(at 2.075 -1.075 180)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Earth")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2.075 1.075 180)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 73 "Net-(R11-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.075 1.075 180)
			(size 1.05 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 73 "Net-(R11-Pad2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_PTS810.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 229.01768 112.044984)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C13"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1.5pF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "Net-(DA1-ANT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 217.4 122.6 90)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP9"
			(at 0 -1.448 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 90)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0 90)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 48 "Net-(DD3-SWDIO)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 215.2 111.4 180)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C40"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7uF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "VCC-5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 229.019214 110.58942)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.3pF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "Net-(DA1-ANT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0201_0603Metric"
		(layer "F.Cu")
		(at 220.1 111.515 90)
		(descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R8"
			(at 0 -1.1176 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1K"
			(at 0 1.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.4 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 19 "Net-(D3-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 222.68 116.4)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7uF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm"
		(layer "F.Cu")
		(at 216.1 115.95)
		(descr "SMD3225/4, Crystal, 3.2x2.5mm package, SMD, generated with kicad-footprint-generator make_crystal.py, http://www.txccrystal.com/images/pdf/7m-accuracy.pdf")
		(property "Reference" "Y2"
			(at 0 -2.45 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "16MHz"
			(at 0 2.45 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Four pin crystal, GND on pins 2 and 4"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Crystal*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1 0.85)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 15 "Net-(DD3-XIN)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.1 0.85)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "Earth")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 1.1 -0.85)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 14 "Net-(DD3-XOUT)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -1.1 -0.85)
			(size 1.4 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.208333)
			(net 1 "Earth")
			(pinfunction "4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0201_0603Metric"
		(layer "F.Cu")
		(at 226.9 118.7 90)
		(descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 -1.1176 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1M"
			(at 0 1.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.4 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(DD1-XC2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 4 "Net-(DD1-XC1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 200.1 118.42 -90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C34"
			(at 0 -1.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7uF"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0603_1608Metric"
		(layer "F.Cu")
		(at 204.6 109.3 180)
		(descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L6"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "VHF160808H33NJT"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "3.3V")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "Net-(DD3-ADC_AVDD)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 212.8 122.6)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP4"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 87 "Net-(DD3-GPIO22)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 193 118 180)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C17"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0201_0603Metric"
		(layer "F.Cu")
		(at 223.8 115.42 90)
		(descr "Inductor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L2"
			(at 0 -1.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "3.9nH"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 35 "Net-(DD1-ANT2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 8 "Net-(C7-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 214.1 110.3 -90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C39"
			(at 0 -1.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7uF"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "VCC-5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 218.4 110 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C44"
			(at 0 -1.16 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "22uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "RFX2401C:RFX2401C"
		(layer "F.Cu")
		(at 226.1 111.05)
		(descr "QFN16(H=0.6mm)")
		(tags "Integrated Circuit")
		(property "Reference" "DA1"
			(at 0.125 -2.8 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "RFX2401C"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://eu.mouser.com/datasheet/2/472/RFX2401C_204359B-1524606.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "RF Front End 2.4GHz ZigBee/ISM RFeIC PA+LNA+SPDT"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Skyworks"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "RFX2401C"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "477-RFX2401C"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Skyworks-Solutions-Inc/RFX2401C?qs=dBWc1juS%252B3ydEXrKsuxQ7A%3D%3D"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" "RFX2401C"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/rfx2401c/skyworks-solutions?utm_currency=USD&region=nac"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.025 -0.025 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.5 -0.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 23 "unconnected-(DA1-N{slash}C_1-Pad1)")
			(pinfunction "N/C_1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.5 -0.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Earth")
			(pinfunction "GND_1")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.5 0.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Earth")
			(pinfunction "GND_2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.5 0.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "Net-(DA1-TXRX)")
			(pinfunction "TXRX")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -0.75 1.5)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "Net-(DA1-TXEN)")
			(pinfunction "TXEN")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -0.25 1.5)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 25 "Net-(DA1-RXEN)")
			(pinfunction "RXEN")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 0.25 1.5)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 26 "unconnected-(DA1-N{slash}C_2-Pad7)")
			(pinfunction "N/C_2")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 0.75 1.5)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Earth")
			(pinfunction "GND_3")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 1.5 0.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Earth")
			(pinfunction "GND_4")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 1.5 0.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 10 "Net-(DA1-ANT)")
			(pinfunction "ANT")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at 1.5 -0.25 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Earth")
			(pinfunction "GND_5")
			(pintype "passive")
		)
		(pad "12" smd rect
			(at 1.5 -0.75 90)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 27 "unconnected-(DA1-N{slash}C_3-Pad12)")
			(pinfunction "N/C_3")
			(pintype "passive")
		)
		(pad "13" smd rect
			(at 0.75 -1.5)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 21 "unconnected-(DA1-DNC-Pad13)")
			(pinfunction "DNC")
			(pintype "passive")
		)
		(pad "14" smd rect
			(at 0.25 -1.5)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 24 "unconnected-(DA1-VDD_1-Pad14)")
			(pinfunction "VDD_1")
			(pintype "passive+no_connect")
		)
		(pad "15" smd rect
			(at -0.25 -1.5)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 20 "unconnected-(DA1-N{slash}C_4-Pad15)")
			(pinfunction "N/C_4")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at -0.75 -1.5)
			(size 0.3 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "3.3V")
			(pinfunction "VDD_2")
			(pintype "passive")
		)
		(pad "17" smd rect
			(at 0 0)
			(size 1.75 1.75)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Earth")
			(pinfunction "GND_6")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/Library/RFX2401C.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "RP2350B:QFN40P1000X1000X90-81N-D"
		(layer "F.Cu")
		(at 206.149755 115.742755 90)
		(descr "80QFN")
		(tags "Integrated Circuit")
		(property "Reference" "DD3"
			(at -4.5 -6.5 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "RP2350B"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/rp2350/rp2350-product-brief.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Dual Arm Cortex-M33 or dual Hazard3 RISC-V processors @ 150MHz"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.9"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "RASPBERRY-PI"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "RP2350B"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 6.5 90)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -4.95 -3.8 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 95 "unconnected-(DD3-GPIO4-Pad1)")
			(pinfunction "GPIO4")
			(pintype "passive+no_connect")
		)
		(pad "2" smd rect
			(at -4.95 -3.4 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 80 "unconnected-(DD3-GPIO5-Pad2)")
			(pinfunction "GPIO5")
			(pintype "passive+no_connect")
		)
		(pad "3" smd rect
			(at -4.95 -3 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 89 "unconnected-(DD3-GPIO6-Pad3)")
			(pinfunction "GPIO6")
			(pintype "passive+no_connect")
		)
		(pad "4" smd rect
			(at -4.95 -2.6 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 82 "unconnected-(DD3-GPIO7-Pad4)")
			(pinfunction "GPIO7")
			(pintype "passive+no_connect")
		)
		(pad "5" smd rect
			(at -4.95 -2.2 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "3.3V")
			(pinfunction "IOVDD_1")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at -4.95 -1.8 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 86 "unconnected-(DD3-GPIO8-Pad6)")
			(pinfunction "GPIO8")
			(pintype "passive+no_connect")
		)
		(pad "7" smd rect
			(at -4.95 -1.4 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 81 "unconnected-(DD3-GPIO9-Pad7)")
			(pinfunction "GPIO9")
			(pintype "passive+no_connect")
		)
		(pad "8" smd rect
			(at -4.95 -1 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 93 "unconnected-(DD3-GPIO10-Pad8)")
			(pinfunction "GPIO10")
			(pintype "passive+no_connect")
		)
		(pad "9" smd rect
			(at -4.95 -0.6 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 88 "unconnected-(DD3-GPIO11-Pad9)")
			(pinfunction "GPIO11")
			(pintype "passive+no_connect")
		)
		(pad "10" smd rect
			(at -4.95 -0.2 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(DD3-DVDD_1)")
			(pinfunction "DVDD_1")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at -4.95 0.2 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 92 "unconnected-(DD3-GPIO12-Pad11)")
			(pinfunction "GPIO12")
			(pintype "passive+no_connect")
		)
		(pad "12" smd rect
			(at -4.95 0.6 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 83 "unconnected-(DD3-GPIO13-Pad12)")
			(pinfunction "GPIO13")
			(pintype "passive+no_connect")
		)
		(pad "13" smd rect
			(at -4.95 1 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 85 "unconnected-(DD3-GPIO14-Pad13)")
			(pinfunction "GPIO14")
			(pintype "passive+no_connect")
		)
		(pad "14" smd rect
			(at -4.95 1.4 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 94 "unconnected-(DD3-GPIO15-Pad14)")
			(pinfunction "GPIO15")
			(pintype "passive+no_connect")
		)
		(pad "15" smd rect
			(at -4.95 1.8 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "3.3V")
			(pinfunction "IOVDD_2")
			(pintype "passive")
		)
		(pad "16" smd rect
			(at -4.95 2.2 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 91 "unconnected-(DD3-GPIO16-Pad16)")
			(pinfunction "GPIO16")
			(pintype "passive+no_connect")
		)
		(pad "17" smd rect
			(at -4.95 2.6 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 49 "LED1")
			(pinfunction "GPIO17")
			(pintype "passive")
		)
		(pad "18" smd rect
			(at -4.95 3 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 62 "LED2")
			(pinfunction "GPIO18")
			(pintype "passive")
		)
		(pad "19" smd rect
			(at -4.95 3.4 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 78 "Net-(DD3-GPIO19)")
			(pinfunction "GPIO19")
			(pintype "passive")
		)
		(pad "20" smd rect
			(at -4.95 3.8 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "Net-(DD3-GPIO20)")
			(pinfunction "GPIO20")
			(pintype "passive")
		)
		(pad "21" smd rect
			(at -3.8 4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 79 "Net-(DD3-GPIO21)")
			(pinfunction "GPIO21")
			(pintype "passive")
		)
		(pad "22" smd rect
			(at -3.4 4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 87 "Net-(DD3-GPIO22)")
			(pinfunction "GPIO22")
			(pintype "passive")
		)
		(pad "23" smd rect
			(at -3 4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 90 "Net-(DD3-GPIO23)")
			(pinfunction "GPIO23")
			(pintype "passive")
		)
		(pad "24" smd rect
			(at -2.6 4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "3.3V")
			(pinfunction "IOVDD_3")
			(pintype "passive")
		)
		(pad "25" smd rect
			(at -2.2 4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 98 "Net-(DD3-GPIO24)")
			(pinfunction "GPIO24")
			(pintype "passive")
		)
		(pad "26" smd rect
			(at -1.8 4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 97 "Net-(DD3-GPIO25)")
			(pinfunction "GPIO25")
			(pintype "passive")
		)
		(pad "27" smd rect
			(at -1.4 4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 99 "Net-(DD3-GPIO26)")
			(pinfunction "GPIO26")
			(pintype "passive")
		)
		(pad "28" smd rect
			(at -1 4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 28 "SPI_MOSI")
			(pinfunction "GPIO27")
			(pintype "passive")
		)
		(pad "29" smd rect
			(at -0.6 4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "3.3V")
			(pinfunction "IOVDD_4")
			(pintype "passive")
		)
		(pad "30" smd rect
			(at -0.2 4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "Net-(DD3-XIN)")
			(pinfunction "XIN")
			(pintype "passive")
		)
		(pad "31" smd rect
			(at 0.2 4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "Net-(DD3-XOUT)")
			(pinfunction "XOUT")
			(pintype "passive")
		)
		(pad "32" smd rect
			(at 0.6 4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(DD3-DVDD_1)")
			(pinfunction "DVDD_2")
			(pintype "passive")
		)
		(pad "33" smd rect
			(at 1 4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 44 "Net-(DD3-SWCLK)")
			(pinfunction "SWCLK")
			(pintype "passive")
		)
		(pad "34" smd rect
			(at 1.4 4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 48 "Net-(DD3-SWDIO)")
			(pinfunction "SWDIO")
			(pintype "passive")
		)
		(pad "35" smd rect
			(at 1.8 4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 59 "RUN")
			(pinfunction "RUN")
			(pintype "passive")
		)
		(pad "36" smd rect
			(at 2.2 4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "SPI_MISO")
			(pinfunction "GPIO28")
			(pintype "passive")
		)
		(pad "37" smd rect
			(at 2.6 4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 31 "SPI_SCK")
			(pinfunction "GPIO29")
			(pintype "passive")
		)
		(pad "38" smd rect
			(at 3 4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 30 "NRF_CS")
			(pinfunction "GPIO30")
			(pintype "passive")
		)
		(pad "39" smd rect
			(at 3.4 4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 29 "NRF_CE")
			(pinfunction "GPIO31")
			(pintype "passive")
		)
		(pad "40" smd rect
			(at 3.8 4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 34 "NRF_IRQ")
			(pinfunction "GPIO32")
			(pintype "passive")
		)
		(pad "41" smd rect
			(at 4.95 3.8 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "3.3V")
			(pinfunction "IOVDD_5")
			(pintype "passive")
		)
		(pad "42" smd rect
			(at 4.95 3.4 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 56 "unconnected-(DD3-GPIO33-Pad42)")
			(pinfunction "GPIO33")
			(pintype "passive+no_connect")
		)
		(pad "43" smd rect
			(at 4.95 3 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 45 "unconnected-(DD3-GPIO34-Pad43)")
			(pinfunction "GPIO34")
			(pintype "passive+no_connect")
		)
		(pad "44" smd rect
			(at 4.95 2.6 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 67 "unconnected-(DD3-GPIO35-Pad44)")
			(pinfunction "GPIO35")
			(pintype "passive+no_connect")
		)
		(pad "45" smd rect
			(at 4.95 2.2 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 54 "unconnected-(DD3-GPIO36-Pad45)")
			(pinfunction "GPIO36")
			(pintype "passive+no_connect")
		)
		(pad "46" smd rect
			(at 4.95 1.8 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 61 "unconnected-(DD3-GPIO37-Pad46)")
			(pinfunction "GPIO37")
			(pintype "passive+no_connect")
		)
		(pad "47" smd rect
			(at 4.95 1.4 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 47 "unconnected-(DD3-GPIO38-Pad47)")
			(pinfunction "GPIO38")
			(pintype "passive+no_connect")
		)
		(pad "48" smd rect
			(at 4.95 1 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 57 "unconnected-(DD3-GPIO39-Pad48)")
			(pinfunction "GPIO39")
			(pintype "passive+no_connect")
		)
		(pad "49" smd rect
			(at 4.95 0.6 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 69 "unconnected-(DD3-GPIO40_ADC0-Pad49)")
			(pinfunction "GPIO40_ADC0")
			(pintype "passive+no_connect")
		)
		(pad "50" smd rect
			(at 4.95 0.2 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "3.3V")
			(pinfunction "IOVDD_6")
			(pintype "passive")
		)
		(pad "51" smd rect
			(at 4.95 -0.2 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(DD3-DVDD_1)")
			(pinfunction "DVDD_3")
			(pintype "passive")
		)
		(pad "52" smd rect
			(at 4.95 -0.6 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 53 "unconnected-(DD3-GPIO41_ADC1-Pad52)")
			(pinfunction "GPIO41_ADC1")
			(pintype "passive+no_connect")
		)
		(pad "53" smd rect
			(at 4.95 -1 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 55 "unconnected-(DD3-GPIO42_ADC2-Pad53)")
			(pinfunction "GPIO42_ADC2")
			(pintype "passive+no_connect")
		)
		(pad "54" smd rect
			(at 4.95 -1.4 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 46 "unconnected-(DD3-GPIO43_ADC3-Pad54)")
			(pinfunction "GPIO43_ADC3")
			(pintype "passive+no_connect")
		)
		(pad "55" smd rect
			(at 4.95 -1.8 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "unconnected-(DD3-GPIO44_ADC4-Pad55)")
			(pinfunction "GPIO44_ADC4")
			(pintype "passive+no_connect")
		)
		(pad "56" smd rect
			(at 4.95 -2.2 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 60 "unconnected-(DD3-GPIO45_ADC5-Pad56)")
			(pinfunction "GPIO45_ADC5")
			(pintype "passive+no_connect")
		)
		(pad "57" smd rect
			(at 4.95 -2.6 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "unconnected-(DD3-GPIO46_ADC6-Pad57)")
			(pinfunction "GPIO46_ADC6")
			(pintype "passive+no_connect")
		)
		(pad "58" smd rect
			(at 4.95 -3 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 63 "unconnected-(DD3-GPIO47_ADC7-Pad58)")
			(pinfunction "GPIO47_ADC7")
			(pintype "passive+no_connect")
		)
		(pad "59" smd rect
			(at 4.95 -3.4 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(DD3-ADC_AVDD)")
			(pinfunction "ADC_AVDD")
			(pintype "passive")
		)
		(pad "60" smd rect
			(at 4.95 -3.8 180)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "3.3V")
			(pinfunction "IOVDD_7")
			(pintype "passive")
		)
		(pad "61" smd rect
			(at 3.8 -4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(DD3-ADC_AVDD)")
			(pinfunction "VREG_AVDD")
			(pintype "passive")
		)
		(pad "62" smd rect
			(at 3.4 -4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Earth")
			(pinfunction "VREG_PGND")
			(pintype "passive")
		)
		(pad "63" smd rect
			(at 3 -4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 50 "Net-(DD3-VREG_LX)")
			(pinfunction "VREG_LX")
			(pintype "passive")
		)
		(pad "64" smd rect
			(at 2.6 -4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "3.3V")
			(pinfunction "VREG_VIN")
			(pintype "passive")
		)
		(pad "65" smd rect
			(at 2.2 -4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(DD3-DVDD_1)")
			(pinfunction "VREG_FB")
			(pintype "passive")
		)
		(pad "66" smd rect
			(at 1.8 -4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 68 "USB_R-")
			(pinfunction "USB_DM")
			(pintype "passive")
		)
		(pad "67" smd rect
			(at 1.4 -4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 65 "USB_R+")
			(pinfunction "USB_DP")
			(pintype "passive")
		)
		(pad "68" smd rect
			(at 1 -4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "3.3V")
			(pinfunction "USB_OTP_VDD")
			(pintype "passive")
		)
		(pad "69" smd rect
			(at 0.6 -4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "3.3V")
			(pinfunction "QSPI_IOVDD")
			(pintype "passive")
		)
		(pad "70" smd rect
			(at 0.2 -4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "QSPI_SD3")
			(pinfunction "QSPI_SD3")
			(pintype "passive")
		)
		(pad "71" smd rect
			(at -0.2 -4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "QSPI_SCLK")
			(pinfunction "QSPI_SCLK")
			(pintype "passive")
		)
		(pad "72" smd rect
			(at -0.6 -4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "QSPI_SD0")
			(pinfunction "QSPI_SD0")
			(pintype "passive")
		)
		(pad "73" smd rect
			(at -1 -4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "QSPI_SD2")
			(pinfunction "QSPI_SD2")
			(pintype "passive")
		)
		(pad "74" smd rect
			(at -1.4 -4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 38 "QSPI_SD1")
			(pinfunction "QSPI_SD1")
			(pintype "passive")
		)
		(pad "75" smd rect
			(at -1.8 -4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 40 "QSPI_SS")
			(pinfunction "QSPI_SS")
			(pintype "passive")
		)
		(pad "76" smd rect
			(at -2.2 -4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "3.3V")
			(pinfunction "IOVDD_8")
			(pintype "passive")
		)
		(pad "77" smd rect
			(at -2.6 -4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 58 "unconnected-(DD3-GPIO0-Pad77)")
			(pinfunction "GPIO0")
			(pintype "passive+no_connect")
		)
		(pad "78" smd rect
			(at -3 -4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 64 "unconnected-(DD3-GPIO1-Pad78)")
			(pinfunction "GPIO1")
			(pintype "passive+no_connect")
		)
		(pad "79" smd rect
			(at -3.4 -4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "unconnected-(DD3-GPIO2-Pad79)")
			(pinfunction "GPIO2")
			(pintype "passive+no_connect")
		)
		(pad "80" smd rect
			(at -3.8 -4.95 90)
			(size 0.2 0.85)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 96 "unconnected-(DD3-GPIO3-Pad80)")
			(pinfunction "GPIO3")
			(pintype "passive+no_connect")
		)
		(pad "81" smd rect
			(at 0 0 90)
			(size 3.45 3.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Earth")
			(pinfunction "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/library/RP2350B.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:QFN-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm"
		(layer "F.Cu")
		(at 223.897621 119.42 90)
		(descr "QFN, 20 Pin (http://ww1.microchip.com/downloads/en/PackagingSpec/00000049BQ.pdf#page=274), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "QFN NoLead")
		(property "Reference" "DD1"
			(at 0 -3.3 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "nRF24L01P"
			(at 0 3.3 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.nordicsemi.com/eng/content/download/2726/34069/file/nRF24L01P_Product_Specification_1_0.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "nRF24L01+, Ultra low power 2.4GHz RF Transceiver, QFN20 4x4mm"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "QFN*4x4*0.5mm*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.625 -0.625 90)
			(size 1.01 1.01)
			(layers "F.Paste")
			(roundrect_rratio 0.247525)
		)
		(pad "" smd roundrect
			(at -0.625 0.625 90)
			(size 1.01 1.01)
			(layers "F.Paste")
			(roundrect_rratio 0.247525)
		)
		(pad "" smd roundrect
			(at 0.625 -0.625 90)
			(size 1.01 1.01)
			(layers "F.Paste")
			(roundrect_rratio 0.247525)
		)
		(pad "" smd roundrect
			(at 0.625 0.625 90)
			(size 1.01 1.01)
			(layers "F.Paste")
			(roundrect_rratio 0.247525)
		)
		(pad "1" smd roundrect
			(at -1.9375 -1 90)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "NRF_CE")
			(pinfunction "CE")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -1.9375 -0.5 90)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "NRF_CS")
			(pinfunction "CSN")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at -1.9375 0 90)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "SPI_SCK")
			(pinfunction "SCK")
			(pintype "input")
		)
		(pad "4" smd roundrect
			(at -1.9375 0.5 90)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "SPI_MOSI")
			(pinfunction "MOSI")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -1.9375 1 90)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "SPI_MISO")
			(pinfunction "MISO")
			(pintype "output")
		)
		(pad "6" smd roundrect
			(at -1 1.9375 90)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "NRF_IRQ")
			(pinfunction "IRQ")
			(pintype "output")
		)
		(pad "7" smd roundrect
			(at -0.5 1.9375 90)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "8" smd roundrect
			(at 0 1.9375 90)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "9" smd roundrect
			(at 0.5 1.9375 90)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "Net-(DD1-XC2)")
			(pinfunction "XC2")
			(pintype "passive")
		)
		(pad "10" smd roundrect
			(at 1 1.9375 90)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(DD1-XC1)")
			(pinfunction "XC1")
			(pintype "passive")
		)
		(pad "11" smd roundrect
			(at 1.9375 1 90)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "VDD_PA")
			(pinfunction "VDD_PA")
			(pintype "power_out")
		)
		(pad "12" smd roundrect
			(at 1.9375 0.5 90)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "Net-(DD1-ANT1)")
			(pinfunction "ANT1")
			(pintype "passive")
		)
		(pad "13" smd roundrect
			(at 1.9375 0 90)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "Net-(DD1-ANT2)")
			(pinfunction "ANT2")
			(pintype "passive")
		)
		(pad "14" smd roundrect
			(at 1.9375 -0.5 90)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "15" smd roundrect
			(at 1.9375 -1 90)
			(size 0.825 0.25)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "16" smd roundrect
			(at 1 -1.9375 90)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "Net-(DD1-IREF)")
			(pinfunction "IREF")
			(pintype "passive")
		)
		(pad "17" smd roundrect
			(at 0.5 -1.9375 90)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "18" smd roundrect
			(at 0 -1.9375 90)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "19" smd roundrect
			(at -0.5 -1.9375 90)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(DD1-DVDD)")
			(pinfunction "DVDD")
			(pintype "power_out")
		)
		(pad "20" smd roundrect
			(at -1 -1.9375 90)
			(size 0.25 0.825)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pinfunction "VSS")
			(pintype "power_in")
		)
		(pad "21" smd rect
			(at 0 0 90)
			(size 2.5 2.5)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 1 "Earth")
			(pinfunction "PAD")
			(pintype "power_in")
			(zone_connect 2)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-20-1EP_4x4mm_P0.5mm_EP2.5x2.5mm.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 226.893117 120.098013 90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 0 -1.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10nF"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "RF_Antenna:Texas_SWRA117D_2.4GHz_Right"
		(layer "F.Cu")
		(at 232.275 111.25 -90)
		(descr "http://www.ti.com/lit/an/swra117d/swra117d.pdf")
		(tags "PCB antenna")
		(property "Reference" "AE1"
			(at 4.55 -6.41 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Antenna_Shield"
			(at 4.55 1.21 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Antenna with extra pin for shielding"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr exclude_from_pos_files)
		(net_tie_pad_groups "1,2")
		(fp_text user "${REFERENCE}"
			(at 4.55 -6.4 90)
			(layer "F.Fab")
		)
		(pad "1" connect rect
			(at 0 0 270)
			(size 0.5 0.5)
			(layers "F.Cu")
			(net 2 "Net-(AE1-A)")
			(pinfunction "A")
			(pintype "input")
		)
		(pad "2" thru_hole rect
			(at -2.1 0 270)
			(size 0.9 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 1 "Earth")
			(pinfunction "Shield")
			(pintype "input")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0201_0603Metric"
		(layer "F.Cu")
		(at 199.183612 113.790734 180)
		(descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R14"
			(at 0 -1.1176 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "27R"
			(at 0 1.05 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.4 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 68 "USB_R-")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 75 "USB_ESD-")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 203.9 122.1 -90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C31"
			(at 0 -1.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 199.822255 115.255489 180)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C35"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7uF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 223.2 109.3 180)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C15"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7uF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 191.92 111.88 90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C42"
			(at 0 -1.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7uF"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 16 "VCC-5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 216.6 111.4 180)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C46"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7uF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 212.48 115)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C22"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7uF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "Net-(DD3-DVDD_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0201_0603Metric"
		(layer "F.Cu")
		(at 225.3 113.98 90)
		(descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R5"
			(at 0 -1.1176 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1K"
			(at 0 1.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.4 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 7 "VDD_PA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 22 "Net-(DA1-TXEN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0201_0603Metric"
		(layer "F.Cu")
		(at 199.559428 109.34433 180)
		(descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R9"
			(at 0 -1.1176 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10K"
			(at 0 1.05 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.4 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 59 "RUN")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "3.3V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 209.9 109.38 90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C38"
			(at 0 -1.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7uF"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 207.9 122.1 -90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C37"
			(at 0 -1.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7uF"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0201_0603Metric"
		(layer "F.Cu")
		(at 220.527713 118.702632)
		(descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 -1.1176 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "22K"
			(at 0 1.05 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.4 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 36 "Net-(DD1-IREF)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0603_1608Metric"
		(layer "F.Cu")
		(at 199.8 111.9 -90)
		(descr "Inductor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L7"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "FHW0603UF3R3JST"
			(at 0 1.43 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "Net-(DD3-VREG_LX)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 270)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "Net-(DD3-DVDD_1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0402_1005Metric"
		(layer "F.Cu")
		(at 221.8 109.815 -90)
		(descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D1"
			(at 0 -1.17 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED 0402"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 270)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.485 0 270)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 17 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 212.3 121.3)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP3"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 79 "Net-(DD3-GPIO21)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 202.7 109.28 -90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C26"
			(at 0 -1.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7uF"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "Net-(DD3-ADC_AVDD)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0201_0603Metric"
		(layer "F.Cu")
		(at 229.011024 111.298977)
		(descr "Inductor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L4"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "2.4nH"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "Net-(DA1-ANT)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 11 "Net-(C16-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 229 121.4 180)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "22pF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "Net-(DD1-XC2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 230 114.6 -90)
		(property "Reference" "G***"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "W25Q16JVUXIQ:W25Q16JVUXIQ"
		(layer "F.Cu")
		(at 196.1 117.9 180)
		(descr "USON 2x3x0.6-mm")
		(tags "Integrated Circuit")
		(property "Reference" "DD2"
			(at 0.53 -1.93 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "W25Q16JVUXIQ_TR"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://componentsearchengine.com/Datasheets/1/W25Q16JVUXIQ TR.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "NOR Flash spiFlash, 3V, 16M-bit, 4Kb Uniform Sector, DTR"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.6"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Winbond"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "W25Q16JVUXIQ TR"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "454-W25Q16JVUXIQTR"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Winbond/W25Q16JVUXIQ-TR?qs=qSfuJ%252Bfl%2Fd7SDdIHLGOd1g%3D%3D"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" "W25Q16JVUXIQ TR"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/w25q16jvuxiqtr/winbond-electronics?utm_currency=USD&region=nac"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.4 -0.75 270)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 40 "QSPI_SS")
			(pinfunction "~{CS}")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.4 -0.25 270)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 38 "QSPI_SD1")
			(pinfunction "DO(IO1)")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.4 0.25 270)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 41 "QSPI_SD2")
			(pinfunction "IO2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.4 0.75 270)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Earth")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 1.4 0.75 270)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 37 "QSPI_SD0")
			(pinfunction "DI(IO0)")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 1.4 0.25 270)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 43 "QSPI_SCLK")
			(pinfunction "CLK")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 1.4 -0.25 270)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 39 "QSPI_SD3")
			(pinfunction "IO3")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 1.4 -0.75 270)
			(size 0.3 0.9)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "3.3V")
			(pinfunction "VCC")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 0 0 180)
			(size 0.25 1.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 42 "unconnected-(DD2-EP-Pad9)")
			(pinfunction "EP")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/library/W25Q16JVUXIQ_TR.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 210 122.6)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP1"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 78 "Net-(DD3-GPIO19)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 198.726001 112.670668 90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C23"
			(at 0 -1.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7uF"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 12 "Net-(DD3-DVDD_1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0201_0603Metric"
		(layer "F.Cu")
		(at 213.604822 115.960393 90)
		(descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R12"
			(at 0 -1.1176 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1M"
			(at 0 1.05 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.4 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 15 "Net-(DD3-XIN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 14 "Net-(DD3-XOUT)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 223.2 110 180)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C12"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7uF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0201_0603Metric"
		(layer "F.Cu")
		(at 224.149372 116.460142)
		(descr "Inductor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L1"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "8.2nH"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 35 "Net-(DD1-ANT2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 33 "Net-(DD1-ANT1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 224.5 114 -90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at 0 -1.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1pF"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 -0.000001 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 9 "Net-(DA1-TXRX)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0.000001 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 212.5 118.3)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C32"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7uF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 212.5 116.5)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C27"
			(at 0 -1.05 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 200.6 109.3 -90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C24"
			(at 0 -1.05 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7uF"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 13 "Net-(DD3-ADC_AVDD)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kibuzzard-68BDB1BF"
		(layer "B.Cu")
		(at 202.7 113.3 180)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiLyIsICJDYXBSaWdodENob2ljZSI6ICIvIiwgIkZvbnRDb21ib0JveCI6ICJGcmVkZHlTcGFyay1SZWd1bGFyIiwgIkhlaWdodEN0cmwiOiAxLjAsICJMYXllckNvbWJvQm94IjogIkYuU2lsa1MiLCAiTGluZVNwYWNpbmdDdHJsIjogMS4wLCAiTXVsdGlMaW5lVGV4dCI6ICJieSBAbWFkam9nZ2VyIiwgIlBhZGRpbmdCb3R0b21DdHJsIjogMi4wLCAiUGFkZGluZ0xlZnRDdHJsIjogMS4wLCAiUGFkZGluZ1JpZ2h0Q3RybCI6IDEuMCwgIlBhZGRpbmdUb3BDdHJsIjogMS4wLCAiV2lkdGhDdHJsIjogMi4wLCAiYWR2YW5jZWRDaGVja2JveCI6IHRydWUsICJpbmxpbmVGb3JtYXRUZXh0Ym94IjogZmFsc2UsICJsaW5lb3ZlclN0eWxlQ2hvaWNlIjogIlJvdW5kZWQiLCAibGluZW92ZXJUaGlja25lc3NDdHJsIjogMX0=")
		(property "Reference" "kibuzzard-68BDB1BF"
			(at 0 3.916383 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 -3.916383 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 226.2 117.8 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 216.7 118.3 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "kibuzzard-68BDB1AB"
		(layer "B.Cu")
		(at 213.064303 111.007975 180)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiLyIsICJDYXBSaWdodENob2ljZSI6ICIvIiwgIkZvbnRDb21ib0JveCI6ICJGcmVkZHlTcGFyay1SZWd1bGFyIiwgIkhlaWdodEN0cmwiOiAyLjAsICJMYXllckNvbWJvQm94IjogIkYuU2lsa1MiLCAiTGluZVNwYWNpbmdDdHJsIjogMS4wLCAiTXVsdGlMaW5lVGV4dCI6ICJOUkYyNEwwMS1SRi1VU0ItU3RpY2tcclxuIiwgIlBhZGRpbmdCb3R0b21DdHJsIjogMi4wLCAiUGFkZGluZ0xlZnRDdHJsIjogMS4wLCAiUGFkZGluZ1JpZ2h0Q3RybCI6IDEuMCwgIlBhZGRpbmdUb3BDdHJsIjogMS4wLCAiV2lkdGhDdHJsIjogMi4wLCAiYWR2YW5jZWRDaGVja2JveCI6IHRydWUsICJpbmxpbmVGb3JtYXRUZXh0Ym94IjogZmFsc2UsICJsaW5lb3ZlclN0eWxlQ2hvaWNlIjogIlJvdW5kZWQiLCAibGluZW92ZXJUaGlja25lc3NDdHJsIjogMX0=")
		(property "Reference" "kibuzzard-68BDB1AB"
			(at 0 4.481476 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 -4.481476 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Connector_USB:USB_A_CNCTech_1001-011-01101_Horizontal"
		(layer "B.Cu")
		(at 184 115.8 180)
		(descr "USB type A Plug, Horizontal, http://cnctech.us/pdfs/1001-011-01101.pdf")
		(tags "USB-A")
		(property "Reference" "X1"
			(at -6.9 8 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "USB_A"
			(at 0 -8 0)
			(layer "B.Fab")
		)
		(property "Datasheet" "~"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "USB Type A connector"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "USB*")
		(sheetname "/")
		(sheetfile "NRF24L01-RF-USB-Stick.kicad_sch")
		(attr smd)
		(fp_text user "PCB Edge"
			(at -4.55 0.05 90)
			(layer "Dwgs.User")
		)
		(fp_text user "${REFERENCE}"
			(at -6 0 90)
			(layer "B.Fab")
		)
		(pad "" np_thru_hole circle
			(at -6.9 -2.3 180)
			(size 1.1 1.1)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -6.9 2.3 180)
			(size 1.1 1.1)
			(drill 1.1)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at -9.65 3.5 180)
			(size 2.5 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 16 "VCC-5V")
			(pinfunction "VBUS")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at -9.65 1 180)
			(size 2.5 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 77 "USB_Conn-")
			(pinfunction "D-")
			(pintype "bidirectional")
		)
		(pad "3" smd rect
			(at -9.65 -1 180)
			(size 2.5 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 76 "USB_Conn+")
			(pinfunction "D+")
			(pintype "bidirectional")
		)
		(pad "4" smd rect
			(at -9.65 -3.5 180)
			(size 2.5 1.1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "Earth")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" thru_hole oval
			(at -6.9 -5.7 180)
			(size 3.5 1.9)
			(drill oval 2.5 0.9)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Earth")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at -6.9 5.7 180)
			(size 3.5 1.9)
			(drill oval 2.5 0.9)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Earth")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_A_CNCTech_1001-011-01101_Horizontal.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 187.8 109.8)
		(end 189 108.6)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 187.8 121.8)
		(end 189 123)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189 123)
		(end 189.5 123.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 187.8 115.8)
		(end 187.8 109.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 238.3 122.9)
		(end 238.3 115.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 187.8 115.8)
		(end 187.8 121.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.5 108.1)
		(end 237.7 108.1)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189.5 123.5)
		(end 237.7 123.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 189 108.6)
		(end 189.5 108.1)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 237.7 123.5)
		(end 238.3 122.9)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 237.7 108.1)
		(end 238.3 108.7)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 238.3 108.7)
		(end 238.3 115.8)
		(layer "Edge.Cuts")
	)
	(gr_text "@madjogger"
		(at 189.2 119.4 90)
		(layer "F.SilkS")
	)
	(gr_text "RP2350B"
		(at 210.3 117.5 0)
		(layer "B.SilkS")
	)
	(gr_text "RFX2401C"
		(at 210.3 120.5 0)
		(layer "B.SilkS")
	)
	(gr_text "NRF24l01+"
		(at 210.3 119 0)
		(layer "B.SilkS")
	)
	(zone
		(net 6)
		(net_name "3.3V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.1016)
		)
		(min_thickness 0.1016)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 216.45 110.65) (xy 216.45 111.35) (xy 217 111.9) (xy 217.9 111.9) (xy 218.15 111.65) (xy 218.15 111.3)
				(xy 218.3 111.15) (xy 218.55 111.15) (xy 219.15 111.75) (xy 219.15 111.85) (xy 219.55 112.25) (xy 220.3 112.25)
				(xy 220.45 112.1) (xy 220.45 111.5) (xy 220.2 111.25) (xy 219.9 111.25) (xy 219.05 110.4) (xy 219.05 110.3)
				(xy 218.9 110.15) (xy 216.95 110.15)
			)
		)
	)
	(zone
		(net 13)
		(net_name "Net-(DD3-ADC_AVDD)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 8)
		(connect_pads yes
			(clearance 0.1016)
		)
		(min_thickness 0.1016)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 202.598906 110.333246) (xy 202.598906 111.25) (xy 201.75 111.25) (xy 201.25 111.75) (xy 201.75 112.25)
				(xy 202.5 112.25) (xy 203 111.75) (xy 203 110.5) (xy 202.833246 110.333246)
			)
		)
	)
	(zone
		(net 16)
		(net_name "VCC-5V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads yes
			(clearance 0.1016)
		)
		(min_thickness 0.1016)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 216.2 110.7) (xy 216.2 111) (xy 215.8 111.4) (xy 215.35 111.4) (xy 214.9 110.95) (xy 214.55 110.95)
				(xy 214.35 110.75) (xy 214.35 110.35) (xy 213.75 110.35) (xy 213.15 109.75) (xy 213.15 108.6) (xy 213.3 108.45)
				(xy 215.55 108.45) (xy 215.7 108.6) (xy 215.7 109.55) (xy 215.55 109.7) (xy 215.55 110.3) (xy 215.6 110.35)
				(xy 215.85 110.35)
			)
		)
	)
	(zone
		(net 50)
		(net_name "Net-(DD3-VREG_LX)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.1016)
		)
		(min_thickness 0.1016)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 201.75 112.55) (xy 201.75 112.9) (xy 201.7 112.95) (xy 200.4 112.95) (xy 200.3 112.85) (xy 200.3 112.3)
				(xy 200.1 112.1) (xy 199.55 112.1) (xy 199.3 111.85) (xy 199.3 110.85) (xy 199.5 110.65) (xy 200.55 110.65)
				(xy 200.8 110.9) (xy 200.8 112.45) (xy 201.65 112.45)
			)
		)
	)
	(zone
		(net 6)
		(net_name "3.3V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.1016)
		)
		(min_thickness 0.1016)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 207.7 109.6) (xy 207.7 109.9) (xy 207.3 110.3) (xy 206.7 110.3) (xy 206.6 110.4) (xy 206.6 111.3)
				(xy 206.9 111.6) (xy 209.2 111.6) (xy 209.7 111.1) (xy 209.7 110) (xy 209.5 109.8) (xy 209.5 109.4)
				(xy 209.6 109.3) (xy 210.1 109.3) (xy 210.3 109.5) (xy 210.3 111.4) (xy 209.6 112.1) (xy 209.6 115)
				(xy 210.6 116) (xy 212 116) (xy 212.4 116.4) (xy 212.1 116.7) (xy 211.8 116.7) (xy 211.7 116.6)
				(xy 210.6 116.6) (xy 210.4 116.8) (xy 210.4 117.7) (xy 210.7 118) (xy 212.4 118) (xy 212.5 118.1)
				(xy 212.5 118.5) (xy 212.3 118.7) (xy 212 118.7) (xy 211.9 118.6) (xy 210.5 118.6) (xy 209.3 119.8)
				(xy 208.3 119.8) (xy 208.1 120) (xy 208.1 121.1) (xy 208.2 121.2) (xy 208.2 121.9) (xy 208.1 122)
				(xy 207.7 122) (xy 207.6 121.9) (xy 207.6 121.3) (xy 207.7 121.2) (xy 207.7 120) (xy 207.4 119.7)
				(xy 204.6 119.7) (xy 204.2 120.1) (xy 204.2 121.3) (xy 204.3 121.4) (xy 204.3 121.9) (xy 204.1 122.1)
				(xy 203.7 122.1) (xy 203.5 121.9) (xy 203.5 121.4) (xy 203.6 121.3) (xy 203.6 120.2) (xy 201.7 118.3)
				(xy 200.7 118.3) (xy 200.5 118.5) (xy 200.1 118.5) (xy 199.9 118.3) (xy 199.9 118) (xy 200.1 117.8)
				(xy 201.5 117.8) (xy 201.8 117.5) (xy 201.8 115.6) (xy 201.6 115.4) (xy 200.8 115.4) (xy 200.7 115.5)
				(xy 199.9 115.5) (xy 199.822255 115.422255) (xy 199.822255 115.177745) (xy 199.9 115.1) (xy 200 115.1)
				(xy 200.6 114.5) (xy 202 114.5) (xy 202.1 114.4) (xy 202.1 113.5) (xy 202 113.4) (xy 200.8 113.4)
				(xy 200.7 113.3) (xy 200.7 113) (xy 200.8 112.9) (xy 202 112.9) (xy 202.1 112.8) (xy 202.1 110.9)
				(xy 201.3 110.1) (xy 201.2 110.1) (xy 200.9 109.8) (xy 200.9 109.6) (xy 201.1 109.4) (xy 201.8 109.4)
				(xy 202.6 110.2) (xy 202.6 111.4) (xy 203 111.8) (xy 205.6 111.8) (xy 206.1 111.3) (xy 206.1 110.2)
				(xy 206.3 110) (xy 206.7 110) (xy 206.8 109.9) (xy 206.8 109.4) (xy 206.9 109.3) (xy 207.4 109.3)
			)
		)
		(polygon
			(pts
				(xy 203.8 113) (xy 203.5 113.3) (xy 203.3 113.5) (xy 203.1 113.7) (xy 203.1 117.6) (xy 203.1 117.6)
				(xy 203.1 118.2) (xy 203.1 118.2) (xy 203.6 118.7) (xy 208.1 118.7) (xy 208.7 118.1) (xy 208.7 113.6)
				(xy 208.1 113)
			)
		)
	)
	(zone
		(net 13)
		(net_name "Net-(DD3-ADC_AVDD)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads yes
			(clearance 0.1016)
		)
		(min_thickness 0.1016)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 200.2 109.4) (xy 200.2 110) (xy 200.5 110.3) (xy 200.5 110.6) (xy 200.8 110.9) (xy 200.8 111.9)
				(xy 200.9 112) (xy 201.6 112) (xy 201.9 111.7) (xy 201.9 110.7) (xy 200.9 109.7) (xy 200.9 109.4)
			)
		)
	)
	(zone
		(net 13)
		(net_name "Net-(DD3-ADC_AVDD)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.1016)
		)
		(min_thickness 0.1016)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 204.1 109.5) (xy 203.7 110.2) (xy 203.2 110.2) (xy 203 110.4) (xy 203 111.3) (xy 202.9 111.4)
				(xy 202.7 111.4) (xy 202.6 111.3) (xy 202.6 109.4) (xy 202.72 109.28) (xy 203.92 109.28) (xy 204.1 109.1)
				(xy 204.2 109.1)
			)
		)
	)
	(zone
		(net 1)
		(net_name "Earth")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.1016)
		)
		(min_thickness 0.1016)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 189.55 108.2) (xy 187.85 109.9) (xy 187.85 121.85) (xy 189.5 123.5) (xy 230.9 123.5) (xy 232.25 122.15)
				(xy 232.25 109.55) (xy 230.9 108.2)
			)
		)
	)
	(zone
		(net 16)
		(net_name "VCC-5V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads yes
			(clearance 0.1016)
		)
		(min_thickness 0.1016)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 215.2 108.6) (xy 215.2 109.65) (xy 214.85 110) (xy 196.6 110) (xy 195.35 111.25) (xy 195.35 112.4)
				(xy 194.8 112.95) (xy 192.35 112.95) (xy 192.2 112.8) (xy 192.2 111.3) (xy 195.3 108.2) (xy 214.8 108.2)
			)
		)
	)
	(zone
		(net 6)
		(net_name "3.3V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.1016)
		)
		(min_thickness 0.1016)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 220.3 111.1) (xy 220.3 111.65) (xy 219.55 112.4) (xy 218.1 112.4) (xy 217.2 111.5) (xy 212.15 111.5)
				(xy 210.65 113) (xy 209 113) (xy 208.25 112.25) (xy 208.25 111.8) (xy 208.75 111.3) (xy 210.65 111.3)
				(xy 211.6 110.35) (xy 219.55 110.35)
			)
		)
	)
	(embedded_fonts no)
)
