(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(stackup
			(layer "F.SilkS"
				(type "Top Silk Screen")
			)
			(layer "F.Paste"
				(type "Top Solder Paste")
			)
			(layer "F.Mask"
				(type "Top Solder Mask")
				(thickness 0.01)
			)
			(layer "F.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "dielectric 1"
				(type "core")
				(thickness 1.51)
				(material "FR4")
				(epsilon_r 4.5)
				(loss_tangent 0.02)
			)
			(layer "B.Cu"
				(type "copper")
				(thickness 0.035)
			)
			(layer "B.Mask"
				(type "Bottom Solder Mask")
				(thickness 0.01)
			)
			(layer "B.Paste"
				(type "Bottom Solder Paste")
			)
			(layer "B.SilkS"
				(type "Bottom Silk Screen")
			)
			(copper_finish "None")
			(dielectric_constraints no)
		)
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 1)
			(scaleselection 1)
			(outputdirectory "")
		)
	)
	(net 0 "")
	(net 1 "Net-(AE1-A)")
	(net 2 "Earth")
	(net 3 "VCC-5V")
	(net 4 "Net-(C3-Pad2)")
	(net 5 "+3V3")
	(net 6 "XTAL_IN")
	(net 7 "Net-(C10-Pad1)")
	(net 8 "+1V2")
	(net 9 "+2V8")
	(net 10 "Net-(U3-LNA_IN)")
	(net 11 "PCLK")
	(net 12 "Net-(VK1-VREFH)")
	(net 13 "Net-(VK1-VREFN)")
	(net 14 "unconnected-(DD1-PG-Pad3)")
	(net 15 "Net-(DD1-FB)")
	(net 16 "Net-(DD1-EN)")
	(net 17 "Net-(DD1-LX)")
	(net 18 "Net-(DD2-SIO[3])")
	(net 19 "Net-(DD2-SI{slash}SIO[0])")
	(net 20 "Net-(DD2-SCLK)")
	(net 21 "Net-(DD2-CE#)")
	(net 22 "unconnected-(VK1-NC-PadD6)")
	(net 23 "Net-(DD2-SIO[2])")
	(net 24 "Net-(DD2-SO{slash}SIO[1])")
	(net 25 "USB_mcu-")
	(net 26 "USB_mcu+")
	(net 27 "USB_filter-")
	(net 28 "USB_filter+")
	(net 29 "USB_con-")
	(net 30 "Net-(J1-CC1)")
	(net 31 "Net-(J1-CC2)")
	(net 32 "USB_con+")
	(net 33 "U0TX")
	(net 34 "U0RX")
	(net 35 "USB_res-")
	(net 36 "USB_res+")
	(net 37 "XTAL_OUT")
	(net 38 "Net-(U3-U0TXD)")
	(net 39 "SPICS0")
	(net 40 "Net-(U5-~{CS})")
	(net 41 "SPICLK")
	(net 42 "Net-(U5-CLK)")
	(net 43 "SPID")
	(net 44 "Net-(U5-DI{slash}IO_{0})")
	(net 45 "Net-(U5-DO{slash}IO_{1})")
	(net 46 "SPIQ")
	(net 47 "SPIWP")
	(net 48 "Net-(U5-~{WP}{slash}IO_{2})")
	(net 49 "Net-(U5-~{HOLD}{slash}~{RESET}{slash}IO_{3})")
	(net 50 "SPIHD")
	(net 51 "CHIP_PU")
	(net 52 "GPIO0")
	(net 53 "GPIO1")
	(net 54 "Y2")
	(net 55 "GPIO2")
	(net 56 "Y3")
	(net 57 "Y4")
	(net 58 "GPIO3")
	(net 59 "Y5")
	(net 60 "GPIO4")
	(net 61 "Y6")
	(net 62 "GPIO5")
	(net 63 "Y7")
	(net 64 "GPIO6")
	(net 65 "GPIO7")
	(net 66 "Y8")
	(net 67 "GPIO8")
	(net 68 "Y9")
	(net 69 "GPIO9")
	(net 70 "GPIO10")
	(net 71 "XVCLK")
	(net 72 "HREF")
	(net 73 "GPIO11")
	(net 74 "GPIO12")
	(net 75 "VSYNC")
	(net 76 "GPIO13")
	(net 77 "RESETB")
	(net 78 "GPIO18")
	(net 79 "SIO_C")
	(net 80 "GPIO17")
	(net 81 "SIO_D")
	(net 82 "GPIO14")
	(net 83 "STROBE")
	(net 84 "FREX")
	(net 85 "GPIO38")
	(net 86 "GPIO37")
	(net 87 "EXPST_B")
	(net 88 "SPICS1")
	(net 89 "PWDN")
	(net 90 "GPIO33")
	(net 91 "GPIO34")
	(net 92 "GPIO35")
	(net 93 "GPIO36")
	(net 94 "GPIO45")
	(net 95 "GPIO46")
	(net 96 "GPIO21")
	(net 97 "GPIO15")
	(net 98 "GPIO16")
	(net 99 "MTCK")
	(net 100 "MTDO")
	(net 101 "MTDI")
	(net 102 "MTMS")
	(net 103 "Net-(U3-SPICLK_N)")
	(net 104 "Net-(U3-SPICLK_P)")
	(net 105 "Y0")
	(net 106 "Y1")
	(net 107 "Net-(VK1-EVDD_1)")
	(net 108 "Net-(VK1-EVDD_2)")
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 112.9 71.28 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R23"
			(at 0 -1.3335 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 57 "Y4")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 64 "GPIO6")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinSocket_2.54mm:PinSocket_1x04_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 124.4 90.54 180)
		(descr "Through hole straight socket strip, 1x04, 2.54mm pitch, single row (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 1x04 2.54mm single row")
		(property "Reference" "J2"
			(at 0.6 -1.86 0)
			(layer "F.SilkS" knockout)
		)
		(property "Value" "Conn_01x04_Pin"
			(at 0 10.39 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, single row, 01x04, script generated"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*_1x??_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr through_hole)
		(fp_text user "${REFERENCE}"
			(at 0 3.81 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 5 "+3V3")
			(pinfunction "Pin_1")
			(pintype "passive")
		)
		(pad "2" thru_hole oval
			(at 0 2.54 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 33 "U0TX")
			(pinfunction "Pin_2")
			(pintype "passive")
		)
		(pad "3" thru_hole oval
			(at 0 5.08 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 34 "U0RX")
			(pinfunction "Pin_3")
			(pintype "passive")
		)
		(pad "4" thru_hole oval
			(at 0 7.62 180)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 2 "Earth")
			(pinfunction "Pin_4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x04_P2.54mm_Vertical.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 99.635 76.56 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R2"
			(at 0 -1.3335 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "5.1K"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "Net-(J1-CC1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 113.1 52.8 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C31"
			(at -0.4 2.2 270)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "100nF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -2.3 -0.83 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "+1V2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_USB:USB_C_Receptacle_GCT_USB4105-xx-A_16P_TopMnt_Horizontal"
		(layer "F.Cu")
		(at 94.335 79.35 -90)
		(descr "USB 2.0 Type C Receptacle, GCT, 16P, top mounted, horizontal, 5A: https://gct.co/files/drawings/usb4105.pdf")
		(tags "USB C Type-C Receptacle SMD USB 2.0 16P 16C USB4105-15-A USB4105-15-A-060 USB4105-15-A-120 USB4105-GF-A USB4105-GF-A-060 USB4105-GF-A-120")
		(property "Reference" "J1"
			(at -5.75 -3.965 0)
			(unlocked yes)
			(layer "F.SilkS" knockout)
		)
		(property "Value" "USB_C_Receptacle_USB2.0_14P"
			(at 0 5 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.usb.org/sites/default/files/documents/usb_type-c.zip"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "USB 2.0-only 14P Type-C Receptacle connector"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "USB*C*Receptacle*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "PCB Edge"
			(at 0 3.1 270)
			(unlocked yes)
			(layer "Dwgs.User")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -2.89 -2.605 270)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2.89 -2.605 270)
			(size 0.65 0.65)
			(drill 0.65)
			(layers "*.Cu" "*.Mask")
		)
		(pad "A1" smd roundrect
			(at -3.2 -3.68 270)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "A4" smd roundrect
			(at -2.4 -3.68 270)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VCC-5V")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "A5" smd roundrect
			(at -1.25 -3.68 270)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "Net-(J1-CC1)")
			(pinfunction "CC1")
			(pintype "bidirectional")
		)
		(pad "A6" smd roundrect
			(at -0.25 -3.68 270)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "USB_con+")
			(pinfunction "D+")
			(pintype "bidirectional")
		)
		(pad "A7" smd roundrect
			(at 0.25 -3.68 270)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "USB_con-")
			(pinfunction "D-")
			(pintype "bidirectional")
		)
		(pad "A8" smd roundrect
			(at 1.25 -3.68 270)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "A9" smd roundrect
			(at 2.4 -3.68 270)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VCC-5V")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "A12" smd roundrect
			(at 3.2 -3.68 270)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "B1" smd roundrect
			(at 3.2 -3.68 270)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "B4" smd roundrect
			(at 2.4 -3.68 270)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VCC-5V")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "B5" smd roundrect
			(at 1.75 -3.68 270)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "Net-(J1-CC2)")
			(pinfunction "CC2")
			(pintype "bidirectional")
		)
		(pad "B6" smd roundrect
			(at 0.75 -3.68 270)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "USB_con+")
			(pinfunction "D+")
			(pintype "bidirectional")
		)
		(pad "B7" smd roundrect
			(at -0.75 -3.68 270)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "USB_con-")
			(pinfunction "D-")
			(pintype "bidirectional")
		)
		(pad "B8" smd roundrect
			(at -1.75 -3.68 270)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "B9" smd roundrect
			(at -2.4 -3.68 270)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VCC-5V")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "B12" smd roundrect
			(at -3.2 -3.68 270)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at -4.32 -3.105 270)
			(size 1 2.1)
			(drill oval 0.6 1.7)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask" "F.Paste")
			(remove_unused_layers no)
			(net 2 "Earth")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at -4.32 1.075 270)
			(size 1 1.8)
			(drill oval 0.6 1.4)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask" "F.Paste")
			(remove_unused_layers no)
			(net 2 "Earth")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at 4.32 -3.105 270)
			(size 1 2.1)
			(drill oval 0.6 1.7)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask" "F.Paste")
			(remove_unused_layers no)
			(net 2 "Earth")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(pad "S1" thru_hole oval
			(at 4.32 1.075 270)
			(size 1 1.8)
			(drill oval 0.6 1.4)
			(property pad_prop_heatsink)
			(layers "*.Cu" "*.Mask" "F.Paste")
			(remove_unused_layers no)
			(net 2 "Earth")
			(pinfunction "SHIELD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_USB.3dshapes/USB_C_Receptacle_GCT_USB4105-xx-A_16P_TopMnt_Horizontal.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 125.7 69.98 -90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C25"
			(at 0 -1.05 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "1.8pF"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Net-(AE1-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 121.5 79.7 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R34"
			(at -0.8 -2.6 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.17 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 84 "FREX")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 85 "GPIO38")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 119.9 82.3 90)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP3"
			(at -2.8 -1.5 180)
			(layer "F.SilkS" knockout)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 90)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0 90)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 92 "GPIO35")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Inductor_SMD:L_0201_0603Metric"
		(layer "F.Cu")
		(at 124.6 69.58)
		(descr "Inductor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L3"
			(at 0 -1.05 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "3nH"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "Net-(U3-LNA_IN)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Net-(AE1-A)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 93.9699 85.575)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at 0 -1.16 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "100nF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_SPST_B3U-1000P"
		(layer "F.Cu")
		(at 93.4 70.65 180)
		(descr "Ultra-small-sized Tactile Switch with High Contact Reliability, Top-actuated Model, without Ground Terminal, without Boss")
		(tags "Tactile Switch")
		(property "Reference" "RST"
			(at 0.642474 -1.999163 0)
			(layer "F.SilkS" knockout)
		)
		(property "Value" "TS-1088-AR02016"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0 180)
			(size 0.9 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "CHIP_PU")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0 180)
			(size 0.9 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Earth")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 101.712388 59.89935 -90)
		(property "Reference" "G***"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 112.1 85.09 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R10"
			(at 0 -1.3335 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "Net-(U5-~{CS})")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 39 "SPICS0")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 96.5 73.5)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 0 -1.16 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "22uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VCC-5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "SY8843QWC:SY8843QWC"
		(layer "F.Cu")
		(at 94.42995 89.85505 90)
		(property "Reference" "DD1"
			(at -1.64495 2.47005 0)
			(unlocked yes)
			(layer "F.SilkS" knockout)
		)
		(property "Value" "~"
			(at 1.5 4.5 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "SY8843QWC"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.51995 2.06985)
			(size 0.25 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 15 "Net-(DD1-FB)")
			(pinfunction "FB")
			(pintype "input")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 0)
		)
		(pad "2" smd rect
			(at -0.51995 2.51995)
			(size 0.25 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "+3V3")
			(pinfunction "OUT")
			(pintype "input")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 0)
		)
		(pad "3" smd rect
			(at -0.32005 3.19505 270)
			(size 0.25 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 14 "unconnected-(DD1-PG-Pad3)")
			(pinfunction "PG")
			(pintype "input")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 0)
		)
		(pad "4" smd rect
			(at 0.12995 3.19505 270)
			(size 0.25 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 16 "Net-(DD1-EN)")
			(pinfunction "EN")
			(pintype "input")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 0)
		)
		(pad "5" smd rect
			(at 0.58005 3.19505 270)
			(size 0.25 0.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "VCC-5V")
			(pinfunction "IN")
			(pintype "input")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 0)
		)
		(pad "6" smd rect
			(at 0.58005 2.51995)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 17 "Net-(DD1-LX)")
			(pinfunction "LX")
			(pintype "input")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 0)
		)
		(pad "7" smd rect
			(at 0.58005 2.06985)
			(size 0.25 1.1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Earth")
			(pinfunction "GND")
			(pintype "input")
			(solder_mask_margin 0.05)
			(thermal_bridge_angle 0)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "User.3")
			(hatch edge 0.5)
			(priority 100)
			(connect_pads yes
				(clearance 0)
			)
			(min_thickness 0)
			(filled_areas_thickness no)
			(fill yes
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 97.7305 90.475) (xy 96.2305 90.475) (xy 96.2305 88.975) (xy 97.7305 88.975)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "User.4")
			(hatch edge 0.5)
			(priority 100)
			(connect_pads yes
				(clearance 0)
			)
			(min_thickness 0)
			(filled_areas_thickness no)
			(fill yes
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 96.5998 89.775) (xy 96.3998 89.775) (xy 96.3998 88.975) (xy 96.5998 88.975)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "User.4")
			(hatch edge 0.5)
			(priority 100)
			(connect_pads yes
				(clearance 0)
			)
			(min_thickness 0)
			(filled_areas_thickness no)
			(fill yes
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 96.5998 90.4751) (xy 96.3998 90.4751) (xy 96.3998 90.0751) (xy 96.5998 90.0751)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "User.4")
			(hatch edge 0.5)
			(priority 100)
			(connect_pads yes
				(clearance 0)
			)
			(min_thickness 0)
			(filled_areas_thickness no)
			(fill yes
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 97.0499 89.775) (xy 96.8499 89.775) (xy 96.8499 88.975) (xy 97.0499 88.975)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "User.4")
			(hatch edge 0.5)
			(priority 100)
			(connect_pads yes
				(clearance 0)
			)
			(min_thickness 0)
			(filled_areas_thickness no)
			(fill yes
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 97.0499 90.4751) (xy 96.8499 90.4751) (xy 96.8499 90.0751) (xy 97.0499 90.0751)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "User.4")
			(hatch edge 0.5)
			(priority 100)
			(connect_pads yes
				(clearance 0)
			)
			(min_thickness 0)
			(filled_areas_thickness no)
			(fill yes
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 97.7305 89.175) (xy 97.7305 89.375) (xy 97.3305 89.375) (xy 97.3305 89.175)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "User.4")
			(hatch edge 0.5)
			(priority 100)
			(connect_pads yes
				(clearance 0)
			)
			(min_thickness 0)
			(filled_areas_thickness no)
			(fill yes
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 97.7305 89.6251) (xy 97.7305 89.8251) (xy 97.3305 89.8251) (xy 97.3305 89.6251)
				)
			)
		)
		(zone
			(net 0)
			(net_name "")
			(layer "User.4")
			(hatch edge 0.5)
			(priority 100)
			(connect_pads yes
				(clearance 0)
			)
			(min_thickness 0)
			(filled_areas_thickness no)
			(fill yes
				(thermal_gap 0.5)
				(thermal_bridge_width 0.5)
			)
			(polygon
				(pts
					(xy 97.7305 90.0751) (xy 97.7305 90.2751) (xy 97.3305 90.2751) (xy 97.3305 90.0751)
				)
			)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/TDFN-8_1.4x1.6mm_P0.4mm.step"
			(offset
				(xyz 0.2 -2.6 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 120.8 83.8 90)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP2"
			(at -2.432647 -0.310548 180)
			(layer "F.SilkS" knockout)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 90)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0 90)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 91 "GPIO34")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 104.7 86.2 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C23"
			(at 0 -1.16 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "22uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+2V8")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 110.4 69.39 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R28"
			(at 0 -1.3335 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 72 "HREF")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 73 "GPIO11")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 98.1 67.5)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP8"
			(at 0 -1.2 0)
			(layer "F.SilkS" knockout)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 97 "GPIO15")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 96.818024 87.53785)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R8"
			(at 0 -1.17 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "9.1K"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "Net-(DD1-FB)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 100.22 90.6)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at 0 -1.16 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "22uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kibuzzard-68B606AE"
		(layer "F.Cu")
		(at 121.1 61.4 -90)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiXFwiLCAiQ2FwUmlnaHRDaG9pY2UiOiAiLyIsICJGb250Q29tYm9Cb3giOiAiVWJ1bnR1TW9uby1CIiwgIkhlaWdodEN0cmwiOiAxLjQsICJMYXllckNvbWJvQm94IjogIkYuU2lsa1MiLCAiTGluZVNwYWNpbmdDdHJsIjogMS4wLCAiTXVsdGlMaW5lVGV4dCI6ICJFU1AzMi1TMyIsICJQYWRkaW5nQm90dG9tQ3RybCI6IDIuMCwgIlBhZGRpbmdMZWZ0Q3RybCI6IDEuMCwgIlBhZGRpbmdSaWdodEN0cmwiOiAxLjAsICJQYWRkaW5nVG9wQ3RybCI6IDEuMCwgIldpZHRoQ3RybCI6IDIuNSwgImFkdmFuY2VkQ2hlY2tib3giOiB0cnVlLCAiaW5saW5lRm9ybWF0VGV4dGJveCI6IGZhbHNlLCAibGluZW92ZXJTdHlsZUNob2ljZSI6ICJSb3VuZGVkIiwgImxpbmVvdmVyVGhpY2tuZXNzQ3RybCI6IDF9")
		(property "Reference" "kibuzzard-68B606AE"
			(at 0 -4.061247 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 4.061247 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 120.9 91 90)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP15"
			(at 2.4 -0.4 90)
			(layer "F.SilkS" knockout)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 90)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0 90)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 104 "Net-(U3-SPICLK_P)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 94.6 73.5 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0 -1.16 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "100nF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VCC-5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "RF_Antenna:Texas_SWRA117D_2.4GHz_Left"
		(layer "F.Cu")
		(at 127.5 69.5 -90)
		(descr "http://www.ti.com/lit/an/swra117d/swra117d.pdf")
		(tags "PCB antenna")
		(property "Reference" "AE1"
			(at -4.55 -6.41 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "Antenna_Shield"
			(at -3.95 1.21 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Antenna with extra pin for shielding"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr exclude_from_pos_files)
		(net_tie_pad_groups "1,2")
		(fp_text user "${REFERENCE}"
			(at -4.55 -6.4 90)
			(layer "F.Fab")
		)
		(pad "1" connect rect
			(at 0 0 270)
			(size 0.5 0.5)
			(layers "F.Cu")
			(net 1 "Net-(AE1-A)")
			(pinfunction "A")
			(pintype "input")
		)
		(pad "2" thru_hole rect
			(at 2.1 0 270)
			(size 0.9 0.5)
			(drill 0.3)
			(layers "*.Cu")
			(remove_unused_layers no)
			(net 2 "Earth")
			(pinfunction "Shield")
			(pintype "input")
			(zone_connect 2)
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 115.8 62.3 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP19"
			(at -0.7 -2.8 0)
			(layer "F.SilkS" knockout)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 108 "Net-(VK1-EVDD_2)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 123.5 69.88 -90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C24"
			(at 0 -1.05 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "1.2pF"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 10 "Net-(U3-LNA_IN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 121.6 82.3)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP4"
			(at -0.7 2.832647 0)
			(layer "F.SilkS" knockout)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 93 "GPIO36")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 110.1 85.09 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R15"
			(at 0 -1.3335 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "Net-(U5-~{HOLD}{slash}~{RESET}{slash}IO_{3})")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "SPIHD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 100.613298 78.344107 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R5"
			(at 0 -1.3335 180)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "18R"
			(at 0 1.17 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "USB_res-")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "USB_con-")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 126.1 78.9)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP11"
			(at 3.9 0 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 100 "MTDO")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 110.9 71.29 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R27"
			(at 0 -1.3335 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 71 "XVCLK")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 70 "GPIO10")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Crystal:Crystal_SMD_2520-4Pin_2.5x2.0mm"
		(layer "F.Cu")
		(at 122.675 75.5)
		(descr "SMD Crystal SERIES SMD2520/4 http://www.newxtal.com/UploadFiles/Images/2012-11-12-09-29-09-776.pdf, 2.5x2.0mm^2 package")
		(tags "SMD SMT crystal")
		(property "Reference" "Y1"
			(at 0 -2.2 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "XTM25040000JT00351005"
			(at 0 2.2 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Four pin crystal, GND on pins 2 and 4"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Crystal*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.875 0.7)
			(size 1.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 6 "XTAL_IN")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 0.875 0.7)
			(size 1.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Earth")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 0.875 -0.7)
			(size 1.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 4 "Net-(C3-Pad2)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -0.875 -0.7)
			(size 1.15 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Earth")
			(pinfunction "4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_2520-4Pin_2.5x2.0mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 119.6 73.5 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C13"
			(at 0 -1.16 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "22uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 108.9 71.29 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R33"
			(at 0 -1.3335 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 83 "STROBE")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 82 "GPIO14")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 108.2 75.1 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R40"
			(at 0.7 -0.1 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "4.7K"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 81 "SIO_D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 112.1 52.8 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C28"
			(at -0.4 2.1 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "100nF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "Net-(VK1-VREFH)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 115.5 63.5 180)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP18"
			(at -1 -2.7 0)
			(layer "F.SilkS" knockout)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0 180)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 107 "Net-(VK1-EVDD_1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Button_Switch_SMD:SW_SPST_B3U-1000P"
		(layer "F.Cu")
		(at 93.4 67.3 180)
		(descr "Ultra-small-sized Tactile Switch with High Contact Reliability, Top-actuated Model, without Ground Terminal, without Boss")
		(tags "Tactile Switch")
		(property "Reference" "BOOT"
			(at 0.165687 1.914783 0)
			(layer "F.SilkS" knockout)
		)
		(property "Value" "TS-1088-AR02016"
			(at 0 2.5 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.7 0 180)
			(size 0.9 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 52 "GPIO0")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.7 0 180)
			(size 0.9 1.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Earth")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Button_Switch_SMD.3dshapes/SW_SPST_B3U-1000P.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 96.3 68.1 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R17"
			(at 0 -1.3335 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "10K"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "GPIO0")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 114.4 69.39 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R20"
			(at 0 -1.3335 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 63 "Y7")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 58 "GPIO3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0402_1005Metric"
		(layer "F.Cu")
		(at 117.4 68.7 180)
		(descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L2"
			(at 0 -1.17 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "2nH"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 180)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.485 0 180)
			(size 0.59 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(C10-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 110.5 62.6 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C26"
			(at 0 -1.16 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "15pF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "PCLK")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 121.1 77.92 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C19"
			(at -0.88 -1 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "22uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 111.7 81.8 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C18"
			(at 0 -1.16 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "22uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 118.4 87.6 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C21"
			(at 0 -1.16 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "22uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 120.516815 73.5 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C14"
			(at 0 -1.16 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "22uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_Cenker_CKCS4020"
		(layer "F.Cu")
		(at 93.6 88.515 90)
		(descr "Inductor, Cenker, CKCS4020, 4.0x4.0x2.0mm, (https://www.ckcoil.com/file/upload/spae532/2023-07/11/202307110955366446.pdf), generated with kicad-footprint-generator gen_inductor.py")
		(tags "Inductor ckcs")
		(property "Reference" "L1"
			(at -2.985 1.2 180)
			(layer "F.SilkS" knockout)
		)
		(property "Value" "0.68uH"
			(at 0 3 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.35 0 90)
			(size 1.7 3.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.147059)
			(net 17 "Net-(DD1-LX)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.35 0 90)
			(size 1.7 3.7)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.147059)
			(net 5 "+3V3")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_Cenker_CKCS4020.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 101.4 68.8 -90)
		(property "Reference" "G***"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 102.5 86.2)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C15"
			(at 0 -1.16 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "22uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "+1V2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 109.9 71.3 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R29"
			(at 0 -1.3335 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 75 "VSYNC")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 74 "GPIO12")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 124.5 80.3)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP10"
			(at 2.6 1 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 99 "MTCK")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 108.5 82 90)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP7"
			(at 0 -1.8 180)
			(layer "F.SilkS" knockout)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 90)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0 90)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 96 "GPIO21")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 96.818024 86.53785 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R7"
			(at 0 -1.17 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "41К"
			(at 0 1.17 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 15 "Net-(DD1-FB)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 123.1 73.2)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 -1.43 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "18pF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(C3-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_CommonModeChoke_Coilcraft_0805USB"
		(layer "F.Cu")
		(at 107.6 78.8 90)
		(descr "Coilcraft 0805USB Series Common Mode Choke, https://www.coilcraft.com/pdfs/0805usb.pdf")
		(tags "surface mount common mode bead")
		(property "Reference" "FL1"
			(at -1.5 -0.1 180)
			(layer "F.SilkS" knockout)
		)
		(property "Value" "DLW21SZ900HQ2L"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "EMI 2-inductor common mode filter"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "L_* L_CommonMode*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.435 -0.835 90)
			(size 0.51 0.76)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 28 "USB_filter+")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -0.435 0.835 90)
			(size 0.51 0.76)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 26 "USB_mcu+")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.435 0.835 90)
			(size 0.51 0.76)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 25 "USB_mcu-")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 0.435 -0.835 90)
			(size 0.51 0.76)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.05)
			(net 27 "USB_filter-")
			(pinfunction "4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/library/DLW21SZ900HQ2L.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -90)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 108.9 62.1 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C33"
			(at 0 -1.16 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "100nF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 117.4 70.6)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at 0 -1.16 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "22uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(C10-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 107.2 75.1 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R32"
			(at 0.7 -0.1 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 81 "SIO_D")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 80 "GPIO17")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 122.1 87.6 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R9"
			(at 0 -1.3335 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "499"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "U0TX")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 38 "Net-(U3-U0TXD)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP4x4mm"
		(layer "F.Cu")
		(at 114.95 77.2 -90)
		(descr "QFN, 56 Pin (https://www.espressif.com/sites/default/files/documentation/esp32-s2_datasheet_en.pdf#page=41), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "QFN NoLead")
		(property "Reference" "U3"
			(at 4.8 0.35 180)
			(layer "F.SilkS" knockout)
		)
		(property "Value" "ESP32-S3"
			(at 0 4.8 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.espressif.com/sites/default/files/documentation/esp32-s3_datasheet_en.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Microcontroller, Wi-Fi 802.11b/g/n, Bluetooth, 32bit"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "QFN*1EP*7x7mm*P0.4mm*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -1.33 -1.33 270)
			(size 1.07 1.07)
			(layers "F.Paste")
			(roundrect_rratio 0.233645)
		)
		(pad "" smd roundrect
			(at -1.33 0 270)
			(size 1.07 1.07)
			(layers "F.Paste")
			(roundrect_rratio 0.233645)
		)
		(pad "" smd roundrect
			(at -1.33 1.33 270)
			(size 1.07 1.07)
			(layers "F.Paste")
			(roundrect_rratio 0.233645)
		)
		(pad "" smd roundrect
			(at 0 -1.33 270)
			(size 1.07 1.07)
			(layers "F.Paste")
			(roundrect_rratio 0.233645)
		)
		(pad "" smd roundrect
			(at 0 0 270)
			(size 1.07 1.07)
			(layers "F.Paste")
			(roundrect_rratio 0.233645)
		)
		(pad "" smd roundrect
			(at 0 1.33 270)
			(size 1.07 1.07)
			(layers "F.Paste")
			(roundrect_rratio 0.233645)
		)
		(pad "" smd roundrect
			(at 1.33 -1.33 270)
			(size 1.07 1.07)
			(layers "F.Paste")
			(roundrect_rratio 0.233645)
		)
		(pad "" smd roundrect
			(at 1.33 0 270)
			(size 1.07 1.07)
			(layers "F.Paste")
			(roundrect_rratio 0.233645)
		)
		(pad "" smd roundrect
			(at 1.33 1.33 270)
			(size 1.07 1.07)
			(layers "F.Paste")
			(roundrect_rratio 0.233645)
		)
		(pad "1" smd roundrect
			(at -3.45 -2.6 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "Net-(U3-LNA_IN)")
			(pinfunction "LNA_IN")
			(pintype "bidirectional")
		)
		(pad "2" smd roundrect
			(at -3.45 -2.2 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(C10-Pad1)")
			(pinfunction "VDD3P3")
			(pintype "power_in")
		)
		(pad "3" smd roundrect
			(at -3.45 -1.8 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(C10-Pad1)")
			(pinfunction "VDD3P3")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at -3.45 -1.4 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "CHIP_PU")
			(pinfunction "CHIP_PU")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at -3.45 -1 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "GPIO0")
			(pinfunction "GPIO0")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at -3.45 -0.6 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "GPIO1")
			(pinfunction "GPIO1")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at -3.45 -0.2 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 55 "GPIO2")
			(pinfunction "GPIO2")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at -3.45 0.2 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 58 "GPIO3")
			(pinfunction "GPIO3")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at -3.45 0.6 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 60 "GPIO4")
			(pinfunction "GPIO4")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at -3.45 1 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 62 "GPIO5")
			(pinfunction "GPIO5")
			(pintype "bidirectional")
		)
		(pad "11" smd roundrect
			(at -3.45 1.4 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 64 "GPIO6")
			(pinfunction "GPIO6")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at -3.45 1.8 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "GPIO7")
			(pinfunction "GPIO7")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at -3.45 2.2 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 67 "GPIO8")
			(pinfunction "GPIO8")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at -3.45 2.6 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 69 "GPIO9")
			(pinfunction "GPIO9")
			(pintype "bidirectional")
		)
		(pad "15" smd roundrect
			(at -2.6 3.45 270)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 70 "GPIO10")
			(pinfunction "GPIO10")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at -2.2 3.45 270)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 73 "GPIO11")
			(pinfunction "GPIO11")
			(pintype "bidirectional")
		)
		(pad "17" smd roundrect
			(at -1.8 3.45 270)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 74 "GPIO12")
			(pinfunction "GPIO12")
			(pintype "bidirectional")
		)
		(pad "18" smd roundrect
			(at -1.4 3.45 270)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 76 "GPIO13")
			(pinfunction "GPIO13")
			(pintype "bidirectional")
		)
		(pad "19" smd roundrect
			(at -1 3.45 270)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 82 "GPIO14")
			(pinfunction "GPIO14")
			(pintype "bidirectional")
		)
		(pad "20" smd roundrect
			(at -0.6 3.45 270)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pinfunction "VDD3P3_RTC")
			(pintype "power_in")
		)
		(pad "21" smd roundrect
			(at -0.2 3.45 270)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 97 "GPIO15")
			(pinfunction "XTAL_32K_P")
			(pintype "passive")
		)
		(pad "22" smd roundrect
			(at 0.2 3.45 270)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 98 "GPIO16")
			(pinfunction "XTAL_32K_N")
			(pintype "passive")
		)
		(pad "23" smd roundrect
			(at 0.6 3.45 270)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 80 "GPIO17")
			(pinfunction "GPIO17")
			(pintype "bidirectional")
		)
		(pad "24" smd roundrect
			(at 1 3.45 270)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 78 "GPIO18")
			(pinfunction "GPIO18")
			(pintype "bidirectional")
		)
		(pad "25" smd roundrect
			(at 1.4 3.45 270)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "USB_mcu-")
			(pinfunction "GPIO19/USB_D-")
			(pintype "bidirectional")
		)
		(pad "26" smd roundrect
			(at 1.8 3.45 270)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "USB_mcu+")
			(pinfunction "GPIO20/USB_D+")
			(pintype "bidirectional")
		)
		(pad "27" smd roundrect
			(at 2.2 3.45 270)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 96 "GPIO21")
			(pinfunction "GPIO21")
			(pintype "bidirectional")
		)
		(pad "28" smd roundrect
			(at 2.6 3.45 270)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 88 "SPICS1")
			(pinfunction "SPICS1")
			(pintype "bidirectional")
		)
		(pad "29" smd roundrect
			(at 3.45 2.6 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pinfunction "VDD_SPI")
			(pintype "power_in")
		)
		(pad "30" smd roundrect
			(at 3.45 2.2 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "SPIHD")
			(pinfunction "SPIHD")
			(pintype "bidirectional")
		)
		(pad "31" smd roundrect
			(at 3.45 1.8 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 47 "SPIWP")
			(pinfunction "SPIWP")
			(pintype "bidirectional")
		)
		(pad "32" smd roundrect
			(at 3.45 1.4 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 39 "SPICS0")
			(pinfunction "SPICS0")
			(pintype "bidirectional")
		)
		(pad "33" smd roundrect
			(at 3.45 1 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "SPICLK")
			(pinfunction "SPICLK")
			(pintype "bidirectional")
		)
		(pad "34" smd roundrect
			(at 3.45 0.6 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 46 "SPIQ")
			(pinfunction "SPIQ")
			(pintype "bidirectional")
		)
		(pad "35" smd roundrect
			(at 3.45 0.2 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "SPID")
			(pinfunction "SPID")
			(pintype "bidirectional")
		)
		(pad "36" smd roundrect
			(at 3.45 -0.2 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 103 "Net-(U3-SPICLK_N)")
			(pinfunction "SPICLK_N")
			(pintype "bidirectional")
		)
		(pad "37" smd roundrect
			(at 3.45 -0.6 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 104 "Net-(U3-SPICLK_P)")
			(pinfunction "SPICLK_P")
			(pintype "bidirectional")
		)
		(pad "38" smd roundrect
			(at 3.45 -1 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 90 "GPIO33")
			(pinfunction "GPIO33")
			(pintype "bidirectional")
		)
		(pad "39" smd roundrect
			(at 3.45 -1.4 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 91 "GPIO34")
			(pinfunction "GPIO34")
			(pintype "bidirectional")
		)
		(pad "40" smd roundrect
			(at 3.45 -1.8 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 92 "GPIO35")
			(pinfunction "GPIO35")
			(pintype "bidirectional")
		)
		(pad "41" smd roundrect
			(at 3.45 -2.2 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 93 "GPIO36")
			(pinfunction "GPIO36")
			(pintype "bidirectional")
		)
		(pad "42" smd roundrect
			(at 3.45 -2.6 270)
			(size 0.8 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 86 "GPIO37")
			(pinfunction "GPIO37")
			(pintype "bidirectional")
		)
		(pad "43" smd roundrect
			(at 2.6 -3.45 270)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 85 "GPIO38")
			(pinfunction "GPIO38")
			(pintype "bidirectional")
		)
		(pad "44" smd roundrect
			(at 2.2 -3.45 270)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 99 "MTCK")
			(pinfunction "MTCK")
			(pintype "bidirectional")
		)
		(pad "45" smd roundrect
			(at 1.8 -3.45 270)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 100 "MTDO")
			(pinfunction "MTDO")
			(pintype "bidirectional")
		)
		(pad "46" smd roundrect
			(at 1.4 -3.45 270)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pinfunction "VDD3P3_CPU")
			(pintype "power_in")
		)
		(pad "47" smd roundrect
			(at 1 -3.45 270)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 101 "MTDI")
			(pinfunction "MTDI")
			(pintype "bidirectional")
		)
		(pad "48" smd roundrect
			(at 0.6 -3.45 270)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 102 "MTMS")
			(pinfunction "MTMS")
			(pintype "bidirectional")
		)
		(pad "49" smd roundrect
			(at 0.2 -3.45 270)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 38 "Net-(U3-U0TXD)")
			(pinfunction "U0TXD")
			(pintype "bidirectional")
		)
		(pad "50" smd roundrect
			(at -0.2 -3.45 270)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "U0RX")
			(pinfunction "U0RXD")
			(pintype "bidirectional")
		)
		(pad "51" smd roundrect
			(at -0.6 -3.45 270)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 94 "GPIO45")
			(pinfunction "GPIO45")
			(pintype "bidirectional")
		)
		(pad "52" smd roundrect
			(at -1 -3.45 270)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 95 "GPIO46")
			(pinfunction "GPIO46")
			(pintype "bidirectional")
		)
		(pad "53" smd roundrect
			(at -1.4 -3.45 270)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "XTAL_IN")
			(pinfunction "XTAL_N")
			(pintype "output")
		)
		(pad "54" smd roundrect
			(at -1.8 -3.45 270)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "XTAL_OUT")
			(pinfunction "XTAL_P")
			(pintype "input")
		)
		(pad "55" smd roundrect
			(at -2.2 -3.45 270)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pinfunction "VDDA")
			(pintype "power_in")
		)
		(pad "56" smd roundrect
			(at -2.6 -3.45 270)
			(size 0.2 0.8)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pinfunction "VDDA")
			(pintype "passive")
		)
		(pad "57" smd rect
			(at 0 0 270)
			(size 4 4)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 2 "Earth")
			(pinfunction "GND")
			(pintype "power_in")
			(zone_connect 2)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-56-1EP_7x7mm_P0.4mm_EP4x4mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 126.1 76.9)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP12"
			(at 7.5 -1.3 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 101 "MTDI")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 113.4 69.39 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R22"
			(at 0 -1.3335 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 59 "Y5")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 62 "GPIO5")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 111.9 71.28 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R25"
			(at 0 -1.3335 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 54 "Y2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 67 "GPIO8")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "OV2640:OV2640"
		(layer "F.Cu")
		(at 112.3 57.7 90)
		(descr "38-PIN CSP2")
		(tags "Integrated Circuit")
		(property "Reference" "VK1"
			(at 1.8 3.8 270)
			(layer "F.SilkS" knockout)
		)
		(property "Value" "OV2640-VL9A"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://www.uctronics.com/download/cam_module/OV2640DS.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "OV2640-VL9A"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Height" "0.965"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "OmniVision Technologies Inc"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "OV2640-VL9A"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at -0.0005 4.475 90)
			(layer "F.Fab")
		)
		(pad "A1" smd circle
			(at -2 -2.4 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Earth")
			(pinfunction "DOGND")
			(pintype "passive")
		)
		(pad "A2" smd circle
			(at -1.2 -2.4 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 87 "EXPST_B")
			(pinfunction "EXPST_B")
			(pintype "passive")
		)
		(pad "A3" smd circle
			(at -0.4 -2.4 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Earth")
			(pinfunction "AGND")
			(pintype "passive")
		)
		(pad "A4" smd circle
			(at 0.4 -2.4 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Earth")
			(pinfunction "SGND")
			(pintype "passive")
		)
		(pad "A5" smd circle
			(at 1.2 -2.4 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 13 "Net-(VK1-VREFN)")
			(pinfunction "VREFN")
			(pintype "passive")
		)
		(pad "A6" smd circle
			(at 2 -2.4 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 83 "STROBE")
			(pinfunction "STROBE")
			(pintype "passive")
		)
		(pad "B1" smd circle
			(at -2 -1.6 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 5 "+3V3")
			(pinfunction "DOVDD")
			(pintype "passive")
		)
		(pad "B2" smd circle
			(at -1.2 -1.6 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 84 "FREX")
			(pinfunction "FREX")
			(pintype "passive")
		)
		(pad "B3" smd circle
			(at -0.4 -1.6 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "+2V8")
			(pinfunction "AVDD")
			(pintype "passive")
		)
		(pad "B4" smd circle
			(at 0.4 -1.6 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "+2V8")
			(pinfunction "SVDD_1")
			(pintype "passive")
		)
		(pad "B5" smd circle
			(at 1.2 -1.6 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 9 "+2V8")
			(pinfunction "SVDD_2")
			(pintype "passive")
		)
		(pad "B6" smd circle
			(at 2 -1.6 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 89 "PWDN")
			(pinfunction "PWDN")
			(pintype "passive")
		)
		(pad "C1" smd circle
			(at -2 -0.8 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 81 "SIO_D")
			(pinfunction "SIO_D")
			(pintype "passive")
		)
		(pad "C2" smd circle
			(at -1.2 -0.8 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 79 "SIO_C")
			(pinfunction "SIO_C")
			(pintype "passive")
		)
		(pad "C3" smd circle
			(at -0.4 -0.8 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 72 "HREF")
			(pinfunction "HREF")
			(pintype "passive")
		)
		(pad "C4" smd circle
			(at 0.4 -0.8 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 71 "XVCLK")
			(pinfunction "XVCLK")
			(pintype "passive")
		)
		(pad "C5" smd circle
			(at 1.2 -0.8 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 12 "Net-(VK1-VREFH)")
			(pinfunction "VREFH")
			(pintype "passive")
		)
		(pad "C6" smd circle
			(at 2 -0.8 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 77 "RESETB")
			(pinfunction "RESETB")
			(pintype "passive")
		)
		(pad "D2" smd circle
			(at -1.2 0 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 75 "VSYNC")
			(pinfunction "VSYNC")
			(pintype "passive")
		)
		(pad "D6" smd circle
			(at 2 0 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 22 "unconnected-(VK1-NC-PadD6)")
			(pinfunction "NC")
			(pintype "no_connect")
		)
		(pad "E1" smd circle
			(at -2 0.8 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 106 "Y1")
			(pinfunction "Y1")
			(pintype "passive")
		)
		(pad "E2" smd circle
			(at -1.2 0.8 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 105 "Y0")
			(pinfunction "Y0")
			(pintype "passive")
		)
		(pad "E3" smd circle
			(at -0.4 0.8 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 11 "PCLK")
			(pinfunction "PCLK")
			(pintype "passive")
		)
		(pad "E4" smd circle
			(at 0.4 0.8 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Earth")
			(pinfunction "EGND")
			(pintype "passive")
		)
		(pad "E5" smd circle
			(at 1.2 0.8 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 61 "Y6")
			(pinfunction "Y6")
			(pintype "passive")
		)
		(pad "E6" smd circle
			(at 2 0.8 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Earth")
			(pinfunction "DGND_1")
			(pintype "passive")
		)
		(pad "F1" smd circle
			(at -2 1.6 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 107 "Net-(VK1-EVDD_1)")
			(pinfunction "EVDD_1")
			(pintype "passive")
		)
		(pad "F2" smd circle
			(at -1.2 1.6 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "+1V2")
			(pinfunction "DVDD_1")
			(pintype "passive")
		)
		(pad "F3" smd circle
			(at -0.4 1.6 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 54 "Y2")
			(pinfunction "Y2")
			(pintype "passive")
		)
		(pad "F4" smd circle
			(at 0.4 1.6 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 57 "Y4")
			(pinfunction "Y4")
			(pintype "passive")
		)
		(pad "F5" smd circle
			(at 1.2 1.6 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 66 "Y8")
			(pinfunction "Y8")
			(pintype "passive")
		)
		(pad "F6" smd circle
			(at 2 1.6 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 8 "+1V2")
			(pinfunction "DVDD_2")
			(pintype "passive")
		)
		(pad "G1" smd circle
			(at -2 2.4 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 108 "Net-(VK1-EVDD_2)")
			(pinfunction "EVDD_2")
			(pintype "passive")
		)
		(pad "G2" smd circle
			(at -1.2 2.4 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 2 "Earth")
			(pinfunction "DGND_2")
			(pintype "passive")
		)
		(pad "G3" smd circle
			(at -0.4 2.4 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 56 "Y3")
			(pinfunction "Y3")
			(pintype "passive")
		)
		(pad "G4" smd circle
			(at 0.4 2.4 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 59 "Y5")
			(pinfunction "Y5")
			(pintype "passive")
		)
		(pad "G5" smd circle
			(at 1.2 2.4 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 63 "Y7")
			(pinfunction "Y7")
			(pintype "passive")
		)
		(pad "G6" smd circle
			(at 2 2.4 180)
			(size 0.33 0.33)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 68 "Y9")
			(pinfunction "Y9")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/library/OV2640-VL9A.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 114.3 62.6 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C34"
			(at 0.2 -1.2 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "100nF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "+1V2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 105.2 75.1 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R41"
			(at 0.7 -0.1 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "4.7K"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 79 "SIO_C")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 107.2 56.6 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C32"
			(at 0 -1.16 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "100nF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "Net-(VK1-VREFN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 107.6 60.6 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C35"
			(at 0 -1.16 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "100nF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+2V8")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_SO:SOIC-8_5.3x5.3mm_P1.27mm"
		(layer "F.Cu")
		(at 112.29 89.1)
		(descr "SOIC, 8 Pin (JEITA/EIAJ 08-001-BBA and Atmel/Microchip, 208 mils width, https://www.jeita.or.jp/japanese/standard/book/ED-7311-19/#target/page_no=21, https://ww1.microchip.com/downloads/en/DeviceDoc/20005045C.pdf#page=23, https://ww1.microchip.com/downloads/en/DeviceDoc/doc2535.pdf#page=162), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOIC SO P-SOP SOP SOP-8 SO SO-8 8S2 S2AE/F K04-056 CASE-751BE SO8W 8-Pin-SOIC PSA W8-2 W8-4 W8MS-1")
		(property "Reference" "U5"
			(at -3.69 -3.4 0)
			(layer "F.SilkS" knockout)
		)
		(property "Value" "W25Q64JVSSIQ"
			(at 0 3.6 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://www.winbond.com/resource-files/w25q32jv%20revg%2003272018%20plus.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "32Mbit / 4MiB Serial Flash Memory, Standard/Dual/Quad SPI, 2.7-3.6V, SOIC-8 (208 mil)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*SOIC*5.3x5.3mm*P1.27mm*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -3.5875 -1.905)
			(size 1.625 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "Net-(U5-~{CS})")
			(pinfunction "~{CS}")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -3.5875 -0.635)
			(size 1.625 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 45 "Net-(U5-DO{slash}IO_{1})")
			(pinfunction "DO/IO_{1}")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -3.5875 0.635)
			(size 1.625 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "Net-(U5-~{WP}{slash}IO_{2})")
			(pinfunction "~{WP}/IO_{2}")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -3.5875 1.905)
			(size 1.625 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" smd roundrect
			(at 3.5875 1.905)
			(size 1.625 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 44 "Net-(U5-DI{slash}IO_{0})")
			(pinfunction "DI/IO_{0}")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at 3.5875 0.635)
			(size 1.625 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 42 "Net-(U5-CLK)")
			(pinfunction "CLK")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at 3.5875 -0.635)
			(size 1.625 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "Net-(U5-~{HOLD}{slash}~{RESET}{slash}IO_{3})")
			(pinfunction "~{HOLD}/~{RESET}/IO_{3}")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at 3.5875 -1.905)
			(size 1.625 0.65)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pinfunction "VCC")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_SO.3dshapes/SOIC-8_5.3x5.3mm_P1.27mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 98.1 69.7)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP9"
			(at 0 1.3 0)
			(layer "F.SilkS" knockout)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 98 "GPIO16")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 96.3 70 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R16"
			(at 0 -1.3335 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "10K"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "CHIP_PU")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-3"
		(layer "F.Cu")
		(at 105.5 88.4 180)
		(descr "SOT, 3 Pin (JEDEC MO-178 inferred 3-pin variant https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U4"
			(at -1.1 -2.5 0)
			(layer "F.SilkS" knockout)
		)
		(property "Value" "XC6206-2.8V"
			(at 0 2.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.torexsemi.com/file/xc6206/XC6206.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Positive 60-250mA Low Dropout Regulator, Fixed Output, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23?3*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -1.1375 0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+2V8")
			(pinfunction "VO")
			(pintype "power_out")
		)
		(pad "3" smd roundrect
			(at 1.1375 0 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pinfunction "VI")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-3.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 115.4 69.39 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R18"
			(at 0 -1.3335 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 68 "Y9")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 53 "GPIO1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 111.1 85.09 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R14"
			(at 0 -1.3335 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "Net-(U5-~{WP}{slash}IO_{2})")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 47 "SPIWP")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 110.1 52.81 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R39"
			(at 0.39 1 270)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "1K"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 89 "PWDN")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 92.1499 85.575 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 0 -1.16 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "22uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 113.1 63.8 90)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP16"
			(at -2.4 0.2 180)
			(layer "F.SilkS" knockout)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 90)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0 90)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 105 "Y0")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 111.4 69.39 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R26"
			(at 0 -1.3335 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "PCLK")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 69 "GPIO9")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-6"
		(layer "F.Cu")
		(at 104 78.8 180)
		(descr "SOT, 6 Pin (JEDEC MO-178 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U1"
			(at 0 -2.2 0)
			(layer "F.SilkS" knockout)
		)
		(property "Value" "USBLC6-2SC6"
			(at 0 2.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.st.com/resource/en/datasheet/usblc6-2.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Very low capacitance ESD protection diode, 2 data-line, SOT-23-6"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "USB_filter+")
			(pinfunction "I/O1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -1.1375 0 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at -1.1375 0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "USB_filter-")
			(pinfunction "I/O2")
			(pintype "passive")
		)
		(pad "4" smd roundrect
			(at 1.1375 0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "USB_res-")
			(pinfunction "I/O2")
			(pintype "passive")
		)
		(pad "5" smd roundrect
			(at 1.1375 0 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VCC-5V")
			(pinfunction "VBUS")
			(pintype "passive")
		)
		(pad "6" smd roundrect
			(at 1.1375 -0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "USB_res+")
			(pinfunction "I/O1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-6.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "kibuzzard-68B606C1"
		(layer "F.Cu")
		(at 123.150432 61.412112 -90)
		(descr "Generated with KiBuzzard")
		(tags "kb_params=eyJBbGlnbm1lbnRDaG9pY2UiOiAiQ2VudGVyIiwgIkNhcExlZnRDaG9pY2UiOiAiXFwiLCAiQ2FwUmlnaHRDaG9pY2UiOiAiLyIsICJGb250Q29tYm9Cb3giOiAiVWJ1bnR1TW9uby1CIiwgIkhlaWdodEN0cmwiOiAxLjQsICJMYXllckNvbWJvQm94IjogIkYuU2lsa1MiLCAiTGluZVNwYWNpbmdDdHJsIjogMS4wLCAiTXVsdGlMaW5lVGV4dCI6ICJPVjI2NDAtVVNCIiwgIlBhZGRpbmdCb3R0b21DdHJsIjogMi4wLCAiUGFkZGluZ0xlZnRDdHJsIjogMS4wLCAiUGFkZGluZ1JpZ2h0Q3RybCI6IDEuMCwgIlBhZGRpbmdUb3BDdHJsIjogMS4wLCAiV2lkdGhDdHJsIjogMi41LCAiYWR2YW5jZWRDaGVja2JveCI6IHRydWUsICJpbmxpbmVGb3JtYXRUZXh0Ym94IjogZmFsc2UsICJsaW5lb3ZlclN0eWxlQ2hvaWNlIjogIlJvdW5kZWQiLCAibGluZW92ZXJUaGlja25lc3NDdHJsIjogMX0=")
		(property "Reference" "kibuzzard-68B606C1"
			(at 0 -4.061247 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "G***"
			(at 0 4.061247 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 113.9 71.29 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R21"
			(at 0 -1.3335 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 61 "Y6")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 60 "GPIO4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 99.635 82.15 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R3"
			(at 0 -1.3335 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "5.1K"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "Net-(J1-CC2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 128.8 76.3)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP6"
			(at 8.4 -1.8 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 95 "GPIO46")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 95.8499 85.575)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at 0 -1.16 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "22uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 113.1 62.4 90)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP17"
			(at -2.7 0.2 180)
			(layer "F.SilkS" knockout)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 90)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0 90)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 106 "Y1")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 106.2 75.1 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R31"
			(at 0.7 -0.1 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 79 "SIO_C")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 78 "GPIO18")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 127.6 77.5)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP13"
			(at 9.2 -1.9 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 102 "MTMS")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 114.1 85.09 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R13"
			(at -3.71 -2.3 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 45 "Net-(U5-DO{slash}IO_{1})")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 46 "SPIQ")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 113.1 85.09 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R11"
			(at 0 -1.3335 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 42 "Net-(U5-CLK)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "SPICLK")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 121.5 80.7 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R35"
			(at 0 -1.3335 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.17 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 87 "EXPST_B")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 86 "GPIO37")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 107.2 58 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C27"
			(at 0 -1.16 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "100nF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+2V8")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 100.6 86.2 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C16"
			(at 0 -1.16 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "22uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "+1V2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 114.9 71.28 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R19"
			(at 0 -1.3335 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 66 "Y8")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 55 "GPIO2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 106.6 86.2)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C22"
			(at -0.3 -1.4 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "22uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+2V8")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 115.1 85.09 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R12"
			(at 0 -1.3335 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 44 "Net-(U5-DI{slash}IO_{0})")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "SPID")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 109.4 69.39 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R30"
			(at 0 -1.3335 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 77 "RESETB")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 76 "GPIO13")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 111.1 52.8 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C30"
			(at -0.4 -3.1 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "100nF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "+2V8")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 100.613298 79.344107 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R4"
			(at 0 -1.3335 180)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "18R"
			(at 0 1.17 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "USB_res+")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "USB_con+")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 112.4 69.39 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R24"
			(at 0 -1.3335 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "Y3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 65 "GPIO7")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 109.7 76.4 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C20"
			(at 0 -1.16 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "22uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 120 75.1 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R6"
			(at 0 -1.3335 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "0"
			(at 0 1.17 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(C3-Pad2)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "XTAL_OUT")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 127.3 75.8)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP5"
			(at 7 -1.3 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 94 "GPIO45")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 117.40736 69.678716)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C12"
			(at 0 -1.16 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "22uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(C10-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 119 83.8 90)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP1"
			(at -2.4 -0.96 180)
			(layer "F.SilkS" knockout)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 90)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0 90)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 90 "GPIO33")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 117.395835 67.771122 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at 0 -1.16 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "22uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 98.1499 88.475)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 -1.16 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "22uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VCC-5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0603_1608Metric"
		(layer "F.Cu")
		(at 123.1 77.8 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 0 -1.43 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "18pF"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "XTAL_IN")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23-3"
		(layer "F.Cu")
		(at 101.4 88.4 180)
		(descr "SOT, 3 Pin (JEDEC MO-178 inferred 3-pin variant https://www.jedec.org/document_search?search_api_views_fulltext=MO-178), generated with kicad-footprint-generator ipc_gullwing_generator.py")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "U2"
			(at -1.3 -2.5 0)
			(layer "F.SilkS" knockout)
		)
		(property "Value" "XC6206-1.2V"
			(at 0 2.4 0)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.torexsemi.com/file/xc6206/XC6206.pdf"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Positive 60-250mA Low Dropout Regulator, Fixed Output, SOT-23"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23?3*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.1375 -0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -1.1375 0.95 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "+1V2")
			(pinfunction "VO")
			(pintype "power_out")
		)
		(pad "3" smd roundrect
			(at 1.1375 0 180)
			(size 1.325 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pinfunction "VI")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23-3.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 118.9 91 90)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP14"
			(at 2.4 0.4 90)
			(layer "F.SilkS" knockout)
		)
		(property "Value" "TestPoint"
			(at 0 1.55 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 90)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0 90)
			(size 1 1)
			(layers "F.Cu" "F.Mask")
			(net 103 "Net-(U3-SPICLK_N)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Resistor_SMD:R_0402_1005Metric"
		(layer "F.Cu")
		(at 98.5499 90.075 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R1"
			(at 0 -1.17 90)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "10K"
			(at 0 1.17 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "Net-(DD1-EN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "VCC-5V")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 104.4 90.6)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C17"
			(at 0 -1.16 0)
			(layer "F.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "22uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "B.Cu")
		(at 114.1 85.1 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R37"
			(at 2.2 0 90)
			(layer "B.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "0"
			(at 0 -1.17 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 24 "Net-(DD2-SO{slash}SIO[1])")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 46 "SPIQ")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "B.Cu")
		(at 111.1 85.1 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R38"
			(at 2.2 0 90)
			(layer "B.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "0"
			(at 0 -1.17 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 23 "Net-(DD2-SIO[2])")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 47 "SPIWP")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LOGO"
		(layer "B.Cu")
		(at 112.7 66.3 180)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(embedded_fonts no)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "B.Cu")
		(at 112.1 85.1 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R36"
			(at 2.2 0 90)
			(layer "B.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "0"
			(at 0 -1.17 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 21 "Net-(DD2-CE#)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 88 "SPICS1")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 116.7 90.6 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C29"
			(at 0 1.16 90)
			(layer "B.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "22uF"
			(at 0 -1.16 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 5 "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "B.Cu")
		(at 115.1 85.1 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R44"
			(at 2.2 0 90)
			(layer "B.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "0"
			(at 0 -1.17 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 19 "Net-(DD2-SI{slash}SIO[0])")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 43 "SPID")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "B.Cu")
		(at 113.1 85.1 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R43"
			(at 2.2 0 90)
			(layer "B.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "0"
			(at 0 -1.17 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 20 "Net-(DD2-SCLK)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 41 "SPICLK")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LY68L6400SLIT:LY68L6400SLIT"
		(layer "B.Cu")
		(at 112.4 89.1)
		(descr "8-pin (150mil) SOP")
		(tags "Integrated Circuit")
		(property "Reference" "DD2"
			(at -4.3 1.1 270)
			(layer "B.SilkS" knockout)
		)
		(property "Value" "LY68L6400SLIT"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://datasheet.lcsc.com/szlcsc/Lyontek-Inc-LY68L6400SLIT_C261881.pdf"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "AM SRAM 64Mb (8M x 8) SPI/ QPI SOP-8_150mil RoHS"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Height" "1.75"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Lyontek Inc."
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "LY68L6400SLIT"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0.05 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -2.7 1.905 270)
			(size 0.65 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 21 "Net-(DD2-CE#)")
			(pinfunction "CE#")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2.7 0.635 270)
			(size 0.65 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 24 "Net-(DD2-SO{slash}SIO[1])")
			(pinfunction "SO/SIO[1]")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -2.7 -0.635 270)
			(size 0.65 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 23 "Net-(DD2-SIO[2])")
			(pinfunction "SIO[2]")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -2.7 -1.905 270)
			(size 0.65 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "Earth")
			(pinfunction "VSS")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 2.7 -1.905 270)
			(size 0.65 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 19 "Net-(DD2-SI{slash}SIO[0])")
			(pinfunction "SI/SIO[0]")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 2.7 -0.635 270)
			(size 0.65 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 20 "Net-(DD2-SCLK)")
			(pinfunction "SCLK")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 2.7 0.635 270)
			(size 0.65 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 18 "Net-(DD2-SIO[3])")
			(pinfunction "SIO[3]")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 2.7 1.905 270)
			(size 0.65 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 5 "+3V3")
			(pinfunction "VCC")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/library/LY68L6400SLIT.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "B.Cu")
		(at 110.1 85.1 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R42"
			(at 2.2 0 90)
			(layer "B.SilkS" knockout)
			(hide yes)
		)
		(property "Value" "0"
			(at 0 -1.17 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "USB-OV2640-module.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 18 "Net-(DD2-SIO[3])")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 50 "SPIHD")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 128.999999 51.7)
		(end 104.6 51.7)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 90.7 91.4)
		(end 90.7 65.6)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 133 55.700001)
		(end 128.999999 51.7)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 92.4 93.1)
		(end 90.7 91.4)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 124.5 93.1)
		(end 92.4 93.1)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 133 73.7)
		(end 126 80.7)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 126 91.6)
		(end 124.5 93.1)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 133 55.7)
		(mid 136.727922 64.7)
		(end 133 73.7)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 126 80.7)
		(end 126 91.6)
		(layer "Edge.Cuts")
	)
	(gr_arc
		(start 90.7 65.6)
		(mid 94.771216 55.771216)
		(end 104.6 51.7)
		(layer "Edge.Cuts")
	)
	(gr_text "6"
		(at 130.573442 72.869638 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "11"
		(at 130.2 75.1 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "10"
		(at 128.7 75.1 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "TP:"
		(at 128.3 72.9 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "13"
		(at 129.324683 73.990571 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "by @madjogger"
		(at 125 61.3 270)
		(layer "F.SilkS")
	)
	(gr_text "12"
		(at 128.6 74 0)
		(layer "F.SilkS" knockout)
	)
	(gr_text "5"
		(at 129.7 72.9 0)
		(layer "F.SilkS" knockout)
	)
	(zone
		(net 3)
		(net_name "VCC-5V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.1016)
		)
		(min_thickness 0.1016)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 98.8 82.2) (xy 97.5 82.2) (xy 97.2 81.9) (xy 97.2 81.8) (xy 96.6 81.8) (xy 96.4 82) (xy 96.4 83.3)
				(xy 96.3 83.4) (xy 96.3 83.9) (xy 96.6 84.2) (xy 98.1 84.2) (xy 98.5 84.6) (xy 98.5 88.2) (xy 98.4 88.3)
				(xy 98.4 88.7) (xy 98.5 88.8) (xy 98.9 88.8) (xy 99.1 89) (xy 99.1 89.8) (xy 99 89.9) (xy 98.2 89.9)
				(xy 97.8 89.5) (xy 97.3 89.5) (xy 97.2 89.4) (xy 97.2 88.1) (xy 97.5 87.8) (xy 97.7 87.8) (xy 97.8 87.7)
				(xy 97.8 86.2) (xy 96.7 85.1) (xy 96.3 85.1) (xy 94.3 83.1) (xy 94.3 73.8) (xy 95 73.1) (xy 96.3 73.1)
				(xy 96.6 73.4) (xy 96.6 73.9) (xy 96.2 74.3) (xy 96.2 76.3) (xy 96.5 76.6) (xy 98.7 76.6) (xy 98.9 76.8)
				(xy 98.9 77.2) (xy 98.7 77.4) (xy 97.4 77.4) (xy 97 77.8) (xy 97 80.9) (xy 97.4 81.3) (xy 98.7 81.3)
				(xy 98.9 81.5) (xy 98.9 82.1)
			)
		)
	)
	(zone
		(net 5)
		(net_name "+3V3")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.1016)
		)
		(min_thickness 0.1016)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 92.1499 85.575) (xy 92.1499 86.0501) (xy 91.7 86.5) (xy 91.7 88.1501) (xy 92.1499 88.6) (xy 95.2 88.6)
				(xy 95.9 87.9) (xy 95.9 87.1) (xy 96 87) (xy 96.5 87) (xy 96.7 86.8) (xy 96.7 86.3) (xy 96.3 85.9)
				(xy 95.9 85.9) (xy 95.8499 85.8499) (xy 95.8499 85.575) (xy 95.5749 85.3) (xy 95.175 85.3) (xy 94.8 85.675)
				(xy 94.8 85.9) (xy 94.7 86) (xy 94.1 86) (xy 93.8 85.7) (xy 93.8 85.575) (xy 93.525 85.3) (xy 92.4249 85.3)
			)
		)
	)
	(zone
		(net 17)
		(net_name "Net-(DD1-LX)")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads yes
			(clearance 0.1016)
		)
		(min_thickness 0.1016)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 97.2 89.8) (xy 96.8 89.8) (xy 96.7 89.7) (xy 96.7 88.7) (xy 96.6 88.6) (xy 96.3 88.6) (xy 95.7 89.2)
				(xy 95.7 90.2) (xy 95.6 90.3) (xy 95.6 90.5) (xy 95.4 90.7) (xy 92.1 90.7) (xy 91.7 90.3) (xy 91.7 89.2)
				(xy 92.3 88.6) (xy 95.2 88.6) (xy 95.8 88) (xy 97.1 88) (xy 97.2 88.1)
			)
		)
	)
	(zone
		(net 2)
		(net_name "Earth")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.1016)
		)
		(min_thickness 0.1016)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 96.7 88.7) (xy 96.7 89.9) (xy 95.929925 89.9) (xy 95.7 89.670075) (xy 95.7 89.2) (xy 96.2 88.7)
			)
		)
	)
	(zone
		(net 2)
		(net_name "Earth")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.1016)
		)
		(min_thickness 0.1016)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 124.5 92.8) (xy 92.6 92.8) (xy 91 91.2) (xy 91 64.9) (xy 103.8 52.1) (xy 125 52.1) (xy 127.7 54.8)
				(xy 127.7 78.1) (xy 125.8 80) (xy 125.8 91.5)
			)
		)
	)
	(zone
		(net 5)
		(net_name "+3V3")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.1016)
		)
		(min_thickness 0.1016)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 93 85.4) (xy 91.2 87.2) (xy 91.2 91.4) (xy 92.6 92.8) (xy 124.5 92.8) (xy 125.8 91.5) (xy 125.8 89.4)
				(xy 125.5 89.1) (xy 122 89.1) (xy 119 86.1) (xy 117.5 86.1) (xy 116.2 87.4) (xy 116.2 88.4) (xy 117 89.2)
				(xy 117.5 89.2) (xy 117.8 89.5) (xy 117.8 90.3) (xy 117.3 90.8) (xy 106.6 90.8) (xy 103.1 87.3)
				(xy 100.3 87.3) (xy 97.4 90.8) (xy 95.8 90.9) (xy 95.7 85.4)
			)
		)
	)
	(embedded_fonts no)
)
