(kicad_pcb
	(version 20241229)
	(generator "pcbnew")
	(generator_version "9.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "A4")
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting front back)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12.000000)
			(dashed_line_gap_ratio 3.000000)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(hpglpennumber 1)
			(hpglpenspeed 20)
			(hpglpendiameter 15.000000)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(plotinvisibletext no)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 1)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "Gerbers/")
		)
	)
	(net 0 "")
	(net 1 "Earth")
	(net 2 "+5V")
	(net 3 "+3.3V")
	(net 4 "Net-(DD3-XOUT)")
	(net 5 "Net-(DD3-XIN)")
	(net 6 "+1.1V")
	(net 7 "Net-(D1-A)")
	(net 8 "LVL_LED_1")
	(net 9 "Net-(D2-A)")
	(net 10 "LVL_LED_2")
	(net 11 "Net-(D3-A)")
	(net 12 "LVL_LED_3")
	(net 13 "Net-(D4-A)")
	(net 14 "LVL_LED_4")
	(net 15 "Net-(D5-A)")
	(net 16 "STATUS_LED_1")
	(net 17 "Net-(D6-A)")
	(net 18 "STATUS_LED_2")
	(net 19 "Net-(DD1-EN)")
	(net 20 "Net-(DD1-PS)")
	(net 21 "Net-(DD1-LX1)")
	(net 22 "Net-(DD1-LX2)")
	(net 23 "Net-(DD2-IO2)")
	(net 24 "unconnected-(DD2-EP-Pad9)")
	(net 25 "Net-(DD2-IO3)")
	(net 26 "Net-(DD2-~{CS})")
	(net 27 "Net-(DD2-DO(IO1))")
	(net 28 "Net-(DD2-DI(IO0))")
	(net 29 "Net-(DD2-CLK)")
	(net 30 "USB-_")
	(net 31 "unconnected-(DD3-GPIO16-Pad27)")
	(net 32 "CLK4")
	(net 33 "unconnected-(DD3-GPIO1-Pad3)")
	(net 34 "unconnected-(DD3-GPIO0-Pad2)")
	(net 35 "CLK1")
	(net 36 "CLK2")
	(net 37 "DAT2")
	(net 38 "CLK3")
	(net 39 "unconnected-(DD3-GPIO27_ADC1-Pad39)")
	(net 40 "DAT3")
	(net 41 "unconnected-(DD3-GPIO26_ADC0-Pad38)")
	(net 42 "Net-(DD3-RUN)")
	(net 43 "SPH0645_WS")
	(net 44 "unconnected-(DD3-GPIO28_ADC2-Pad40)")
	(net 45 "DAT4")
	(net 46 "unconnected-(DD3-GPIO23-Pad35)")
	(net 47 "USB+_")
	(net 48 "unconnected-(DD3-SWD-Pad25)")
	(net 49 "unconnected-(DD3-GPIO4-Pad6)")
	(net 50 "unconnected-(DD3-GPIO29_ADC3-Pad41)")
	(net 51 "DAT1")
	(net 52 "unconnected-(DD3-SWCLK-Pad24)")
	(net 53 "USB+")
	(net 54 "USB-")
	(net 55 "Net-(R11-Pad1)")
	(net 56 "unconnected-(DD3-GPIO22-Pad34)")
	(net 57 "unconnected-(DD3-GPIO3-Pad5)")
	(net 58 "unconnected-(DD3-GPIO6-Pad8)")
	(net 59 "unconnected-(DD3-GPIO5-Pad7)")
	(net 60 "unconnected-(DD3-GPIO2-Pad4)")
	(net 61 "unconnected-(DD3-GPIO7-Pad9)")
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 135.38 102.7)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at -0.058299 1.546799 180)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 6 "+1.1V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Sensor_Audio:Knowles_SPH0645LM4H-6_3.5x2.65mm"
		(layer "F.Cu")
		(at 140.67 97.452884 90)
		(descr "Knowles MEMS I2S Microphone: https://www.knowles.com/subdepartment/dpt-microphones/subdpt-sisonic-surface-mount-mems")
		(tags "microphone MEMS I2S SPH0645LM4H Knowles")
		(property "Reference" "MK3"
			(at 1.952884 -0.07 180)
			(layer "F.SilkS")
		)
		(property "Value" "SPH0645LM4H"
			(at 0 2.9 90)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://www.knowles.com/docs/default-source/default-document-library/sph0645lm4h-1-datasheet.pdf"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Knowles MEMS Microphone, 24-bit I2S, 65 dBA SNR, LGA-6"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Knowles*SPH0645LM4H*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.01 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at 0 0.71 90)
			(size 0.5 0.5)
			(drill 0.5)
			(layers "*.Mask")
		)
		(pad "1" smd roundrect
			(at -0.9 -1.364 90)
			(size 0.6 0.522)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "SPH0645_WS")
			(pinfunction "WS")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9 -0.542 90)
			(size 0.6 0.522)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pinfunction "SEL")
			(pintype "input")
		)
		(pad "3" smd custom
			(at 0.662 0.71 180)
			(size 0.3 0.3)
			(layers "F.Cu" "F.Mask")
			(net 1 "Earth")
			(pinfunction "GND")
			(pintype "power_in")
			(options
				(clearance outline)
				(anchor circle)
			)
			(primitives
				(gr_circle
					(center 0 -0.662)
					(end 0.662 -0.662)
					(width 0.3)
					(fill no)
				)
			)
		)
		(pad "4" smd roundrect
			(at 0.9 -0.542 90)
			(size 0.6 0.522)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 38 "CLK3")
			(pinfunction "BCLK")
			(pintype "input")
		)
		(pad "5" smd roundrect
			(at 0.9 -1.364 90)
			(size 0.6 0.522)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
		)
		(pad "6" smd roundrect
			(at 0 -1.364 90)
			(size 0.6 0.522)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "DAT3")
			(pinfunction "DATA")
			(pintype "output")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Sensor_Audio.3dshapes/Knowles_SPH0645LM4H-6_3.5x2.65mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 127.9 108.6 -90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C16"
			(at 1.8 0.6 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 270)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 270)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 131.5 98.8 90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C15"
			(at 0.3 0.9 90)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MP23DB01HPTR:MP23DB01HPTR"
		(layer "F.Cu")
		(at 140.55 103.77 90)
		(property "Reference" "MK1"
			(at -0.207676 -2.90999 180)
			(layer "F.SilkS")
		)
		(property "Value" "MP23DB01HPTR"
			(at 0 2.7215 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://item.szlcsc.com/datasheet/MP23DB01HPTR/3733773.html"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Direction:Omnidirectional Voltage - Supply:1.8V Voltage - Supply:1.8V Current Consumption:800uA Current Consumption:800uA S/N Ratio:64dB Sensitivity:-24dB Sensitivity:-24dB Impedance:-"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer Part" "MP23DB01HPTR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Manufacturer" "ST(意法半导体)"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier Part" "C3171836"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Supplier" "LCSC"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "LCSC Part Name" "MP23DB01HPTR"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(pad "1" smd rect
			(at -0.838 -1.2595 90)
			(size 0.73 0.53)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 45 "DAT4")
			(pinfunction "DOUT")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at -0.838 -0.4375 90)
			(size 0.73 0.53)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Earth")
			(pinfunction "L/R")
			(pintype "unspecified")
		)
		(pad "3" thru_hole circle
			(at 0 0.82 90)
			(size 1.640488 1.640488)
			(drill 0.8)
			(layers "*.Cu" "F.Mask" "F.Paste")
			(remove_unused_layers no)
			(net 1 "Earth")
			(pinfunction "GND")
			(pintype "unspecified")
			(thermal_bridge_angle 90)
		)
		(pad "4" smd rect
			(at 0.838 -0.4375 90)
			(size 0.73 0.53)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 32 "CLK4")
			(pinfunction "CLK")
			(pintype "unspecified")
		)
		(pad "5" smd rect
			(at 0.838 -1.2595 90)
			(size 0.73 0.53)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "+3.3V")
			(pinfunction "VDD")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/library/MP23DB01HPTR.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 126.9 108.79 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R11"
			(at -0.01 -1.1 270)
			(layer "F.SilkS")
		)
		(property "Value" "1K"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 55 "Net-(R11-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "Net-(DD2-~{CS})")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 133.731619 109.617841 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R6"
			(at 0.682159 -2.163224 90)
			(layer "F.SilkS")
		)
		(property "Value" "300R"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Net-(D2-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 125.9 100 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at -0.1 -1.2 180)
			(layer "F.SilkS")
		)
		(property "Value" "2.2uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+1.1V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 135.42 103.4)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at 0.140134 1.854911 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "TestPoint:TestPoint_Pad_D1.0mm"
		(layer "F.Cu")
		(at 135.2 101.8)
		(descr "SMD pad as test Point, diameter 1.0mm")
		(tags "test point SMD pad")
		(property "Reference" "TP1"
			(at 0 -1.448 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "TestPoint 1mm"
			(at 0.305 0.01 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "test point"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Pin* Test*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr exclude_from_pos_files)
		(fp_text user "${REFERENCE}"
			(at 0 -1.45 0)
			(layer "F.Fab")
		)
		(pad "1" smd circle
			(at 0 0)
			(size 0.6 0.6)
			(layers "F.Cu" "F.Mask")
			(net 42 "Net-(DD3-RUN)")
			(pinfunction "1")
			(pintype "passive")
		)
		(embedded_fonts no)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 131.75 108.25)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at -1.85 0.15 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 128.9 98.8 90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C13"
			(at 0.317627 1.888224 90)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0201_0603Metric"
		(layer "F.Cu")
		(at 124.8 101.7)
		(descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R4"
			(at -1.6 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "27R"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 54 "USB-")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 30 "USB-_")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 137.635784 103.128783 180)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C18"
			(at 2.435784 4.428783 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_DFN_QFN:QFN-56-1EP_7x7mm_P0.4mm_EP3.2x3.2mm"
		(layer "F.Cu")
		(at 130.5375 103.7 90)
		(descr "QFN, 56 Pin (https://datasheets.raspberrypi.com/rp2040/rp2040-datasheet.pdf#page=634), generated with kicad-footprint-generator ipc_noLead_generator.py")
		(tags "QFN NoLead")
		(property "Reference" "DD3"
			(at 1.45059 -4.473183 90)
			(layer "F.SilkS")
		)
		(property "Value" "RP2040"
			(at 0 4.83 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "https://datasheets.raspberrypi.com/rp2040/rp2040-datasheet.pdf"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "A microcontroller by Raspberry Pi"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "QFN*1EP*7x7mm?P0.4mm*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.8 -0.8 90)
			(size 1.29 1.29)
			(layers "F.Paste")
			(roundrect_rratio 0.193798)
		)
		(pad "" smd roundrect
			(at -0.8 0.8 90)
			(size 1.29 1.29)
			(layers "F.Paste")
			(roundrect_rratio 0.193798)
		)
		(pad "" smd roundrect
			(at 0.8 -0.8 90)
			(size 1.29 1.29)
			(layers "F.Paste")
			(roundrect_rratio 0.193798)
		)
		(pad "" smd roundrect
			(at 0.8 0.8 90)
			(size 1.29 1.29)
			(layers "F.Paste")
			(roundrect_rratio 0.193798)
		)
		(pad "1" smd roundrect
			(at -3.4375 -2.6 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "IOVDD")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -3.4375 -2.2 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 34 "unconnected-(DD3-GPIO0-Pad2)")
			(pinfunction "GPIO0")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -3.4375 -1.8 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 33 "unconnected-(DD3-GPIO1-Pad3)")
			(pinfunction "GPIO1")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -3.4375 -1.4 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 60 "unconnected-(DD3-GPIO2-Pad4)")
			(pinfunction "GPIO2")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at -3.4375 -1 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 57 "unconnected-(DD3-GPIO3-Pad5)")
			(pinfunction "GPIO3")
			(pintype "bidirectional")
		)
		(pad "6" smd roundrect
			(at -3.4375 -0.6 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 49 "unconnected-(DD3-GPIO4-Pad6)")
			(pinfunction "GPIO4")
			(pintype "bidirectional")
		)
		(pad "7" smd roundrect
			(at -3.4375 -0.2 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 59 "unconnected-(DD3-GPIO5-Pad7)")
			(pinfunction "GPIO5")
			(pintype "bidirectional")
		)
		(pad "8" smd roundrect
			(at -3.4375 0.2 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 58 "unconnected-(DD3-GPIO6-Pad8)")
			(pinfunction "GPIO6")
			(pintype "bidirectional")
		)
		(pad "9" smd roundrect
			(at -3.4375 0.6 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 61 "unconnected-(DD3-GPIO7-Pad9)")
			(pinfunction "GPIO7")
			(pintype "bidirectional")
		)
		(pad "10" smd roundrect
			(at -3.4375 1 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "IOVDD")
			(pintype "passive")
		)
		(pad "11" smd roundrect
			(at -3.4375 1.4 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 14 "LVL_LED_4")
			(pinfunction "GPIO8")
			(pintype "bidirectional")
		)
		(pad "12" smd roundrect
			(at -3.4375 1.8 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 12 "LVL_LED_3")
			(pinfunction "GPIO9")
			(pintype "bidirectional")
		)
		(pad "13" smd roundrect
			(at -3.4375 2.2 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 10 "LVL_LED_2")
			(pinfunction "GPIO10")
			(pintype "bidirectional")
		)
		(pad "14" smd roundrect
			(at -3.4375 2.6 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 8 "LVL_LED_1")
			(pinfunction "GPIO11")
			(pintype "bidirectional")
		)
		(pad "15" smd roundrect
			(at -2.6 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 36 "CLK2")
			(pinfunction "GPIO12")
			(pintype "bidirectional")
		)
		(pad "16" smd roundrect
			(at -2.2 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 37 "DAT2")
			(pinfunction "GPIO13")
			(pintype "bidirectional")
		)
		(pad "17" smd roundrect
			(at -1.8 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 45 "DAT4")
			(pinfunction "GPIO14")
			(pintype "bidirectional")
		)
		(pad "18" smd roundrect
			(at -1.4 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 32 "CLK4")
			(pinfunction "GPIO15")
			(pintype "bidirectional")
		)
		(pad "19" smd roundrect
			(at -1 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pinfunction "TESTEN")
			(pintype "input")
		)
		(pad "20" smd roundrect
			(at -0.6 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 5 "Net-(DD3-XIN)")
			(pinfunction "XIN")
			(pintype "input")
		)
		(pad "21" smd roundrect
			(at -0.2 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 4 "Net-(DD3-XOUT)")
			(pinfunction "XOUT")
			(pintype "passive")
		)
		(pad "22" smd roundrect
			(at 0.2 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "IOVDD")
			(pintype "passive")
		)
		(pad "23" smd roundrect
			(at 0.6 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+1.1V")
			(pinfunction "DVDD")
			(pintype "power_in")
		)
		(pad "24" smd roundrect
			(at 1 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 52 "unconnected-(DD3-SWCLK-Pad24)")
			(pinfunction "SWCLK")
			(pintype "input+no_connect")
		)
		(pad "25" smd roundrect
			(at 1.4 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 48 "unconnected-(DD3-SWD-Pad25)")
			(pinfunction "SWD")
			(pintype "bidirectional+no_connect")
		)
		(pad "26" smd roundrect
			(at 1.8 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 42 "Net-(DD3-RUN)")
			(pinfunction "RUN")
			(pintype "input")
		)
		(pad "27" smd roundrect
			(at 2.2 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 31 "unconnected-(DD3-GPIO16-Pad27)")
			(pinfunction "GPIO16")
			(pintype "bidirectional")
		)
		(pad "28" smd roundrect
			(at 2.6 3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 43 "SPH0645_WS")
			(pinfunction "GPIO17")
			(pintype "bidirectional")
		)
		(pad "29" smd roundrect
			(at 3.4375 2.6 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 51 "DAT1")
			(pinfunction "GPIO18")
			(pintype "bidirectional")
		)
		(pad "30" smd roundrect
			(at 3.4375 2.2 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 35 "CLK1")
			(pinfunction "GPIO19")
			(pintype "bidirectional")
		)
		(pad "31" smd roundrect
			(at 3.4375 1.8 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 40 "DAT3")
			(pinfunction "GPIO20")
			(pintype "bidirectional")
		)
		(pad "32" smd roundrect
			(at 3.4375 1.4 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 38 "CLK3")
			(pinfunction "GPIO21")
			(pintype "bidirectional")
		)
		(pad "33" smd roundrect
			(at 3.4375 1 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "IOVDD")
			(pintype "passive")
		)
		(pad "34" smd roundrect
			(at 3.4375 0.6 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 56 "unconnected-(DD3-GPIO22-Pad34)")
			(pinfunction "GPIO22")
			(pintype "bidirectional")
		)
		(pad "35" smd roundrect
			(at 3.4375 0.2 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 46 "unconnected-(DD3-GPIO23-Pad35)")
			(pinfunction "GPIO23")
			(pintype "bidirectional")
		)
		(pad "36" smd roundrect
			(at 3.4375 -0.2 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 16 "STATUS_LED_1")
			(pinfunction "GPIO24")
			(pintype "bidirectional")
		)
		(pad "37" smd roundrect
			(at 3.4375 -0.6 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 18 "STATUS_LED_2")
			(pinfunction "GPIO25")
			(pintype "bidirectional")
		)
		(pad "38" smd roundrect
			(at 3.4375 -1 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 41 "unconnected-(DD3-GPIO26_ADC0-Pad38)")
			(pinfunction "GPIO26_ADC0")
			(pintype "bidirectional")
		)
		(pad "39" smd roundrect
			(at 3.4375 -1.4 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 39 "unconnected-(DD3-GPIO27_ADC1-Pad39)")
			(pinfunction "GPIO27_ADC1")
			(pintype "bidirectional")
		)
		(pad "40" smd roundrect
			(at 3.4375 -1.8 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 44 "unconnected-(DD3-GPIO28_ADC2-Pad40)")
			(pinfunction "GPIO28_ADC2")
			(pintype "bidirectional")
		)
		(pad "41" smd roundrect
			(at 3.4375 -2.2 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 50 "unconnected-(DD3-GPIO29_ADC3-Pad41)")
			(pinfunction "GPIO29_ADC3")
			(pintype "bidirectional")
		)
		(pad "42" smd roundrect
			(at 3.4375 -2.6 90)
			(size 0.875 0.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "IOVDD")
			(pintype "passive")
		)
		(pad "43" smd roundrect
			(at 2.6 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "ADC_AVDD")
			(pintype "power_in")
		)
		(pad "44" smd roundrect
			(at 2.2 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "VREG_IN")
			(pintype "power_in")
		)
		(pad "45" smd roundrect
			(at 1.8 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+1.1V")
			(pinfunction "VREG_VOUT")
			(pintype "power_out")
		)
		(pad "46" smd roundrect
			(at 1.4 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 30 "USB-_")
			(pinfunction "USB_DM")
			(pintype "bidirectional")
		)
		(pad "47" smd roundrect
			(at 1 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 47 "USB+_")
			(pinfunction "USB_DP")
			(pintype "bidirectional")
		)
		(pad "48" smd roundrect
			(at 0.6 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "USB_VDD")
			(pintype "power_in")
		)
		(pad "49" smd roundrect
			(at 0.2 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pinfunction "IOVDD")
			(pintype "passive")
		)
		(pad "50" smd roundrect
			(at -0.2 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+1.1V")
			(pinfunction "DVDD")
			(pintype "passive")
		)
		(pad "51" smd roundrect
			(at -0.6 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 25 "Net-(DD2-IO3)")
			(pinfunction "QSPI_SD3")
			(pintype "bidirectional")
		)
		(pad "52" smd roundrect
			(at -1 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 29 "Net-(DD2-CLK)")
			(pinfunction "QSPI_SCLK")
			(pintype "output")
		)
		(pad "53" smd roundrect
			(at -1.4 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 28 "Net-(DD2-DI(IO0))")
			(pinfunction "QSPI_SD0")
			(pintype "bidirectional")
		)
		(pad "54" smd roundrect
			(at -1.8 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 23 "Net-(DD2-IO2)")
			(pinfunction "QSPI_SD2")
			(pintype "bidirectional")
		)
		(pad "55" smd roundrect
			(at -2.2 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 27 "Net-(DD2-DO(IO1))")
			(pinfunction "QSPI_SD1")
			(pintype "bidirectional")
		)
		(pad "56" smd roundrect
			(at -2.6 -3.4375 90)
			(size 0.2 0.875)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 26 "Net-(DD2-~{CS})")
			(pinfunction "QSPI_SS")
			(pintype "bidirectional")
		)
		(pad "57" smd rect
			(at 0 0 90)
			(size 3.2 3.2)
			(property pad_prop_heatsink)
			(layers "F.Cu" "F.Mask")
			(net 1 "Earth")
			(pinfunction "GND")
			(pintype "power_in")
			(zone_connect 2)
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Package_DFN_QFN.3dshapes/QFN-56-1EP_7x7mm_P0.4mm_EP3.2x3.2mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 125 103.6 180)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C14"
			(at 0.1 -1.9 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 131.731619 109.617841 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R8"
			(at 0.682159 2.136776 90)
			(layer "F.SilkS")
		)
		(property "Value" "300R"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 13 "Net-(D4-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 132.731619 109.617841 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R7"
			(at 0.682159 2.036776 90)
			(layer "F.SilkS")
		)
		(property "Value" "300R"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 11 "Net-(D3-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 124.9 104.5 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at 0.4 -2.1 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.2uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 6 "+1.1V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 137.7 96.3 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C24"
			(at 0.1 0.9 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.2uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Resistor_SMD:R_0201_0603Metric"
		(layer "F.Cu")
		(at 124.8 102.4)
		(descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "resistor")
		(property "Reference" "R3"
			(at -1.6 0.4 0)
			(layer "F.SilkS")
		)
		(property "Value" "27R"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 53 "USB+")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 47 "USB+_")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "F.Cu")
		(at 134.731619 109.617841 -90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R5"
			(at 0.682159 -2.263224 90)
			(layer "F.SilkS")
		)
		(property "Value" "300R"
			(at 0 1.17 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 270)
			(size 0.54 0.64)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(D1-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_1008_2520Metric"
		(layer "F.Cu")
		(at 127.4 96.6 180)
		(descr "Inductor SMD 1008 (2520 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://ecsxtal.com/store/pdf/ECS-MPI2520-SMD-POWER-INDUCTOR.pdf), generated with kicad-footprint-generator")
		(tags "inductor")
		(property "Reference" "L1"
			(at 0 1.7 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.2uH"
			(at 0 2.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.075 0 180)
			(size 1.25 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 21 "Net-(DD1-LX1)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.075 0 180)
			(size 1.25 2.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.2)
			(net 22 "Net-(DD1-LX2)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_1008_2520Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 137.6 97.2 180)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C20"
			(at 0 -0.9 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 137.504575 102.310519 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C21"
			(at 2.304575 4.710519 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.2uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "MP34DT01:MP34DT01"
		(layer "F.Cu")
		(at 140.647083 100.732 90)
		(property "Reference" "MK2"
			(at 1.032 -3.247083 180)
			(layer "F.SilkS")
		)
		(property "Value" "MP34DT01TR-M"
			(at 8.37112 3.039045 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "MP34DT01-M Series MEMS Audio Sensor Omnidirectional Digital Microphone - HCLGA"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "STMicroelectronics"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PACKAGE" "HCLGA"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MPN" "MP34DT01TR-M"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PRICE" "--"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "None"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/MP34DT01TRM/STMicroelectronics/view-part/?ref=eda"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturers recommendation"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "3"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/MP34DT01TRM/STMicroelectronics/view-part/?ref=snap"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "MP34DT01TRM"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "AVAILABILITY" "In stock"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "20 Hz ~ 10 kHz Digital, PDM Microphone MEMS (Silicon) 1.64 V ~ 3.6 V Omnidirectional (-26dB ±3dB @ 94dB SPL) Solder Pads"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(pad "1" smd rect
			(at -0.425 -0.675 90)
			(size 0.45 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 3 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at -0.425 0.675 90)
			(size 0.45 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Earth")
			(pinfunction "LR")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at 0.425 0.675 90)
			(size 0.45 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 35 "CLK1")
			(pinfunction "CLK")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd rect
			(at 0.425 -0.675 90)
			(size 0.45 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 51 "DAT1")
			(pinfunction "DOUT")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd custom
			(at -1 -1.75 90)
			(size 0.05 0.05)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net 1 "Earth")
			(pinfunction "GND")
			(pintype "power_in")
			(solder_mask_margin 0.102)
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.1 -0.15) (xy 2.4 -0.15) (xy 2.4 3.65) (xy 1 3.65) (xy 1 3.3) (xy 1.925 3.3) (xy 1.932 3.3)
						(xy 1.938 3.299) (xy 1.945 3.298) (xy 1.951 3.297) (xy 1.957 3.296) (xy 1.964 3.294) (xy 1.97 3.292)
						(xy 1.976 3.289) (xy 1.982 3.286) (xy 1.988 3.283) (xy 1.993 3.28) (xy 1.998 3.276) (xy 2.004 3.272)
						(xy 2.009 3.268) (xy 2.013 3.263) (xy 2.018 3.259) (xy 2.022 3.254) (xy 2.026 3.248) (xy 2.03 3.243)
						(xy 2.033 3.238) (xy 2.036 3.232) (xy 2.039 3.226) (xy 2.042 3.22) (xy 2.044 3.214) (xy 2.046 3.207)
						(xy 2.047 3.201) (xy 2.048 3.195) (xy 2.049 3.188) (xy 2.05 3.182) (xy 2.05 3.175) (xy 2.05 0.325)
						(xy 2.05 0.318) (xy 2.049 0.312) (xy 2.048 0.305) (xy 2.047 0.299) (xy 2.046 0.293) (xy 2.044 0.286)
						(xy 2.042 0.28) (xy 2.039 0.274) (xy 2.036 0.268) (xy 2.033 0.262) (xy 2.03 0.257) (xy 2.026 0.252)
						(xy 2.022 0.246) (xy 2.018 0.241) (xy 2.013 0.237) (xy 2.009 0.232) (xy 2.004 0.228) (xy 1.998 0.224)
						(xy 1.993 0.22) (xy 1.988 0.217) (xy 1.982 0.214) (xy 1.976 0.211) (xy 1.97 0.208) (xy 1.964 0.206)
						(xy 1.957 0.204) (xy 1.951 0.203) (xy 1.945 0.202) (xy 1.938 0.201) (xy 1.932 0.2) (xy 1.925 0.2)
						(xy 0.075 0.2) (xy 0.068 0.2) (xy 0.062 0.201) (xy 0.055 0.202) (xy 0.049 0.203) (xy 0.043 0.204)
						(xy 0.036 0.206) (xy 0.03 0.208) (xy 0.024 0.211) (xy 0.018 0.214) (xy 0.012 0.217) (xy 0.007 0.22)
						(xy 0.002 0.224) (xy -0.004 0.228) (xy -0.009 0.232) (xy -0.013 0.237) (xy -0.018 0.241) (xy -0.022 0.246)
						(xy -0.026 0.252) (xy -0.03 0.257) (xy -0.033 0.262) (xy -0.036 0.268) (xy -0.039 0.274) (xy -0.042 0.28)
						(xy -0.044 0.286) (xy -0.046 0.293) (xy -0.047 0.299) (xy -0.048 0.305) (xy -0.049 0.312) (xy -0.05 0.318)
						(xy -0.05 0.325) (xy -0.05 3.175) (xy -0.05 3.182) (xy -0.049 3.188) (xy -0.048 3.195) (xy -0.047 3.201)
						(xy -0.046 3.207) (xy -0.044 3.214) (xy -0.042 3.22) (xy -0.039 3.226) (xy -0.036 3.232) (xy -0.033 3.238)
						(xy -0.03 3.243) (xy -0.026 3.248) (xy -0.022 3.254) (xy -0.018 3.259) (xy -0.013 3.263) (xy -0.009 3.268)
						(xy -0.004 3.272) (xy 0.002 3.276) (xy 0.007 3.28) (xy 0.012 3.283) (xy 0.018 3.286) (xy 0.024 3.289)
						(xy 0.03 3.292) (xy 0.036 3.294) (xy 0.043 3.296) (xy 0.049 3.297) (xy 0.055 3.298) (xy 0.062 3.299)
						(xy 0.068 3.3) (xy 0.075 3.3) (xy 1 3.3) (xy 1 3.65) (xy -0.4 3.65) (xy -0.4 0.15) (xy -0.1 -0.15)
					)
					(width 0)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/library/MP34DT01TRM--3DModel-STEP-510211.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 137.5 101.4 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C22"
			(at 2.3 4.9 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.2uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 137.399608 100.564255 180)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C19"
			(at 2.199608 5.164255 0)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.05 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 0)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "INMP441:INMP441"
		(layer "F.Cu")
		(at 139.97 107.27 180)
		(property "Reference" "MK4"
			(at 0.07 -2.53 0)
			(layer "F.SilkS")
		)
		(property "Value" "INMP441ACEZ-R7"
			(at 6.644 3.258 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "TDK InvenSense"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "1.05 mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "LGA-9 TDK InvenSense"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/INMP441ACEZ-R7/TDK/view-part/?ref=eda"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "1.1"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/INMP441ACEZ-R7/TDK/view-part/?ref=snap"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "INMP441ACEZ-R7"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "60 Hz ~ 15 kHz Digital, I2S Microphone MEMS (Silicon) 1.62 V ~ 3.63 V Omnidirectional (-26dB ±3dB @ 94dB SPL) Solder Pads"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "TDK InvenSense"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(pad "" np_thru_hole circle
			(at -1.29 0 180)
			(size 0.75 0.75)
			(drill 0.75)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" smd rect
			(at 1.87 -1.33 180)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask")
			(net 36 "CLK2")
			(pinfunction "SCK")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0.82 -1.33 180)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask")
			(net 37 "DAT2")
			(pinfunction "SD")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at -0.23 -1.33 180)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask")
			(net 43 "SPH0645_WS")
			(pinfunction "WS")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd rect
			(at -1.28 -1.33 180)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask")
			(net 1 "Earth")
			(pinfunction "L/R")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd custom
			(at -1.92 0 180)
			(size 0.1 0.1)
			(layers "F.Cu")
			(net 1 "Earth")
			(pinfunction "GND")
			(pintype "power_in")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 1.41 -0.0025) (xy 1.11 -0.003) (xy 1.109 -0.026) (xy 1.107 -0.051) (xy 1.104 -0.076) (xy 1.1 -0.101)
						(xy 1.094 -0.125) (xy 1.087 -0.149) (xy 1.078 -0.173) (xy 1.069 -0.196) (xy 1.058 -0.219) (xy 1.046 -0.241)
						(xy 1.033 -0.262) (xy 1.019 -0.283) (xy 1.003 -0.303) (xy 0.987 -0.322) (xy 0.97 -0.34) (xy 0.952 -0.357)
						(xy 0.933 -0.373) (xy 0.913 -0.389) (xy 0.892 -0.403) (xy 0.871 -0.416) (xy 0.849 -0.428) (xy 0.826 -0.439)
						(xy 0.803 -0.448) (xy 0.779 -0.457) (xy 0.755 -0.464) (xy 0.731 -0.47) (xy 0.706 -0.474) (xy 0.681 -0.477)
						(xy 0.656 -0.479) (xy 0.63 -0.48) (xy 0.605 -0.479) (xy 0.58 -0.477) (xy 0.555 -0.474) (xy 0.53 -0.47)
						(xy 0.506 -0.464) (xy 0.482 -0.457) (xy 0.458 -0.448) (xy 0.435 -0.439) (xy 0.412 -0.428) (xy 0.39 -0.416)
						(xy 0.369 -0.403) (xy 0.348 -0.388) (xy 0.328 -0.373) (xy 0.309 -0.357) (xy 0.291 -0.339) (xy 0.273 -0.321)
						(xy 0.257 -0.302) (xy 0.242 -0.282) (xy 0.227 -0.261) (xy 0.214 -0.24) (xy 0.202 -0.218) (xy 0.191 -0.195)
						(xy 0.182 -0.172) (xy 0.173 -0.148) (xy 0.166 -0.124) (xy 0.16 -0.1) (xy 0.156 -0.075) (xy 0.153 -0.05)
						(xy 0.151 -0.025) (xy 0.15 0) (xy 0.151 0.025) (xy 0.153 0.05) (xy 0.156 0.075) (xy 0.16 0.1)
						(xy 0.166 0.124) (xy 0.173 0.148) (xy 0.182 0.172) (xy 0.191 0.195) (xy 0.202 0.218) (xy 0.214 0.24)
						(xy 0.227 0.261) (xy 0.242 0.282) (xy 0.257 0.302) (xy 0.273 0.321) (xy 0.291 0.339) (xy 0.309 0.357)
						(xy 0.328 0.373) (xy 0.348 0.388) (xy 0.369 0.403) (xy 0.39 0.416) (xy 0.412 0.428) (xy 0.435 0.439)
						(xy 0.458 0.448) (xy 0.482 0.457) (xy 0.506 0.464) (xy 0.53 0.47) (xy 0.555 0.474) (xy 0.58 0.477)
						(xy 0.605 0.479) (xy 0.63 0.48) (xy 0.656 0.479) (xy 0.681 0.477) (xy 0.706 0.474) (xy 0.731 0.47)
						(xy 0.755 0.464) (xy 0.779 0.457) (xy 0.803 0.448) (xy 0.826 0.439) (xy 0.849 0.428) (xy 0.871 0.416)
						(xy 0.892 0.403) (xy 0.913 0.389) (xy 0.933 0.373) (xy 0.952 0.357) (xy 0.97 0.34) (xy 0.987 0.322)
						(xy 1.003 0.303) (xy 1.019 0.283) (xy 1.033 0.262) (xy 1.046 0.241) (xy 1.058 0.219) (xy 1.069 0.196)
						(xy 1.078 0.173) (xy 1.087 0.149) (xy 1.094 0.125) (xy 1.1 0.101) (xy 1.104 0.076) (xy 1.107 0.051)
						(xy 1.109 0.026) (xy 1.11 0.003) (xy 1.41 0.003) (xy 1.409 0.042) (xy 1.406 0.083) (xy 1.4 0.123)
						(xy 1.393 0.163) (xy 1.383 0.203) (xy 1.372 0.242) (xy 1.358 0.28) (xy 1.343 0.318) (xy 1.325 0.355)
						(xy 1.306 0.391) (xy 1.284 0.425) (xy 1.261 0.459) (xy 1.236 0.491) (xy 1.21 0.522) (xy 1.182 0.552)
						(xy 1.152 0.58) (xy 1.121 0.606) (xy 1.089 0.631) (xy 1.055 0.654) (xy 1.021 0.676) (xy 0.985 0.695)
						(xy 0.948 0.713) (xy 0.91 0.728) (xy 0.872 0.742) (xy 0.833 0.753) (xy 0.793 0.763) (xy 0.753 0.77)
						(xy 0.713 0.776) (xy 0.672 0.779) (xy 0.63 0.78) (xy 0.589 0.779) (xy 0.548 0.776) (xy 0.508 0.77)
						(xy 0.468 0.763) (xy 0.428 0.753) (xy 0.389 0.742) (xy 0.35 0.728) (xy 0.313 0.713) (xy 0.276 0.695)
						(xy 0.24 0.675) (xy 0.205 0.654) (xy 0.172 0.631) (xy 0.139 0.606) (xy 0.108 0.58) (xy 0.078 0.552)
						(xy 0.05 0.522) (xy 0.024 0.491) (xy -0.001 0.458) (xy -0.024 0.425) (xy -0.045 0.39) (xy -0.065 0.354)
						(xy -0.083 0.317) (xy -0.098 0.28) (xy -0.112 0.241) (xy -0.123 0.202) (xy -0.133 0.162) (xy -0.14 0.122)
						(xy -0.146 0.082) (xy -0.149 0.041) (xy -0.15 0) (xy -0.149 -0.041) (xy -0.146 -0.082) (xy -0.14 -0.122)
						(xy -0.133 -0.162) (xy -0.123 -0.202) (xy -0.112 -0.241) (xy -0.098 -0.28) (xy -0.083 -0.317)
						(xy -0.065 -0.354) (xy -0.045 -0.39) (xy -0.024 -0.425) (xy -0.001 -0.458) (xy 0.024 -0.491) (xy 0.05 -0.522)
						(xy 0.078 -0.552) (xy 0.108 -0.58) (xy 0.139 -0.606) (xy 0.172 -0.631) (xy 0.205 -0.654) (xy 0.24 -0.675)
						(xy 0.276 -0.695) (xy 0.313 -0.713) (xy 0.35 -0.728) (xy 0.389 -0.742) (xy 0.428 -0.753) (xy 0.468 -0.763)
						(xy 0.508 -0.77) (xy 0.548 -0.776) (xy 0.589 -0.779) (xy 0.63 -0.78) (xy 0.672 -0.779) (xy 0.713 -0.776)
						(xy 0.753 -0.77) (xy 0.793 -0.763) (xy 0.833 -0.753) (xy 0.872 -0.742) (xy 0.91 -0.728) (xy 0.948 -0.713)
						(xy 0.985 -0.695) (xy 1.021 -0.676) (xy 1.055 -0.654) (xy 1.089 -0.631) (xy 1.121 -0.606) (xy 1.152 -0.58)
						(xy 1.182 -0.552) (xy 1.21 -0.522) (xy 1.236 -0.491) (xy 1.261 -0.459) (xy 1.284 -0.425) (xy 1.306 -0.391)
						(xy 1.325 -0.355) (xy 1.343 -0.318) (xy 1.358 -0.28) (xy 1.372 -0.242) (xy 1.383 -0.203) (xy 1.393 -0.163)
						(xy 1.4 -0.123) (xy 1.406 -0.083) (xy 1.409 -0.042) (xy 1.41 -0.003) (xy 1.41 -0.0025)
					)
					(width 0.01)
					(fill yes)
				)
			)
		)
		(pad "6" smd rect
			(at -1.28 1.33 180)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask")
			(net 1 "Earth")
			(pinfunction "GND__1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "7" smd rect
			(at -0.23 1.33 180)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask")
			(net 3 "+3.3V")
			(pinfunction "VDD")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "8" smd rect
			(at 0.82 1.33 180)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask")
			(net 3 "+3.3V")
			(pinfunction "CHIPEN")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "9" smd rect
			(at 1.87 1.33 180)
			(size 0.4 0.6)
			(layers "F.Cu" "F.Mask")
			(net 1 "Earth")
			(pinfunction "GND__2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/library/INMP441ACEZ-R7.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 136.9 106.2 90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C25"
			(at -2.016466 0.044707 90)
			(layer "F.SilkS")
		)
		(property "Value" "2.2uF"
			(at 0 1.16 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 90)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "F.Cu")
		(at 126.8 98.6 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C17"
			(at 2.2 0 0)
			(layer "F.SilkS")
		)
		(property "Value" "2.2uF"
			(at 0 1.16 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 136.01 106.4 90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C23"
			(at -1.82274 -0.150791 90)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "F.Cu")
		(at 128.1 98.8 90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C12"
			(at 0.317627 1.588224 90)
			(layer "F.SilkS")
		)
		(property "Value" "100nF"
			(at 0 1.05 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 -0.68 90)
			(layer "F.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "F.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 90)
			(size 0.46 0.4)
			(layers "F.Cu" "F.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "B.Cu")
		(at 131.9 101.2)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R2"
			(at 1.8 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "100K"
			(at 0 -1.17 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 20 "Net-(DD1-PS)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_USB:USB_A_Connfly_DS1098_Horizontal"
		(layer "B.Cu")
		(at 114.7 102.55 180)
		(descr "USB type A Plug, Horizontal, https://en.connfly.com/static/upload/file//DS1098.pdf")
		(tags "USB-A")
		(property "Reference" "J1"
			(at -8.1 7.45 0)
			(layer "B.SilkS")
		)
		(property "Value" "USB_A"
			(at 0 -9 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "USB Type A connector"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "USB*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "PCB Edge"
			(at -4.3 0 90)
			(layer "Dwgs.User")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "" np_thru_hole circle
			(at -8.3 -2.25 180)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at -8.3 2.25 180)
			(size 1.2 1.2)
			(drill 1.2)
			(layers "*.Mask")
		)
		(pad "1" smd roundrect
			(at -10.55 3.5 180)
			(size 2.5 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+5V")
			(pinfunction "VBUS")
			(pintype "power_in")
		)
		(pad "2" smd roundrect
			(at -10.55 1 180)
			(size 2.5 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 54 "USB-")
			(pinfunction "D-")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at -10.55 -1 180)
			(size 2.5 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 53 "USB+")
			(pinfunction "D+")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at -10.55 -3.5 180)
			(size 2.5 1)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pinfunction "GND")
			(pintype "power_in")
		)
		(pad "5" thru_hole oval
			(at -8.3 -5.85 180)
			(size 3.8 1.4)
			(drill oval 2.5 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Earth")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(pad "5" thru_hole oval
			(at -8.3 5.85 180)
			(size 3.8 1.4)
			(drill oval 2.5 0.9)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net 1 "Earth")
			(pinfunction "Shield")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/library/USB Type A.step"
			(offset
				(xyz 0 0 -1.2)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -90)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "B.Cu")
		(at 133.9 102)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 1.7 -0.1 0)
			(layer "B.SilkS")
		)
		(property "Value" "15pF"
			(at 0 -1.05 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.68 0)
			(layer "B.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0)
			(size 0.46 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 4 "Net-(DD3-XOUT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0)
			(size 0.46 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "W25Q16JVUXIQ:W25Q16JVUXIQ"
		(layer "B.Cu")
		(at 129.1 105.8)
		(descr "USON 2x3x0.6-mm")
		(tags "Integrated Circuit")
		(property "Reference" "DD2"
			(at 0.1 -1.7 0)
			(layer "B.SilkS")
		)
		(property "Value" "W25Q16JVUXIQ_TR"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://componentsearchengine.com/Datasheets/1/W25Q16JVUXIQ TR.pdf"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "NOR Flash spiFlash, 3V, 16M-bit, 4Kb Uniform Sector, DTR"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Height" "0.6"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "Winbond"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "W25Q16JVUXIQ TR"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "454-W25Q16JVUXIQTR"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Winbond/W25Q16JVUXIQ-TR?qs=qSfuJ%252Bfl%2Fd7SDdIHLGOd1g%3D%3D"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" "W25Q16JVUXIQ TR"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" "https://www.arrow.com/en/products/w25q16jvuxiqtr/winbond-electronics?utm_currency=USD&region=nac"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.4 0.75 270)
			(size 0.3 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 26 "Net-(DD2-~{CS})")
			(pinfunction "~{CS}")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.4 0.25 270)
			(size 0.3 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 27 "Net-(DD2-DO(IO1))")
			(pinfunction "DO(IO1)")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.4 -0.25 270)
			(size 0.3 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 23 "Net-(DD2-IO2)")
			(pinfunction "IO2")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.4 -0.75 270)
			(size 0.3 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "Earth")
			(pinfunction "GND")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at 1.4 -0.75 270)
			(size 0.3 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 28 "Net-(DD2-DI(IO0))")
			(pinfunction "DI(IO0)")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 1.4 -0.25 270)
			(size 0.3 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 29 "Net-(DD2-CLK)")
			(pinfunction "CLK")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 1.4 0.25 270)
			(size 0.3 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 25 "Net-(DD2-IO3)")
			(pinfunction "IO3")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 1.4 0.75 270)
			(size 0.3 0.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "+3.3V")
			(pinfunction "VCC")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 0 0)
			(size 0.25 1.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 24 "unconnected-(DD2-EP-Pad9)")
			(pinfunction "EP")
			(pintype "passive+no_connect")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/library/W25Q16JVUXIQ_TR.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0402_1005Metric"
		(layer "B.Cu")
		(at 132.645737 109.616661 -90)
		(descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D3"
			(at -1.701661 -0.954263 90)
			(layer "B.SilkS")
		)
		(property "Value" "LED"
			(at 0 -1.17 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 270)
			(size 0.59 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 12 "LVL_LED_3")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.485 0 270)
			(size 0.59 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 11 "Net-(D3-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0402_1005Metric"
		(layer "B.Cu")
		(at 131.645737 109.601661 -90)
		(descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D4"
			(at -1.701661 -0.954263 90)
			(layer "B.SilkS")
		)
		(property "Value" "LED"
			(at 0 -1.17 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 270)
			(size 0.59 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 14 "LVL_LED_4")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.485 0 270)
			(size 0.59 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 13 "Net-(D4-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0402_1005Metric"
		(layer "B.Cu")
		(at 133.71 96.685 -90)
		(descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D5"
			(at 0.015 -2.19 90)
			(layer "B.SilkS")
		)
		(property "Value" "LED"
			(at 0 -1.17 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 270)
			(size 0.59 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 16 "STATUS_LED_1")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.485 0 270)
			(size 0.59 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 15 "Net-(D5-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "B.Cu")
		(at 131.9 100.2 180)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R1"
			(at -1.8 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "100K"
			(at 0 -1.17 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 180)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 180)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 19 "Net-(DD1-EN)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Crystal:Crystal_SMD_3225-4Pin_3.2x2.5mm"
		(layer "B.Cu")
		(at 134 104.1)
		(descr "SMD Crystal SERIES SMD3225/4 http://www.txccrystal.com/images/pdf/7m-accuracy.pdf, 3.2x2.5mm^2 package")
		(tags "SMD SMT crystal")
		(property "Reference" "Y1"
			(at -2.8 -1.1 0)
			(layer "B.SilkS")
		)
		(property "Value" "ABM8-272-T3"
			(at 0 -2.45 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Four pin crystal, GND on pins 2 and 4"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Crystal*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.1 -0.85)
			(size 1.4 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 4 "Net-(DD3-XOUT)")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 1.1 -0.85)
			(size 1.4 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "Earth")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at 1.1 0.85)
			(size 1.4 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 5 "Net-(DD3-XIN)")
			(pinfunction "3")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.1 0.85)
			(size 1.4 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "Earth")
			(pinfunction "4")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Crystal.3dshapes/Crystal_SMD_3225-4Pin_3.2x2.5mm.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Button_Switch_SMD:SW_SPST_PTS810"
		(layer "B.Cu")
		(at 128.283017 108.950846 180)
		(descr "C&K Components, PTS 810 Series, Microminiature SMT Top Actuated, http://www.ckswitches.com/media/1476/pts810.pdf")
		(tags "SPST Button Switch")
		(property "Reference" "SW1"
			(at 3.983017 -1.149154 180)
			(layer "B.SilkS")
		)
		(property "Value" "KMR221GLFS"
			(at 0 -2.6 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -2.075 1.075 180)
			(size 1.05 0.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "Earth")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "1" smd rect
			(at 2.075 1.075 180)
			(size 1.05 0.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "Earth")
			(pinfunction "1")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -2.075 -1.075 180)
			(size 1.05 0.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 55 "Net-(R11-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at 2.075 -1.075 180)
			(size 1.05 0.65)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 55 "Net-(R11-Pad1)")
			(pinfunction "2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/library/KMR221GLFS--3DModel-STEP-56544.STEP"
			(offset
				(xyz 0 0 1.4)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "LED_SMD:LED_0402_1005Metric"
		(layer "B.Cu")
		(at 132.71 96.685 -90)
		(descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D6"
			(at 0.015 -2.09 90)
			(layer "B.SilkS")
		)
		(property "Value" "LED"
			(at 0 -1.17 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 270)
			(size 0.59 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 18 "STATUS_LED_2")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.485 0 270)
			(size 0.59 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 17 "Net-(D6-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "RT6150B-33GQW:RT6150B-33GQW"
		(layer "B.Cu")
		(at 128.5625 98.3 -90)
		(descr "W-Type 10L DFN 2.5x2.5 Package")
		(tags "Integrated Circuit")
		(property "Reference" "DD1"
			(at -2.4 -0.1375 180)
			(layer "B.SilkS")
		)
		(property "Value" "RT6150B-33GQW"
			(at 0 0 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Datasheet" "https://datasheet.octopart.com/RT6150B-33GQW-Richtek-datasheet-82510503.pdf"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "IC REG BCK BST 3.3V 800MA 10WDFN"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Height" "0.8"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer_Name" "RICHTEK"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Manufacturer_Part_Number" "RT6150B-33GQW"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mouser Part Number" "835-RT6150B-33GQW"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Mouser Price/Stock" "https://www.mouser.co.uk/ProductDetail/Richtek/RT6150B-33GQW?qs=amGC7iS6iy8r3kS79wnzgg%3D%3D"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Arrow Part Number" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Arrow Price/Stock" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd rect
			(at -1.25 1 180)
			(size 0.3 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "+3.3V")
			(pinfunction "VOUT")
			(pintype "passive")
		)
		(pad "2" smd rect
			(at -1.25 0.5 180)
			(size 0.3 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 22 "Net-(DD1-LX2)")
			(pinfunction "LX2")
			(pintype "passive")
		)
		(pad "3" smd rect
			(at -1.25 0 180)
			(size 0.3 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "Earth")
			(pinfunction "GND_1")
			(pintype "passive")
		)
		(pad "4" smd rect
			(at -1.25 -0.5 180)
			(size 0.3 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 21 "Net-(DD1-LX1)")
			(pinfunction "LX1")
			(pintype "passive")
		)
		(pad "5" smd rect
			(at -1.25 -1 180)
			(size 0.3 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "+5V")
			(pinfunction "VIN")
			(pintype "passive")
		)
		(pad "6" smd rect
			(at 1.25 -1 180)
			(size 0.3 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 19 "Net-(DD1-EN)")
			(pinfunction "EN")
			(pintype "passive")
		)
		(pad "7" smd rect
			(at 1.25 -0.5 180)
			(size 0.3 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 20 "Net-(DD1-PS)")
			(pinfunction "PS")
			(pintype "passive")
		)
		(pad "8" smd rect
			(at 1.25 0 180)
			(size 0.3 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 2 "+5V")
			(pinfunction "VINA")
			(pintype "passive")
		)
		(pad "9" smd rect
			(at 1.25 0.5 180)
			(size 0.3 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "Earth")
			(pinfunction "GND_2")
			(pintype "passive")
		)
		(pad "10" smd rect
			(at 1.25 1 180)
			(size 0.3 0.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 3 "+3.3V")
			(pinfunction "FB")
			(pintype "passive")
		)
		(pad "11" smd rect
			(at 0 0 270)
			(size 1.25 2.05)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net 1 "Earth")
			(pinfunction "GND_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KIPRJMOD}/library/RT6150B-33GQW.stp"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 131.676295 106.725911 -90)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 0.021674 -1.131678 0)
			(layer "B.SilkS")
		)
		(property "Value" "2.2uF"
			(at 0 -1.16 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 270)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 270)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0402_1005Metric"
		(layer "B.Cu")
		(at 134.645737 109.616661 -90)
		(descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D1"
			(at -1.701661 -0.954263 90)
			(layer "B.SilkS")
		)
		(property "Value" "LED"
			(at 0 -1.17 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 270)
			(size 0.59 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 8 "LVL_LED_1")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.485 0 270)
			(size 0.59 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 7 "Net-(D1-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 131.2 98 -90)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at -2.1 0 0)
			(layer "B.SilkS")
		)
		(property "Value" "47uF"
			(at 0 -1.68 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 2 "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0 270)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0402_1005Metric"
		(layer "B.Cu")
		(at 133.625737 109.601661 -90)
		(descr "LED SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf), generated with kicad-footprint-generator")
		(tags "LED")
		(property "Reference" "D2"
			(at -1.701661 -0.954263 90)
			(layer "B.SilkS")
		)
		(property "Value" "LED"
			(at 0 -1.17 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 270)
			(size 0.59 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 10 "LVL_LED_2")
			(pinfunction "K")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.485 0 270)
			(size 0.59 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 9 "Net-(D2-A)")
			(pinfunction "A")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "B.Cu")
		(at 134 106.2 180)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at -1.6 -0.1 0)
			(layer "B.SilkS")
		)
		(property "Value" "15pF"
			(at 0 -1.05 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.68 0)
			(layer "B.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 180)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 180)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 180)
			(size 0.46 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 5 "Net-(DD3-XIN)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 180)
			(size 0.46 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "B.Cu")
		(at 132.7 98.6 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R10"
			(at 0.017633 2.127081 90)
			(layer "B.SilkS")
		)
		(property "Value" "300R"
			(at 0 -1.17 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 17 "Net-(D6-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "PCM_Resistor_SMD_AKL:R_0402_1005Metric"
		(layer "B.Cu")
		(at 133.71 98.6 90)
		(descr "Resistor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 72, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), Alternate KiCad Library")
		(tags "resistor")
		(property "Reference" "R9"
			(at 0.4 2.19 90)
			(layer "B.SilkS")
		)
		(property "Value" "300R"
			(at 0 -1.17 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Resistor"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.51 0 90)
			(size 0.54 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 15 "Net-(D5-A)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD6_3DMODEL_DIR}/Resistor_SMD.3dshapes/R_0402_1005Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0805_2012Metric"
		(layer "B.Cu")
		(at 128.7 101.2)
		(descr "Capacitor SMD 0805 (2012 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf, https://docs.google.com/spreadsheets/d/1BsfQQcO9C6DZCsRaXUlFlo91Tg2WpOkGARC1WS5S8t0/edit?usp=sharing), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0.1 1.3 0)
			(layer "B.SilkS")
		)
		(property "Value" "47uF"
			(at 0 -1.68 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.95 0)
			(size 1 1.45)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0805_2012Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0201_0603Metric"
		(layer "B.Cu")
		(at 131.55726 105.104568 90)
		(descr "Capacitor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 1.004568 -0.35726 0)
			(layer "B.SilkS")
		)
		(property "Value" "100nF"
			(at 0 -1.05 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "Daredevil-mini.kicad_sch")
		(attr smd)
		(fp_text user "${REFERENCE}"
			(at 0 0.68 90)
			(layer "B.Fab")
		)
		(pad "" smd roundrect
			(at -0.345 0 90)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "" smd roundrect
			(at 0.345 0 90)
			(size 0.318 0.36)
			(layers "B.Paste")
			(roundrect_rratio 0.25)
		)
		(pad "1" smd roundrect
			(at -0.32 0 90)
			(size 0.46 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 3 "+3.3V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.32 0 90)
			(size 0.46 0.4)
			(layers "B.Cu" "B.Mask")
			(roundrect_rratio 0.25)
			(net 1 "Earth")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_line
		(start 141.2 111.4)
		(end 121.2 111.4)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 141.2 93.8)
		(end 143 96)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 120 108.5)
		(end 120 96.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 121.2 93.8)
		(end 141.2 93.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143 109.25)
		(end 141.2 111.4)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 143 96)
		(end 143 109.25)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 120 96.75)
		(end 120 95.5)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 121.2 111.4)
		(end 120 109.75)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 120 95.5)
		(end 121.2 93.8)
		(layer "Edge.Cuts")
	)
	(gr_line
		(start 120 109.75)
		(end 120 108.5)
		(layer "Edge.Cuts")
	)
	(gr_text "@madjogger"
		(at 137.6 102.4 270)
		(layer "B.SilkS")
	)
	(gr_text "Daredevil-mini"
		(at 139.7 102.5 270)
		(layer "B.SilkS" knockout)
	)
	(zone
		(net 3)
		(net_name "+3.3V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 7)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 139.6 96.1) (xy 137.9 96.1) (xy 137.7 96.3) (xy 137.7 97.2) (xy 137.9 97.4) (xy 138.5 97.4)
				(xy 139 96.9) (xy 139.6 96.9)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+3.3V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 5)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 131.3 98.9) (xy 131.2 99) (xy 131.2 99.7) (xy 131.3 99.8) (xy 131.3 100.6) (xy 131.4 100.7)
				(xy 131.7 100.7) (xy 131.8 100.6) (xy 131.8 99.8) (xy 131.9 99.7) (xy 131.9 99) (xy 131.8 98.9)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+3.3V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 135.8 106.4) (xy 138.3 106.4) (xy 138.7 106) (xy 138.7 105.5) (xy 138.8 105.4) (xy 140.4 105.4)
				(xy 140.5 105.5) (xy 140.5 106.6) (xy 139.9 107.2) (xy 135.9 107.2) (xy 135.8 107.1)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+3.3V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 4)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 126.7 101.7) (xy 126.3 101.3) (xy 126.3 99.3) (xy 126.7 98.9) (xy 126.8 98.9) (xy 126.8 98.4)
				(xy 126.9 98.3) (xy 127.4 98.3) (xy 127.7 98.6) (xy 127.7 98.8) (xy 127.8 98.9) (xy 128.9 98.9)
				(xy 129 99) (xy 129 99.5) (xy 128.9 99.6) (xy 128.2 99.6) (xy 128 99.8) (xy 128 101.2) (xy 127.5 101.7)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+3.3V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 8)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 139.6 102.5) (xy 139.6 103.3) (xy 137.807001 103.3) (xy 137.635784 103.128783) (xy 137.635784 100.664216)
				(xy 137.9 100.4) (xy 138.3 100.4) (xy 138.5 100.6) (xy 138.5 102.1) (xy 138.8 102.4) (xy 139.5 102.4)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+3.3V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 2)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 1)
			(island_area_min 10)
		)
		(polygon
			(pts
				(xy 131.3 106.7) (xy 131.3 107.7) (xy 131.1 107.9) (xy 131.1 109.1) (xy 131.4 109.4) (xy 135 109.4)
				(xy 135.1 109.3) (xy 135.1 108.9) (xy 135 108.8) (xy 131.9 108.8) (xy 131.7 108.6) (xy 131.7 106.7)
			)
		)
	)
	(zone
		(net 6)
		(net_name "+1.1V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 127.6 103.8) (xy 127.488351 103.705824) (xy 126.594176 103.705824) (xy 126.3 104) (xy 125.3 104)
				(xy 125 104.3) (xy 125 104.7) (xy 125.2 104.9) (xy 125.6 104.9) (xy 126.2 104.3) (xy 126.5 104.3)
				(xy 126.6 104.2) (xy 126.6 104.1) (xy 127.5 104.1) (xy 127.6 104)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+3.3V")
		(layer "F.Cu")
		(hatch edge 0.5)
		(priority 1)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 125.2 103.8) (xy 127.6 103.8) (xy 127.6 103) (xy 126.4 103) (xy 126 103.4) (xy 125.1 103.4)
				(xy 125.1 103.7)
			)
		)
	)
	(zone
		(net 1)
		(net_name "Earth")
		(layers "F.Cu" "B.Cu")
		(hatch edge 0.5)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 121.4 94.5) (xy 120.2 95.7) (xy 120.2 109.5) (xy 121.4 110.7) (xy 140.9 110.7) (xy 142.5 109.1)
				(xy 142.5 96.2) (xy 140.8 94.5)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+3.3V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 9)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 130 106.3) (xy 130 106.7) (xy 130.1 106.8) (xy 131.602206 106.8) (xy 132 106.402206) (xy 132 105.5)
				(xy 131.7 105.2) (xy 131.3 105.2) (xy 131.1 105.4) (xy 131.1 106.2) (xy 131 106.3)
			)
		)
	)
	(zone
		(net 3)
		(net_name "+3.3V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 3)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 127.2 101.6) (xy 127.2 101.2) (xy 127.2 100.7) (xy 126.7 100.2) (xy 126.7 97.1) (xy 127.3 96.5)
				(xy 127.7 96.5) (xy 127.8 96.6) (xy 127.8 97.5) (xy 127.7 97.6) (xy 127.4 97.6) (xy 127.4 98.9)
				(xy 127.6 99.1) (xy 127.8 99.1) (xy 127.8 100.1) (xy 128.2 100.5) (xy 128.3 100.5) (xy 128.4 100.6)
				(xy 128.4 101) (xy 128.4 101.6)
			)
		)
	)
	(zone
		(net 2)
		(net_name "+5V")
		(layer "B.Cu")
		(hatch edge 0.5)
		(priority 6)
		(connect_pads yes
			(clearance 0.127)
		)
		(min_thickness 0.127)
		(filled_areas_thickness no)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
		)
		(polygon
			(pts
				(xy 129.4 97.5) (xy 131.9 97.5) (xy 132 97.4) (xy 132 95.2) (xy 131.3 94.5) (xy 126.2 94.5) (xy 125 95.7)
				(xy 125 97.2) (xy 124.7 97.5) (xy 124.4 97.5) (xy 123.9 98) (xy 123.9 99.4) (xy 124.1 99.6) (xy 126.4 99.6)
				(xy 126.6 99.4) (xy 126.6 97.5) (xy 126.4 97.3) (xy 126.4 95.8) (xy 126.7 95.5) (xy 128.7 95.5)
				(xy 129.4 96.2)
			)
		)
	)
	(embedded_fonts no)
)
