(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A4")
	(title_block
		(title "TACHYMETRE")
		(date "2025-11-16")
		(rev "1")
		(company "PRONOE")
		(comment 2 "Needs an external KY-033 tracking sensor")
		(comment 3 "Needs an external DC 9V power supply")
	)
	(lib_symbols
		(symbol "Connector:Barrel_Jack_Switch"
			(pin_names
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 5.334 0)
			)
			(property "Value" "Barrel_Jack_Switch"
				(at 0 -5.08 0)
			)
			(property "Footprint" ""
				(at 1.27 -1.016 0)
			)
			(property "Datasheet" "~"
				(at 1.27 -1.016 0)
			)
			(property "Description" "DC Barrel Jack with an internal switch"
				(at 0 0 0)
			)
			(property "ki_keywords" "DC power barrel jack connector"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "BarrelJack*"
				(at 0 0 0)
			)
			(symbol "Barrel_Jack_Switch_0_1"
				(rectangle
					(start -5.08 3.81)
					(end 5.08 -3.81)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -3.81 -2.54) (xy -2.54 -2.54) (xy -1.27 -1.27) (xy 0 -2.54) (xy 2.54 -2.54) (xy 5.08 -2.54)
					)
					(fill
						(type none)
					)
				)
				(arc
					(start -3.302 1.905)
					(mid -3.9343 2.54)
					(end -3.302 3.175)
					(fill
						(type none)
					)
				)
				(arc
					(start -3.302 1.905)
					(mid -3.9343 2.54)
					(end -3.302 3.175)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 1.27 -2.286) (xy 1.905 -1.651)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 3.683 3.175)
					(end -3.302 1.905)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 5.08 2.54) (xy 3.81 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.08 0) (xy 1.27 0) (xy 1.27 -2.286) (xy 0.635 -1.651)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "Barrel_Jack_Switch_1_1"
				(pin passive line
					(at 7.62 2.54 180)
					(length 2.54)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 7.62 0 180)
					(length 2.54)
					(name "~")
					(number "3")
				)
				(pin passive line
					(at 7.62 -2.54 180)
					(length 2.54)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Connector:Conn_01x01_Pin"
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 2.54 0)
			)
			(property "Value" "Conn_01x01_Pin"
				(at 0 -2.54 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Generic connector, single row, 01x01, script generated"
				(at 0 0 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "connector"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Connector*:*_1x??_*"
				(at 0 0 0)
			)
			(symbol "Conn_01x01_Pin_1_1"
				(rectangle
					(start 0.8636 0.127)
					(end 0 -0.127)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 1.27 0) (xy 0.8636 0)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at 5.08 0 180)
					(length 3.81)
					(name "Pin_1")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Connector_Audio:AudioJack2_Ground"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "J"
				(at 0 8.89 0)
			)
			(property "Value" "AudioJack2_Ground"
				(at 0 6.35 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Audio Jack, 2 Poles (Mono / TS), Grounded Sleeve"
				(at 0 0 0)
			)
			(property "ki_keywords" "audio jack receptacle mono phone headphone TS connector"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Jack*"
				(at 0 0 0)
			)
			(symbol "AudioJack2_Ground_0_1"
				(rectangle
					(start -2.54 -2.54)
					(end -3.81 0)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0.635 -0.635) (xy 1.27 0) (xy 2.54 0)
					)
					(fill
						(type none)
					)
				)
				(rectangle
					(start 2.54 3.81)
					(end -2.54 -2.54)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy 2.54 2.54) (xy -0.635 2.54) (xy -0.635 0) (xy -1.27 -0.635) (xy -1.905 0)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "AudioJack2_Ground_1_1"
				(pin passive line
					(at 0 -5.08 90)
					(length 2.54)
					(name "~")
					(number "G")
				)
				(pin passive line
					(at 5.08 2.54 180)
					(length 2.54)
					(name "~")
					(number "S")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 2.54)
					(name "~")
					(number "T")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Device:R"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 2.032 0 90)
			)
			(property "Value" "R"
				(at 0 0 90)
			)
			(property "Footprint" ""
				(at -1.778 0 90)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Resistor"
				(at 0 0 0)
			)
			(property "ki_keywords" "R res resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "R_*"
				(at 0 0 0)
			)
			(symbol "R_0_1"
				(rectangle
					(start -1.016 -2.54)
					(end 1.016 2.54)
					(fill
						(type none)
					)
				)
			)
			(symbol "R_1_1"
				(pin passive line
					(at 0 3.81 270)
					(length 1.27)
					(name "~")
					(number "1")
				)
				(pin passive line
					(at 0 -3.81 90)
					(length 1.27)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Display_Character:CA56-12EWA"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -24.13 13.97 0)
			)
			(property "Value" "CA56-12EWA"
				(at 19.05 13.97 0)
			)
			(property "Footprint" "Display_7Segment:CA56-12EWA"
				(at 0 -15.24 0)
			)
			(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/CA56-12EWA.pdf"
				(at -10.922 0.762 0)
			)
			(property "Description" "4 digit 7 segment high efficiency red LED, common anode"
				(at 0 0 0)
			)
			(property "ki_keywords" "display LED 7-segment"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "*CA56*12EWA*"
				(at 0 0 0)
			)
			(symbol "CA56-12EWA_0_0"
				(rectangle
					(start -25.4 12.7)
					(end 25.4 -12.7)
					(fill
						(type background)
					)
				)
				(polyline
					(pts
						(xy -20.32 -3.81) (xy -19.05 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -19.05 -3.81) (xy -16.51 -3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -18.796 1.27) (xy -17.526 5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -17.78 0) (xy -15.24 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -16.256 5.08) (xy -13.716 5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -15.24 -3.81) (xy -13.97 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -13.716 1.27) (xy -12.446 5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -8.89 -3.81) (xy -7.62 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -7.62 -3.81) (xy -5.08 -3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -7.366 1.27) (xy -6.096 5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -6.35 0) (xy -3.81 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -4.826 5.08) (xy -2.286 5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -3.81 -3.81) (xy -2.54 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -2.286 1.27) (xy -1.016 5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 -3.81) (xy 2.54 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 -3.81) (xy 5.08 -3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.794 1.27) (xy 4.064 5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.81 0) (xy 6.35 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.334 5.08) (xy 7.874 5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.35 -3.81) (xy 7.62 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 7.874 1.27) (xy 9.144 5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 11.176 -3.81) (xy 12.446 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 12.446 -3.81) (xy 14.986 -3.81)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 12.7 1.27) (xy 13.97 5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 13.716 0) (xy 16.256 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 15.24 5.08) (xy 17.78 5.08)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 16.256 -3.81) (xy 17.526 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 17.78 1.27) (xy 19.05 5.08)
					)
					(fill
						(type none)
					)
				)
				(text "e"
					(at -21.336 -1.524 0)
				)
				(text "f"
					(at -19.558 3.048 0)
				)
				(text "d"
					(at -17.78 -2.794 0)
				)
				(text "g"
					(at -16.51 1.524 0)
				)
				(text "a"
					(at -15.24 6.35 0)
				)
				(text "DP1"
					(at -13.716 -6.35 0)
				)
				(text "c"
					(at -13.208 -1.778 0)
				)
				(text "b"
					(at -12.192 2.794 0)
				)
				(text "DP2"
					(at -2.286 -6.35 0)
				)
				(text "DP3"
					(at 7.62 -6.35 0)
				)
				(text "DP4"
					(at 17.78 -6.096 0)
				)
			)
			(symbol "CA56-12EWA_0_1"
				(circle
					(center -13.716 -3.81)
					(radius 0.3556)
					(fill
						(type outline)
					)
				)
				(circle
					(center -2.54 -3.81)
					(radius 0.3556)
					(fill
						(type outline)
					)
				)
			)
			(symbol "CA56-12EWA_1_0"
				(circle
					(center 7.62 -4.064)
					(radius 0.3556)
					(fill
						(type outline)
					)
				)
				(circle
					(center 17.78 -3.81)
					(radius 0.3556)
					(fill
						(type outline)
					)
				)
			)
			(symbol "CA56-12EWA_1_1"
				(pin input line
					(at -27.94 7.62 0)
					(length 2.54)
					(name "a")
					(number "11")
				)
				(pin input line
					(at -27.94 5.08 0)
					(length 2.54)
					(name "b")
					(number "7")
				)
				(pin input line
					(at -27.94 2.54 0)
					(length 2.54)
					(name "c")
					(number "4")
				)
				(pin input line
					(at -27.94 0 0)
					(length 2.54)
					(name "d")
					(number "2")
				)
				(pin input line
					(at -27.94 -2.54 0)
					(length 2.54)
					(name "e")
					(number "1")
				)
				(pin input line
					(at -27.94 -5.08 0)
					(length 2.54)
					(name "f")
					(number "10")
				)
				(pin input line
					(at -27.94 -7.62 0)
					(length 2.54)
					(name "g")
					(number "5")
				)
				(pin input line
					(at -27.94 -10.16 0)
					(length 2.54)
					(name "DPX")
					(number "3")
				)
				(pin input line
					(at 27.94 -2.54 180)
					(length 2.54)
					(name "CA1")
					(number "12")
				)
				(pin input line
					(at 27.94 -5.08 180)
					(length 2.54)
					(name "CA2")
					(number "9")
				)
				(pin input line
					(at 27.94 -7.62 180)
					(length 2.54)
					(name "CA3")
					(number "8")
				)
				(pin input line
					(at 27.94 -10.16 180)
					(length 2.54)
					(name "CA4")
					(number "6")
				)
			)
			(embedded_fonts no)
		)
		(symbol "MCU_Module:Arduino_Nano_v2.x"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "A"
				(at -10.16 23.495 0)
			)
			(property "Value" "Arduino_Nano_v2.x"
				(at 5.08 -24.13 0)
			)
			(property "Footprint" "Module:Arduino_Nano"
				(at 0 0 0)
			)
			(property "Datasheet" "https://www.arduino.cc/en/uploads/Main/ArduinoNanoManual23.pdf"
				(at 0 0 0)
			)
			(property "Description" "Arduino Nano v2.x"
				(at 0 0 0)
			)
			(property "ki_keywords" "Arduino nano microcontroller module USB"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Arduino*Nano*"
				(at 0 0 0)
			)
			(symbol "Arduino_Nano_v2.x_0_1"
				(rectangle
					(start -10.16 22.86)
					(end 10.16 -22.86)
					(fill
						(type background)
					)
				)
			)
			(symbol "Arduino_Nano_v2.x_1_1"
				(pin bidirectional line
					(at -12.7 15.24 0)
					(length 2.54)
					(name "D0/RX")
					(number "2")
				)
				(pin bidirectional line
					(at -12.7 12.7 0)
					(length 2.54)
					(name "D1/TX")
					(number "1")
				)
				(pin bidirectional line
					(at -12.7 10.16 0)
					(length 2.54)
					(name "D2")
					(number "5")
				)
				(pin bidirectional line
					(at -12.7 7.62 0)
					(length 2.54)
					(name "D3")
					(number "6")
				)
				(pin bidirectional line
					(at -12.7 5.08 0)
					(length 2.54)
					(name "D4")
					(number "7")
				)
				(pin bidirectional line
					(at -12.7 2.54 0)
					(length 2.54)
					(name "D5")
					(number "8")
				)
				(pin bidirectional line
					(at -12.7 0 0)
					(length 2.54)
					(name "D6")
					(number "9")
				)
				(pin bidirectional line
					(at -12.7 -2.54 0)
					(length 2.54)
					(name "D7")
					(number "10")
				)
				(pin bidirectional line
					(at -12.7 -5.08 0)
					(length 2.54)
					(name "D8")
					(number "11")
				)
				(pin bidirectional line
					(at -12.7 -7.62 0)
					(length 2.54)
					(name "D9")
					(number "12")
				)
				(pin bidirectional line
					(at -12.7 -10.16 0)
					(length 2.54)
					(name "D10")
					(number "13")
				)
				(pin bidirectional line
					(at -12.7 -12.7 0)
					(length 2.54)
					(name "D11")
					(number "14")
				)
				(pin bidirectional line
					(at -12.7 -15.24 0)
					(length 2.54)
					(name "D12")
					(number "15")
				)
				(pin bidirectional line
					(at -12.7 -17.78 0)
					(length 2.54)
					(name "D13")
					(number "16")
				)
				(pin power_in line
					(at -2.54 25.4 270)
					(length 2.54)
					(name "VIN")
					(number "30")
				)
				(pin power_in line
					(at 0 -25.4 90)
					(length 2.54)
					(name "GND")
					(number "4")
				)
				(pin power_out line
					(at 2.54 25.4 270)
					(length 2.54)
					(name "3V3")
					(number "17")
				)
				(pin power_in line
					(at 2.54 -25.4 90)
					(length 2.54)
					(name "GND")
					(number "29")
				)
				(pin power_out line
					(at 5.08 25.4 270)
					(length 2.54)
					(name "+5V")
					(number "27")
				)
				(pin input line
					(at 12.7 15.24 180)
					(length 2.54)
					(name "~{RESET}")
					(number "28")
				)
				(pin input line
					(at 12.7 12.7 180)
					(length 2.54)
					(name "~{RESET}")
					(number "3")
				)
				(pin input line
					(at 12.7 5.08 180)
					(length 2.54)
					(name "AREF")
					(number "18")
				)
				(pin bidirectional line
					(at 12.7 0 180)
					(length 2.54)
					(name "A0")
					(number "19")
				)
				(pin bidirectional line
					(at 12.7 -2.54 180)
					(length 2.54)
					(name "A1")
					(number "20")
				)
				(pin bidirectional line
					(at 12.7 -5.08 180)
					(length 2.54)
					(name "A2")
					(number "21")
				)
				(pin bidirectional line
					(at 12.7 -7.62 180)
					(length 2.54)
					(name "A3")
					(number "22")
				)
				(pin bidirectional line
					(at 12.7 -10.16 180)
					(length 2.54)
					(name "A4")
					(number "23")
				)
				(pin bidirectional line
					(at 12.7 -12.7 180)
					(length 2.54)
					(name "A5")
					(number "24")
				)
				(pin bidirectional line
					(at 12.7 -15.24 180)
					(length 2.54)
					(name "A6")
					(number "25")
				)
				(pin bidirectional line
					(at 12.7 -17.78 180)
					(length 2.54)
					(name "A7")
					(number "26")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Mechanical:MountingHole"
			(pin_names
				(offset 1.016)
			)
			(exclude_from_sim no)
			(in_bom no)
			(on_board yes)
			(property "Reference" "H"
				(at 0 5.08 0)
			)
			(property "Value" "MountingHole"
				(at 0 3.175 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Mounting Hole without connection"
				(at 0 0 0)
			)
			(property "ki_keywords" "mounting hole"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "MountingHole*"
				(at 0 0 0)
			)
			(symbol "MountingHole_0_1"
				(circle
					(center 0 0)
					(radius 1.27)
					(fill
						(type none)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:+5V"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "+5V"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"+5V\""
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "+5V_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "+5V_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(name "~")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "~")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:VCC"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "VCC"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"VCC\""
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "VCC_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "VCC_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(name "~")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
	)
	(junction
		(at 48.26 140.97)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 45.72 50.8)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 48.26 134.62)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 39.37 55.88)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 45.72 146.05)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 85.09 102.87)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 41.91 50.8)
		(diameter 0)
		(color 0 0 0 0)
	)
	(no_connect
		(at 97.79 95.25)
	)
	(no_connect
		(at 72.39 95.25)
	)
	(no_connect
		(at 97.79 92.71)
	)
	(no_connect
		(at 97.79 64.77)
	)
	(no_connect
		(at 97.79 77.47)
	)
	(no_connect
		(at 97.79 80.01)
	)
	(no_connect
		(at 72.39 92.71)
	)
	(no_connect
		(at 87.63 52.07)
	)
	(no_connect
		(at 97.79 72.39)
	)
	(no_connect
		(at 72.39 90.17)
	)
	(no_connect
		(at 72.39 64.77)
	)
	(no_connect
		(at 72.39 62.23)
	)
	(no_connect
		(at 97.79 62.23)
	)
	(wire
		(pts
			(xy 118.11 67.31) (xy 118.11 124.46)
		)
	)
	(wire
		(pts
			(xy 212.09 64.77) (xy 220.98 64.77)
		)
	)
	(wire
		(pts
			(xy 55.88 69.85) (xy 72.39 69.85)
		)
	)
	(wire
		(pts
			(xy 52.07 74.93) (xy 52.07 36.83)
		)
	)
	(wire
		(pts
			(xy 85.09 102.87) (xy 85.09 105.41)
		)
	)
	(wire
		(pts
			(xy 48.26 128.27) (xy 48.26 134.62)
		)
	)
	(wire
		(pts
			(xy 102.87 64.77) (xy 102.87 85.09)
		)
	)
	(wire
		(pts
			(xy 198.12 64.77) (xy 204.47 64.77)
		)
	)
	(wire
		(pts
			(xy 63.5 67.31) (xy 72.39 67.31)
		)
	)
	(wire
		(pts
			(xy 52.07 77.47) (xy 52.07 128.27)
		)
	)
	(wire
		(pts
			(xy 48.26 146.05) (xy 48.26 152.4)
		)
	)
	(wire
		(pts
			(xy 38.1 55.88) (xy 39.37 55.88)
		)
	)
	(wire
		(pts
			(xy 33.02 135.89) (xy 33.02 128.27)
		)
	)
	(wire
		(pts
			(xy 55.88 80.01) (xy 72.39 80.01)
		)
	)
	(wire
		(pts
			(xy 33.02 128.27) (xy 48.26 128.27)
		)
	)
	(wire
		(pts
			(xy 45.72 48.26) (xy 45.72 50.8)
		)
	)
	(wire
		(pts
			(xy 220.98 64.77) (xy 220.98 43.18)
		)
	)
	(wire
		(pts
			(xy 118.11 124.46) (xy 55.88 124.46)
		)
	)
	(wire
		(pts
			(xy 90.17 50.8) (xy 102.87 50.8)
		)
	)
	(wire
		(pts
			(xy 105.41 74.93) (xy 134.62 74.93)
		)
	)
	(wire
		(pts
			(xy 198.12 74.93) (xy 198.12 64.77)
		)
	)
	(wire
		(pts
			(xy 63.5 85.09) (xy 72.39 85.09)
		)
	)
	(wire
		(pts
			(xy 27.94 143.51) (xy 27.94 151.13)
		)
	)
	(wire
		(pts
			(xy 59.69 120.65) (xy 59.69 82.55)
		)
	)
	(wire
		(pts
			(xy 107.95 128.27) (xy 52.07 128.27)
		)
	)
	(wire
		(pts
			(xy 120.65 80.01) (xy 120.65 120.65)
		)
	)
	(wire
		(pts
			(xy 195.58 57.15) (xy 204.47 57.15)
		)
	)
	(wire
		(pts
			(xy 190.5 80.01) (xy 204.47 80.01)
		)
	)
	(wire
		(pts
			(xy 67.31 87.63) (xy 72.39 87.63)
		)
	)
	(wire
		(pts
			(xy 190.5 77.47) (xy 195.58 77.47)
		)
	)
	(wire
		(pts
			(xy 97.79 87.63) (xy 105.41 87.63)
		)
	)
	(wire
		(pts
			(xy 55.88 40.64) (xy 55.88 69.85)
		)
	)
	(wire
		(pts
			(xy 52.07 36.83) (xy 226.06 36.83)
		)
	)
	(wire
		(pts
			(xy 124.46 116.84) (xy 63.5 116.84)
		)
	)
	(wire
		(pts
			(xy 223.52 72.39) (xy 223.52 40.64)
		)
	)
	(wire
		(pts
			(xy 63.5 45.72) (xy 63.5 67.31)
		)
	)
	(wire
		(pts
			(xy 114.3 62.23) (xy 134.62 62.23)
		)
	)
	(wire
		(pts
			(xy 48.26 140.97) (xy 121.92 140.97)
		)
	)
	(wire
		(pts
			(xy 114.3 62.23) (xy 114.3 90.17)
		)
	)
	(wire
		(pts
			(xy 63.5 116.84) (xy 63.5 85.09)
		)
	)
	(wire
		(pts
			(xy 190.5 74.93) (xy 198.12 74.93)
		)
	)
	(wire
		(pts
			(xy 134.62 80.01) (xy 120.65 80.01)
		)
	)
	(wire
		(pts
			(xy 120.65 120.65) (xy 59.69 120.65)
		)
	)
	(wire
		(pts
			(xy 82.55 50.8) (xy 82.55 52.07)
		)
	)
	(wire
		(pts
			(xy 110.49 82.55) (xy 110.49 134.62)
		)
	)
	(wire
		(pts
			(xy 134.62 77.47) (xy 107.95 77.47)
		)
	)
	(wire
		(pts
			(xy 97.79 82.55) (xy 110.49 82.55)
		)
	)
	(wire
		(pts
			(xy 67.31 113.03) (xy 67.31 87.63)
		)
	)
	(wire
		(pts
			(xy 59.69 82.55) (xy 72.39 82.55)
		)
	)
	(wire
		(pts
			(xy 97.79 90.17) (xy 114.3 90.17)
		)
	)
	(wire
		(pts
			(xy 55.88 80.01) (xy 55.88 124.46)
		)
	)
	(wire
		(pts
			(xy 48.26 138.43) (xy 48.26 140.97)
		)
	)
	(wire
		(pts
			(xy 128.27 72.39) (xy 128.27 113.03)
		)
	)
	(wire
		(pts
			(xy 59.69 72.39) (xy 72.39 72.39)
		)
	)
	(wire
		(pts
			(xy 45.72 146.05) (xy 45.72 151.13)
		)
	)
	(wire
		(pts
			(xy 128.27 113.03) (xy 67.31 113.03)
		)
	)
	(wire
		(pts
			(xy 124.46 69.85) (xy 124.46 116.84)
		)
	)
	(wire
		(pts
			(xy 212.09 72.39) (xy 223.52 72.39)
		)
	)
	(wire
		(pts
			(xy 52.07 77.47) (xy 72.39 77.47)
		)
	)
	(wire
		(pts
			(xy 121.92 140.97) (xy 121.92 139.7)
		)
	)
	(wire
		(pts
			(xy 41.91 50.8) (xy 41.91 35.56)
		)
	)
	(wire
		(pts
			(xy 35.56 35.56) (xy 41.91 35.56)
		)
	)
	(wire
		(pts
			(xy 45.72 146.05) (xy 48.26 146.05)
		)
	)
	(wire
		(pts
			(xy 72.39 74.93) (xy 52.07 74.93)
		)
	)
	(wire
		(pts
			(xy 102.87 64.77) (xy 134.62 64.77)
		)
	)
	(wire
		(pts
			(xy 85.09 102.87) (xy 87.63 102.87)
		)
	)
	(wire
		(pts
			(xy 39.37 55.88) (xy 44.45 55.88)
		)
	)
	(wire
		(pts
			(xy 38.1 50.8) (xy 41.91 50.8)
		)
	)
	(wire
		(pts
			(xy 118.11 67.31) (xy 134.62 67.31)
		)
	)
	(wire
		(pts
			(xy 48.26 138.43) (xy 33.02 138.43)
		)
	)
	(wire
		(pts
			(xy 35.56 40.64) (xy 39.37 40.64)
		)
	)
	(wire
		(pts
			(xy 48.26 134.62) (xy 110.49 134.62)
		)
	)
	(wire
		(pts
			(xy 226.06 36.83) (xy 226.06 80.01)
		)
	)
	(wire
		(pts
			(xy 90.17 50.8) (xy 90.17 52.07)
		)
	)
	(wire
		(pts
			(xy 134.62 72.39) (xy 128.27 72.39)
		)
	)
	(wire
		(pts
			(xy 218.44 45.72) (xy 63.5 45.72)
		)
	)
	(wire
		(pts
			(xy 44.45 55.88) (xy 44.45 66.04)
		)
	)
	(wire
		(pts
			(xy 45.72 134.62) (xy 48.26 134.62)
		)
	)
	(wire
		(pts
			(xy 27.94 151.13) (xy 45.72 151.13)
		)
	)
	(wire
		(pts
			(xy 39.37 40.64) (xy 39.37 55.88)
		)
	)
	(wire
		(pts
			(xy 226.06 80.01) (xy 212.09 80.01)
		)
	)
	(wire
		(pts
			(xy 59.69 43.18) (xy 59.69 72.39)
		)
	)
	(wire
		(pts
			(xy 134.62 69.85) (xy 124.46 69.85)
		)
	)
	(wire
		(pts
			(xy 190.5 72.39) (xy 204.47 72.39)
		)
	)
	(wire
		(pts
			(xy 45.72 50.8) (xy 82.55 50.8)
		)
	)
	(wire
		(pts
			(xy 220.98 43.18) (xy 59.69 43.18)
		)
	)
	(wire
		(pts
			(xy 223.52 40.64) (xy 55.88 40.64)
		)
	)
	(wire
		(pts
			(xy 195.58 57.15) (xy 195.58 77.47)
		)
	)
	(wire
		(pts
			(xy 218.44 57.15) (xy 218.44 45.72)
		)
	)
	(wire
		(pts
			(xy 45.72 140.97) (xy 48.26 140.97)
		)
	)
	(wire
		(pts
			(xy 105.41 74.93) (xy 105.41 87.63)
		)
	)
	(wire
		(pts
			(xy 97.79 85.09) (xy 102.87 85.09)
		)
	)
	(wire
		(pts
			(xy 107.95 77.47) (xy 107.95 128.27)
		)
	)
	(wire
		(pts
			(xy 41.91 50.8) (xy 45.72 50.8)
		)
	)
	(wire
		(pts
			(xy 212.09 57.15) (xy 218.44 57.15)
		)
	)
	(symbol
		(lib_id "power:VCC")
		(at 45.72 48.26 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR04"
			(at 45.72 52.07 0)
		)
		(property "Value" "VCC"
			(at 45.72 43.18 0)
		)
		(property "Footprint" ""
			(at 45.72 48.26 0)
		)
		(property "Datasheet" ""
			(at 45.72 48.26 0)
		)
		(property "Description" "Power symbol creates a global label with name \"VCC\""
			(at 45.72 48.26 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR04")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x01_Pin")
		(at 40.64 146.05 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J7"
			(at 37.338 145.796 0)
		)
		(property "Value" "GND"
			(at 36.068 149.352 0)
		)
		(property "Footprint" "Connector_Wire:SolderWire-0.15sqmm_1x01_D0.5mm_OD1.5mm"
			(at 40.64 146.05 0)
		)
		(property "Datasheet" "~"
			(at 40.64 146.05 0)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 40.64 146.05 0)
		)
		(pin "1")
		(instances
			(project "tachy_PCB"
				(path
					(reference "J7")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Mechanical:MountingHole")
		(at 21.59 161.29 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom no)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "H3"
			(at 24.13 160.0199 0)
		)
		(property "Value" "MountingHole"
			(at 24.13 162.5599 0)
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3"
			(at 21.59 161.29 0)
		)
		(property "Datasheet" "~"
			(at 21.59 161.29 0)
		)
		(property "Description" "Mounting Hole without connection"
			(at 21.59 161.29 0)
		)
		(instances
			(project "tachy_PCB"
				(path
					(reference "H3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 208.28 80.01 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R4"
			(at 208.28 75.946 90)
		)
		(property "Value" "220"
			(at 208.28 77.724 90)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 208.28 81.788 90)
		)
		(property "Datasheet" "~"
			(at 208.28 80.01 0)
		)
		(property "Description" "Resistor"
			(at 208.28 80.01 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "tachy_PCB"
				(path
					(reference "R4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 208.28 72.39 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R3"
			(at 208.28 68.326 90)
		)
		(property "Value" "220"
			(at 208.28 70.104 90)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 208.28 74.168 90)
		)
		(property "Datasheet" "~"
			(at 208.28 72.39 0)
		)
		(property "Description" "Resistor"
			(at 208.28 72.39 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "tachy_PCB"
				(path
					(reference "R3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+5V")
		(at 121.92 139.7 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR06"
			(at 121.92 143.51 0)
		)
		(property "Value" "+5V"
			(at 121.92 134.62 0)
		)
		(property "Footprint" ""
			(at 121.92 139.7 0)
		)
		(property "Datasheet" ""
			(at 121.92 139.7 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 121.92 139.7 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR06")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Mechanical:MountingHole")
		(at 21.59 22.86 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom no)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "H1"
			(at 24.13 21.5899 0)
		)
		(property "Value" "MountingHole"
			(at 24.13 24.1299 0)
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3"
			(at 21.59 22.86 0)
		)
		(property "Datasheet" "~"
			(at 21.59 22.86 0)
		)
		(property "Description" "Mounting Hole without connection"
			(at 21.59 22.86 0)
		)
		(instances
			(project ""
				(path
					(reference "H1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 44.45 66.04 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR03"
			(at 44.45 72.39 0)
		)
		(property "Value" "GND"
			(at 44.45 71.12 0)
		)
		(property "Footprint" ""
			(at 44.45 66.04 0)
		)
		(property "Datasheet" ""
			(at 44.45 66.04 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 44.45 66.04 0)
		)
		(pin "1")
		(instances
			(project "tachy_PCB"
				(path
					(reference "#PWR03")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x01_Pin")
		(at 40.64 140.97 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J6"
			(at 37.338 140.716 0)
		)
		(property "Value" "V5V"
			(at 36.068 144.272 0)
		)
		(property "Footprint" "Connector_Wire:SolderWire-0.15sqmm_1x01_D0.5mm_OD1.5mm"
			(at 40.64 140.97 0)
		)
		(property "Datasheet" "~"
			(at 40.64 140.97 0)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 40.64 140.97 0)
		)
		(pin "1")
		(instances
			(project "tachy_PCB"
				(path
					(reference "J6")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector_Audio:AudioJack2_Ground")
		(at 27.94 138.43 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board no)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J5"
			(at 27.305 129.54 0)
		)
		(property "Value" "AudioJack2_Ground"
			(at 27.305 132.08 0)
		)
		(property "Footprint" ""
			(at 27.94 138.43 0)
		)
		(property "Datasheet" "~"
			(at 27.94 138.43 0)
		)
		(property "Description" "Audio Jack, 2 Poles (Mono / TS), Grounded Sleeve"
			(at 27.94 138.43 0)
		)
		(pin "G")
		(pin "T")
		(pin "S")
		(instances
			(project ""
				(path
					(reference "J5")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x01_Pin")
		(at 33.02 50.8 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J4"
			(at 29.464 50.8 0)
		)
		(property "Value" "VIN"
			(at 27.432 48.514 0)
		)
		(property "Footprint" "Connector_Wire:SolderWire-0.15sqmm_1x01_D0.5mm_OD1.5mm"
			(at 33.02 50.8 0)
		)
		(property "Datasheet" "~"
			(at 33.02 50.8 0)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 33.02 50.8 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "J4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Barrel_Jack_Switch")
		(at 27.94 38.1 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board no)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "J2"
			(at 27.94 29.21 0)
		)
		(property "Value" "Barrel_Jack_Switch"
			(at 27.94 31.75 0)
		)
		(property "Footprint" "Connector_BarrelJack:BarrelJack_CUI_PJ-063AH_Horizontal_CircularHoles"
			(at 29.21 39.116 0)
		)
		(property "Datasheet" "~"
			(at 29.21 39.116 0)
		)
		(property "Description" "DC Barrel Jack with an internal switch"
			(at 27.94 38.1 0)
		)
		(pin "1")
		(pin "3")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "J2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x01_Pin")
		(at 33.02 55.88 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J3"
			(at 29.718 55.626 0)
		)
		(property "Value" "GND"
			(at 28.448 59.182 0)
		)
		(property "Footprint" "Connector_Wire:SolderWire-0.15sqmm_1x01_D0.5mm_OD1.5mm"
			(at 33.02 55.88 0)
		)
		(property "Datasheet" "~"
			(at 33.02 55.88 0)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 33.02 55.88 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "J3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:+5V")
		(at 102.87 50.8 270)
		(mirror x)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "#PWR05"
			(at 99.06 50.8 0)
		)
		(property "Value" "+5V"
			(at 107.95 50.8 0)
		)
		(property "Footprint" ""
			(at 102.87 50.8 0)
		)
		(property "Datasheet" ""
			(at 102.87 50.8 0)
		)
		(property "Description" "Power symbol creates a global label with name \"+5V\""
			(at 102.87 50.8 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR05")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Mechanical:MountingHole")
		(at 232.41 25.4 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom no)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "H2"
			(at 234.95 24.1299 0)
		)
		(property "Value" "MountingHole"
			(at 234.95 26.6699 0)
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3"
			(at 232.41 25.4 0)
		)
		(property "Datasheet" "~"
			(at 232.41 25.4 0)
		)
		(property "Description" "Mounting Hole without connection"
			(at 232.41 25.4 0)
		)
		(instances
			(project "tachy_PCB"
				(path
					(reference "H2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 208.28 57.15 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R1"
			(at 208.28 53.086 90)
		)
		(property "Value" "220"
			(at 208.28 54.864 90)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 208.28 58.928 90)
		)
		(property "Datasheet" "~"
			(at 208.28 57.15 0)
		)
		(property "Description" "Resistor"
			(at 208.28 57.15 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Device:R")
		(at 208.28 64.77 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R2"
			(at 208.28 60.706 90)
		)
		(property "Value" "220"
			(at 208.28 62.484 90)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 208.28 66.548 90)
		)
		(property "Datasheet" "~"
			(at 208.28 64.77 0)
		)
		(property "Description" "Resistor"
			(at 208.28 64.77 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "tachy_PCB"
				(path
					(reference "R2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 85.09 105.41 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01"
			(at 85.09 111.76 0)
		)
		(property "Value" "GND"
			(at 85.09 110.49 0)
		)
		(property "Footprint" ""
			(at 85.09 105.41 0)
		)
		(property "Datasheet" ""
			(at 85.09 105.41 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 85.09 105.41 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR01")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Connector:Conn_01x01_Pin")
		(at 40.64 134.62 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "J1"
			(at 37.338 134.366 0)
		)
		(property "Value" "Sensor IN"
			(at 36.068 137.922 0)
		)
		(property "Footprint" "Connector_Wire:SolderWire-0.15sqmm_1x01_D0.5mm_OD1.5mm"
			(at 40.64 134.62 0)
		)
		(property "Datasheet" "~"
			(at 40.64 134.62 0)
		)
		(property "Description" "Generic connector, single row, 01x01, script generated"
			(at 40.64 134.62 0)
		)
		(pin "1")
		(instances
			(project "tachy_PCB"
				(path
					(reference "J1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "MCU_Module:Arduino_Nano_v2.x")
		(at 85.09 77.47 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "A2"
			(at 89.7733 102.87 0)
		)
		(property "Value" "Arduino_Nano_v2.x"
			(at 89.7733 105.41 0)
		)
		(property "Footprint" "MyFootprints:Arduino_Nano"
			(at 85.09 77.47 0)
		)
		(property "Datasheet" "https://www.arduino.cc/en/uploads/Main/ArduinoNanoManual23.pdf"
			(at 85.09 77.47 0)
		)
		(property "Description" "Arduino Nano v2.x"
			(at 85.09 77.47 0)
		)
		(pin "13")
		(pin "29")
		(pin "4")
		(pin "1")
		(pin "24")
		(pin "2")
		(pin "5")
		(pin "15")
		(pin "27")
		(pin "30")
		(pin "28")
		(pin "10")
		(pin "21")
		(pin "16")
		(pin "6")
		(pin "12")
		(pin "8")
		(pin "9")
		(pin "11")
		(pin "14")
		(pin "3")
		(pin "7")
		(pin "17")
		(pin "18")
		(pin "20")
		(pin "22")
		(pin "19")
		(pin "23")
		(pin "26")
		(pin "25")
		(instances
			(project ""
				(path
					(reference "A2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Mechanical:MountingHole")
		(at 231.14 135.89 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom no)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "H4"
			(at 233.68 134.6199 0)
		)
		(property "Value" "MountingHole"
			(at 233.68 137.1599 0)
		)
		(property "Footprint" "MountingHole:MountingHole_3.2mm_M3"
			(at 231.14 135.89 0)
		)
		(property "Datasheet" "~"
			(at 231.14 135.89 0)
		)
		(property "Description" "Mounting Hole without connection"
			(at 231.14 135.89 0)
		)
		(instances
			(project "tachy_PCB"
				(path
					(reference "H4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Display_Character:CA56-12EWA")
		(at 162.56 69.85 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U1"
			(at 162.56 52.07 0)
		)
		(property "Value" "3641BS"
			(at 162.56 54.61 0)
		)
		(property "Footprint" "MyFootprints:3416BS"
			(at 162.56 85.09 0)
		)
		(property "Datasheet" "http://www.kingbrightusa.com/images/catalog/SPEC/CA56-12EWA.pdf"
			(at 151.638 69.088 0)
		)
		(property "Description" "4 digit 7 segment high efficiency red LED, common anode"
			(at 162.56 69.85 0)
		)
		(pin "3")
		(pin "8")
		(pin "7")
		(pin "2")
		(pin "1")
		(pin "4")
		(pin "11")
		(pin "5")
		(pin "9")
		(pin "6")
		(pin "12")
		(pin "10")
		(instances
			(project ""
				(path
					(reference "U1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 48.26 152.4 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR02"
			(at 48.26 158.75 0)
		)
		(property "Value" "GND"
			(at 48.26 157.48 0)
		)
		(property "Footprint" ""
			(at 48.26 152.4 0)
		)
		(property "Datasheet" ""
			(at 48.26 152.4 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 48.26 152.4 0)
		)
		(pin "1")
		(instances
			(project "tachy_PCB"
				(path
					(reference "#PWR02")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
	(embedded_fonts no)
)
