(kicad_sch
	(version 20250114)
	(generator "eeschema")
	(generator_version "9.0")
	(paper "A4")
	(title_block
		(title "Binary Dice v1")
		(date "2026-01-19")
		(rev "1.0.0")
		(company "Aiden FLynn")
	)
	(lib_symbols
		(symbol "MCU_Microchip_ATtiny:ATtiny85-20P"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "U"
				(at -12.7 13.97 0)
			)
			(property "Value" "ATtiny85-20P"
				(at 2.54 -13.97 0)
			)
			(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
				(at 0 0 0)
			)
			(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2586-avr-8-bit-microcontroller-attiny25-attiny45-attiny85_datasheet.pdf"
				(at 0 0 0)
			)
			(property "Description" "20MHz, 8kB Flash, 512B SRAM, 512B EEPROM, debugWIRE, DIP-8"
				(at 0 0 0)
			)
			(property "ki_keywords" "AVR 8bit Microcontroller tinyAVR"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "DIP*W7.62mm*"
				(at 0 0 0)
			)
			(symbol "ATtiny85-20P_0_1"
				(rectangle
					(start -12.7 -12.7)
					(end 12.7 12.7)
					(fill
						(type background)
					)
				)
			)
			(symbol "ATtiny85-20P_1_1"
				(pin power_in line
					(at 0 15.24 270)
					(length 2.54)
					(name "VCC")
					(number "8")
				)
				(pin power_in line
					(at 0 -15.24 90)
					(length 2.54)
					(name "GND")
					(number "4")
				)
				(pin bidirectional line
					(at 15.24 7.62 180)
					(length 2.54)
					(name "AREF/PB0")
					(number "5")
				)
				(pin bidirectional line
					(at 15.24 5.08 180)
					(length 2.54)
					(name "PB1")
					(number "6")
				)
				(pin bidirectional line
					(at 15.24 2.54 180)
					(length 2.54)
					(name "PB2")
					(number "7")
				)
				(pin bidirectional line
					(at 15.24 0 180)
					(length 2.54)
					(name "XTAL1/PB3")
					(number "2")
				)
				(pin bidirectional line
					(at 15.24 -2.54 180)
					(length 2.54)
					(name "XTAL2/PB4")
					(number "3")
				)
				(pin bidirectional line
					(at 15.24 -5.08 180)
					(length 2.54)
					(name "~{RESET}/PB5")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "New_Library:BS-7"
			(pin_names
				(offset 0.254)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "B"
				(at 4.826 3.81 0)
			)
			(property "Value" "BS-7"
				(at 4.826 -3.81 0)
			)
			(property "Footprint" "BS-7_MPD"
				(at 0 0 0)
			)
			(property "Datasheet" "BS-7"
				(at 0 0 0)
			)
			(property "Description" ""
				(at 0 0 0)
			)
			(property "ki_locked" ""
				(at 0 0 0)
			)
			(property "ki_keywords" "BS-7"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "BS-7_MPD"
				(at 0 0 0)
			)
			(symbol "BS-7_0_1"
				(polyline
					(pts
						(xy 1.778 1.27) (xy 2.794 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.286 0.762) (xy 2.286 1.778)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 0) (xy 3.4798 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 3.556 -1.778) (xy 3.556 1.778)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 4.572 0.762) (xy 4.572 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 5.588 -1.778) (xy 5.588 1.778)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.604 0.762) (xy 6.604 -0.762)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 6.604 0) (xy 7.62 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 7.366 1.27) (xy 8.382 1.27)
					)
					(fill
						(type none)
					)
				)
				(pin unspecified line
					(at 0 0 0)
					(length 2.54)
					(name "")
					(number "2")
				)
				(pin unspecified line
					(at 10.16 0 180)
					(length 2.54)
					(name "")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "PCM_SL_Devices:LED_5mm"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "D"
				(at -0.508 5.334 0)
			)
			(property "Value" "LED_5mm"
				(at -0.508 2.794 0)
			)
			(property "Footprint" "LED_THT:LED_D5.0mm"
				(at -1.016 -2.794 0)
			)
			(property "Datasheet" ""
				(at -1.27 0 0)
			)
			(property "Description" "Common 5mm diameter LED"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "LED_D5.0mm_Clear LED_D5.0mm_Horizontal_O1.27mm_Z3.0mm LED_D5.0mm_Horizontal_O3.81mm_Z3.0mm LED_D5.0mm_Horizontal_O6.35mm_Z3.0mm"
				(at 0 0 0)
			)
			(symbol "LED_5mm_0_1"
				(polyline
					(pts
						(xy -1.27 0) (xy -2.54 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy -1.27 -1.27) (xy -1.27 1.27) (xy 0 0) (xy 1.27 0)
					)
					(fill
						(type outline)
					)
				)
				(polyline
					(pts
						(xy 0.508 0.508) (xy 1.524 1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.27 0) (xy 2.54 0)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 1.524) (xy 0.889 1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 1.524) (xy 1.524 0.889)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 1.524 0.508) (xy 2.54 1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 1.524) (xy 1.905 1.524)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 1.524) (xy 2.54 0.889)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "LED_5mm_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 1.5)
					(name "")
					(number "2")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 1.5)
					(name "~")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "PCM_SL_Resistors:Resistor"
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "R"
				(at 0 5.08 0)
			)
			(property "Value" "Resistor"
				(at 0 2.54 0)
			)
			(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
				(at 0.889 -4.318 0)
			)
			(property "Datasheet" ""
				(at 0.508 0 0)
			)
			(property "Description" "1/4W Resistor"
				(at 0 0 0)
			)
			(property "ki_keywords" "Resistor"
				(at 0 0 0)
			)
			(property "ki_fp_filters" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm*"
				(at 0 0 0)
			)
			(symbol "Resistor_0_1"
				(rectangle
					(start -2.286 0.889)
					(end 2.286 -0.889)
					(fill
						(type none)
					)
				)
			)
			(symbol "Resistor_1_1"
				(pin passive line
					(at -3.81 0 0)
					(length 1.5)
					(name "")
					(number "1")
				)
				(pin passive line
					(at 3.81 0 180)
					(length 1.5)
					(name "~")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Switch:SW_Push"
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 1.016)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "SW"
				(at 1.27 2.54 0)
			)
			(property "Value" "SW_Push"
				(at 0 -1.524 0)
			)
			(property "Footprint" ""
				(at 0 5.08 0)
			)
			(property "Datasheet" "~"
				(at 0 5.08 0)
			)
			(property "Description" "Push button switch, generic, two pins"
				(at 0 0 0)
			)
			(property "ki_keywords" "switch normally-open pushbutton push-button"
				(at 0 0 0)
			)
			(symbol "SW_Push_0_1"
				(circle
					(center -2.032 0)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 1.27) (xy 0 3.048)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.032 0)
					(radius 0.508)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 2.54 1.27) (xy -2.54 1.27)
					)
					(fill
						(type none)
					)
				)
				(pin passive line
					(at -5.08 0 0)
					(length 2.54)
					(name "1")
					(number "1")
				)
				(pin passive line
					(at 5.08 0 180)
					(length 2.54)
					(name "2")
					(number "2")
				)
			)
			(embedded_fonts no)
		)
		(symbol "Switch:SW_SPDT"
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "SW"
				(at 0 5.08 0)
			)
			(property "Value" "SW_SPDT"
				(at 0 -5.08 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 -7.62 0)
			)
			(property "Description" "Switch, single pole double throw"
				(at 0 0 0)
			)
			(property "ki_keywords" "switch single-pole double-throw spdt ON-ON"
				(at 0 0 0)
			)
			(symbol "SW_SPDT_0_1"
				(circle
					(center -2.032 0)
					(radius 0.4572)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy -1.651 0.254) (xy 1.651 2.286)
					)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.032 2.54)
					(radius 0.4572)
					(fill
						(type none)
					)
				)
				(circle
					(center 2.032 -2.54)
					(radius 0.4572)
					(fill
						(type none)
					)
				)
			)
			(symbol "SW_SPDT_1_1"
				(rectangle
					(start -3.175 3.81)
					(end 3.175 -3.81)
					(fill
						(type background)
					)
				)
				(pin passive line
					(at -5.08 0 0)
					(length 2.54)
					(name "B")
					(number "2")
				)
				(pin passive line
					(at 5.08 2.54 180)
					(length 2.54)
					(name "A")
					(number "1")
				)
				(pin passive line
					(at 5.08 -2.54 180)
					(length 2.54)
					(name "C")
					(number "3")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:GND"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -6.35 0)
			)
			(property "Value" "GND"
				(at 0 -3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "GND_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 -1.27) (xy 1.27 -1.27) (xy 0 -2.54) (xy -1.27 -1.27) (xy 0 -1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "GND_1_1"
				(pin power_in line
					(at 0 0 270)
					(length 0)
					(name "~")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:PWR_FLAG"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#FLG"
				(at 0 1.905 0)
			)
			(property "Value" "PWR_FLAG"
				(at 0 3.81 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" "~"
				(at 0 0 0)
			)
			(property "Description" "Special symbol for telling ERC where power comes from"
				(at 0 0 0)
			)
			(property "ki_keywords" "flag power"
				(at 0 0 0)
			)
			(symbol "PWR_FLAG_0_0"
				(pin power_out line
					(at 0 0 90)
					(length 0)
					(name "~")
					(number "1")
				)
			)
			(symbol "PWR_FLAG_0_1"
				(polyline
					(pts
						(xy 0 0) (xy 0 1.27) (xy -1.016 1.905) (xy 0 2.54) (xy 1.016 1.905) (xy 0 1.27)
					)
					(fill
						(type none)
					)
				)
			)
			(embedded_fonts no)
		)
		(symbol "power:VCC"
			(power)
			(pin_numbers
				(hide yes)
			)
			(pin_names
				(offset 0)
				(hide yes)
			)
			(exclude_from_sim no)
			(in_bom yes)
			(on_board yes)
			(property "Reference" "#PWR"
				(at 0 -3.81 0)
			)
			(property "Value" "VCC"
				(at 0 3.556 0)
			)
			(property "Footprint" ""
				(at 0 0 0)
			)
			(property "Datasheet" ""
				(at 0 0 0)
			)
			(property "Description" "Power symbol creates a global label with name \"VCC\""
				(at 0 0 0)
			)
			(property "ki_keywords" "global power"
				(at 0 0 0)
			)
			(symbol "VCC_0_1"
				(polyline
					(pts
						(xy -0.762 1.27) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 2.54) (xy 0.762 1.27)
					)
					(fill
						(type none)
					)
				)
				(polyline
					(pts
						(xy 0 0) (xy 0 2.54)
					)
					(fill
						(type none)
					)
				)
			)
			(symbol "VCC_1_1"
				(pin power_in line
					(at 0 0 90)
					(length 0)
					(name "~")
					(number "1")
				)
			)
			(embedded_fonts no)
		)
	)
	(junction
		(at 132.08 113.03)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 125.73 113.03)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 104.14 113.03)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 119.38 113.03)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 106.68 113.03)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 138.43 113.03)
		(diameter 0)
		(color 0 0 0 0)
	)
	(junction
		(at 86.36 67.31)
		(diameter 0)
		(color 0 0 0 0)
	)
	(no_connect
		(at 184.15 72.39)
	)
	(no_connect
		(at 101.6 88.9)
	)
	(wire
		(pts
			(xy 138.43 80.01) (xy 138.43 82.55)
		)
	)
	(wire
		(pts
			(xy 101.6 81.28) (xy 105.41 81.28)
		)
	)
	(wire
		(pts
			(xy 119.38 69.85) (xy 119.38 72.39)
		)
	)
	(wire
		(pts
			(xy 125.73 69.85) (xy 125.73 72.39)
		)
	)
	(wire
		(pts
			(xy 101.6 83.82) (xy 105.41 83.82)
		)
	)
	(wire
		(pts
			(xy 132.08 113.03) (xy 138.43 113.03)
		)
	)
	(wire
		(pts
			(xy 138.43 90.17) (xy 138.43 113.03)
		)
	)
	(wire
		(pts
			(xy 143.51 58.42) (xy 143.51 113.03)
		)
	)
	(wire
		(pts
			(xy 86.36 64.77) (xy 86.36 67.31)
		)
	)
	(wire
		(pts
			(xy 184.15 77.47) (xy 195.58 77.47)
		)
	)
	(wire
		(pts
			(xy 101.6 76.2) (xy 105.41 76.2)
		)
	)
	(wire
		(pts
			(xy 86.36 99.06) (xy 86.36 113.03)
		)
	)
	(wire
		(pts
			(xy 162.56 74.93) (xy 173.99 74.93)
		)
	)
	(wire
		(pts
			(xy 135.89 58.42) (xy 143.51 58.42)
		)
	)
	(wire
		(pts
			(xy 125.73 113.03) (xy 132.08 113.03)
		)
	)
	(wire
		(pts
			(xy 138.43 69.85) (xy 138.43 72.39)
		)
	)
	(wire
		(pts
			(xy 119.38 80.01) (xy 119.38 82.55)
		)
	)
	(wire
		(pts
			(xy 101.6 78.74) (xy 105.41 78.74)
		)
	)
	(wire
		(pts
			(xy 195.58 71.12) (xy 195.58 77.47)
		)
	)
	(wire
		(pts
			(xy 86.36 113.03) (xy 104.14 113.03)
		)
	)
	(wire
		(pts
			(xy 125.73 80.01) (xy 125.73 82.55)
		)
	)
	(wire
		(pts
			(xy 106.68 115.57) (xy 106.68 113.03)
		)
	)
	(wire
		(pts
			(xy 162.56 86.36) (xy 162.56 99.06)
		)
	)
	(wire
		(pts
			(xy 104.14 113.03) (xy 106.68 113.03)
		)
	)
	(wire
		(pts
			(xy 162.56 76.2) (xy 162.56 74.93)
		)
	)
	(wire
		(pts
			(xy 132.08 90.17) (xy 132.08 113.03)
		)
	)
	(wire
		(pts
			(xy 132.08 80.01) (xy 132.08 82.55)
		)
	)
	(wire
		(pts
			(xy 132.08 69.85) (xy 132.08 72.39)
		)
	)
	(wire
		(pts
			(xy 101.6 86.36) (xy 105.41 86.36)
		)
	)
	(wire
		(pts
			(xy 138.43 113.03) (xy 143.51 113.03)
		)
	)
	(wire
		(pts
			(xy 106.68 113.03) (xy 119.38 113.03)
		)
	)
	(wire
		(pts
			(xy 125.73 90.17) (xy 125.73 113.03)
		)
	)
	(wire
		(pts
			(xy 119.38 113.03) (xy 125.73 113.03)
		)
	)
	(wire
		(pts
			(xy 119.38 90.17) (xy 119.38 113.03)
		)
	)
	(wire
		(pts
			(xy 86.36 67.31) (xy 86.36 68.58)
		)
	)
	(global_label "LED3"
		(shape input)
		(at 132.08 69.85 90)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 132.08 62.2082 90)
		)
	)
	(global_label "LED1"
		(shape input)
		(at 119.38 69.85 90)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 119.38 62.2082 90)
		)
	)
	(global_label "LED2"
		(shape input)
		(at 125.73 69.85 90)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 125.73 62.2082 90)
		)
	)
	(global_label "LED4"
		(shape input)
		(at 105.41 86.36 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 113.0518 86.36 0)
		)
	)
	(global_label "BTN"
		(shape input)
		(at 105.41 83.82 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 111.9633 83.82 0)
		)
	)
	(global_label "LED3"
		(shape input)
		(at 105.41 81.28 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 113.0518 81.28 0)
		)
	)
	(global_label "LED2"
		(shape input)
		(at 105.41 78.74 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 113.0518 78.74 0)
		)
	)
	(global_label "BTN"
		(shape input)
		(at 125.73 58.42 180)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 119.1767 58.42 0)
		)
	)
	(global_label "LED4"
		(shape input)
		(at 138.43 69.85 90)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 138.43 62.2082 90)
		)
	)
	(global_label "LED1"
		(shape input)
		(at 105.41 76.2 0)
		(fields_autoplaced yes)
		(property "Intersheetrefs" "${INTERSHEET_REFS}"
			(at 113.0518 76.2 0)
		)
	)
	(symbol
		(lib_id "PCM_SL_Resistors:Resistor")
		(at 119.38 86.36 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R1"
			(at 117.094 85.09 90)
		)
		(property "Value" "220"
			(at 116.332 87.376 90)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 115.062 87.249 0)
		)
		(property "Datasheet" ""
			(at 119.38 86.868 0)
		)
		(property "Description" "1/4W Resistor"
			(at 119.38 86.36 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "attiny_dice_final"
				(path
					(reference "R1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:VCC")
		(at 195.58 71.12 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR04"
			(at 195.58 74.93 0)
		)
		(property "Value" "VCC"
			(at 195.58 66.04 0)
		)
		(property "Footprint" ""
			(at 195.58 71.12 0)
		)
		(property "Datasheet" ""
			(at 195.58 71.12 0)
		)
		(property "Description" "Power symbol creates a global label with name \"VCC\""
			(at 195.58 71.12 0)
		)
		(pin "1")
		(instances
			(project "attiny_dice_final"
				(path
					(reference "#PWR04")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 106.68 115.57 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR01"
			(at 106.68 121.92 0)
		)
		(property "Value" "GND"
			(at 106.68 120.65 0)
		)
		(property "Footprint" ""
			(at 106.68 115.57 0)
		)
		(property "Datasheet" ""
			(at 106.68 115.57 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 106.68 115.57 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR01")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:PWR_FLAG")
		(at 86.36 67.31 90)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#FLG02"
			(at 84.455 67.31 0)
		)
		(property "Value" "PWR_FLAG"
			(at 82.55 67.3099 90)
		)
		(property "Footprint" ""
			(at 86.36 67.31 0)
		)
		(property "Datasheet" "~"
			(at 86.36 67.31 0)
		)
		(property "Description" "Special symbol for telling ERC where power comes from"
			(at 86.36 67.31 0)
		)
		(pin "1")
		(instances
			(project "attiny_dice_final"
				(path
					(reference "#FLG02")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "PCM_SL_Devices:LED_5mm")
		(at 132.08 76.2 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "D3"
			(at 129.286 75.438 90)
		)
		(property "Value" "LED_5mm"
			(at 135.89 76.2 0)
		)
		(property "Footprint" "LED_THT:LED_D5.0mm"
			(at 129.286 75.184 0)
		)
		(property "Datasheet" ""
			(at 132.08 74.93 0)
		)
		(property "Description" "Common 5mm diameter LED"
			(at 132.08 76.2 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "attiny_dice_final"
				(path
					(reference "D3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "PCM_SL_Devices:LED_5mm")
		(at 119.38 76.2 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "D1"
			(at 116.586 75.438 90)
		)
		(property "Value" "LED_5mm"
			(at 123.19 76.2 0)
		)
		(property "Footprint" "LED_THT:LED_D5.0mm"
			(at 116.586 75.184 0)
		)
		(property "Datasheet" ""
			(at 119.38 74.93 0)
		)
		(property "Description" "Common 5mm diameter LED"
			(at 119.38 76.2 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "attiny_dice_final"
				(path
					(reference "D1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "PCM_SL_Resistors:Resistor")
		(at 132.08 86.36 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R3"
			(at 129.794 85.09 90)
		)
		(property "Value" "220"
			(at 129.032 87.376 90)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 127.762 87.249 0)
		)
		(property "Datasheet" ""
			(at 132.08 86.868 0)
		)
		(property "Description" "1/4W Resistor"
			(at 132.08 86.36 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "attiny_dice_final"
				(path
					(reference "R3")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:GND")
		(at 162.56 99.06 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR03"
			(at 162.56 105.41 0)
		)
		(property "Value" "GND"
			(at 162.56 104.14 0)
		)
		(property "Footprint" ""
			(at 162.56 99.06 0)
		)
		(property "Datasheet" ""
			(at 162.56 99.06 0)
		)
		(property "Description" "Power symbol creates a global label with name \"GND\" , ground"
			(at 162.56 99.06 0)
		)
		(pin "1")
		(instances
			(project "attiny_dice_final"
				(path
					(reference "#PWR03")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "PCM_SL_Resistors:Resistor")
		(at 138.43 86.36 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R4"
			(at 136.144 85.09 90)
		)
		(property "Value" "220"
			(at 135.382 87.376 90)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 134.112 87.249 0)
		)
		(property "Datasheet" ""
			(at 138.43 86.868 0)
		)
		(property "Description" "1/4W Resistor"
			(at 138.43 86.36 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "attiny_dice_final"
				(path
					(reference "R4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:VCC")
		(at 86.36 64.77 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#PWR02"
			(at 86.36 68.58 0)
		)
		(property "Value" "VCC"
			(at 86.36 59.69 0)
		)
		(property "Footprint" ""
			(at 86.36 64.77 0)
		)
		(property "Datasheet" ""
			(at 86.36 64.77 0)
		)
		(property "Description" "Power symbol creates a global label with name \"VCC\""
			(at 86.36 64.77 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#PWR02")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "PCM_SL_Devices:LED_5mm")
		(at 125.73 76.2 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "D2"
			(at 122.936 75.438 90)
		)
		(property "Value" "LED_5mm"
			(at 129.54 76.2 0)
		)
		(property "Footprint" "LED_THT:LED_D5.0mm"
			(at 122.936 75.184 0)
		)
		(property "Datasheet" ""
			(at 125.73 74.93 0)
		)
		(property "Description" "Common 5mm diameter LED"
			(at 125.73 76.2 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "attiny_dice_final"
				(path
					(reference "D2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_SPDT")
		(at 179.07 74.93 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "SW2"
			(at 179.07 66.04 0)
		)
		(property "Value" "SW_SPDT"
			(at 179.07 68.58 0)
		)
		(property "Footprint" "Library:right angle switch"
			(at 179.07 74.93 0)
		)
		(property "Datasheet" "~"
			(at 179.07 82.55 0)
		)
		(property "Description" "Switch, single pole double throw"
			(at 179.07 74.93 0)
		)
		(pin "2")
		(pin "3")
		(pin "1")
		(instances
			(project "attiny_dice_final"
				(path
					(reference "SW2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "PCM_SL_Devices:LED_5mm")
		(at 138.43 76.2 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "D4"
			(at 135.636 75.438 90)
		)
		(property "Value" "LED_5mm"
			(at 142.24 76.2 0)
		)
		(property "Footprint" "LED_THT:LED_D5.0mm"
			(at 135.636 75.184 0)
		)
		(property "Datasheet" ""
			(at 138.43 74.93 0)
		)
		(property "Description" "Common 5mm diameter LED"
			(at 138.43 76.2 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project "attiny_dice_final"
				(path
					(reference "D4")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "power:PWR_FLAG")
		(at 104.14 113.03 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "#FLG01"
			(at 104.14 111.125 0)
		)
		(property "Value" "PWR_FLAG"
			(at 104.14 107.95 0)
		)
		(property "Footprint" ""
			(at 104.14 113.03 0)
		)
		(property "Datasheet" "~"
			(at 104.14 113.03 0)
		)
		(property "Description" "Special symbol for telling ERC where power comes from"
			(at 104.14 113.03 0)
		)
		(pin "1")
		(instances
			(project ""
				(path
					(reference "#FLG01")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "PCM_SL_Resistors:Resistor")
		(at 125.73 86.36 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "R2"
			(at 123.444 85.09 90)
		)
		(property "Value" "220"
			(at 122.682 87.376 90)
		)
		(property "Footprint" "Resistor_THT:R_Axial_DIN0207_L6.3mm_D2.5mm_P10.16mm_Horizontal"
			(at 121.412 87.249 0)
		)
		(property "Datasheet" ""
			(at 125.73 86.868 0)
		)
		(property "Description" "1/4W Resistor"
			(at 125.73 86.36 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project "attiny_dice_final"
				(path
					(reference "R2")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "MCU_Microchip_ATtiny:ATtiny85-20P")
		(at 86.36 83.82 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "U1"
			(at 72.39 82.5499 0)
		)
		(property "Value" "ATtiny85-20P"
			(at 72.39 85.0899 0)
		)
		(property "Footprint" "Package_DIP:DIP-8_W7.62mm"
			(at 86.36 83.82 0)
		)
		(property "Datasheet" "http://ww1.microchip.com/downloads/en/DeviceDoc/atmel-2586-avr-8-bit-microcontroller-attiny25-attiny45-attiny85_datasheet.pdf"
			(at 86.36 83.82 0)
		)
		(property "Description" "20MHz, 8kB Flash, 512B SRAM, 512B EEPROM, debugWIRE, DIP-8"
			(at 86.36 83.82 0)
		)
		(pin "4")
		(pin "8")
		(pin "6")
		(pin "7")
		(pin "1")
		(pin "5")
		(pin "3")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "U1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "New_Library:BS-7")
		(at 162.56 76.2 270)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(fields_autoplaced yes)
		(property "Reference" "B1"
			(at 165.1 80.0099 90)
		)
		(property "Value" "BS-7"
			(at 165.1 82.5499 90)
		)
		(property "Footprint" "Library:BS-7_MPD"
			(at 162.56 76.2 0)
		)
		(property "Datasheet" "BS-7"
			(at 162.56 76.2 0)
		)
		(property "Description" ""
			(at 162.56 76.2 0)
		)
		(pin "2")
		(pin "1")
		(instances
			(project ""
				(path
					(reference "B1")
					(unit 1)
				)
			)
		)
	)
	(symbol
		(lib_id "Switch:SW_Push")
		(at 130.81 58.42 0)
		(unit 1)
		(exclude_from_sim no)
		(in_bom yes)
		(on_board yes)
		(dnp no)
		(property "Reference" "SW1"
			(at 130.81 54.102 0)
		)
		(property "Value" "SW_Push"
			(at 130.81 53.34 0)
		)
		(property "Footprint" "Library:SW_PUSH-12mm"
			(at 130.81 53.34 0)
		)
		(property "Datasheet" "~"
			(at 130.81 53.34 0)
		)
		(property "Description" "Push button switch, generic, two pins"
			(at 130.81 58.42 0)
		)
		(pin "1")
		(pin "2")
		(instances
			(project ""
				(path
					(reference "SW1")
					(unit 1)
				)
			)
		)
	)
	(sheet_instances
		(path
			(page "1")
		)
	)
	(embedded_fonts no)
)
