(kicad_pcb
	(version 20260206)
	(generator "pcbnew")
	(generator_version "10.0")
	(general
		(thickness 1.6)
		(legacy_teardrops no)
	)
	(paper "User" 200 200)
	(layers
		(0 "F.Cu" signal)
		(2 "B.Cu" signal)
		(9 "F.Adhes" user "F.Adhesive")
		(11 "B.Adhes" user "B.Adhesive")
		(13 "F.Paste" user)
		(15 "B.Paste" user)
		(5 "F.SilkS" user "F.Silkscreen")
		(7 "B.SilkS" user "B.Silkscreen")
		(1 "F.Mask" user)
		(3 "B.Mask" user)
		(17 "Dwgs.User" user "User.Drawings")
		(19 "Cmts.User" user "User.Comments")
		(21 "Eco1.User" user "User.Eco1")
		(23 "Eco2.User" user "User.Eco2")
		(25 "Edge.Cuts" user)
		(27 "Margin" user)
		(31 "F.CrtYd" user "F.Courtyard")
		(29 "B.CrtYd" user "B.Courtyard")
		(35 "F.Fab" user)
		(33 "B.Fab" user)
		(39 "User.1" user)
		(41 "User.2" user)
		(43 "User.3" user)
		(45 "User.4" user)
	)
	(setup
		(pad_to_mask_clearance 0)
		(allow_soldermask_bridges_in_footprints no)
		(tenting
			(front yes)
			(back yes)
		)
		(covering
			(front no)
			(back no)
		)
		(plugging
			(front no)
			(back no)
		)
		(capping no)
		(filling no)
		(pcbplotparams
			(layerselection 0x00000000_00000000_55555555_5755f5ff)
			(plot_on_all_layers_selection 0x00000000_00000000_00000000_00000000)
			(disableapertmacros no)
			(usegerberextensions no)
			(usegerberattributes yes)
			(usegerberadvancedattributes yes)
			(creategerberjobfile yes)
			(dashed_line_dash_ratio 12)
			(dashed_line_gap_ratio 3)
			(svgprecision 4)
			(plotframeref no)
			(mode 1)
			(useauxorigin no)
			(pdf_front_fp_property_popups yes)
			(pdf_back_fp_property_popups yes)
			(pdf_metadata yes)
			(pdf_single_document no)
			(dxfpolygonmode yes)
			(dxfimperialunits yes)
			(dxfusepcbnewfont yes)
			(psnegative no)
			(psa4output no)
			(plot_black_and_white yes)
			(sketchpadsonfab no)
			(plotpadnumbers no)
			(hidednponfab no)
			(sketchdnponfab yes)
			(crossoutdnponfab yes)
			(subtractmaskfromsilk no)
			(outputformat 4)
			(mirror no)
			(drillshape 0)
			(scaleselection 1)
			(outputdirectory "./")
		)
	)
	(variants
		(variant
			(name "v0.1")
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 81.4 117.7375 -90)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "M4"
			(at 0 -2.38 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Motor_Servo"
			(at 0 7.46 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://forums.parallax.com/uploads/attachments/46831/74481.png"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Servo Motor (Futaba, HiTec, JR connector)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "PinHeader*P2.54mm*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "3")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/Servo3")
			(pinfunction "PWM_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+5V")
			(pinfunction "+_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "-_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "F.Cu")
		(at 91.325 76.3375 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C8"
			(at 0 -1.43 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nf"
			(at 0 1.43 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fc:OST_OSTTE020104"
		(layer "F.Cu")
		(at 77.1 94.6875 -90)
		(property "Reference" "P2"
			(at -1.125645 -4.337545 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "PYRO1"
			(at 5.229005 4.568475 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "On Shore Technology Inc."
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole rect
			(at -1.75 0 270)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(Q1-D)")
			(pinfunction "1_1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 1.75 0 270)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+BATT")
			(pinfunction "2_2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "/home/Gary/Downloads/OSTTE020104/OSTTE020104.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "fc:Wio-SX1262"
		(layer "F.Cu")
		(at 75.38 85.8375)
		(property "Reference" "M1"
			(at 5.95 -6.05 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Wio-SX1262"
			(at 0 1 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "3" "4" "5" "6" "7" "8" "12" "11" "10" "9")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 2.5 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at 1.33 0 90)
			(size 2.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net "/RF_SW")
			(pinfunction "RF_SW_1")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at 2.6 0 90)
			(size 2.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net "/MISO")
			(pinfunction "SPI_MISO_2")
			(pintype "bidirectional")
		)
		(pad "3" smd roundrect
			(at 3.87 0 90)
			(size 2.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net "/MOSI")
			(pinfunction "SPI_MOSI_3")
			(pintype "bidirectional")
		)
		(pad "4" smd roundrect
			(at 5.14 0 90)
			(size 2.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net "/SCK")
			(pinfunction "SPI_SCK_4")
			(pintype "bidirectional")
		)
		(pad "5" smd roundrect
			(at 6.41 0 90)
			(size 2.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net "Net-(M1-NRST)")
			(pinfunction "NRST_5")
			(pintype "input")
		)
		(pad "6" smd roundrect
			(at 7.68 0 90)
			(size 2.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net "/RF_CS")
			(pinfunction "SPI_NSS_6")
			(pintype "input")
		)
		(pad "7" smd roundrect
			(at 8.95 0 90)
			(size 2.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net "GND")
			(pinfunction "GND_7")
			(pintype "power_in")
		)
		(pad "8" smd roundrect
			(at 10.22 0 90)
			(size 2.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net "unconnected-(M1-VCC-Pad8)")
			(pinfunction "VCC_8")
			(pintype "power_in")
		)
		(pad "9" smd roundrect
			(at 2.6 -11 90)
			(size 2.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net "Net-(M1-ANT)")
			(pinfunction "ANT_9")
			(pintype "input")
		)
		(pad "10" smd roundrect
			(at 3.87 -11 90)
			(size 2.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net "GND")
			(pinfunction "GND_10")
			(pintype "power_in")
		)
		(pad "11" smd roundrect
			(at 5.14 -11 90)
			(size 2.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net "Net-(M1-BUSY)")
			(pinfunction "BUSY_11")
			(pintype "input")
		)
		(pad "12" smd roundrect
			(at 6.41 -11 90)
			(size 2.2 0.6)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.15)
			(net "Net-(M1-DIO1)")
			(pinfunction "DIO1_12")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "/home/Gary/Downloads/Wio-SX1262 file.step"
			(offset
				(xyz 0 0 0.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "fc:TO252-2-3.3V_DIO"
		(layer "F.Cu")
		(at 90.164 107.8986)
		(tags "AZ1117CD-3.3TRG1 ")
		(property "Reference" "U6"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "AZ1117CD-3.3TRG1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "AZ1117CD-3.3TRG1"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO252-2-3.3V_DIO TO252-2-3.3V_DIO-M TO252-2-3.3V_DIO-L")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "3" "2" "1")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "*"
			(at -2.414 2.8889 0)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -2.414 2.8889 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -2.286 2.8448 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -2.286 2.8448 0)
			(layer "F.Fab")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -2.286 6.4389)
			(size 0.9398 2.413)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "ADJ/GND_1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 0 -1.8923)
			(size 5.5118 5.969)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+3V3")
			(pinfunction "OUTPUT_2")
			(pintype "output")
		)
		(pad "3" smd rect
			(at 2.286 6.4389)
			(size 0.9398 2.413)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+5V")
			(pinfunction "INPUT_3")
			(pintype "input")
		)
		(embedded_fonts no)
		(model "/home/Gary/Downloads/AZ1117CD_3_3TRG1/TO252-2-3_3V_DIO.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "F.Cu")
		(at 111.55 111.9875 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C3"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "1uf"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "F.Cu")
		(at 108.65 87.7375)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R3"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "5"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/rgb-blue")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(D1-Pad6)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 109.65 97.1375 180)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf)")
		(tags "LED")
		(property "Reference" "D6"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(D6-A)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "F.Cu")
		(at 105.25 67.4625 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R14"
			(at 0 -1.43 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "330"
			(at 0 1.43 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/Reset")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(R14-Pad2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "F.Cu")
		(at 100.65 78.3625 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C6"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nf"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "F.Cu")
		(at 98.35 76.4375)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C7"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nf"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "F.Cu")
		(at 111.675 87.7375)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R2"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "65"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/rgb-red")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(D1-Pad5)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fc:ATSAMD21G18-AU"
		(layer "F.Cu")
		(at 97.3 91.6375 -90)
		(property "Reference" "U1"
			(at -2.932823 -5.696648 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "ATSAMD21G18A-AU"
			(at -11.797101 -17.82248 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "ATMEL"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "40" "1" "2" "3" "4" "9" "10" "11" "12" "13" "14" "15" "16" "21"
					"22" "23" "24" "25" "26" "27" "28" "29" "30" "31" "32" "33" "34" "39"
					"41" "45" "46" "6" "17" "36" "44" "43" "47" "48" "7" "8" "19" "20" "37"
					"38" "5" "18" "35" "42"
				)
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" smd rect
			(at -4.2 -2.75 270)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(U1-PA00)")
			(pinfunction "PA00_1")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at -4.2 -2.25 270)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(U1-PA01)")
			(pinfunction "PA01_2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at -4.2 -1.75 270)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/PYRO2")
			(pinfunction "PA02_3")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd rect
			(at -4.2 -1.25 270)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/AREF")
			(pinfunction "PA03_4")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd rect
			(at -4.2 -0.75 270)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "GNDANA_5")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "6" smd rect
			(at -4.2 -0.25 270)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+3V3")
			(pinfunction "VDDANA_6")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "7" smd rect
			(at -4.2 0.25 270)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/RF_NRST")
			(pinfunction "PB08_7")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "8" smd rect
			(at -4.2 0.75 270)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(U1-PB09-Pad8)")
			(pinfunction "PB09_8")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "9" smd rect
			(at -4.2 1.25 270)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/rgb-blue")
			(pinfunction "PA04_9")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "10" smd rect
			(at -4.2 1.75 270)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/rgb-green")
			(pinfunction "PA05_10")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "11" smd rect
			(at -4.2 2.25 270)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/FLASH_CS")
			(pinfunction "PA06_11")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "12" smd rect
			(at -4.2 2.75 270)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/RF_SW")
			(pinfunction "PA07_12")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "13" smd rect
			(at -2.75 4.2 270)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/RF_INT")
			(pinfunction "PA08_13")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "14" smd rect
			(at -2.25 4.2 270)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/RF_BUSY")
			(pinfunction "PA09_14")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "15" smd rect
			(at -1.75 4.2 270)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/RF_CS")
			(pinfunction "PA10_15")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "16" smd rect
			(at -1.25 4.2 270)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/SD_DETECT")
			(pinfunction "PA11_16")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "17" smd rect
			(at -0.75 4.2 270)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+3V3")
			(pinfunction "VDDIO1_17")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "18" smd rect
			(at -0.25 4.2 270)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "GND1_18")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "19" smd rect
			(at 0.25 4.2 270)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/MOSI")
			(pinfunction "PB10_19")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "20" smd rect
			(at 0.75 4.2 270)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/SCK")
			(pinfunction "PB11_20")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "21" smd rect
			(at 1.25 4.2 270)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/MISO")
			(pinfunction "PA12_21")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "22" smd rect
			(at 1.75 4.2 270)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/BUZZER")
			(pinfunction "PA13_22")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "23" smd rect
			(at 2.25 4.2 270)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/SD_CS")
			(pinfunction "PA14_23")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "24" smd rect
			(at 2.75 4.2 270)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(U1-PA15-Pad24)")
			(pinfunction "PA15_24")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "25" smd rect
			(at 4.17 2.75 270)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/Servo1")
			(pinfunction "PA16_25")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "26" smd rect
			(at 4.2 2.25 270)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/LED")
			(pinfunction "PA17_26")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "27" smd rect
			(at 4.2 1.75 270)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/Servo2")
			(pinfunction "PA18_27")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "28" smd rect
			(at 4.2 1.25 270)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/Servo3")
			(pinfunction "PA19_28")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "29" smd rect
			(at 4.2 0.75 270)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/FLASH_EN")
			(pinfunction "PA20_29")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "30" smd rect
			(at 4.2 0.25 270)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/rgb-red")
			(pinfunction "PA21_30")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "31" smd rect
			(at 4.2 -0.25 270)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/SDA")
			(pinfunction "PA22_31")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "32" smd rect
			(at 4.2 -0.75 270)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/SCL")
			(pinfunction "PA23_32")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "33" smd rect
			(at 4.2 -1.25 270)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(U1-PA24)")
			(pinfunction "PA24_33")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "34" smd rect
			(at 4.2 -1.75 270)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(U1-PA25)")
			(pinfunction "PA25_34")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "35" smd rect
			(at 4.2 -2.25 270)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "GND2_35")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "36" smd rect
			(at 4.2 -2.75 270)
			(size 1.45 0.3)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+3V3")
			(pinfunction "VDDIO2_36")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "37" smd rect
			(at 2.75 -4.2 270)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(U1-PB22-Pad37)")
			(pinfunction "PB22_37")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "38" smd rect
			(at 2.25 -4.2 270)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(U1-PB23-Pad38)")
			(pinfunction "PB23_38")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "39" smd rect
			(at 1.75 -4.2 270)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(U1-PA27-Pad39)")
			(pinfunction "PA27_39")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "40" smd rect
			(at 1.25 -4.2 270)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/Reset")
			(pinfunction "~{RESETN}_40")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "41" smd rect
			(at 0.75 -4.2 270)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(U1-PA28-Pad41)")
			(pinfunction "PA28_41")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "42" smd rect
			(at 0.25 -4.2 270)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "GND3_42")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "43" smd rect
			(at -0.25 -4.2 270)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(U1-VDDCORE)")
			(pinfunction "VDDCORE_43")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "44" smd rect
			(at -0.75 -4.2 270)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+3V3")
			(pinfunction "VDDIN_44")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "45" smd rect
			(at -1.25 -4.2 270)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/SWCLK")
			(pinfunction "PA30_45")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "46" smd rect
			(at -1.75 -4.2 270)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/SWDIO")
			(pinfunction "PA31_46")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "47" smd rect
			(at -2.25 -4.2 270)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/PYRO1")
			(pinfunction "PB02_47")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "48" smd rect
			(at -2.75 -4.2 270)
			(size 0.3 1.45)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(U1-PB03-Pad48)")
			(pinfunction "PB03_48")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "/home/Gary/Downloads/ATSAMD21G18A-AU.step"
			(offset
				(xyz 0 0 0.65)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -180)
			)
		)
	)
	(footprint "fc:XTAL_FC-135_EPS"
		(layer "F.Cu")
		(at 101.41505 84.8105 180)
		(tags "FC-135 32.7680KA-A5 ")
		(property "Reference" "X1"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "FC-135 32.7680KA-A5"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "FC-135 32.7680KA-A5"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "XTAL_FC-135_EPS")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "2" "1")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.25 0 180)
			(size 0.9906 1.8034)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(U1-PA00)")
			(pinfunction "1_1")
			(pintype "unspecified")
		)
		(pad "2" smd rect
			(at 1.25 0 180)
			(size 0.9906 1.8034)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(U1-PA01)")
			(pinfunction "2_2")
			(pintype "unspecified")
		)
		(embedded_fonts no)
		(model "/home/Gary/Downloads/FC_135_32_7680KA_A5/XTAL_FC-135_EPS.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fc:OST_OSTTE020104"
		(layer "F.Cu")
		(at 77.15 103.6375 -90)
		(property "Reference" "P3"
			(at -1.125645 -4.337545 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "PYRO2"
			(at 20.379006 28.229875 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "On Shore Technology Inc."
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole rect
			(at -1.75 0 270)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(Q2-D)")
			(pinfunction "1_1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 1.75 0 270)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+BATT")
			(pinfunction "2_2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "/home/Gary/Downloads/OSTTE020104/OSTTE020104.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "F.Cu")
		(at 104.3 84.8875 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C16"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "15pf"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U1-PA00)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fc:OST_OSTTE020104"
		(layer "F.Cu")
		(at 119.15 113.8375 90)
		(property "Reference" "P1"
			(at -1.125645 -4.337545 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "OSTTE020104"
			(at 5.229005 4.568475 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "On Shore Technology Inc."
			(at 0 0 90)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" thru_hole rect
			(at -1.75 0 90)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+BATT")
			(pinfunction "1_1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 1.75 0 90)
			(size 1.8 1.8)
			(drill 1.2)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "2_2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "/home/Gary/Downloads/OSTTE020104/OSTTE020104.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "F.Cu")
		(at 105.35 119.6875 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R5"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "5.1k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(J2-CC2)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "F.Cu")
		(at 103.7 67.4625 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C17"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nf"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/Reset")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "F.Cu")
		(at 82.575 90.2375)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R18"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(M1-NRST)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/RF_NRST")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "F.Cu")
		(at 94.2 102.7875 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R12"
			(at 0 -1.43 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7k"
			(at 0 1.43 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/SDA")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fc:SW_OS102011MS2QN1"
		(layer "F.Cu")
		(at 119.95 102.8875 90)
		(property "Reference" "SW1"
			(at -2.976555 -3.305417 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "SW_SPDT"
			(at 0.682908 3.201326 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Switch, single pole double throw"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "2" "1" "3")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "" np_thru_hole circle
			(at -4.1 0 90)
			(size 1.5 1.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 4.1 0 90)
			(size 1.5 1.5)
			(drill 1.5)
			(layers "*.Cu" "*.Mask")
		)
		(pad "1" thru_hole rect
			(at -2 0 90)
			(size 1.308 1.308)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "unconnected-(SW1-A-Pad1)")
			(pinfunction "A_1")
			(pintype "passive+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "2" thru_hole circle
			(at 0 0 90)
			(size 1.308 1.308)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(D2-K)")
			(pinfunction "B_2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" thru_hole circle
			(at 2 0 90)
			(size 1.308 1.308)
			(drill 0.8)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "Net-(SW1-C)")
			(pinfunction "C_3")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "/home/Gary/Downloads/OS102011MS2QN1/OS102011MS2QN1.step"
			(offset
				(xyz 0 0 4.5)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "F.Cu")
		(at 108.65 80.5875)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R1"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "5"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/rgb-green")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(D1-Pad4)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fc:AMPHENOL_GSB1C41110SSHR"
		(layer "F.Cu")
		(at 97.25 121.0375)
		(property "Reference" "J2"
			(at -1.27 -7.3675 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "GSB1C41110SSHR"
			(at 20.06 -5.08 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "DigiKey_Part_Number" "664-GSB1C41110SSHRCT-ND"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/GSB1C41110SSHR/Amphenol/view-part/?ref=snap"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "3.21mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "None"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/GSB1C41110SSHR/Amphenol/view-part/?ref=eda"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "AX1"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "Amphenol Canada"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "GSB1C41110SSHR"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "USB2.0, Type C, Top mount, Center Height 1.63mm, Single Row Surface Mount"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Amphenol"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "A4_B9" "A5" "A6" "A7" "A8" "A1_B12" "SH1" "SH2" "SH3" "SH4" "B4_A9"
					"B8" "B7" "B6" "B5" "B1_A12"
				)
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "PCB EDGE"
			(at 6.35 3.4275 0)
			(layer "F.Fab")
		)
		(pad "" np_thru_hole circle
			(at -2.89 -2.605)
			(size 0.7 0.7)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
		)
		(pad "" np_thru_hole circle
			(at 2.89 -2.605)
			(size 0.7 0.7)
			(drill 0.7)
			(layers "*.Cu" "*.Mask")
		)
		(pad "A1_B12" smd rect
			(at -3.2 -3.68)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Paste")
			(net "GND")
			(pinfunction "GND_A_A1_B12")
			(pintype "power_in")
		)
		(pad "A4_B9" smd rect
			(at -2.4 -3.68)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Paste")
			(net "VBUS")
			(pinfunction "VBUS_A_A4_B9")
			(pintype "power_in")
		)
		(pad "A5" smd rect
			(at -1.25 -3.68)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste")
			(net "Net-(J2-CC1)")
			(pinfunction "CC1_A5")
			(pintype "bidirectional")
		)
		(pad "A6" smd rect
			(at -0.25 -3.68)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste")
			(net "/D+")
			(pinfunction "DP1_A6")
			(pintype "bidirectional")
		)
		(pad "A7" smd rect
			(at 0.25 -3.68)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste")
			(net "/D-")
			(pinfunction "DN1_A7")
			(pintype "bidirectional")
		)
		(pad "A8" smd rect
			(at 1.25 -3.68)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste")
			(net "unconnected-(J2-SBU1-PadA8)")
			(pinfunction "SBU1_A8")
			(pintype "bidirectional")
		)
		(pad "B1_A12" smd rect
			(at 3.2 -3.68)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Paste")
			(net "GND")
			(pinfunction "GND_B_B1_A12")
			(pintype "power_in")
		)
		(pad "B4_A9" smd rect
			(at 2.4 -3.68)
			(size 0.6 1.15)
			(layers "F.Cu" "F.Paste")
			(net "VBUS")
			(pinfunction "VBUS_B_B4_A9")
			(pintype "power_in")
		)
		(pad "B5" smd rect
			(at 1.75 -3.68)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste")
			(net "Net-(J2-CC2)")
			(pinfunction "CC2_B5")
			(pintype "bidirectional")
		)
		(pad "B6" smd rect
			(at 0.75 -3.68)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste")
			(net "/D-")
			(pinfunction "DP2_B6")
			(pintype "bidirectional")
		)
		(pad "B7" smd rect
			(at -0.75 -3.68)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste")
			(net "/D+")
			(pinfunction "DN2_B7")
			(pintype "bidirectional")
		)
		(pad "B8" smd rect
			(at -1.75 -3.68)
			(size 0.3 1.15)
			(layers "F.Cu" "F.Paste")
			(net "unconnected-(J2-SBU2-PadB8)")
			(pinfunction "SBU2_B8")
			(pintype "bidirectional")
		)
		(pad "SH1" smd rect
			(at -5.12 -3.105)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "SHIELD_SH1")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "SH2" smd rect
			(at 5.12 -3.105)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "SHIELD_SH2")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "SH3" smd rect
			(at -5.12 0.825)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "SHIELD_SH3")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "SH4" smd rect
			(at 5.12 0.825)
			(size 1.5 1.5)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "SHIELD_SH4")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "/home/Gary/Downloads/GSB1C41110SSHR--3DModel-STEP-533217.STEP"
			(offset
				(xyz 0 7.25 1.625)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -180)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "F.Cu")
		(at 115.55 93.0625 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R22"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/SWCLK")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 81.38 110.1875 -90)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "M2"
			(at 0 -2.38 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Motor_Servo"
			(at 0 7.46 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://forums.parallax.com/uploads/attachments/46831/74481.png"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Servo Motor (Futaba, HiTec, JR connector)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "PinHeader*P2.54mm*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "3")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/Servo1")
			(pinfunction "PWM_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+5V")
			(pinfunction "+_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "-_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "LED_SMD:LED_0603_1608Metric"
		(layer "F.Cu")
		(at 109.7 94.6875 180)
		(descr "LED SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf)")
		(tags "LED")
		(property "Reference" "D5"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LED"
			(at 0 1.43 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Light emitting diode"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "LED* LED_SMD:* LED_THT:*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 180)
			(size 0.875 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(D5-A)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/LED_SMD.3dshapes/LED_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "F.Cu")
		(at 99.05 113.7625 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R7"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "22"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/D+")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U1-PA25)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "F.Cu")
		(at 94.05 112.8875 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C5"
			(at 0 -1.43 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10uf"
			(at 0 1.43 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+5V")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fc:DPAK229P990X238-4N"
		(layer "F.Cu")
		(at 107.09 109.9975)
		(property "Reference" "U5"
			(at 0.635 -7.239 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "MC7805BDTRKG"
			(at 22.092 8.701 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "27"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "IPC-7351B"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "ON Semiconductor"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "3" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" smd rect
			(at -2.29 4.14)
			(size 0.97 2.83)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(SW1-C)")
			(pinfunction "IN_1")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 0 -2.51)
			(size 5.63 6.09)
			(layers "F.Cu" "F.Mask")
			(net "GND")
			(pinfunction "GND_2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at 2.29 4.14)
			(size 0.97 2.83)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+5V")
			(pinfunction "OUT_3")
			(pintype "output")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "/home/Gary/Downloads/MC7805BDTRKG/MC7805BDTRKG.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -90)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "F.Cu")
		(at 102.65 110.5375 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C2"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "0.33uf"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(SW1-C)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "F.Cu")
		(at 95.75 102.7875 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R11"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "4.7k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/SCL")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Connector_PinHeader_2.54mm:PinHeader_1x03_P2.54mm_Vertical"
		(layer "F.Cu")
		(at 81.38 113.8875 -90)
		(descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
		(tags "Through hole pin header THT 1x03 2.54mm single row")
		(property "Reference" "M3"
			(at 0 -2.38 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Motor_Servo"
			(at 0 7.46 90)
			(layer "F.Fab")
		)
		(property "Datasheet" "http://forums.parallax.com/uploads/attachments/46831/74481.png"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Servo Motor (Futaba, HiTec, JR connector)"
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "PinHeader*P2.54mm*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "3")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 2.54 0)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/Servo2")
			(pinfunction "PWM_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at 0 2.54 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+5V")
			(pinfunction "+_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 5.08 270)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "-_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "F.Cu")
		(at 97.5 113.7625 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R6"
			(at 0 -1.43 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "22"
			(at 0 1.43 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U1-PA24)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/D-")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "F.Cu")
		(at 102.15 67.4625 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R8"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "/Reset")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "F.Cu")
		(at 90.8 78.7625 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C9"
			(at 0 -1.43 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "100nf"
			(at 0 1.43 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fc:SW_PTS_647_SN50_SMTR2_LFS"
		(layer "F.Cu")
		(at 97.625 67.7375)
		(property "Reference" "S1"
			(at -0.475 -3.635 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "PTS_647_SN50_SMTR2_LFS"
			(at 12.225 3.635 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MF" "C&K"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "5.0 mm"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Package" "None"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Price" "None"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Check_prices" "https://www.snapeda.com/parts/PTS%20647%20SN50%20SMTR2%20LFS/C%2526K/view-part/?ref=eda"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "4 Apr 22"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SnapEDA_Link" "https://www.snapeda.com/parts/PTS%20647%20SN50%20SMTR2%20LFS/C%2526K/view-part/?ref=snap"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MP" "PTS 647 SN50 SMTR2 LFS"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description_1" "Tactile Switch SPST-NO Top Actuated Surface Mount"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "SNAPEDA_PN" "PTS 647 SN50 SMTR2 LFS"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Availability" "In Stock"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "C&K"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "3" "4" "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" smd rect
			(at -2.625 -1.6)
			(size 1.55 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(R14-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at 2.625 -1.6)
			(size 1.55 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(R14-Pad2)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at -2.625 1.6)
			(size 1.55 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd rect
			(at 2.625 1.6)
			(size 1.55 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "/home/Gary/Downloads/PTS 647 SN50 SMTR2 LFS--3DModel-STEP-269445.STEP"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "fc:LED_IN-P55TATRGB"
		(layer "F.Cu")
		(at 110.6 84.1875 180)
		(property "Reference" "D1"
			(at -1.36 -3.508 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "IN-P55TATRGB"
			(at 4.228 3.508 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "PARTREV" "1.0"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommended"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "1.5mm"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Inolux"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "4" "5" "6" "3" "2" "1")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" smd rect
			(at -2.2 -1.8 180)
			(size 2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd rect
			(at -2.2 0 180)
			(size 2 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd rect
			(at -2.2 1.8 180)
			(size 2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd rect
			(at 2.2 1.8 180)
			(size 2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(D1-Pad4)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd rect
			(at 2.2 0 180)
			(size 2 1)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(D1-Pad5)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(pad "6" smd rect
			(at 2.2 -1.8 180)
			(size 2 1.4)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "Net-(D1-Pad6)")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "/home/Gary/Downloads/IN_P55TATRGB/IN-P55TATRGB.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 90)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "F.Cu")
		(at 94.65 109.8375 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C15"
			(at 0 -1.43 270)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "22uf"
			(at 0 1.43 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "F.Cu")
		(at 89.1 121.6375 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R4"
			(at 0 -1.43 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "5.1k"
			(at 0 1.43 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(J2-CC1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fc:PinSocket_2x03_odd"
		(layer "F.Cu")
		(at 121.34 89.5475)
		(descr "Through hole straight socket strip, 2x03, 2.54mm pitch, double cols (from Kicad 4.0.7), script generated")
		(tags "Through hole socket strip THT 2x03 2.54mm double row")
		(property "Reference" "J3"
			(at -1.27 -2.77 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "Conn_2Rows-05Pins"
			(at -1.27 7.85 0)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "Generic connector, double row, 05 pins, odd/even pin numbering scheme (row 1 odd numbers, row 2 even numbers), script generated (kicad-library-utils/schlib/autogen/connector/)"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Connector*:*2Rows*Pins__* *FCC*2Rows*Pins__*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "3" "5" "2" "4")
			)
		)
		(attr through_hole)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at -1.27 2.54 90)
			(layer "F.Fab")
		)
		(pad "1" thru_hole rect
			(at 0 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "+3V3")
			(pinfunction "Pin_1_1")
			(pintype "passive")
		)
		(pad "2" thru_hole circle
			(at -2.54 0)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/SWDIO")
			(pinfunction "Pin_2_2")
			(pintype "passive")
		)
		(pad "3" thru_hole circle
			(at 0 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "GND")
			(pinfunction "Pin_3_3")
			(pintype "passive")
		)
		(pad "4" thru_hole circle
			(at -2.54 2.54)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/SWCLK")
			(pinfunction "Pin_4_4")
			(pintype "passive")
		)
		(pad "5" thru_hole circle
			(at 0 5.08)
			(size 1.7 1.7)
			(drill 1)
			(layers "*.Cu" "*.Mask")
			(remove_unused_layers no)
			(net "/Reset")
			(pinfunction "Pin_5_5")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinSocket_2.54mm.3dshapes/PinSocket_2x03_P2.54mm_Vertical.step"
			(hide yes)
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
		(model "${KICAD9_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.step"
			(offset
				(xyz -2.5 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -0)
			)
		)
	)
	(footprint "LOGO"
		(layer "F.Cu")
		(at 114.45 71.4875)
		(property "Reference" "G***"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "LOGO"
			(at 0.75 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(attr board_only exclude_from_pos_files exclude_from_bom)
		(duplicate_pad_numbers_are_jumpers no)
		(embedded_fonts no)
	)
	(footprint "fc:BMI323_BOS"
		(layer "F.Cu")
		(at 93.5 78.6519 180)
		(tags "BMI323 ")
		(property "Reference" "U2"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "BMI323"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "BMI323"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "BMI323_BOS BMI323_BOS-M BMI323_BOS-L")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "3" "4" "5" "6" "7" "14" "13" "12" "11" "10" "9" "8")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "*"
			(at -1.35 -1.2356 0)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -1.45 -1.6356 180)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -0.9144 -1 0)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at -0.9144 -1 180)
			(unlocked yes)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -1.1557 -0.750001 270)
			(size 0.254 0.4826)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "SDO_1")
			(pintype "bidirectional")
		)
		(pad "2" smd rect
			(at -1.1557 -0.25 270)
			(size 0.254 0.4826)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(U2-NC-Pad2)")
			(pinfunction "NC_2")
			(pintype "no_connect")
		)
		(pad "3" smd rect
			(at -1.1557 0.25 270)
			(size 0.254 0.4826)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(U2-NC-Pad3)")
			(pinfunction "NC_3")
			(pintype "no_connect")
		)
		(pad "4" smd rect
			(at -1.1557 0.750001 270)
			(size 0.254 0.4826)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/IMU_INT")
			(pinfunction "INT1_4")
			(pintype "bidirectional")
		)
		(pad "5" smd rect
			(at -0.499999 0.9144 180)
			(size 0.254 0.4826)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+3V3")
			(pinfunction "VDDIO_5")
			(pintype "power_in")
		)
		(pad "6" smd rect
			(at 0 0.9144 180)
			(size 0.254 0.4826)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "GNDIO_6")
			(pintype "power_out")
		)
		(pad "7" smd rect
			(at 0.499999 0.9144 180)
			(size 0.254 0.4826)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "GND_7")
			(pintype "power_out")
		)
		(pad "8" smd rect
			(at 1.1557 0.750001 270)
			(size 0.254 0.4826)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+3V3")
			(pinfunction "VDD_8")
			(pintype "power_in")
		)
		(pad "9" smd rect
			(at 1.1557 0.25 270)
			(size 0.254 0.4826)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(U2-INT2-Pad9)")
			(pinfunction "INT2_9")
			(pintype "bidirectional")
		)
		(pad "10" smd rect
			(at 1.1557 -0.25 270)
			(size 0.254 0.4826)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(U2-NC-Pad10)")
			(pinfunction "NC_10")
			(pintype "no_connect")
		)
		(pad "11" smd rect
			(at 1.1557 -0.750001 270)
			(size 0.254 0.4826)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(U2-NC-Pad11)")
			(pinfunction "NC_11")
			(pintype "no_connect")
		)
		(pad "12" smd rect
			(at 0.499999 -0.9144 180)
			(size 0.254 0.4826)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+3V3")
			(pinfunction "CSB_12")
			(pintype "input")
		)
		(pad "13" smd rect
			(at 0 -0.9144 180)
			(size 0.254 0.4826)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/SCL")
			(pinfunction "SCX_13")
			(pintype "input")
		)
		(pad "14" smd rect
			(at -0.499999 -0.9144 180)
			(size 0.254 0.4826)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/SDA")
			(pinfunction "SDX_14")
			(pintype "bidirectional")
		)
		(embedded_fonts no)
		(model "/home/Gary/Downloads/BMI323/BMI323_BOS.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "F.Cu")
		(at 114.3 113.9375 -90)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D2"
			(at 0 -2 90)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "~"
			(at 0 2.1 90)
			(layer "F.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" "75V 0.15A Fast Switching Diode, SOD-123"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*SOD?123*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -2 90)
			(layer "F.Fab")
		)
		(pad "1" smd roundrect
			(at -1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(D2-K)")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0 270)
			(size 0.9 1.2)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+BATT")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "F.Cu")
		(at 100.825 82.7875 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C10"
			(at 0 -1.43 180)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "15pf"
			(at 0 1.43 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U1-PA01)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "F.Cu")
		(at 82.575 88.6375)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R16"
			(at 0 -1.43 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 1.43 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "F.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(M1-NRST)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fc:BMP390"
		(layer "F.Cu")
		(at 98.25 78.6001)
		(tags "BMP390 ")
		(property "Reference" "U3"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.SilkS")
			(hide yes)
		)
		(property "Value" "BMP390"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(property "Datasheet" "BMP390"
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "F.Fab")
			(hide yes)
		)
		(property ki_fp_filters "10LGA_2X2X0p75_BOS 10LGA_2X2X0p75_BOS-M 10LGA_2X2X0p75_BOS-L")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2" "3" "4" "5" "10" "9" "8" "7" "6")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "*"
			(at -1.7145 -0.25 0)
			(unlocked yes)
			(layer "F.SilkS")
		)
		(fp_text user "*"
			(at -1.7145 -0.25 0)
			(layer "F.SilkS")
		)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at 0.1397 -0.25 0)
			(unlocked yes)
			(layer "F.Fab")
		)
		(fp_text user "*"
			(at 0.1397 -0.25 0)
			(layer "F.Fab")
		)
		(pad "1" smd rect
			(at -0.7874 -0.25 90)
			(size 0.254 0.2794)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+3V3")
			(pinfunction "VDDIO_1")
			(pintype "power_in")
		)
		(pad "2" smd rect
			(at -0.7874 0.25 90)
			(size 0.254 0.2794)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/SCL")
			(pinfunction "SCK_2")
			(pintype "input")
		)
		(pad "3" smd rect
			(at -0.499999 0.7874)
			(size 0.254 0.2794)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "VSS_3")
			(pintype "power_out")
		)
		(pad "4" smd rect
			(at 0 0.7874)
			(size 0.254 0.2794)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "/SDA")
			(pinfunction "SDI_4")
			(pintype "bidirectional")
		)
		(pad "5" smd rect
			(at 0.499999 0.7874)
			(size 0.254 0.2794)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+3V3")
			(pinfunction "SDO_5")
			(pintype "bidirectional")
		)
		(pad "6" smd rect
			(at 0.7874 0.25 90)
			(size 0.254 0.2794)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+3V3")
			(pinfunction "CSB_6")
			(pintype "input")
		)
		(pad "7" smd rect
			(at 0.7874 -0.25 90)
			(size 0.254 0.2794)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "unconnected-(U3-INT-Pad7)")
			(pinfunction "INT_7")
			(pintype "input")
		)
		(pad "8" smd rect
			(at 0.499999 -0.7874)
			(size 0.254 0.2794)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "VSS_8")
			(pintype "power_out")
		)
		(pad "9" smd rect
			(at 0 -0.7874)
			(size 0.254 0.2794)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "GND")
			(pinfunction "VSS_9")
			(pintype "power_out")
		)
		(pad "10" smd rect
			(at -0.499999 -0.7874)
			(size 0.254 0.2794)
			(layers "F.Cu" "F.Mask" "F.Paste")
			(net "+3V3")
			(pinfunction "VDD_10")
			(pintype "power_in")
		)
		(embedded_fonts no)
		(model "/home/Gary/Downloads/bmp390.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -0 -0 -90)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 83.9 85.1875 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C14"
			(at 0 1.16 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "NC"
			(at 0 -1.16 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(C14-Pad1)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "B.Cu")
		(at 95.65 75.7125 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R10"
			(at 0 1.43 270)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "1k"
			(at 0 -1.43 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "B.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "/PYRO2")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(Q2-G)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Fuse:Fuse_0603_1608Metric"
		(layer "B.Cu")
		(at 89.3 80.225 90)
		(descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf)")
		(tags "fuse")
		(property "Reference" "F2"
			(at 0 1.43 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Fuse"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Fuse"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*Fuse*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 90)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 90)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(Q2-S)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Fuse.3dshapes/Fuse_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "B.Cu")
		(at 115.325 87.8875)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C12"
			(at 0 1.43 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "100nf"
			(at 0 -1.43 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "B.Cu")
		(at 97.47 115.6125)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D3"
			(at 0 2 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "~"
			(at 0 -2.1 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Schottky diode"
			(at 0 0 180)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO-???* *_Diode_* *SingleDiode* D_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 2 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.65 0)
			(size 0.9 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "+5V")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0)
			(size 0.9 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "VBUS")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "B.Cu")
		(at 79.95 84.3875 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R13"
			(at 0 1.43 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "1k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "/BUZZER")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(Q3-B)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fc:MCU75N06YHE3-TP"
		(layer "B.Cu")
		(at 101.75 73.4875 180)
		(property "Reference" "Q1"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "MCU75N06YHE3-TP"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO?92*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "2" "1" "3")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at 0 3.9375 180)
			(size 6.2 5.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.15)
			(net "Net-(Q1-D)")
			(pinfunction "D_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -2.285 -3.26 180)
			(size 1.6 3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.15)
			(net "Net-(Q1-G)")
			(pinfunction "G_2")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at 2.285 -3.28 180)
			(size 1.6 3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.15)
			(net "Net-(Q1-S)")
			(pinfunction "S_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "/home/Gary/Downloads/IRLR7843TRPBF/IRLR7843TRPBF.step"
			(offset
				(xyz 0 1 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -90)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "B.Cu")
		(at 87.7 80.2125 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R19"
			(at 0 1.43 270)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "100"
			(at 0 -1.43 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "B.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "/RF_BUSY")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(M1-BUSY)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fc:XDCR_SMT-0827-S-HT-R"
		(layer "B.Cu")
		(at 79.05 75.8375 90)
		(property "Reference" "LS1"
			(at -1.425 6.235 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "SMT-0827-S-HT-R"
			(at 7.735 -6.6 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTREV" "31/03/20"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "3.3mm"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "PUI Audio"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "P" "N")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "2" smd custom
			(at 3.45 3.45 90)
			(size 1 1)
			(layers "B.Cu")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy -1.44056 0.34792) (xy 0.39792 -1.49056) (xy 1.55 -0.23848) (xy -0.28848 1.6)
					)
					(width 0.01)
					(fill yes)
				)
			)
		)
		(pad "4" smd custom
			(at 3.6 -3.6 90)
			(size 1 1)
			(layers "B.Cu")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 0.24792 1.64056) (xy -1.59056 -0.19792) (xy -0.68848 -1.15) (xy 1.15 -1.15) (xy 1.15 0.68848)
					)
					(width 0.01)
					(fill yes)
				)
			)
		)
		(pad "N" smd custom
			(at -3.6 -3.6 90)
			(size 1 1)
			(layers "B.Cu")
			(net "Net-(D4-A)")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy 1.59056 -0.19792) (xy -0.24792 1.64056) (xy -1.15 0.68848) (xy -1.15 -1.15) (xy 0.68848 -1.15)
					)
					(width 0.01)
					(fill yes)
				)
			)
		)
		(pad "P" smd custom
			(at -3.6 3.6 90)
			(size 1 1)
			(layers "B.Cu")
			(net "+3V3")
			(pintype "passive")
			(options
				(clearance outline)
				(anchor rect)
			)
			(primitives
				(gr_poly
					(pts
						(xy -0.24792 -1.64056) (xy 1.59056 0.19792) (xy 0.68848 1.15) (xy -1.15 1.15) (xy -1.15 -0.68848)
					)
					(width 0.01)
					(fill yes)
				)
			)
		)
		(embedded_fonts no)
		(model "/home/Gary/Downloads/SMT-0827-S-HT-R.step"
			(offset
				(xyz 0 0 1.25)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -180)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "B.Cu")
		(at 108 90.5875 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R15"
			(at 0 1.43 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "10k"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U4-~{HOLD}{slash}RESET(IO3))")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Package_TO_SOT_SMD:SOT-23"
		(layer "B.Cu")
		(at 76.45 82.975 90)
		(descr "SOT, 3 Pin (JEDEC TO-236 Var AB https://www.jedec.org/document_search?search_api_views_fulltext=TO-236)")
		(tags "SOT TO_SOT_SMD")
		(property "Reference" "Q3"
			(at 0 2.4 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "BC847"
			(at 0 -2.4 90)
			(layer "B.Fab")
		)
		(property "Datasheet" "http://www.infineon.com/dgdl/Infineon-BC847SERIES_BC848SERIES_BC849SERIES_BC850SERIES-DS-v01_01-en.pdf?fileId=db3a304314dca389011541d4630a1657"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "0.1A Ic, 45V Vce, NPN Transistor, SOT-23"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "SOT?23*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "3" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.9375 0.95 90)
			(size 1.475 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(Q3-B)")
			(pinfunction "B_1")
			(pintype "input")
		)
		(pad "2" smd roundrect
			(at -0.9375 -0.95 90)
			(size 1.475 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "E_2")
			(pintype "passive")
		)
		(pad "3" smd roundrect
			(at 0.9375 0 90)
			(size 1.475 0.6)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(D4-A)")
			(pinfunction "C_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Package_TO_SOT_SMD.3dshapes/SOT-23.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "B.Cu")
		(at 106.725 71.0875)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R9"
			(at 0 1.43 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "1k"
			(at 0 -1.43 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "/PYRO1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(Q1-G)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Diode_SMD:D_SOD-123"
		(layer "B.Cu")
		(at 81.55 82.2375 180)
		(descr "SOD-123")
		(tags "SOD-123")
		(property "Reference" "D4"
			(at 0 2 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "~"
			(at 0 -2.1 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "75V 0.15A Fast Switching Diode, SOD-123"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Device" "D"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Sim.Pins" "1=K 2=A"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "D*SOD?123*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 2 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -1.65 0 180)
			(size 0.9 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
			(pinfunction "K_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 1.65 0 180)
			(size 0.9 1.2)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(D4-A)")
			(pinfunction "A_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Diode_SMD.3dshapes/D_SOD-123.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fc:MCU75N06YHE3-TP"
		(layer "B.Cu")
		(at 91.25 73.3375 180)
		(property "Reference" "Q2"
			(at 0 0.5 0)
			(unlocked yes)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "MCU75N06YHE3-TP"
			(at 0 -1 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "TO?92*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "2" "1" "3")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 -2.5 0)
			(unlocked yes)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at 0 3.9375 180)
			(size 6.2 5.8)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.15)
			(net "Net-(Q2-D)")
			(pinfunction "D_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at -2.285 -3.26 180)
			(size 1.6 3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.15)
			(net "Net-(Q2-G)")
			(pinfunction "G_2")
			(pintype "input")
		)
		(pad "3" smd roundrect
			(at 2.285 -3.28 180)
			(size 1.6 3)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.15)
			(net "Net-(Q2-S)")
			(pinfunction "S_3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "/home/Gary/Downloads/IRLR7843TRPBF/IRLR7843TRPBF.step"
			(offset
				(xyz 0 1 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -90)
			)
		)
	)
	(footprint "fc:W25Q16JVSSIQ"
		(layer "B.Cu")
		(at 111.15 94.3375 180)
		(property "Reference" "U4"
			(at -1.05616 3.50582 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "W25Q16JVSSIQ"
			(at 7.21091 -3.507335 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "3v 16m-Bit Serial Flash Memory With Dual"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MF" "Winbond Electronics"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PACKAGE" "SOIC-8 Winbond"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PRICE" "None"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MP" "W25Q16JVSSIQ"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "AVAILABILITY" "Unavailable"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "6" "5" "2" "8" "3" "7" "4")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "1" smd roundrect
			(at -3.605 1.905 180)
			(size 1.61 0.58)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "/FLASH_CS")
			(pinfunction "~{CS}_1")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "2" smd roundrect
			(at -3.605 0.635 180)
			(size 1.61 0.58)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "/MISO")
			(pinfunction "DO(IO1)_2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "3" smd roundrect
			(at -3.605 -0.635 180)
			(size 1.61 0.58)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "/FLASH_EN")
			(pinfunction "~{WP}(IO2)_3")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "4" smd roundrect
			(at -3.605 -1.905 180)
			(size 1.61 0.58)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pinfunction "GND_4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "5" smd roundrect
			(at 3.605 -1.905 180)
			(size 1.61 0.58)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "/MOSI")
			(pinfunction "DI(IO0)_5")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "6" smd roundrect
			(at 3.605 -0.635 180)
			(size 1.61 0.58)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "/SCK")
			(pinfunction "CLK_6")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "7" smd roundrect
			(at 3.605 0.635 180)
			(size 1.61 0.58)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U4-~{HOLD}{slash}RESET(IO3))")
			(pinfunction "~{HOLD}/RESET(IO3)_7")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "8" smd roundrect
			(at 3.605 1.905 180)
			(size 1.61 0.58)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
			(pinfunction "VCC_8")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(embedded_fonts no)
		(model "/home/Gary/Downloads/W25Q16JVSSIQ/W25Q16JVSSIQ.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "B.Cu")
		(at 98.35 88.2875 -90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C4"
			(at 0 1.43 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "1uf"
			(at 0 -1.43 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "/AREF")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 270)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "B.Cu")
		(at 109.675 98.2875)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R21"
			(at 0 1.43 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "100"
			(at 0 -1.43 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(D6-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "/LED")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Capacitor_SMD:C_0402_1005Metric"
		(layer "B.Cu")
		(at 85.87 85.1875 180)
		(descr "Capacitor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf)")
		(tags "capacitor")
		(property "Reference" "C13"
			(at 0 1.16 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "NC"
			(at 0 -1.16 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Unpolarized capacitor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(M1-ANT)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.48 0 180)
			(size 0.56 0.62)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "fc:GCT_MEM2052-00-195-00-A_REVA"
		(layer "B.Cu")
		(at 114.825 79.6125 -90)
		(property "Reference" "J1"
			(at -4.45 10.6 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "MEM2052-00-195-00-A_REVA"
			(at 10.155 9.22 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "PARTREV" "A"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "STANDARD" "Manufacturer Recommendations"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "SNAPEDA_PN" "MEM2052-00-195-00-A"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MAXIMUM_PACKAGE_HEIGHT" "1.95 mm"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(property "MANUFACTURER" "Global Connector Technology"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.Fab")
			(hide yes)
		)
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "P5" "P7" "P8" "P1" "P2" "P4" "P3" "P9" "P6" "G1" "G2" "G3" "G4")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(pad "G1" smd rect
			(at -6.575 -5.925 270)
			(size 1.4 1.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "GND")
			(pinfunction "SHIELD_GND_G1")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "G2" smd rect
			(at 6.575 -6.925 270)
			(size 1.4 1.9)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "GND")
			(pinfunction "SHIELD_GND__1_G2")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "G3" smd rect
			(at -5.035 7.225 270)
			(size 1.2 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "GND")
			(pinfunction "SHIELD_GND__2_G3")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "G4" smd rect
			(at 0.715 7.225 270)
			(size 1.3 1.4)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "GND")
			(pinfunction "SHIELD_GND__3_G4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "P1" smd rect
			(at 1.905 -3.635 270)
			(size 0.8 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "unconnected-(J1-DAT2-PadP1)")
			(pinfunction "DAT2_P1")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "P2" smd rect
			(at 0.805 -3.235 270)
			(size 0.8 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "/SD_CS")
			(pinfunction "CD/DAT3_P2")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "P3" smd rect
			(at -0.295 -3.635 270)
			(size 0.8 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "/MOSI")
			(pinfunction "CMD_P3")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "P4" smd rect
			(at -1.395 -3.835 270)
			(size 0.8 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "+3V3")
			(pinfunction "VDD_P4")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "P5" smd rect
			(at -2.495 -3.635 270)
			(size 0.8 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "/SCK")
			(pinfunction "CLK_P5")
			(pintype "input")
			(solder_mask_margin 0.102)
		)
		(pad "P6" smd rect
			(at -3.595 -3.835 270)
			(size 0.8 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "GND")
			(pinfunction "VSS_P6")
			(pintype "power_in")
			(solder_mask_margin 0.102)
		)
		(pad "P7" smd rect
			(at -4.695 -3.635 270)
			(size 0.8 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "/MISO")
			(pinfunction "DAT0_P7")
			(pintype "bidirectional")
			(solder_mask_margin 0.102)
		)
		(pad "P8" smd rect
			(at -5.795 -3.635 270)
			(size 0.8 1.5)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "unconnected-(J1-DAT1-PadP8)")
			(pinfunction "DAT1_P8")
			(pintype "bidirectional+no_connect")
			(solder_mask_margin 0.102)
		)
		(pad "P9" smd rect
			(at -3.585 7.595 270)
			(size 1 1.04)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(net "/SD_DETECT")
			(pinfunction "CD_PIN_P9")
			(pintype "passive")
			(solder_mask_margin 0.102)
		)
		(zone
			(layers "F.Cu" "B.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.01)
			(keepout
				(tracks allowed)
				(vias not_allowed)
				(pads allowed)
				(copperpour allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
				(island_removal_mode 0)
			)
			(polygon
				(pts
					(xy 113.59 82.0625) (xy 113.59 73.3025) (xy 111.29 73.3025) (xy 111.29 75.3225) (xy 109.46 75.3225)
					(xy 109.46 76.8225) (xy 111.29 76.8225) (xy 111.29 82.0625)
				)
			)
		)
		(zone
			(layer "B.Cu")
			(hatch full 0.508)
			(connect_pads
				(clearance 0)
			)
			(min_thickness 0.01)
			(keepout
				(tracks not_allowed)
				(vias not_allowed)
				(pads not_allowed)
				(copperpour not_allowed)
				(footprints allowed)
			)
			(placement
				(enabled no)
				(sheetname "")
			)
			(fill
				(thermal_gap 0.508)
				(thermal_bridge_width 0.508)
				(island_removal_mode 0)
			)
			(polygon
				(pts
					(xy 113.59 82.0625) (xy 113.59 73.3025) (xy 111.29 73.3025) (xy 111.29 75.3225) (xy 109.46 75.3225)
					(xy 109.46 76.8225) (xy 111.29 76.8225) (xy 111.29 82.0625)
				)
			)
		)
		(embedded_fonts no)
		(model "/home/Gary/Downloads/173905292-3-mem2052-00-195-00-a/mem2052-00-195-00-a.stp"
			(offset
				(xyz 0 -7.5 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz -90 -0 -0)
			)
		)
	)
	(footprint "Fuse:Fuse_0603_1608Metric"
		(layer "B.Cu")
		(at 103.2 80.075 90)
		(descr "Fuse SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf)")
		(tags "fuse")
		(property "Reference" "F1"
			(at 0 1.43 90)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "Fuse"
			(at 0 -1.43 90)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Fuse"
			(at 0 0 90)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "*Fuse*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 90)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.7875 0 90)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.7875 0 90)
			(size 0.875 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(Q1-S)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Fuse.3dshapes/Fuse_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "B.Cu")
		(at 114.1 90.5875)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C11"
			(at 0 1.43 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "22pf"
			(at 0 -1.43 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "B.Cu")
		(at 111.05 90.5875)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R17"
			(at 0 1.43 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "100"
			(at 0 -1.43 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 180)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 180)
			(layer "B.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 270)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(D5-A)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "+3V3")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "B.Cu")
		(at 100.75 91.5375 180)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "C1"
			(at 0 1.43 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "1uf"
			(at 0 -1.43 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "C_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 90)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(U1-VDDCORE)")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 180)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "GND")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Standard:0603-cap"
		(layer "B.Cu")
		(at 86.05 80.1625 90)
		(descr "Capacitor SMD 0603 (1608 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: IPC-SM-782 page 76, https://www.pcb-3d.com/wordpress/wp-content/uploads/ipc-sm-782a_amendment_1_and_2.pdf), generated with kicad-footprint-generator")
		(tags "capacitor")
		(property "Reference" "R20"
			(at 0 1.43 270)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "100"
			(at 0 -1.43 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Datasheet" ""
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" ""
			(at 0 0 270)
			(layer "B.Fab")
			(hide yes)
		)
		(property "KiLib_Generator" "SMD_2terminal_chip_molded"
			(at 0 0 270)
			(layer "B.SilkS")
			(hide yes)
		)
		(property ki_fp_filters "R_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${VALUE}"
			(at 0 0 0)
			(unlocked yes)
			(layer "B.SilkS")
		)
		(pad "1" smd roundrect
			(at -0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "/RF_INT")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.775 0 90)
			(size 0.9 0.95)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(M1-DIO1)")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD9_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0603_1608Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(footprint "Inductor_SMD:L_0402_1005Metric"
		(layer "B.Cu")
		(at 85.15 83.8875 180)
		(descr "Inductor SMD 0402 (1005 Metric), square (rectangular) end terminal, IPC-7351 nominal, (Body size source: http://www.tortai-tech.com/upload/download/2011102023233369053.pdf)")
		(tags "inductor")
		(property "Reference" "L1"
			(at 0 1.17 0)
			(layer "B.SilkS")
			(hide yes)
		)
		(property "Value" "0"
			(at 0 -1.17 0)
			(layer "B.Fab")
		)
		(property "Datasheet" ""
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property "Description" "Inductor"
			(at 0 0 0)
			(layer "B.Fab")
			(hide yes)
		)
		(property ki_fp_filters "Choke_* *Coil* Inductor_* L_*")
		(sheetname "/")
		(sheetfile "fc.kicad_sch")
		(units
			(unit
				(name "A")
				(pins "1" "2")
			)
		)
		(attr smd)
		(duplicate_pad_numbers_are_jumpers no)
		(fp_text user "${REFERENCE}"
			(at 0 0 0)
			(layer "B.Fab")
		)
		(pad "1" smd roundrect
			(at -0.485 0 180)
			(size 0.59 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(M1-ANT)")
			(pinfunction "1_1")
			(pintype "passive")
		)
		(pad "2" smd roundrect
			(at 0.485 0 180)
			(size 0.59 0.64)
			(layers "B.Cu" "B.Mask" "B.Paste")
			(roundrect_rratio 0.25)
			(net "Net-(C14-Pad1)")
			(pinfunction "2_2")
			(pintype "passive")
		)
		(embedded_fonts no)
		(model "${KICAD10_3DMODEL_DIR}/Inductor_SMD.3dshapes/L_0402_1005Metric.step"
			(offset
				(xyz 0 0 0)
			)
			(scale
				(xyz 1 1 1)
			)
			(rotate
				(xyz 0 0 0)
			)
		)
	)
	(gr_rect
		(start 73.4 64.7875)
		(end 123.399999 124.7875)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 76.4 67.7875)
		(end 77.9 67.7875)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 76.4 121.7875)
		(end 77.9 121.7875)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 120.4 67.7875)
		(end 121.9 67.7875)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_circle
		(center 120.4 121.7875)
		(end 121.9 121.7875)
		(fill no)
		(layer "Edge.Cuts")
	)
	(gr_text "0.1uf"
		(at 115.35 87.8875 90)
		(layer "F.SilkS")
	)
	(gr_text "POWER"
		(at 109.75 93.5375 0)
		(layer "F.SilkS")
	)
	(gr_text "LED\n"
		(at 109.75 95.8875 0)
		(layer "F.SilkS")
	)
	(gr_text "3V3"
		(at 121.35 87.7875 0)
		(layer "F.SilkS")
	)
	(gr_text "RESET"
		(at 121.45 96.4875 0)
		(layer "F.SilkS")
	)
	(gr_text "DIO"
		(at 117.05 89.5875 90)
		(layer "F.SilkS")
	)
	(gr_text "CLK\n"
		(at 117.05 92.1875 90)
		(layer "F.SilkS")
	)
	(gr_text "v1.1"
		(at 114.05 78.9875 0)
		(layer "F.SilkS")
	)
	(gr_text "RESET"
		(at 97.45 70.9875 0)
		(layer "F.SilkS")
	)
	(gr_text "-\n"
		(at 114.15 110.5375 90)
		(layer "F.SilkS")
	)
	(gr_text "+"
		(at 114.15 117.1875 90)
		(layer "F.SilkS")
	)
	(gr_text "BATTERY"
		(at 116.75 103.0375 90)
		(layer "F.SilkS")
	)
	(gr_text "G"
		(at 76.25 108.2875 270)
		(layer "F.SilkS")
	)
	(gr_text "V"
		(at 78.75 108.2875 270)
		(layer "F.SilkS")
	)
	(gr_text "S"
		(at 81.25 108.2875 270)
		(layer "F.SilkS")
	)
	(gr_text "PYRO1"
		(at 81.5 94.7875 270)
		(layer "F.SilkS")
	)
	(gr_text "PYRO2\n"
		(at 81.5 103.7875 270)
		(layer "F.SilkS")
	)
	(gr_text "1"
		(at 84 110.2875 270)
		(layer "F.SilkS")
	)
	(gr_text "2\n"
		(at 84 113.7875 270)
		(layer "F.SilkS")
	)
	(gr_text "3"
		(at 84 117.7875 270)
		(layer "F.SilkS")
	)
	(gr_text "GO"
		(at 107.45 79.1875 0)
		(layer "F.SilkS")
	)
	(gr_text "F"
		(at 89.25 80.2875 0)
		(layer "B.SilkS")
	)
	(gr_text "F"
		(at 103.15 80.0875 0)
		(layer "B.SilkS")
	)
	(zone
		(net "GND")
		(layers "F.Cu" "B.Cu")
		(name "GND")
		(hatch edge 0.5)
		(connect_pads
			(clearance 0.5)
		)
		(min_thickness 0.25)
		(fill yes
			(thermal_gap 0.5)
			(thermal_bridge_width 0.5)
			(island_removal_mode 0)
		)
		(polygon
			(pts
				(xy 123.4 64.8) (xy 123.409429 124.79214) (xy 73.4 124.8) (xy 73.4 64.8)
			)
		)
	)
	(embedded_fonts no)
)
