2.425 GHz Wilkinson Power Splitter

This Wilkinson power splitter is designed for operation at 2.425 GHz and fabrication on a standard two-layer PCB using 1.6 mm thick FR-4 material.

Files for simulation, PCB design, and manufacturing-ready Gerber files are included.