<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<schematic>
<libraries>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08-EIAJ">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
<package name="DIP08">
<description>&lt;b&gt;Dual In Line&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="ATTINY13">
<pin name="VCC"/>
<pin name="PB1(MISO)"/>
<pin name="PB5(NRES)"/>
<pin name="GND"/>
<pin name="PB0(MOSI)"/>
<pin name="PB2(SCK/ADC1)"/>
<pin name="PB3(ADC3)"/>
<pin name="PB4(ADC2)"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ATTINY45" prefix="U" uservalue="yes">
<description>Atmel 8-pin 2/4/8kB flash uC</description>
<gates>
<gate name="G$1" symbol="ATTINY13"/>
</gates>
<devices>
<device name="TINY45-20-SMT" package="SO08-EIAJ">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB0(MOSI)" pad="5"/>
<connect gate="G$1" pin="PB1(MISO)" pad="6"/>
<connect gate="G$1" pin="PB2(SCK/ADC1)" pad="7"/>
<connect gate="G$1" pin="PB3(ADC3)" pad="2"/>
<connect gate="G$1" pin="PB4(ADC2)" pad="3"/>
<connect gate="G$1" pin="PB5(NRES)" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-08922"/>
<attribute name="VALUE" value="Tiny45-20-SMT"/>
</technology>
</technologies>
</device>
<device name="TINY45-20-DIP" package="DIP08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB0(MOSI)" pad="5"/>
<connect gate="G$1" pin="PB1(MISO)" pad="6"/>
<connect gate="G$1" pin="PB2(SCK/ADC1)" pad="7"/>
<connect gate="G$1" pin="PB3(ADC3)" pad="2"/>
<connect gate="G$1" pin="PB4(ADC2)" pad="3"/>
<connect gate="G$1" pin="PB5(NRES)" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09439"/>
<attribute name="VALUE" value="TINY45-20-DIP"/>
</technology>
</technologies>
</device>
<device name="TINY85-20-DIP" package="DIP08">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB0(MOSI)" pad="5"/>
<connect gate="G$1" pin="PB1(MISO)" pad="6"/>
<connect gate="G$1" pin="PB2(SCK/ADC1)" pad="7"/>
<connect gate="G$1" pin="PB3(ADC3)" pad="2"/>
<connect gate="G$1" pin="PB4(ADC2)" pad="3"/>
<connect gate="G$1" pin="PB5(NRES)" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09445"/>
<attribute name="VALUE" value="TINY85-20-DIP"/>
</technology>
</technologies>
</device>
<device name="TINY85-20-SMT" package="SO08-EIAJ">
<connects>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="PB0(MOSI)" pad="5"/>
<connect gate="G$1" pin="PB1(MISO)" pad="6"/>
<connect gate="G$1" pin="PB2(SCK/ADC1)" pad="7"/>
<connect gate="G$1" pin="PB3(ADC3)" pad="2"/>
<connect gate="G$1" pin="PB4(ADC2)" pad="3"/>
<connect gate="G$1" pin="PB5(NRES)" pad="1"/>
<connect gate="G$1" pin="VCC" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="IC-09092"/>
<attribute name="VALUE" value="Tiny85-20-SMT"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-0603">
</package>
<package name="LED-1206">
</package>
<package name="LED-1206-BOTTOM">
</package>
</packages>
<symbols>
<symbol name="LED">
<pin name="C" direction="pas"/>
<pin name="A" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="LED-GREEN" prefix="D" uservalue="yes">
<description>&lt;B&gt;Various green LEDs&lt;br&gt;&lt;br&gt;&lt;/B&gt;
Green LEDs used in SFE Production&lt;br&gt;&lt;br&gt;
0603- DIO-00821&lt;br&gt;
LARGE- DIO-00862&lt;br&gt;
LILYPAD- DIO-09910&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="LED"/>
</gates>
<devices>
<device name="0603" package="LED-0603">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-00821"/>
<attribute name="VALUE" value="GREEN"/>
</technology>
</technologies>
</device>
<device name="LILYPAD" package="LED-1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-09910"/>
<attribute name="VALUE" value="GREEN"/>
</technology>
</technologies>
</device>
<device name="1206" package="LED-1206">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-00862"/>
<attribute name="VALUE" value="GREEN"/>
</technology>
</technologies>
</device>
<device name="1206-BOTTOM" package="LED-1206-BOTTOM">
<connects>
<connect gate="G$1" pin="A" pad="A"/>
<connect gate="G$1" pin="C" pad="C"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="DIO-11076"/>
<attribute name="VALUE" value="Green"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
<package name="AXIAL-0.3">
</package>
<package name="R2010">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="0805">
</package>
<package name="0603-RES">
</package>
<package name="0402-RES">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="1/6W-RES">
<description>1/6W Thru-hole Resistor - *UNPROVEN*</description>
</package>
<package name="R2512">
</package>
<package name="AXIAL-0.4">
<description>1/4W Resistor, 0.4" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="AXIAL-0.5">
<description>1/2W Resistor, 0.5" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="AXIAL-0.6">
<description>1W Resistor, 0.6" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="AXIAL-0.8">
<description>2W Resistor, 0.8" wide&lt;p&gt;

Yageo CFR series &lt;a href="http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf"&gt;http://www.yageo.com/pdf/yageo/Leaded-R_CFR_2008.pdf&lt;/a&gt;</description>
</package>
<package name="AXIAL-0.3-KIT">
<description>&lt;h3&gt;AXIAL-0.3-KIT&lt;/h3&gt;

Commonly used for 1/4W through-hole resistors. 0.3" pitch between holes.&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of the AXIAL-0.3 package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.</description>
</package>
<package name="AXIAL-0.3EZ">
<description>This is the "EZ" version of the standard .3" spaced resistor package.&lt;br&gt;
It has a reduced top mask to make it harder to install upside-down.</description>
</package>
</packages>
<symbols>
<symbol name="RESISTOR">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="RESISTOR" prefix="R" uservalue="yes">
<description>&lt;b&gt;Resistor&lt;/b&gt;
Basic schematic elements and footprints for 0603, 1206, and PTH resistors.</description>
<gates>
<gate name="G$1" symbol="RESISTOR"/>
</gates>
<devices>
<device name="1206" package="1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="AXIAL-0.3" package="AXIAL-0.3">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2010" package="R2010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0805-RES" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0603-RES" package="0603-RES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="0402-RES" package="0402-RES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-1/6W" package="1/6W-RES">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="2512" package="R2512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-1/4W" package="AXIAL-0.4">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-1/2W" package="AXIAL-0.5">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-1W" package="AXIAL-0.6">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="PTH-2W" package="AXIAL-0.8">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="KIT" package="AXIAL-0.3-KIT">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="EZ" package="AXIAL-0.3EZ">
<connects>
<connect gate="G$1" pin="1" pad="P$1"/>
<connect gate="G$1" pin="2" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="Ilya_Teach">
<packages>
<package name="0805">
</package>
</packages>
<symbols>
<symbol name="CAP">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="CAP" prefix="C" uservalue="yes">
<gates>
<gate name="G$1" symbol="CAP"/>
</gates>
<devices>
<device name="" package="0805">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="switch">
<packages>
<package name="3-SLIDESWITCH">
</package>
</packages>
<symbols>
<symbol name="3-SLIDESWITCH">
<pin name="P$1"/>
<pin name="P$2"/>
<pin name="P$3"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="3-SLIDESWITCH">
<gates>
<gate name="G$1" symbol="3-SLIDESWITCH"/>
</gates>
<devices>
<device name="" package="3-SLIDESWITCH">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
<connect gate="G$1" pin="P$3" pad="P$3"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="SparkFun-Batteries">
<description>&lt;h3&gt;SparkFun Batteries&lt;/h3&gt;
This library contains battery clips, connectors, and appropriately sized silk outlines for LiPo batteries. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BATTERY-AAA">
<description>&lt;h3&gt;AAA Battery Clips&lt;/h3&gt;
&lt;p&gt;PCB mount clips properly spaced to hold a AAA battery.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Prototyping/M60-2p9.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="BATTERY-AA">
<description>&lt;h3&gt;AA Battery Clips&lt;/h3&gt;
&lt;p&gt;PCB mount clips properly spaced to hold a AA battery&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Prototyping/M60-2p9.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="BATTCON_12MM_PTH">
<description>&lt;h3&gt;12mm Coin Cell Battery (CR1225) Holder - PTH&lt;/h3&gt;
&lt;p&gt;This is a through hole 12mm coin cell battery holder. Holds battery in place with friction. Metal housing is +, PCB pad underneath is -.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Prototyping/KEY-3001.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="BATTCON_20MM">
<description>&lt;h3&gt;20mm Coin Cell Battery (CR2032) Holder - SMD (Single Pad)&lt;/h3&gt;
&lt;p&gt;Part number: CR2032-THM&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="BATTCOM_20MM_PTH">
<description>&lt;h3&gt;20mm (CR2032) Coin Cell Battery Holder - PTH&lt;/h3&gt;
&lt;p&gt;Basic 20mm coin cell holder. Posts can be inserted into 0.1" perf board! Holds the common CR2032 type batteries.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.sparkfun.com/datasheets/Prototyping/CoinCellHolder-20mm.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="BATTCON_24.5MM_PTH">
<description>&lt;h3&gt;24.5mm Coin Cell Battery (CR2450) Holder - PTH&lt;/h3&gt;
&lt;p&gt;Through hole 24.5 mm coin cell holder. Holds battery in place with friction. Metal housing is +, PCB pad underneath is -.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.sparkfun.com/datasheets/Batteries/Coin_Cell_Holder_245mm-3009.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="BATTCON_12MM">
<description>&lt;h3&gt;12mm Coin Cell (CR1225) Battery Holder - SMD&lt;/h3&gt;
&lt;p&gt;Holds battery in place with friction. The metal housing connects to the positive side of the battery and the PCB pad underneath is connected to the negative side.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Prototyping/KEY-3000.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="BATTCON_20MM_4LEGS">
<description>&lt;h3&gt;20mm Coin Cell Battery (CR2032) Holder - SMD (Dual Pad)&lt;/h3&gt;
&lt;p&gt;This holder fits 20mm Lithium coin cell batteries and holds the battery in place with friction. The metal housing connects to the positive (+) side of the battery and the PCB pad underneath is connected to the negative (-) side.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Prototyping/BAT-BLH-001.jpg"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="BATTERY-AA-KIT">
<description>&lt;h3&gt;AA Battery Clips (KIT Variant)&lt;/h3&gt;
&lt;p&gt;PCB mount clips properly spaced to hold a AA battery&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Prototyping/M60-2p9.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="BATTCON_9V">
<description>&lt;h3&gt;PCMOUNT 9V Battery Holder&lt;/h3&gt;
&lt;p&gt;&lt;a href="http://www.memoryprotectiondevices.com/datasheets/BC9VPC-datasheet.pdf"&gt;Datasheet&lt;/a&gt; (MPD BC9VPC)&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="BATTCON_20MM_4LEGS_OVERPASTE">
<description>&lt;h3&gt;20mm Coin Cell Battery (CR2032) Holder - SMD (Dual Pad) (Overpaste on pads)&lt;/h3&gt;
&lt;p&gt;This holder fits 20mm Lithium coin cell batteries and holds the battery in place with friction. The metal housing connects to the positive (+) side of the battery and the PCB pad underneath is connected to the negative (-) side.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Prototyping/BAT-BLH-001.jpg"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="BATTERY-AAA-KIT">
<description>&lt;h3&gt;AAA Battery Clips (KIT Variant)&lt;/h3&gt;
&lt;p&gt;PCB mount clips properly spaced to hold a AAA battery.&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Warning:&lt;/b&gt; This is the KIT version of this package. This package has a smaller diameter top stop mask, which doesn't cover the diameter of the pad. This means only the bottom side of the pads' copper will be exposed. You'll only be able to solder to the bottom side.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Prototyping/M60-2p9.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
<package name="BATTERY_18650-HOLDER">
<description>&lt;h3&gt;18650 Lithium Ion Cell Battery Holders&lt;/h3&gt;
&lt;p&gt;PCB mount clips properly spaced to hold a 18650 Lithium Ion Cell battery.&lt;/p&gt;
&lt;p&gt;&lt;a href="https://cdn.sparkfun.com/datasheets/Prototyping/54.PDF"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
<symbols>
<symbol name="BATTERY">
<description>&lt;h3&gt;Battery (Single-Cell)&lt;/h3&gt;</description>
<pin name="-" direction="pwr"/>
<pin name="+" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="BATTERY" prefix="BT" uservalue="yes">
<description>&lt;h3&gt;Battery - Single Cell&lt;/h3&gt;
&lt;p&gt;A variety of battery chemistries, sizes, and footprints.&lt;/p&gt;
&lt;p&gt;Device List:
&lt;ul&gt;
&lt;li&gt;&lt;b&gt;20MM_PTH - &lt;/b&gt; &lt;a href="https://www.sparkfun.com/products/783"&gt;Coin Cell Battery Holder - 20mm (PTH)&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;b&gt;12MM_SMD - &lt;/b&gt; &lt;a href="https://www.sparkfun.com/products/10592"&gt;Coin Cell Battery Holder - 12mm (SMD)&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;b&gt;12MM_PTH - &lt;/b&gt;&lt;a href="https://www.sparkfun.com/products/7948"&gt;Coin Cell Battery Holder - 12mm (PTH)&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;b&gt;20MM_SMD - &lt;/b&gt; 20mm Coin Cell Battery Holder (SMD) (2 legs)&lt;/li&gt;
&lt;ul&gt;&lt;li&gt;Used on the &lt;a href="https://www.sparkfun.com/products/11734"&gt;Big Time Watch Kit&lt;/a&gt;&lt;/li&gt;&lt;/ul&gt;
&lt;li&gt;&lt;b&gt;20MM_SMD_4LEGS - &lt;/b&gt; &lt;a href="https://www.sparkfun.com/products/11892"&gt;Coin Cell Battery Holder - 20mm (SMD)&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;b&gt;20MM_SMD_4LEGS_OVERPASTE - &lt;/b&gt; &lt;a href="https://www.sparkfun.com/products/11892"&gt;Coin Cell Battery Holder - 20mm (SMD)&lt;/a&gt; (Over-paste on the legs)&lt;/li&gt;
&lt;li&gt;&lt;b&gt;24.5MM_PTH - &lt;/b&gt; &lt;a href="https://www.sparkfun.com/products/8863"&gt;Coin Cell Battery Holder - 24.5mm (PTH)&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;b&gt;9V - &lt;/b&gt; 9V Battery Holder - PC Mount &lt;/li&gt;
&lt;ul&gt;&lt;li&gt;Used on the &lt;a href="https://www.sparkfun.com/products/11177"&gt;SparkFun SparkPunk Sound Kit &lt;/a&gt; and &lt;a href="https://www.sparkfun.com/products/12707"&gt;SparkFun SparkPunk Sequencer Kit &lt;/a&gt;&lt;/li&gt;&lt;/ul&gt;
&lt;li&gt;&lt;b&gt;18650 - &lt;/b&gt; &lt;a href="https://www.sparkfun.com/products/13113"&gt;Battery Holder - 18650 (PTH)&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;b&gt;AA - &lt;/b&gt; &lt;a href="https://www.sparkfun.com/products/7949"&gt;Battery Holder - 1xAA (PTH)&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;b&gt;AAA - &lt;/b&gt; &lt;a href="https://www.sparkfun.com/products/12718"&gt;Battery Holder - 1xAAA (PTH)&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;b&gt;AA_KIT - &lt;/b&gt; &lt;a href="https://www.sparkfun.com/products/7949"&gt;Battery Holder - 1xAA (PTH)&lt;/a&gt;&lt;/li&gt;
&lt;ul&gt;&lt;li&gt;Special kit package - pads only have exposed copper on one side of the board.&lt;/li&gt;&lt;/ul&gt;
&lt;li&gt;&lt;b&gt;AAA_KIT - &lt;/b&gt; &lt;a href="https://www.sparkfun.com/products/12718"&gt;Battery Holder - 1xAAA (PTH)&lt;/a&gt;&lt;/li&gt;
&lt;ul&gt;&lt;li&gt;Special kit package - pads only have exposed copper on one side of the board.&lt;/li&gt;&lt;/ul&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="BATTERY"/>
</gates>
<devices>
<device name="-AAA" package="BATTERY-AAA">
<connects>
<connect gate="G$1" pin="+" pad="PWR@1"/>
<connect gate="G$1" pin="-" pad="GND@1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="BATT-08571"/>
<attribute name="SF_SKU" value="PRT-12718"/>
</technology>
</technologies>
</device>
<device name="-AA" package="BATTERY-AA">
<connects>
<connect gate="G$1" pin="+" pad="PWR@1"/>
<connect gate="G$1" pin="-" pad="GND@1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="BATT-08316"/>
<attribute name="SF_SKU" value="PRT-07949"/>
</technology>
</technologies>
</device>
<device name="-12MM_PTH" package="BATTCON_12MM_PTH">
<connects>
<connect gate="G$1" pin="+" pad="VCC@1"/>
<connect gate="G$1" pin="-" pad="GND"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="BATT-08315"/>
<attribute name="SF_SKU" value="PRT-07948"/>
</technology>
</technologies>
</device>
<device name="-20MM_SMD" package="BATTCON_20MM">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="BATT-11519"/>
</technology>
</technologies>
</device>
<device name="-20MM_PTH" package="BATTCOM_20MM_PTH">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="BATT-09031"/>
<attribute name="SF_SKU" value="PRT-00783"/>
</technology>
</technologies>
</device>
<device name="-24.5MM_PTH" package="BATTCON_24.5MM_PTH">
<connects>
<connect gate="G$1" pin="+" pad="3"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="SF_SKU" value="PRT-08863"/>
</technology>
</technologies>
</device>
<device name="-12MM_SMD" package="BATTCON_12MM">
<connects>
<connect gate="G$1" pin="+" pad="PWR@1"/>
<connect gate="G$1" pin="-" pad="GND"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="BATT-08044"/>
<attribute name="SF_SKU" value="PRT-10592"/>
</technology>
</technologies>
</device>
<device name="-20MM_SMD_4LEGS" package="BATTCON_20MM_4LEGS">
<connects>
<connect gate="G$1" pin="+" pad="POSITIVE@1 POSITIVE@2 POSITIVE@3 POSITIVE@4"/>
<connect gate="G$1" pin="-" pad="NEGATIVE"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="BATT-10373"/>
<attribute name="SF_SKU" value="PRT-11892"/>
</technology>
</technologies>
</device>
<device name="-AA_KIT" package="BATTERY-AA-KIT">
<connects>
<connect gate="G$1" pin="+" pad="PWR@1"/>
<connect gate="G$1" pin="-" pad="GND@1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="BATT-08316"/>
<attribute name="SF_SKU" value="PRT-07949"/>
</technology>
</technologies>
</device>
<device name="-9V" package="BATTCON_9V">
<connects>
<connect gate="G$1" pin="+" pad="+"/>
<connect gate="G$1" pin="-" pad="-"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="BATT-10855"/>
</technology>
</technologies>
</device>
<device name="-20MM_SMD_4LEGS_OVERPASTE" package="BATTCON_20MM_4LEGS_OVERPASTE">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="PRT-11892 "/>
<attribute name="SF_SKU" value="BATT-10373"/>
</technology>
</technologies>
</device>
<device name="-AAA_KIT" package="BATTERY-AAA-KIT">
<connects>
<connect gate="G$1" pin="+" pad="PWR@1"/>
<connect gate="G$1" pin="-" pad="GND@1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="BATT-08571"/>
<attribute name="SF_SKU" value="PRT-12718"/>
</technology>
</technologies>
</device>
<device name="-18650" package="BATTERY_18650-HOLDER">
<connects>
<connect gate="G$1" pin="+" pad="PWR@1"/>
<connect gate="G$1" pin="-" pad="GND@1"/>
</connects>
<technologies>
<technology name="">
<attribute name="PROD_ID" value="BATT-12327"/>
<attribute name="SF_SKU" value="PRT-13113"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<parts>
<part name="U1" library="SparkFun-DigitalIC" deviceset="ATTINY45" device="TINY85-20-SMT" value="Tiny85-20-SMT"/>
<part name="D3" library="SparkFun-LED" deviceset="LED-GREEN" device="0603" value="GREEN"/>
<part name="D4" library="SparkFun-LED" deviceset="LED-GREEN" device="0603" value="GREEN"/>
<part name="R3" library="SparkFun-Passives" deviceset="RESISTOR" device="0805-RES" value="330R"/>
<part name="R4" library="SparkFun-Passives" deviceset="RESISTOR" device="0805-RES" value="330R"/>
<part name="C1" library="Ilya_Teach" deviceset="CAP" device="" value="0.1uF"/>
<part name="U$2" library="switch" deviceset="3-SLIDESWITCH" device=""/>
<part name="BT1" library="SparkFun-Batteries" deviceset="BATTERY" device="-20MM_SMD_4LEGS"/>
<part name="C2" library="Ilya_Teach" deviceset="CAP" device="" value="4.7uF"/>
</parts>
<sheets>
<sheet>
<plain>
</plain>
<busses>
</busses>
<nets>
<net name="N$3">
<segment>
<pinref part="D3" gate="G$1" pin="C"/>
<pinref part="R3" gate="G$1" pin="2"/>
</segment>
</net>
<net name="N$4">
<segment>
<pinref part="D4" gate="G$1" pin="C"/>
<pinref part="R4" gate="G$1" pin="2"/>
</segment>
</net>
<net name="LED3">
<segment>
<pinref part="U1" gate="G$1" pin="PB3(ADC3)"/>
</segment>
</net>
<net name="LED4">
<segment>
<pinref part="D4" gate="G$1" pin="A"/>
</segment>
<segment>
<pinref part="U1" gate="G$1" pin="PB4(ADC2)"/>
</segment>
</net>
<net name="LED2">
<segment>
<pinref part="U1" gate="G$1" pin="PB2(SCK/ADC1)"/>
</segment>
</net>
<net name="LED1">
<segment>
<pinref part="U1" gate="G$1" pin="PB1(MISO)"/>
</segment>
<segment>
<pinref part="D3" gate="G$1" pin="A"/>
</segment>
</net>
<net name="GND">
<segment>
<pinref part="U1" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="R3" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="R4" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="BT1" gate="G$1" pin="-"/>
</segment>
<segment>
<pinref part="C1" gate="G$1" pin="2"/>
</segment>
<segment>
<pinref part="C2" gate="G$1" pin="2"/>
</segment>
</net>
<net name="VCC">
<segment>
<pinref part="U1" gate="G$1" pin="VCC"/>
</segment>
<segment>
<pinref part="C1" gate="G$1" pin="1"/>
<pinref part="U$2" gate="G$1" pin="P$3"/>
<pinref part="C2" gate="G$1" pin="1"/>
</segment>
</net>
<net name="N$13">
<segment>
<pinref part="U1" gate="G$1" pin="PB0(MOSI)"/>
</segment>
</net>
<net name="N$18">
<segment>
<pinref part="U1" gate="G$1" pin="PB5(NRES)"/>
</segment>
</net>
<net name="SWITCH">
<segment>
<pinref part="U$2" gate="G$1" pin="P$1"/>
<pinref part="BT1" gate="G$1" pin="+"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
