<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.7.0">
<drawing>
<board>
<plain>
<wire x1="19" y1="23" x2="1" y2="23" width="0" layer="20"/>
<wire x1="1" y1="23" x2="0" y2="22" width="0" layer="20" curve="90"/>
<wire x1="0" y1="22" x2="0" y2="1" width="0" layer="20"/>
<wire x1="0" y1="1" x2="1" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1" y1="0" x2="19" y2="0" width="0" layer="20"/>
<wire x1="19" y1="0" x2="20" y2="1" width="0" layer="20" curve="90"/>
<wire x1="20" y1="1" x2="20" y2="22" width="0" layer="20"/>
<wire x1="20" y1="22" x2="19" y2="23" width="0" layer="20" curve="90"/>
<text>E2417CS051 BoB</text>
<text>soniktech.com</text>
</plain>
<libraries>
<library name="MF_Passives">
<packages>
<package name="C0603">
<description>&lt;b&gt;Description:&lt;/b&gt; Standard 0603 Package for Capacitors&lt;br/&gt;</description>
</package>
<package name="C0805">
<description>&lt;b&gt;Description:&lt;/b&gt; Standard 0805 Package for Capacitors&lt;br/&gt;</description>
</package>
<package name="R0805">
<description>&lt;b&gt;Description:&lt;/b&gt; Standard 0805 Package for Resistors&lt;br/&gt;</description>
</package>
</packages>
</library>
<library name="MF_Discrete_Semiconductor">
<packages>
<package name="SOD-123">
<description>&lt;b&gt;Description:&lt;/b&gt; Footprint for Diodes in SOD-123 Standard.&lt;br/&gt;</description>
</package>
<package name="SOT323">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="INDUCTOR-SRP4020">
</package>
</packages>
</library>
<library name="con-hirose">
<description>&lt;b&gt;Hirose Connectors&lt;/b&gt;&lt;p&gt;
www.hirose.co.jp&lt;p&gt;
Include : &lt;br&gt;
con-hirose-df12d(3.0)60dp0.5v80.lbr from Bob Starr &amp;lt;rtzaudio@mindspring.com&amp;gt;&lt;br&gt;
con-hirose.lbr from Bob Starr &amp;lt;rtzaudio@mindspring.com&amp;gt;&lt;br&gt;</description>
<packages>
<package name="XF3M-34">
</package>
</packages>
</library>
<library name="MF_Connectors">
<packages>
<package name="PTH_2.54MM_01X09">
<description>&lt;b&gt;Description:&lt;/b&gt; Package for 2.54MM Pitch Header 9 Position. Based on 4UCON 00834.&lt;br&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="MF_Passives" package="C0603" value="4.7uF / 25V">
<attribute name="MPN" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="VOLTAGE" value=""/>
<attribute name="HOUSEPART" value=""/>
<attribute name="URL" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="DIELECTRIC" value=""/>
<attribute name="NAME"/>
</element>
<element name="C2" library="MF_Passives" package="C0805" value="4.7uF / 50V">
<attribute name="MPN" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="VOLTAGE" value=""/>
<attribute name="HOUSEPART" value=""/>
<attribute name="URL" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="DIELECTRIC" value=""/>
<attribute name="NAME"/>
</element>
<element name="C3" library="MF_Passives" package="C0603" value="4.7uF / 25V">
<attribute name="MPN" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="VOLTAGE" value=""/>
<attribute name="HOUSEPART" value=""/>
<attribute name="URL" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="DIELECTRIC" value=""/>
<attribute name="NAME"/>
</element>
<element name="C4" library="MF_Passives" package="C0603" value="4.7uF / 25V">
<attribute name="MPN" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="VOLTAGE" value=""/>
<attribute name="HOUSEPART" value=""/>
<attribute name="URL" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="DIELECTRIC" value=""/>
<attribute name="NAME"/>
</element>
<element name="C5" library="MF_Passives" package="C0603" value="1uF / 25V">
<attribute name="MPN" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="VOLTAGE" value=""/>
<attribute name="HOUSEPART" value=""/>
<attribute name="URL" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="DIELECTRIC" value=""/>
<attribute name="NAME"/>
</element>
<element name="C6" library="MF_Passives" package="C0603" value="1uF / 25V">
<attribute name="MPN" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="VOLTAGE" value=""/>
<attribute name="HOUSEPART" value=""/>
<attribute name="URL" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="DIELECTRIC" value=""/>
<attribute name="NAME"/>
</element>
<element name="C7" library="MF_Passives" package="C0603" value="4.7uF / 25V">
<attribute name="MPN" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="VOLTAGE" value=""/>
<attribute name="HOUSEPART" value=""/>
<attribute name="URL" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="DIELECTRIC" value=""/>
<attribute name="NAME"/>
</element>
<element name="C8" library="MF_Passives" package="C0603" value="4.7uF / 25V">
<attribute name="MPN" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="VOLTAGE" value=""/>
<attribute name="HOUSEPART" value=""/>
<attribute name="URL" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="DIELECTRIC" value=""/>
<attribute name="NAME"/>
</element>
<element name="C9" library="MF_Passives" package="C0603" value="4.7uF / 25V">
<attribute name="MPN" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="VOLTAGE" value=""/>
<attribute name="HOUSEPART" value=""/>
<attribute name="URL" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="DIELECTRIC" value=""/>
<attribute name="NAME"/>
</element>
<element name="D1" library="MF_Discrete_Semiconductor" package="SOD-123" value="MBR0530">
<attribute name="MPN" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="HOUSEPART" value="NO"/>
<attribute name="URL" value=""/>
<attribute name="NAME"/>
</element>
<element name="D2" library="MF_Discrete_Semiconductor" package="SOD-123" value="MBR0530">
<attribute name="MPN" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="HOUSEPART" value="NO"/>
<attribute name="URL" value=""/>
<attribute name="NAME"/>
</element>
<element name="D3" library="MF_Discrete_Semiconductor" package="SOD-123" value="MBR0530">
<attribute name="MPN" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="HOUSEPART" value="NO"/>
<attribute name="URL" value=""/>
<attribute name="NAME"/>
</element>
<element name="L1" library="SparkFun-Passives" package="INDUCTOR-SRP4020" value="IFSC-1515AH-01">
<attribute name="NAME"/>
</element>
<element name="R1" library="MF_Passives" package="R0805" value="0.47Ω / 1%">
<attribute name="MPN" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="VOLTAGE" value=""/>
<attribute name="HOUSEPART" value=""/>
<attribute name="URL" value=""/>
<attribute name="WATTAGE" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="NAME"/>
</element>
<element name="U1" library="MF_Discrete_Semiconductor" package="SOT323" value="DMN3067LW-7">
<attribute name="NAME"/>
</element>
<element name="X1" library="con-hirose" package="XF3M-34" value="FH12-34S-0.5S&quot;">
<attribute name="NAME"/>
</element>
<element name="J1" library="MF_Connectors" package="PTH_2.54MM_01X09" value="MF-CON-2.54mm-01x09">
<attribute name="LABEL01" value="VCC"/>
<attribute name="LABEL02" value="GND"/>
<attribute name="MPN" value="MF-CON-2.54mm-01x09"/>
<attribute name="POPULATE" value="1"/>
<attribute name="HOUSEPART" value="YES"/>
<attribute name="LABEL04" value="!BUSY"/>
<attribute name="LABEL05" value="!RST"/>
<attribute name="LABEL06" value="D/C"/>
<attribute name="LABEL03" value="BS"/>
<attribute name="URL" value="https://factory.macrofab.com/part/MF-CON-2.54mm-01x09"/>
<attribute name="LABEL07" value="CSB"/>
<attribute name="LABEL08" value="SCL"/>
<attribute name="LABEL09" value="SDA"/>
</element>
<element name="C10" library="MF_Passives" package="C0603" value="0.1uF / 25V">
<attribute name="POPULATE" value="1"/>
<attribute name="HOUSEPART" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="URL" value=""/>
<attribute name="MPN" value=""/>
<attribute name="VOLTAGE" value=""/>
<attribute name="DIELECTRIC" value=""/>
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="NC-6">
<contactref element="X1" pad="6"/>
</signal>
<signal name="NC-9">
<contactref element="X1" pad="12"/>
</signal>
<signal name="SCL">
<contactref element="X1" pad="18"/>
<contactref element="J1" pad="P$8"/>
</signal>
<signal name="NC-10">
<contactref element="X1" pad="24"/>
</signal>
<signal name="NC-11">
<contactref element="X1" pad="30"/>
</signal>
<signal name="NC-15">
<contactref element="X1" pad="34"/>
</signal>
<signal name="NC-1">
<contactref element="X1" pad="1"/>
</signal>
<signal name="NC-2">
<contactref element="X1" pad="2"/>
</signal>
<signal name="NC-3">
<contactref element="X1" pad="3"/>
</signal>
<signal name="NC-4">
<contactref element="X1" pad="4"/>
</signal>
<signal name="NC-5">
<contactref element="X1" pad="5"/>
</signal>
<signal name="GDR">
<contactref element="X1" pad="7"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="RESE">
<contactref element="X1" pad="8"/>
<contactref element="R1" pad="P$1"/>
<contactref element="U1" pad="3"/>
</signal>
<signal name="NC-7">
<contactref element="X1" pad="9"/>
</signal>
<signal name="VDHR">
<contactref element="X1" pad="10"/>
<contactref element="C5" pad="P$1"/>
</signal>
<signal name="NC-8">
<contactref element="X1" pad="11"/>
</signal>
<signal name="BS">
<contactref element="X1" pad="13"/>
<contactref element="J1" pad="P$3"/>
</signal>
<signal name="!BUSY">
<contactref element="X1" pad="14"/>
<contactref element="J1" pad="P$4"/>
</signal>
<signal name="!RST">
<contactref element="X1" pad="15"/>
<contactref element="J1" pad="P$5"/>
</signal>
<signal name="D/C">
<contactref element="X1" pad="16"/>
<contactref element="J1" pad="P$6"/>
</signal>
<signal name="CSB">
<contactref element="X1" pad="17"/>
<contactref element="J1" pad="P$7"/>
</signal>
<signal name="SDA">
<contactref element="X1" pad="19"/>
<contactref element="J1" pad="P$9"/>
</signal>
<signal name="VCC">
<contactref element="X1" pad="20"/>
<contactref element="L1" pad="P$1"/>
<contactref element="C4" pad="P$1"/>
<contactref element="J1" pad="P$1"/>
<contactref element="C10" pad="P$1"/>
<contactref element="X1" pad="21"/>
</signal>
<signal name="GND">
<contactref element="X1" pad="22"/>
<contactref element="R1" pad="P$2"/>
<contactref element="C4" pad="P$2"/>
<contactref element="D1" pad="CATHODE"/>
<contactref element="C3" pad="P$2"/>
<contactref element="C2" pad="P$2"/>
<contactref element="C9" pad="P$2"/>
<contactref element="C8" pad="P$2"/>
<contactref element="C7" pad="P$2"/>
<contactref element="C6" pad="P$2"/>
<contactref element="C5" pad="P$2"/>
<contactref element="J1" pad="P$2"/>
<contactref element="C10" pad="P$2"/>
</signal>
<signal name="VDDD">
<contactref element="X1" pad="23"/>
<contactref element="C6" pad="P$1"/>
</signal>
<signal name="VGH">
<contactref element="X1" pad="26"/>
<contactref element="D3" pad="CATHODE"/>
<contactref element="C2" pad="P$1"/>
</signal>
<signal name="VGL">
<contactref element="X1" pad="28"/>
<contactref element="D2" pad="ANODE"/>
<contactref element="C3" pad="P$1"/>
</signal>
<signal name="VCOM">
<contactref element="X1" pad="29"/>
<contactref element="C9" pad="P$1"/>
</signal>
<signal name="NC-12">
<contactref element="X1" pad="31"/>
</signal>
<signal name="NC-13">
<contactref element="X1" pad="32"/>
</signal>
<signal name="NC-14">
<contactref element="X1" pad="33"/>
</signal>
<signal name="N$1">
<contactref element="L1" pad="P$2"/>
<contactref element="C1" pad="P$1"/>
<contactref element="D3" pad="ANODE"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="C1" pad="P$2"/>
<contactref element="D1" pad="ANODE"/>
<contactref element="D2" pad="CATHODE"/>
</signal>
<signal name="VSH">
<contactref element="C7" pad="P$1"/>
<contactref element="X1" pad="25"/>
</signal>
<signal name="VSL">
<contactref element="X1" pad="27"/>
<contactref element="C8" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
