<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="22.86" y1="68.58" x2="25.4" y2="66.04" width="0" layer="20" curve="90"/>
<wire x1="25.4" y1="66.04" x2="67.31" y2="66.04" width="0" layer="20"/>
<wire x1="67.31" y1="66.04" x2="69.85" y2="68.58" width="0" layer="20"/>
<wire x1="69.85" y1="68.58" x2="77.47" y2="68.58" width="0" layer="20"/>
<wire x1="77.47" y1="68.58" x2="80.01" y2="66.04" width="0" layer="20"/>
<wire x1="80.01" y1="66.04" x2="119.38" y2="66.04" width="0" layer="20"/>
<wire x1="119.38" y1="66.04" x2="121.92" y2="68.58" width="0" layer="20" curve="90"/>
<wire x1="121.92" y1="68.58" x2="121.92" y2="111.76" width="0" layer="20"/>
<wire x1="121.92" y1="111.76" x2="119.38" y2="114.3" width="0" layer="20" curve="90"/>
<wire x1="26.67" y1="114.3" x2="25.4" y2="114.3" width="0" layer="20"/>
<wire x1="25.4" y1="114.3" x2="22.86" y2="111.76" width="0" layer="20" curve="90"/>
<wire x1="22.86" y1="111.76" x2="22.86" y2="68.58" width="0" layer="20"/>
<wire x1="22.86" y1="120.015" x2="25.4" y2="117.475" width="0" layer="20" curve="90"/>
<wire x1="25.4" y1="117.475" x2="26.67" y2="117.475" width="0" layer="20"/>
<wire x1="119.38" y1="117.475" x2="121.92" y2="120.015" width="0" layer="20" curve="90"/>
<wire x1="121.92" y1="120.015" x2="121.92" y2="163.195" width="0" layer="20"/>
<wire x1="121.92" y1="163.195" x2="119.38" y2="165.735" width="0" layer="20" curve="90"/>
<wire x1="119.38" y1="165.735" x2="25.4" y2="165.735" width="0" layer="20"/>
<wire x1="25.4" y1="165.735" x2="22.86" y2="163.195" width="0" layer="20" curve="90"/>
<wire x1="22.86" y1="163.195" x2="22.86" y2="120.015" width="0" layer="20"/>
<circle x="31.75" y="132.715" radius="1.767765625" width="0.002540625" layer="20"/>
<circle x="38.1" y="126.365" radius="1.767765625" width="0.002540625" layer="20"/>
<circle x="44.45" y="132.715" radius="1.767765625" width="0.002540625" layer="20"/>
<circle x="38.1" y="139.065" radius="1.767765625" width="0.002540625" layer="20"/>
<circle x="45.72" y="146.685" radius="1.767765625" width="0.002540625" layer="20"/>
<circle x="104.14" y="132.715" radius="1.767765625" width="0.002540625" layer="20"/>
<circle x="114.3" y="137.795" radius="1.767765625" width="0.002540625" layer="20"/>
<wire x1="56.515" y1="125.095" x2="90.805" y2="125.095" width="0" layer="20"/>
<wire x1="90.805" y1="125.095" x2="91.44" y2="125.73" width="0" layer="20" curve="90"/>
<wire x1="91.44" y1="125.73" x2="91.44" y2="150.495" width="0" layer="20"/>
<wire x1="91.44" y1="150.495" x2="90.805" y2="151.13" width="0" layer="20" curve="90"/>
<wire x1="90.805" y1="151.13" x2="56.515" y2="151.13" width="0" layer="20"/>
<wire x1="56.515" y1="151.13" x2="55.88" y2="150.495" width="0" layer="20" curve="90"/>
<wire x1="55.88" y1="150.495" x2="55.88" y2="125.73" width="0" layer="20"/>
<wire x1="55.88" y1="125.73" x2="56.515" y2="125.095" width="0" layer="20" curve="90"/>
<wire x1="26.67" y1="114.3" x2="26.67" y2="117.475" width="0" layer="20"/>
<wire x1="31.75" y1="114.3" x2="31.75" y2="117.475" width="0" layer="20"/>
<hole x="27.305" y="117.1575" drill="0.6"/>
<hole x="28.2575" y="117.1575" drill="0.6"/>
<hole x="29.21" y="117.1575" drill="0.6"/>
<hole x="30.1625" y="117.1575" drill="0.6"/>
<hole x="31.115" y="117.1575" drill="0.6"/>
<hole x="27.305" y="114.6175" drill="0.6"/>
<hole x="28.2575" y="114.6175" drill="0.6"/>
<hole x="29.21" y="114.6175" drill="0.6"/>
<hole x="30.1625" y="114.6175" drill="0.6"/>
<hole x="31.115" y="114.6175" drill="0.6"/>
<wire x1="113.03" y1="114.3" x2="113.03" y2="117.475" width="0" layer="20"/>
<wire x1="118.11" y1="114.3" x2="118.11" y2="117.475" width="0" layer="20"/>
<hole x="113.665" y="117.1575" drill="0.6"/>
<hole x="114.6175" y="117.1575" drill="0.6"/>
<hole x="115.57" y="117.1575" drill="0.6"/>
<hole x="116.5225" y="117.1575" drill="0.6"/>
<hole x="117.475" y="117.1575" drill="0.6"/>
<hole x="113.665" y="114.6175" drill="0.6"/>
<hole x="114.6175" y="114.6175" drill="0.6"/>
<hole x="115.57" y="114.6175" drill="0.6"/>
<hole x="116.5225" y="114.6175" drill="0.6"/>
<hole x="117.475" y="114.6175" drill="0.6"/>
<wire x1="58.42" y1="114.3" x2="58.42" y2="117.475" width="0" layer="20"/>
<wire x1="63.5" y1="114.3" x2="63.5" y2="117.475" width="0" layer="20"/>
<hole x="59.055" y="117.1575" drill="0.6"/>
<hole x="60.0075" y="117.1575" drill="0.6"/>
<hole x="60.96" y="117.1575" drill="0.6"/>
<hole x="61.9125" y="117.1575" drill="0.6"/>
<hole x="62.865" y="117.1575" drill="0.6"/>
<hole x="59.055" y="114.6175" drill="0.6"/>
<hole x="60.0075" y="114.6175" drill="0.6"/>
<hole x="60.96" y="114.6175" drill="0.6"/>
<hole x="61.9125" y="114.6175" drill="0.6"/>
<hole x="62.865" y="114.6175" drill="0.6"/>
<wire x1="83.82" y1="114.3" x2="83.82" y2="117.475" width="0" layer="20"/>
<wire x1="88.9" y1="114.3" x2="88.9" y2="117.475" width="0" layer="20"/>
<hole x="84.455" y="117.1575" drill="0.6"/>
<hole x="85.4075" y="117.1575" drill="0.6"/>
<hole x="86.36" y="117.1575" drill="0.6"/>
<hole x="87.3125" y="117.1575" drill="0.6"/>
<hole x="88.265" y="117.1575" drill="0.6"/>
<hole x="84.455" y="114.6175" drill="0.6"/>
<hole x="85.4075" y="114.6175" drill="0.6"/>
<hole x="86.36" y="114.6175" drill="0.6"/>
<hole x="87.3125" y="114.6175" drill="0.6"/>
<hole x="88.265" y="114.6175" drill="0.6"/>
<wire x1="31.75" y1="117.475" x2="58.42" y2="117.475" width="0" layer="20"/>
<wire x1="31.75" y1="114.3" x2="58.42" y2="114.3" width="0" layer="20"/>
<wire x1="63.5" y1="117.475" x2="83.82" y2="117.475" width="0" layer="20"/>
<wire x1="83.82" y1="114.3" x2="63.5" y2="114.3" width="0" layer="20"/>
<wire x1="88.9" y1="117.475" x2="113.03" y2="117.475" width="0" layer="20"/>
<wire x1="113.03" y1="114.3" x2="88.9" y2="114.3" width="0" layer="20"/>
<wire x1="118.11" y1="117.475" x2="119.38" y2="117.475" width="0" layer="20"/>
<wire x1="119.38" y1="114.3" x2="118.11" y2="114.3" width="0" layer="20"/>
<hole x="107.6325" y="153.9875" drill="0.6"/>
<hole x="105.7275" y="152.0825" drill="0.6"/>
<hole x="109.5375" y="152.0825" drill="0.6"/>
<hole x="107.6325" y="150.1775" drill="0.6"/>
<hole x="108.9025" y="153.3525" drill="0.6"/>
<hole x="106.3625" y="153.3525" drill="0.6"/>
<hole x="106.3625" y="150.8125" drill="0.6"/>
<hole x="108.9025" y="150.8125" drill="0.6"/>
<text>Open Source
Game Console</text>
<text>Open Source
Game Console</text>
<text>A</text>
<text>B</text>
<text>C</text>
<text>Bobricius
Made in Slovakia</text>
<hole x="30.48" y="162.56" drill="3.2"/>
<text>Charge</text>
<text>MicroSD</text>
<text>RXD</text>
<text>TXD</text>
<text>VCC</text>
<text>GND</text>
<text>SDA</text>
<text>SCL</text>
<text>VCC</text>
<text>GND</text>
<text>SPEAKER</text>
<text>A</text>
<text>B</text>
<text>C</text>
<text>On</text>
<text>Off</text>
<text>CR2032</text>
<text>16Mhz</text>
<text>4K7</text>
<text>10K</text>
<text>220R</text>
<text>LM1117</text>
<text>GND</text>
<text>+3V</text>
<text>+</text>
<text>-</text>
<text>+</text>
<text>-</text>
<text>+</text>
<text>-</text>
<text>+</text>
<text>-</text>
<text>MicroSD</text>
<text>1K</text>
<text>1K</text>
<text>1uF</text>
<text>4.7uF</text>
<text>4.7uF</text>
<text>4.7uF</text>
<text>10K</text>
<text>BSS123</text>
<text>+</text>
<text>-</text>
<text>Charge</text>
<text>AtMega328</text>
</plain>
<libraries>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="SMT-8585-BUZZER">
</package>
<package name="CR2032-THRU">
</package>
</packages>
</library>
<library name="transistor-small-signal">
<packages>
<package name="SOT23">
<description>&lt;b&gt;SOT-23&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="OPL5">
<packages>
<package name="9P-SMD-W-RING">
</package>
</packages>
</library>
<library name="microbuilder">
<packages>
<package name="4UCONN_20329_V2">
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt; - 5 Pin</description>
</package>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED 0603&lt;/b&gt;</description>
</package>
<package name="0603-NO">
</package>
<package name="0805-NO">
</package>
<package name="MOUNTINGHOLE_2.0_PLATED">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X02">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="2X03">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="SOT223">
<description>&lt;b&gt;SOT-223&lt;/b&gt;</description>
</package>
<package name="1X04">
</package>
<package name="SJ_2S-NOTRACE">
</package>
</packages>
</library>
<library name="lph-7366">
<description>&lt;b&gt;LPH-7366: PCD8544-based Nokia 5110 monochrome LCD display&lt;/b&gt;
&lt;p&gt;&lt;b&gt;Doublecheck before using!&lt;/b&gt;&lt;/p&gt;</description>
<packages>
<package name="LPH-7366-SLOTS">
</package>
</packages>
</library>
<library name="atmel">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Configurable logic, microcontrollers, nonvolatile memories&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt;CD-ROM : Configurable Logic Microcontroller Nonvolatile Memory
&lt;li&gt;CadSoft download site, www.cadsoft.de or www.cadsoftusa.com , file at90smcu_v400.zip
&lt;li&gt;avr.lbr
&lt;/ul&gt;
&lt;author&gt;Revised by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="rc-master-smd">
<packages>
<package name="C0603">
<description>&lt;b&gt;SMD CHIP CAP&lt;/b&gt; - 0603</description>
</package>
</packages>
</library>
<library name="samd21-temp">
<packages>
<package name="HC49UP">
<description>&lt;b&gt;CRYSTAL&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3-NS">
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find non-functional items- supply symbols, logos, notations, frame blocks, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-M">
</package>
</packages>
</library>
<library name="logo">
<description>&lt;b&gt;Electronic and CadSoft EAGLE logos&lt;/b&gt;&lt;p&gt;</description>
<packages>
<package name="RADIOACTIVE_10.00">
<description>&lt;b&gt;Logo radioactive 10 mm&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="BTN_UP" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="BTN_RIGHT" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="BTN_DOWN" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="BTN_LEFT" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="BTN_A" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="BTN_B" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="BTN_C" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="SWITCH-MOMENTARY-2PTH">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="Q2" library="transistor-small-signal" package="SOT23" value="BSS123"/>
<element name="U$2" library="adafruit" package="SMT-8585-BUZZER" value="BUZZER"/>
<element name="J1" library="OPL5" package="9P-SMD-W-RING" value="MICRO-SDCARD-CONNECTOR-3300060P1"/>
<element name="X6" library="microbuilder" package="4UCONN_20329_V2" value="microUSB"/>
<element name="U2" library="microbuilder" package="SOT23-5" value="MCP73831T-2ACI/OT"/>
<element name="CHG1" library="microbuilder" package="CHIPLED_0603" value="RED"/>
<element name="R7" library="microbuilder" package="0603-NO" value="1K"/>
<element name="C25" library="microbuilder" package="0805-NO" value="10µF"/>
<element name="R8" library="microbuilder" package="0603-NO" value="10K\"/>
<element name="BAT" library="pinhead" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="JP5" library="pinhead" package="2X03" value="">
<attribute name="VALUE"/>
</element>
<element name="C14" library="microbuilder" package="0805-NO" value="10µF"/>
<element name="U$3" library="lph-7366" package="LPH-7366-SLOTS" value="LPH-7366-SLOTS"/>
<element name="IC1" library="atmel" package="TQFP32-08" value="ATMEGA328P">
<attribute name="MPN" value="ATMEGA8-16AU"/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="9171371"/>
<attribute name="OC_NEWARK" value="73M8863"/>
</element>
<element name="I2C4" library="SparkFun" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="UART" library="SparkFun" package="1X04" value="">
<attribute name="VALUE"/>
</element>
<element name="U$4" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$5" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="IC2" library="SparkFun" package="SOT223" value="">
<attribute name="VALUE"/>
</element>
<element name="C3" library="rc-master-smd" package="C0603" value="100nF"/>
<element name="C5" library="rc-master-smd" package="C0603" value="100nF"/>
<element name="U$6" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$7" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$8" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$9" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$1" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$10" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="C1" library="rc-master-smd" package="C0603" value="1Uf"/>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="U$11" library="adafruit" package="CR2032-THRU" value="">
<attribute name="VALUE"/>
</element>
<element name="C2" library="rc-master-smd" package="C0603" value="15pF"/>
<element name="C7" library="rc-master-smd" package="C0603" value="15pF"/>
<element name="Y2" library="samd21-temp" package="HC49UP" value="16MHz"/>
<element name="LED2" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="JUMPER2" library="SparkFun" package="SJ_2S-NOTRACE" value="SOLDERJUMPERNC2"/>
<element name="LED1" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED3" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="LED4" library="led" package="CHIPLED_0603" value="">
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0603-RES" value="220">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0603-RES" value="220">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0603-RES" value="220">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0603-RES" value="220">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="2X3-NS" value="">
<attribute name="VALUE"/>
</element>
<element name="R10" library="rcl" package="R0603" value="1k"/>
<element name="U$12" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$13" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$14" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$15" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$16" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$17" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$18" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$19" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="SPEAKER" library="pinhead" package="1X02" value="">
<attribute name="VALUE"/>
</element>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-M" value="OSHW-LOGOM"/>
<element name="C4" library="rc-master-smd" package="C0603" value="15pF"/>
<element name="U$21" library="logo" package="RADIOACTIVE_10.00" value=""/>
</elements>
<signals>
<signal name="BTN_C">
<contactref element="BTN_C" pad="3"/>
<contactref element="IC1" pad="26"/>
</signal>
<signal name="BTN_B">
<contactref element="BTN_B" pad="3"/>
<contactref element="IC1" pad="32"/>
</signal>
<signal name="BTN_A">
<contactref element="BTN_A" pad="3"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="BACKLIGHT">
<contactref element="IC1" pad="9"/>
<contactref element="LED2" pad="A"/>
<contactref element="LED1" pad="A"/>
<contactref element="LED3" pad="A"/>
<contactref element="LED4" pad="A"/>
</signal>
<signal name="BTN_RIGHT">
<contactref element="BTN_RIGHT" pad="3"/>
<contactref element="IC1" pad="11"/>
</signal>
<signal name="BTN_LEFT">
<contactref element="BTN_LEFT" pad="3"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="BTN_UP">
<contactref element="BTN_UP" pad="3"/>
<contactref element="IC1" pad="13"/>
</signal>
<signal name="MOSI">
<contactref element="IC1" pad="15"/>
<contactref element="J1" pad="3"/>
<contactref element="U$3" pad="3"/>
<contactref element="JP4" pad="4"/>
</signal>
<signal name="MISO">
<contactref element="IC1" pad="16"/>
<contactref element="J1" pad="7"/>
<contactref element="JP4" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="4"/>
<contactref element="IC1" pad="6"/>
<contactref element="IC1" pad="18"/>
<contactref element="J1" pad="4"/>
<contactref element="U$2" pad="+"/>
<contactref element="IC2" pad="2"/>
<contactref element="IC2" pad="4"/>
<contactref element="C3" pad="1"/>
<contactref element="I2C4" pad="1"/>
<contactref element="UART" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="U$3" pad="1"/>
<contactref element="U$3" pad="6"/>
<contactref element="R2" pad="1"/>
<contactref element="R10" pad="1"/>
<contactref element="JP4" pad="2"/>
<contactref element="JUMPER2" pad="1"/>
<contactref element="SPEAKER" pad="1"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="LCD_RST">
<contactref element="IC1" pad="23"/>
<contactref element="U$3" pad="9"/>
</signal>
<signal name="LCD_CE">
<contactref element="IC1" pad="24"/>
<contactref element="U$3" pad="5"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="LCD_DC">
<contactref element="IC1" pad="25"/>
<contactref element="U$3" pad="4"/>
</signal>
<signal name="RXD">
<contactref element="IC1" pad="30"/>
<contactref element="UART" pad="3"/>
</signal>
<signal name="TXD">
<contactref element="IC1" pad="31"/>
<contactref element="UART" pad="4"/>
</signal>
<signal name="SOUND">
<contactref element="Q2" pad="1"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="BTN_DOWN">
<contactref element="BTN_DOWN" pad="3"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="SD_CS">
<contactref element="IC1" pad="14"/>
<contactref element="J1" pad="2"/>
</signal>
<signal name="RESET">
<contactref element="IC1" pad="29"/>
<contactref element="JP4" pad="5"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="GND">
<contactref element="BTN_UP" pad="1"/>
<contactref element="BTN_RIGHT" pad="1"/>
<contactref element="BTN_DOWN" pad="1"/>
<contactref element="BTN_LEFT" pad="1"/>
<contactref element="BTN_A" pad="1"/>
<contactref element="BTN_B" pad="1"/>
<contactref element="BTN_C" pad="1"/>
<contactref element="Q2" pad="2"/>
<contactref element="J1" pad="6"/>
<contactref element="X6" pad="SPRT@4"/>
<contactref element="X6" pad="BASE@2"/>
<contactref element="X6" pad="BASE@1"/>
<contactref element="X6" pad="SPRT@2"/>
<contactref element="X6" pad="SPRT@1"/>
<contactref element="X6" pad="SPRT@3"/>
<contactref element="X6" pad="GND"/>
<contactref element="C25" pad="2"/>
<contactref element="R8" pad="2"/>
<contactref element="U2" pad="2"/>
<contactref element="C14" pad="2"/>
<contactref element="BAT" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="IC1" pad="5"/>
<contactref element="IC1" pad="21"/>
<contactref element="I2C4" pad="2"/>
<contactref element="UART" pad="1"/>
<contactref element="IC2" pad="1"/>
<contactref element="C5" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="U$3" pad="7"/>
<contactref element="C1" pad="1"/>
<contactref element="U$11" pad="-"/>
<contactref element="C2" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="JP4" pad="6"/>
<contactref element="C4" pad="2"/>
</signal>
<signal name="N$13">
</signal>
<signal name="N$18">
</signal>
<signal name="N$21">
</signal>
<signal name="N$14">
</signal>
<signal name="N$15">
</signal>
<signal name="N$16">
</signal>
<signal name="N$17">
</signal>
<signal name="N$19">
</signal>
<signal name="N$20">
</signal>
<signal name="N$22">
</signal>
<signal name="OUT">
<contactref element="Q2" pad="3"/>
<contactref element="U$2" pad="-"/>
<contactref element="SPEAKER" pad="2"/>
</signal>
<signal name="SCK">
<contactref element="J1" pad="5"/>
<contactref element="IC1" pad="17"/>
<contactref element="U$3" pad="2"/>
<contactref element="JP4" pad="3"/>
</signal>
<signal name="VBUS">
<contactref element="X6" pad="VBUS"/>
<contactref element="U2" pad="4"/>
<contactref element="CHG1" pad="A"/>
<contactref element="C14" pad="1"/>
</signal>
<signal name="VBAT">
<contactref element="JP5" pad="4"/>
<contactref element="JP5" pad="3"/>
<contactref element="JP5" pad="1"/>
<contactref element="JP5" pad="2"/>
<contactref element="IC2" pad="3"/>
<contactref element="C5" pad="1"/>
<contactref element="JUMPER2" pad="2"/>
</signal>
<signal name="N$27">
<contactref element="CHG1" pad="C"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="CHSTAT">
<contactref element="R7" pad="2"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="N$29">
<contactref element="U2" pad="5"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="VBAT1">
<contactref element="U2" pad="3"/>
<contactref element="C25" pad="1"/>
<contactref element="BAT" pad="2"/>
<contactref element="JP5" pad="6"/>
<contactref element="JP5" pad="5"/>
<contactref element="U$11" pad="+2"/>
<contactref element="U$11" pad="+1"/>
</signal>
<signal name="PB6">
<contactref element="IC1" pad="7"/>
<contactref element="C2" pad="1"/>
<contactref element="Y2" pad="1"/>
</signal>
<signal name="PB7">
<contactref element="IC1" pad="8"/>
<contactref element="C7" pad="1"/>
<contactref element="Y2" pad="2"/>
</signal>
<signal name="AREF">
<contactref element="IC1" pad="20"/>
</signal>
<signal name="ADC7">
<contactref element="IC1" pad="22"/>
</signal>
<signal name="ADC6">
<contactref element="IC1" pad="19"/>
</signal>
<signal name="SDA">
<contactref element="IC1" pad="27"/>
<contactref element="I2C4" pad="4"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="SCL">
<contactref element="IC1" pad="28"/>
<contactref element="I2C4" pad="3"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="U$3" pad="8"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="LED2" pad="C"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$2">
<contactref element="LED1" pad="C"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$3">
<contactref element="LED3" pad="C"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="LED4" pad="C"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$5">
</signal>
<signal name="N$8">
</signal>
<signal name="N$12">
</signal>
<signal name="N$23">
</signal>
<signal name="N$24">
</signal>
<signal name="N$25">
</signal>
<signal name="N$28">
</signal>
<signal name="N$31">
</signal>
<signal name="N$32">
</signal>
</signals>
</board>
</drawing>
</eagle>
