<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.1.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="26.5" y2="0" width="0" layer="20"/>
<wire x1="26.5" y1="0" x2="26.5" y2="58" width="0" layer="20"/>
<wire x1="26.5" y1="58" x2="0" y2="58" width="0" layer="20"/>
<wire x1="0" y1="58" x2="0" y2="0" width="0" layer="20"/>
<text>GND</text>
<text>MSCK</text>
<text>MOSI</text>
<text>VSUP</text>
</plain>
<libraries>
<library name="Dust">
<packages>
<package name="LTP5901">
<description>SmartMesh LTP5901 Module</description>
</package>
<package name="4MMX1MMX4SMD">
<description>Four metric (4mm x 1mm) @ 2mm pitch, SMD Pads.</description>
</package>
<package name="8S2">
<description>&lt;b&gt;8S2&lt;/b&gt; 8-lead, 0.208 Body&lt;p&gt;
Plastic Small Outline Package (EIAJ)&lt;br&gt;
Source: http://www.atmel.com/dyn/resources/prod_documents/2535S.pdf</description>
</package>
</packages>
</library>
<library name="nxp_60">
<description>&lt;H1&gt;NXP Library&lt;/H1&gt;
&lt;author&gt;marco.kuystermans@nxp.com&lt;/author&gt;&lt;p&gt;

&lt;H2&gt;Disclaimer:&lt;/H2&gt;
&lt;i&gt;The information contained in this library is made available for general information and public access only. By using our 
library, you accept this disclaimer in full. If you disagree with any part of this disclaimer, you must not use our library.
Use of this library is permitted on the basis that NXP will not be liable for any loss or damage including without limitation, indirect or consequential loss or 
damage, arising out of or in connection with the use of this library.&lt;/i&gt;

&lt;H2&gt;Information:&lt;/H2&gt;
&lt;ul&gt;&lt;li&gt;Footprints are according to NXP footprint information, see &lt;a href=http://www.nxp.com&gt;NXP website&lt;/a&gt;
&lt;li&gt;SMD Footprints in this library are for reflow soldering only.
&lt;li&gt;&lt;b&gt;Library is generated as a courtesy: Information is NOT guaranteed, use at your own risk&lt;/b&gt;
&lt;li&gt;NXP package numbers (SOT/SOD) numbers used
&lt;/ul&gt;
Please send your comments to the mail address above.</description>
<packages>
<package name="SOT457">
<description>&lt;li&gt;&lt;b&gt;SOT457&lt;/b&gt;&lt;hr&gt;
&lt;ul&gt;&lt;li&gt;TSOP6: Plastic surface-mounted package; 6 lead
&lt;li&gt;&lt;u&gt;JEIDA&lt;/u&gt;: SC73
&lt;p&gt;A.K.A. SOT23-6</description>
</package>
</packages>
</library>
<library name="maxim">
<description>&lt;b&gt;Maxim Components&lt;/b&gt;&lt;p&gt;

&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT23">
<description>&lt;b&gt;SMALL OUTLINE TRANSISTOR&lt;/b&gt;&lt;p&gt;
reflow soldering</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="Dust" package="LTP5901" value="LTP5901MODULE"/>
<element name="U10" library="Dust" package="4MMX1MMX4SMD" value="4MMX1MMX4SMDPADS"/>
<element name="U2" library="Dust" package="4MMX1MMX4SMD" value="4MMX1MMX4SMDPADS"/>
<element name="U3" library="Dust" package="4MMX1MMX4SMD" value="4MMX1MMX4SMDPADS"/>
<element name="U4" library="Dust" package="4MMX1MMX4SMD" value="4MMX1MMX4SMDPADS"/>
<element name="U5" library="Dust" package="4MMX1MMX4SMD" value="4MMX1MMX4SMDPADS"/>
<element name="U6" library="Dust" package="4MMX1MMX4SMD" value="4MMX1MMX4SMDPADS"/>
<element name="U7" library="Dust" package="4MMX1MMX4SMD" value="4MMX1MMX4SMDPADS"/>
<element name="U8" library="Dust" package="4MMX1MMX4SMD" value="4MMX1MMX4SMDPADS"/>
<element name="U9" library="Dust" package="4MMX1MMX4SMD" value="4MMX1MMX4SMDPADS"/>
<element name="U11" library="nxp_60" package="SOT457" value="2X1MUX"/>
<element name="U12" library="Dust" package="8S2" value="SERIALFLASH"/>
<element name="IC1" library="maxim" package="SOT23" value="MAX6520">
<attribute name="MF" value="MAXIM"/>
<attribute name="MPN" value="MAX6520EUR-T"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="02J4586"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603" value="22">
<attribute name="PROD_ID" value="RES-08698"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603" value="22">
<attribute name="PROD_ID" value="RES-08698"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="GND2"/>
<contactref element="U1" pad="GND3"/>
<contactref element="U1" pad="GND7"/>
<contactref element="U1" pad="GND8"/>
<contactref element="U1" pad="GND9"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="GND6"/>
<contactref element="U2" pad="PAD4"/>
<contactref element="U1" pad="GND4"/>
<contactref element="U1" pad="GND5"/>
<contactref element="U11" pad="2"/>
<contactref element="U12" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="U2" pad="PAD3"/>
<contactref element="U1" pad="SPIM_MOSI"/>
<contactref element="U12" pad="5"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="SPIM_SCK"/>
<contactref element="U11" pad="3"/>
<contactref element="U12" pad="6"/>
</signal>
<signal name="N$4">
<contactref element="U2" pad="PAD1"/>
<contactref element="U1" pad="VSUPPLY"/>
<contactref element="U11" pad="5"/>
<contactref element="U11" pad="1"/>
<contactref element="U12" pad="8"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="U1" pad="SPIM_MISO"/>
<contactref element="U3" pad="PAD4"/>
<contactref element="U12" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="U3" pad="PAD3"/>
<contactref element="U1" pad="SPIM_SS_1N"/>
<contactref element="U12" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="U3" pad="PAD2"/>
<contactref element="U1" pad="SPIM_SS_0N"/>
<contactref element="U11" pad="6"/>
</signal>
<signal name="N$8">
<contactref element="U3" pad="PAD1"/>
<contactref element="U1" pad="DP1"/>
</signal>
<signal name="N$9">
<contactref element="U4" pad="PAD4"/>
<contactref element="U1" pad="PMW0"/>
</signal>
<signal name="N$10">
<contactref element="U4" pad="PAD3"/>
<contactref element="U1" pad="1_WIRE"/>
</signal>
<signal name="N$11">
<contactref element="U4" pad="PAD2"/>
<contactref element="U1" pad="GPIO26"/>
</signal>
<signal name="N$12">
<contactref element="U1" pad="UART_RX_RTSN"/>
<contactref element="U5" pad="PAD4"/>
</signal>
<signal name="N$13">
<contactref element="U1" pad="UART_RX_CSTN"/>
<contactref element="U5" pad="PAD3"/>
</signal>
<signal name="N$14">
<contactref element="U5" pad="PAD2"/>
</signal>
<signal name="N$15">
<contactref element="U1" pad="UART_TX_RTSN"/>
<contactref element="U5" pad="PAD1"/>
</signal>
<signal name="N$16">
<contactref element="U1" pad="UART_TX_CTSN"/>
<contactref element="U6" pad="PAD4"/>
</signal>
<signal name="N$17">
<contactref element="U1" pad="UART_TX"/>
<contactref element="U6" pad="PAD3"/>
</signal>
<signal name="N$18">
<contactref element="U1" pad="TIMEN"/>
<contactref element="U6" pad="PAD2"/>
</signal>
<signal name="N$19">
<contactref element="U1" pad="RADIO_INHIBIT"/>
<contactref element="U6" pad="PAD1"/>
</signal>
<signal name="N$21">
<contactref element="U1" pad="SDA"/>
<contactref element="U7" pad="PAD1"/>
</signal>
<signal name="N$22">
<contactref element="U1" pad="SCL"/>
<contactref element="U7" pad="PAD2"/>
</signal>
<signal name="N$20">
<contactref element="U1" pad="GND"/>
<contactref element="U8" pad="PAD1"/>
</signal>
<signal name="N$25">
<contactref element="U1" pad="GPIO17"/>
<contactref element="U8" pad="PAD4"/>
</signal>
<signal name="N$26">
<contactref element="U1" pad="GPIO18"/>
<contactref element="U8" pad="PAD3"/>
</signal>
<signal name="N$27">
<contactref element="U1" pad="GPIO19"/>
<contactref element="U8" pad="PAD2"/>
</signal>
<signal name="N$28">
<contactref element="U9" pad="PAD4"/>
<contactref element="U1" pad="AI_2"/>
</signal>
<signal name="N$29">
<contactref element="U1" pad="AI_1"/>
<contactref element="U9" pad="PAD3"/>
</signal>
<signal name="N$30">
<contactref element="U9" pad="PAD2"/>
<contactref element="U1" pad="AI_3"/>
</signal>
<signal name="N$31">
<contactref element="U9" pad="PAD1"/>
<contactref element="U1" pad="AI_0"/>
</signal>
<signal name="N$32">
<contactref element="U1" pad="DP4"/>
<contactref element="U10" pad="PAD4"/>
</signal>
<signal name="N$33">
<contactref element="U1" pad="DP3"/>
<contactref element="U10" pad="PAD3"/>
</signal>
<signal name="N$34">
<contactref element="U1" pad="DP2"/>
<contactref element="U10" pad="PAD2"/>
</signal>
<signal name="N$35">
<contactref element="U1" pad="DP0"/>
<contactref element="U10" pad="PAD1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="N$36">
<contactref element="U2" pad="PAD2"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$37">
<contactref element="U11" pad="4"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$39">
<contactref element="IC1" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$23">
<contactref element="IC1" pad="3"/>
<contactref element="U7" pad="PAD4"/>
</signal>
</signals>
</board>
</drawing>
</eagle>

