<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="3" x2="3" y2="0" width="0" layer="20" curve="90"/>
<wire x1="3" y1="0" x2="43" y2="0" width="0" layer="20"/>
<wire x1="47" y1="0" x2="62" y2="0" width="0" layer="20"/>
<wire x1="62" y1="0" x2="65" y2="3" width="0" layer="20" curve="90"/>
<wire x1="65" y1="3" x2="65" y2="53" width="0" layer="20"/>
<wire x1="65" y1="53" x2="62" y2="56" width="0" layer="20" curve="90"/>
<wire x1="62" y1="56" x2="3" y2="56" width="0" layer="20"/>
<wire x1="3" y1="56" x2="0" y2="53" width="0" layer="20" curve="90"/>
<hole x="3.5" y="3.5" drill="2.8"/>
<hole x="3.5" y="52.5" drill="2.8"/>
<hole x="61.5" y="52.5" drill="2.8"/>
<hole x="61.5" y="3.5" drill="2.8"/>
<wire x1="44" y1="19" x2="44" y2="1" width="0" layer="20"/>
<wire x1="46" y1="19" x2="46" y2="1" width="0" layer="20"/>
<wire x1="45" y1="20" x2="46" y2="19" width="0" layer="20" curve="-90"/>
<wire x1="45" y1="20" x2="44" y2="19" width="0" layer="20" curve="90"/>
<wire x1="44" y1="1" x2="43" y2="0" width="0" layer="20" curve="-90"/>
<wire x1="46" y1="1" x2="47" y2="0" width="0" layer="20" curve="90"/>
<text>HealthyPi</text>
<text>ECG</text>
<text>SpO2 Probe</text>
<text>BP/GLUCO</text>
<text>JTAG</text>
<text>protocentral.com</text>
<text>TEMPERATURE</text>
<text>v3</text>
<text>WARNING: When connected to body,
power only through an isolated source 
or battery</text>
<text>HealthyPi</text>
<text>v3</text>
<wire x1="0" y1="3" x2="0" y2="53" width="0" layer="20"/>
<text>WP</text>
<text>RST</text>
<text>Get Started: http://proty.in/hpi</text>
</plain>
<libraries>
<library name="FLYFISH">
<packages>
<package name="PIN_20X2">
</package>
<package name="SOIC8">
</package>
</packages>
</library>
<library name="resistor">
<packages>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
<package name="C0603">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="circuitects">
<packages>
<package name="SQFP-S-5X5-32">
<description>&lt;b&gt;QFP32&lt;/b&gt;&lt;p&gt;
shrink quad flat pack, square</description>
</package>
<package name="PROTY_WITH_TEXT">
</package>
<package name="QFN-40">
</package>
<package name="LPS">
</package>
<package name="HDR-SMT-50MIL/5X2">
</package>
<package name="MICRO-B">
</package>
<package name="SOT26">
</package>
<package name="HEALTHYPI">
</package>
<package name="DB9-STRIGHT">
</package>
<package name="ABM3">
</package>
<package name="ECX-31B">
</package>
</packages>
</library>
<library name="rcl">
<packages>
<package name="C0402">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;</description>
</package>
<package name="R0402">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;</description>
</package>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="R0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;</description>
</package>
<package name="L1812">
<description>&lt;b&gt;INDUCTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="testpad">
<packages>
<package name="B1,27">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun">
<packages>
<package name="PAD.03X.03">
</package>
<package name="OSHW-LOGO-M">
</package>
</packages>
</library>
<library name="led">
<packages>
<package name="CHIPLED_0603">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY Q971.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="AUDIO-JACK-3.5MM-SMD">
</package>
</packages>
</library>
<library name="zetex">
<description>&lt;b&gt;Zetex Power MOS FETs, Bridges, Diodes&lt;/b&gt;&lt;p&gt;
http://www.zetex.com&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOT323">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="Arduino">
<description>Official Arduino component library &lt;p&gt;&lt;b&gt;www.arduino.cc&lt;b&gt;</description>
<packages>
<package name="TQFP48">
</package>
<package name="C0805">
</package>
<package name="C0603">
</package>
<package name="C0402">
</package>
</packages>
</library>
<library name="con-lstb">
<description>&lt;b&gt;Pin Headers&lt;/b&gt;&lt;p&gt;
Naming:&lt;p&gt;
MA = male&lt;p&gt;
# contacts - # rows&lt;p&gt;
W = angled&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="MA04-1">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="microbuilder">
<packages>
<package name="SOT23-R">
<description>&lt;b&gt;SOT23&lt;/b&gt; - Reflow soldering</description>
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="OSHWA">
<packages>
<package name="CERT-SMALL-SILK">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="K1" library="FLYFISH" package="PIN_20X2" value="PIN20X2">
<attribute name="VALUE"/>
</element>
<element name="U1" library="FLYFISH" package="SOIC8" value="EEPROM24(CAT24C32WI-GT3)">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="resistor" package="M0805" value="3k9">
<attribute name="TOLERANCE" value="5%"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="resistor" package="C0805K" value="100nF">
<attribute name="DIELECTRIC" value="X7R"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="resistor" package="M0805" value="3k9">
<attribute name="TOLERANCE" value="5%"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="resistor" package="M0805" value="1k">
<attribute name="TOLERANCE" value="5%"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$8" library="circuitects" package="SQFP-S-5X5-32" value="ADS1292RIPBSR">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C48" library="rcl" package="C0402" value="1u, NP0/C0G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C49" library="rcl" package="C0402" value="1u, NP0/C0G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C50" library="rcl" package="C0402" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C51" library="resistor" package="C0603" value="10u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C52" library="rcl" package="C0402" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C53" library="rcl" package="C0402" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C54" library="rcl" package="C0402" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C55" library="rcl" package="C0402" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C56" library="rcl" package="C0402" value="47n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C57" library="rcl" package="C0402" value="47n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R20" library="rcl" package="R0402" value="51K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C58" library="rcl" package="C0402" value="47p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R22" library="rcl" package="R0402" value="51K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R24" library="rcl" package="R0402" value="100k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C62" library="rcl" package="C0402" value="47p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="rcl" package="R0402" value="40.2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C22" library="rcl" package="C0402" value="2.2n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C23" library="rcl" package="C0402" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C25" library="rcl" package="C0402" value="2.2n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R10" library="rcl" package="R0402" value="40.2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C31" library="rcl" package="C0402" value="2.2n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C38" library="rcl" package="C0402" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C40" library="rcl" package="C0402" value="2.2n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R12" library="rcl" package="R0402" value="10M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R15" library="rcl" package="R0402" value="10M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R16" library="rcl" package="R0402" value="10M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R18" library="rcl" package="R0402" value="10M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R19" library="rcl" package="R0402" value="1M">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="rcl" package="R0402" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C35" library="rcl" package="C0402" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C37" library="rcl" package="C0402" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="rcl" package="C0402" value="47p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R30" library="rcl" package="R0402" value="330R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="POWER" library="led" package="CHIPLED_0603" value="Red">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP3" library="SparkFun-Connectors" package="AUDIO-JACK-3.5MM-SMD" value="35RASMT4BHNTRX">
<attribute name="PROD_ID" value="CONN-10353"/>
</element>
<element name="U$3" library="circuitects" package="QFN-40" value="AFE4490RHAT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="rcl" package="C0402" value="22p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="rcl" package="C0402" value="22p">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="circuitects" package="DB9-STRIGHT" value="1734354-1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="rcl" package="C0402" value="2.2u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="rcl" package="C0402" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="rcl" package="C0805" value="1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="rcl" package="C0402" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="rcl" package="C0402" value="0.1u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D5" library="zetex" package="SOT323" value="BAV99W-7-F">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="zetex" package="SOT323" value="BAV99W-7-F">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="zetex" package="SOT323" value="BAV99W-7-F">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="zetex" package="SOT323" value="BAV99W-7-F">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="rcl" package="C0402" value="2.2u">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$7" library="circuitects" package="LPS" value="CIG22L100MNE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$9" library="circuitects" package="LPS" value="CIG22L100MNE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$10" library="circuitects" package="LPS" value="CIG22L100MNE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$11" library="circuitects" package="LPS" value="CIG22L100MNE">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C18" library="rcl" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C19" library="rcl" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C27" library="rcl" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C28" library="rcl" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R47" library="rcl" package="R0402" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP4" library="SparkFun" package="PAD.03X.03" value="TEST-POINT3"/>
<element name="IC2" library="Arduino" package="TQFP48" value="SAMD21G18A-AUT">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C102" library="Arduino" package="C0805" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C100" library="Arduino" package="C0805" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C106" library="Arduino" package="C0805" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C105" library="Arduino" package="C0805" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C108" library="Arduino" package="C0805" value="100nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C107" library="Arduino" package="C0805" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L100" library="Arduino" package="C0603" value="BLM18PG471SN1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="CON_JTAG1" library="circuitects" package="HDR-SMT-50MIL/5X2" value="HDR-SMT-50MIL/5X2(20021121-00010C4LF)"/>
<element name="C77" library="rcl" package="C0805" value="100n">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R9" library="rcl" package="R0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="rcl" package="C0402" value="100nf">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP5" library="circuitects" package="MICRO-B" value="MICRO-B">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R11" library="rcl" package="R0805" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP10" library="testpad" package="B1,27" value="TPSQB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="rcl" package="R0402" value="0R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R14" library="rcl" package="R0402" value="0R">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SV1" library="con-lstb" package="MA04-1" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="SV2" library="con-lstb" package="MA04-1" value="">
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="MPN" value=""/>
<attribute name="MF" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="L1" library="rcl" package="L1812" value="MF-MSMF050-2">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q1" library="microbuilder" package="SOT23-R" value="SI2323DS-TI-GE3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="circuitects" package="SOT26" value="DMMT5401">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R37" library="rcl" package="R0805" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R48" library="rcl" package="R0805" value="47K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP3" library="testpad" package="B1,27" value="TPSQB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP13" library="testpad" package="B1,27" value="TPSQB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$15" library="circuitects" package="HEALTHYPI" value="HEALTHYPI"/>
<element name="U$4" library="circuitects" package="ABM3" value="ABM3">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U3" library="SparkFun-PowerIC" package="SOT23-5" value="AP2112K-3.3V">
<attribute name="PROD_ID" value="VREG-12457"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="Arduino" package="C0402" value="12pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="Arduino" package="C0402" value="12pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$19" library="circuitects" package="ECX-31B" value="520-327-12.5-34B(32.768KHZ)"/>
<element name="U$5" library="SparkFun" package="OSHW-LOGO-M" value="OSHW-LOGOM"/>
<element name="U$13" library="OSHWA" package="CERT-SMALL-SILK" value=""/>
<element name="U$6" library="circuitects" package="PROTY_WITH_TEXT" value="PROTY_LOGO_WITH_TEXT"/>
<element name="U$2" library="circuitects" package="PROTY_WITH_TEXT" value="PROTY_LOGO_WITH_TEXT"/>
<element name="R5" library="rcl" package="R0402" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="rcl" package="R0402" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP2" library="testpad" package="B1,27" value="TPSQB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TP1" library="testpad" package="B1,27" value="TPSQB1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="S$28">
</signal>
<signal name="S$33">
</signal>
<signal name="S$39">
</signal>
<signal name="S$40">
</signal>
<signal name="S$60">
</signal>
<signal name="S$61">
</signal>
<signal name="S$213">
</signal>
<signal name="S$234">
</signal>
<signal name="GND">
<contactref element="U1" pad="4"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="1"/>
<contactref element="U1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="K1" pad="9"/>
<contactref element="K1" pad="25"/>
<contactref element="K1" pad="39"/>
<contactref element="K1" pad="6"/>
<contactref element="K1" pad="14"/>
<contactref element="K1" pad="20"/>
<contactref element="K1" pad="30"/>
<contactref element="K1" pad="34"/>
<contactref element="C48" pad="1"/>
<contactref element="C49" pad="1"/>
<contactref element="U$8" pad="24"/>
<contactref element="U$8" pad="13"/>
<contactref element="C52" pad="1"/>
<contactref element="C53" pad="1"/>
<contactref element="C54" pad="1"/>
<contactref element="C55" pad="1"/>
<contactref element="C50" pad="1"/>
<contactref element="C51" pad="2"/>
<contactref element="U$8" pad="10"/>
<contactref element="R15" pad="1"/>
<contactref element="R18" pad="1"/>
<contactref element="C58" pad="1"/>
<contactref element="C35" pad="1"/>
<contactref element="C37" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="R30" pad="1"/>
<contactref element="U$3" pad="19"/>
<contactref element="U$3" pad="32"/>
<contactref element="U$3" pad="36"/>
<contactref element="U$3" pad="40"/>
<contactref element="U$3" pad="8"/>
<contactref element="U$3" pad="3"/>
<contactref element="U$3" pad="12"/>
<contactref element="U$3" pad="13"/>
<contactref element="U$3" pad="16"/>
<contactref element="C6" pad="1"/>
<contactref element="C7" pad="1"/>
<contactref element="X1" pad="7"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="U$3" pad="EXP@10"/>
<contactref element="U$3" pad="EXP@11"/>
<contactref element="U$3" pad="EXP@6"/>
<contactref element="U$3" pad="EXP@7"/>
<contactref element="C19" pad="2"/>
<contactref element="C18" pad="2"/>
<contactref element="C28" pad="2"/>
<contactref element="C27" pad="2"/>
<contactref element="X1" pad="G1"/>
<contactref element="X1" pad="G2"/>
<contactref element="IC2" pad="18"/>
<contactref element="IC2" pad="35"/>
<contactref element="C105" pad="2"/>
<contactref element="IC2" pad="42"/>
<contactref element="C102" pad="2"/>
<contactref element="C100" pad="2"/>
<contactref element="C106" pad="2"/>
<contactref element="IC2" pad="5"/>
<contactref element="C108" pad="1"/>
<contactref element="C107" pad="2"/>
<contactref element="CON_JTAG1" pad="3"/>
<contactref element="CON_JTAG1" pad="5"/>
<contactref element="CON_JTAG1" pad="9"/>
<contactref element="C77" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="JP5" pad="5"/>
<contactref element="JP5" pad="4"/>
<contactref element="JP5" pad="P$6"/>
<contactref element="JP5" pad="P$5"/>
<contactref element="SV1" pad="4"/>
<contactref element="SV2" pad="4"/>
<contactref element="R37" pad="1"/>
<contactref element="R48" pad="1"/>
<contactref element="D3" pad="2"/>
<contactref element="D5" pad="2"/>
<contactref element="D1" pad="2"/>
<contactref element="D2" pad="2"/>
<contactref element="U3" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="C15" pad="1"/>
</signal>
<signal name="+3V3">
<contactref element="U1" pad="8"/>
<contactref element="R3" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="C54" pad="2"/>
<contactref element="C55" pad="2"/>
<contactref element="R16" pad="1"/>
<contactref element="R12" pad="1"/>
<contactref element="U$8" pad="23"/>
<contactref element="C35" pad="2"/>
<contactref element="POWER" pad="A"/>
<contactref element="IC2" pad="36"/>
<contactref element="C105" pad="1"/>
<contactref element="IC2" pad="44"/>
<contactref element="C100" pad="1"/>
<contactref element="L100" pad="2"/>
<contactref element="IC2" pad="17"/>
<contactref element="C108" pad="2"/>
<contactref element="CON_JTAG1" pad="1"/>
<contactref element="C77" pad="1"/>
<contactref element="R9" pad="1"/>
<contactref element="R11" pad="2"/>
<contactref element="U$8" pad="14"/>
<contactref element="TP13" pad="TP"/>
<contactref element="U3" pad="5"/>
<contactref element="U$10" pad="1"/>
<contactref element="U$11" pad="1"/>
<contactref element="U$9" pad="1"/>
<contactref element="U$7" pad="1"/>
<contactref element="C52" pad="2"/>
<contactref element="C53" pad="2"/>
<contactref element="U$8" pad="12"/>
<contactref element="SV2" pad="1"/>
<contactref element="R5" pad="1"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="6"/>
<contactref element="R1" pad="1"/>
<contactref element="K1" pad="28"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="5"/>
<contactref element="R2" pad="1"/>
<contactref element="K1" pad="27"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="7"/>
<contactref element="R3" pad="1"/>
<contactref element="TP3" pad="TP"/>
</signal>
<signal name="+5V">
<contactref element="K1" pad="2"/>
<contactref element="K1" pad="4"/>
<contactref element="C37" pad="2"/>
<contactref element="SV1" pad="3"/>
<contactref element="U$1" pad="5"/>
<contactref element="Q1" pad="2"/>
<contactref element="U3" pad="3"/>
<contactref element="U3" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="U$8" pad="27"/>
<contactref element="C48" pad="2"/>
</signal>
<signal name="N$36">
<contactref element="U$8" pad="11"/>
<contactref element="C49" pad="2"/>
</signal>
<signal name="N$40">
<contactref element="C50" pad="2"/>
<contactref element="C51" pad="1"/>
<contactref element="U$8" pad="9"/>
</signal>
<signal name="N$37">
<contactref element="U$8" pad="8"/>
<contactref element="C56" pad="2"/>
</signal>
<signal name="N$38">
<contactref element="U$8" pad="7"/>
<contactref element="C56" pad="1"/>
</signal>
<signal name="N$41">
<contactref element="U$8" pad="2"/>
<contactref element="C57" pad="2"/>
</signal>
<signal name="N$43">
<contactref element="U$8" pad="1"/>
<contactref element="C57" pad="1"/>
</signal>
<signal name="N$45">
<contactref element="C23" pad="1"/>
<contactref element="C58" pad="2"/>
<contactref element="R22" pad="1"/>
<contactref element="JP3" pad="RING"/>
</signal>
<signal name="N$50">
<contactref element="U$8" pad="30"/>
<contactref element="R21" pad="1"/>
<contactref element="R19" pad="1"/>
<contactref element="C62" pad="1"/>
<contactref element="R24" pad="2"/>
</signal>
<signal name="N$51">
<contactref element="R24" pad="1"/>
<contactref element="JP3" pad="SLEEVE"/>
</signal>
<signal name="N$8">
<contactref element="U$8" pad="31"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="C22" pad="2"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="C22" pad="1"/>
<contactref element="C23" pad="2"/>
<contactref element="C25" pad="1"/>
</signal>
<signal name="N$26">
<contactref element="R10" pad="2"/>
<contactref element="U$8" pad="32"/>
</signal>
<signal name="N$28">
<contactref element="R10" pad="1"/>
<contactref element="C31" pad="2"/>
</signal>
<signal name="N$29">
<contactref element="C38" pad="2"/>
<contactref element="C31" pad="1"/>
<contactref element="C40" pad="1"/>
</signal>
<signal name="N$30">
<contactref element="C38" pad="1"/>
<contactref element="R20" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="JP3" pad="TIP"/>
</signal>
<signal name="N$31">
<contactref element="U$8" pad="3"/>
<contactref element="C40" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="R15" pad="2"/>
</signal>
<signal name="N$32">
<contactref element="R16" pad="2"/>
<contactref element="R18" pad="2"/>
<contactref element="U$8" pad="4"/>
<contactref element="C25" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="U$8" pad="6"/>
<contactref element="R22" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="U$8" pad="5"/>
<contactref element="R20" pad="2"/>
</signal>
<signal name="N$34">
<contactref element="R19" pad="2"/>
<contactref element="U$8" pad="28"/>
<contactref element="C62" pad="2"/>
</signal>
<signal name="N$33">
<contactref element="U$8" pad="29"/>
<contactref element="R21" pad="2"/>
</signal>
<signal name="N$22">
</signal>
<signal name="N$24">
</signal>
<signal name="N$77">
</signal>
<signal name="N$78">
</signal>
<signal name="N$79">
</signal>
<signal name="N$7">
<contactref element="POWER" pad="C"/>
<contactref element="R30" pad="2"/>
</signal>
<signal name="N$47">
</signal>
<signal name="N$48">
</signal>
<signal name="N$74">
</signal>
<signal name="N$75">
</signal>
<signal name="N$76">
</signal>
<signal name="!ADC_RESET">
<contactref element="U$3" pad="29"/>
<contactref element="R47" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="U$3" pad="38"/>
<contactref element="C6" pad="2"/>
<contactref element="U$4" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="U$3" pad="37"/>
<contactref element="C7" pad="2"/>
<contactref element="U$4" pad="1"/>
</signal>
<signal name="PD_ALM">
<contactref element="U$3" pad="23"/>
<contactref element="IC2" pad="19"/>
</signal>
<signal name="LED_ALM">
<contactref element="U$3" pad="22"/>
<contactref element="IC2" pad="20"/>
</signal>
<signal name="INN">
<contactref element="X1" pad="5"/>
<contactref element="D3" pad="1"/>
<contactref element="U$3" pad="1"/>
</signal>
<signal name="INP">
<contactref element="X1" pad="9"/>
<contactref element="D2" pad="1"/>
<contactref element="U$3" pad="2"/>
</signal>
<signal name="TXN">
<contactref element="X1" pad="3"/>
<contactref element="D1" pad="1"/>
<contactref element="U$3" pad="14"/>
</signal>
<signal name="TXP">
<contactref element="X1" pad="2"/>
<contactref element="D5" pad="1"/>
<contactref element="U$3" pad="15"/>
</signal>
<signal name="N$15">
<contactref element="U$3" pad="7"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="N$16">
<contactref element="U$3" pad="30"/>
<contactref element="TP4" pad="P$1"/>
</signal>
<signal name="VCM">
<contactref element="U$3" pad="4"/>
<contactref element="C13" pad="1"/>
</signal>
<signal name="N$49">
</signal>
<signal name="RX_ANA_SUP">
<contactref element="U$3" pad="39"/>
<contactref element="U$3" pad="33"/>
<contactref element="C11" pad="1"/>
<contactref element="U$7" pad="2"/>
<contactref element="C18" pad="1"/>
<contactref element="D3" pad="3"/>
<contactref element="D2" pad="3"/>
</signal>
<signal name="LED_DRV_SUP">
<contactref element="U$3" pad="17"/>
<contactref element="U$3" pad="18"/>
<contactref element="C10" pad="1"/>
<contactref element="U$11" pad="2"/>
<contactref element="C28" pad="1"/>
<contactref element="D1" pad="3"/>
<contactref element="D5" pad="3"/>
</signal>
<signal name="TX_CTRL_SUP">
<contactref element="U$3" pad="11"/>
<contactref element="C9" pad="1"/>
<contactref element="U$10" pad="2"/>
<contactref element="C27" pad="1"/>
</signal>
<signal name="RX_DIG_SUP">
<contactref element="U$3" pad="31"/>
<contactref element="C12" pad="1"/>
<contactref element="U$9" pad="2"/>
<contactref element="C19" pad="1"/>
<contactref element="R47" pad="1"/>
</signal>
<signal name="SPO2_SCK">
<contactref element="IC2" pad="12"/>
<contactref element="U$3" pad="24"/>
</signal>
<signal name="SPO2_MOSI">
<contactref element="IC2" pad="11"/>
<contactref element="U$3" pad="26"/>
</signal>
<signal name="TARGET_USB_N">
<contactref element="IC2" pad="33"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="TARGET_USB_P">
<contactref element="IC2" pad="34"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="VDDCORE">
<contactref element="IC2" pad="43"/>
<contactref element="C102" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="C106" pad="1"/>
<contactref element="IC2" pad="6"/>
<contactref element="C107" pad="1"/>
<contactref element="L100" pad="1"/>
</signal>
<signal name="VCCIO">
<contactref element="C3" pad="1"/>
<contactref element="JP5" pad="1"/>
<contactref element="L1" pad="1"/>
</signal>
<signal name="SAM_RESETN">
<contactref element="CON_JTAG1" pad="10"/>
<contactref element="IC2" pad="40"/>
<contactref element="R9" pad="2"/>
<contactref element="TP2" pad="TP"/>
</signal>
<signal name="SAM_SWDIO">
<contactref element="CON_JTAG1" pad="2"/>
<contactref element="IC2" pad="46"/>
</signal>
<signal name="SAM_SWDCLK">
<contactref element="CON_JTAG1" pad="4"/>
<contactref element="IC2" pad="45"/>
</signal>
<signal name="N$57">
<contactref element="IC2" pad="24"/>
<contactref element="R11" pad="1"/>
<contactref element="TP1" pad="TP"/>
</signal>
<signal name="ECG_PWDN">
<contactref element="U$8" pad="15"/>
<contactref element="IC2" pad="28"/>
</signal>
<signal name="ECG_!DRDY">
<contactref element="IC2" pad="10"/>
<contactref element="U$8" pad="22"/>
</signal>
<signal name="SPO2_DRDY">
<contactref element="IC2" pad="3"/>
<contactref element="U$3" pad="28"/>
</signal>
<signal name="SPO2_START">
<contactref element="IC2" pad="8"/>
<contactref element="U$3" pad="20"/>
</signal>
<signal name="ECG_MISO">
<contactref element="IC2" pad="13"/>
<contactref element="U$8" pad="21"/>
</signal>
<signal name="BP_TX">
<contactref element="IC2" pad="38"/>
<contactref element="SV1" pad="1"/>
</signal>
<signal name="BP_RX">
<contactref element="IC2" pad="37"/>
<contactref element="SV1" pad="2"/>
</signal>
<signal name="ECG_MOSI">
<contactref element="IC2" pad="15"/>
<contactref element="U$8" pad="19"/>
</signal>
<signal name="ECG_SCK">
<contactref element="IC2" pad="16"/>
<contactref element="U$8" pad="20"/>
</signal>
<signal name="ECG_CS">
<contactref element="IC2" pad="14"/>
<contactref element="U$8" pad="18"/>
</signal>
<signal name="N$69">
<contactref element="IC2" pad="29"/>
<contactref element="TP10" pad="TP"/>
</signal>
<signal name="USB_P">
<contactref element="JP5" pad="3"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="USB_N">
<contactref element="JP5" pad="2"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="ECG_START">
<contactref element="U$8" pad="16"/>
<contactref element="IC2" pad="27"/>
</signal>
<signal name="SPO2_MISO">
<contactref element="IC2" pad="9"/>
<contactref element="U$3" pad="25"/>
</signal>
<signal name="SPO2_CS">
<contactref element="IC2" pad="7"/>
<contactref element="U$3" pad="27"/>
</signal>
<signal name="N$72">
<contactref element="U$1" pad="1"/>
<contactref element="U$1" pad="3"/>
<contactref element="U$1" pad="2"/>
<contactref element="R37" pad="2"/>
</signal>
<signal name="N$73">
<contactref element="U$1" pad="4"/>
<contactref element="R48" pad="2"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="N$80">
<contactref element="L1" pad="2"/>
<contactref element="U$1" pad="6"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="RPI_TXD">
<contactref element="K1" pad="8"/>
<contactref element="IC2" pad="22"/>
</signal>
<signal name="RPI_RXD">
<contactref element="K1" pad="10"/>
<contactref element="IC2" pad="21"/>
</signal>
<signal name="N$4">
<contactref element="C15" pad="2"/>
<contactref element="U$19" pad="P$2"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="C4" pad="1"/>
<contactref element="U$19" pad="P$1"/>
<contactref element="IC2" pad="2"/>
</signal>
<signal name="TMP_SCL">
<contactref element="IC2" pad="26"/>
<contactref element="SV2" pad="2"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="TMP_SDA">
<contactref element="IC2" pad="25"/>
<contactref element="SV2" pad="3"/>
<contactref element="R6" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
