(kicad_pcb (version 20171130) (host pcbnew 5.0.2-bee76a0~70~ubuntu16.04.1)
  (general
    (thickness 1.6)
    (drawings 14)
    (tracks 210)
    (zones 0)
    (modules 30)
    (nets 29)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user hide)
  )
  (setup
    (last_trace_width 0.25)
    (user_trace_width 0.153)
    (user_trace_width 0.254)
    (trace_clearance 0.2)
    (zone_clearance 0.154)
    (zone_45_only no)
    (trace_min 0.1)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 0.69 0.331)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (solder_mask_min_width 0.25)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF3F)
    (pcbplotparams
      (layerselection 0x00008_00000000)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (psnegative false)
      (psa4output false)
      (plotreference false)
      (plotvalue false)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 VCC)
  (net 2 GND)
  (net 3 "Net-(D1-Pad1)")
  (net 4 "Net-(D2-Pad1)")
  (net 5 "Net-(D3-Pad1)")
  (net 6 "Net-(D4-Pad1)")
  (net 7 "Net-(D5-Pad1)")
  (net 8 "Net-(D6-Pad1)")
  (net 9 "Net-(D7-Pad1)")
  (net 10 "Net-(U1-Pad6)")
  (net 11 "Net-(U1-Pad7)")
  (net 12 "Net-(U1-Pad10)")
  (net 13 "Net-(U1-Pad17)")
  (net 14 "Net-(U1-Pad18)")
  (net 15 "Net-(U1-Pad19)")
  (net 16 /Reset)
  (net 17 /MOSI)
  (net 18 /MISO)
  (net 19 /SCL)
  (net 20 /PA0)
  (net 21 /PA1)
  (net 22 /PA2)
  (net 23 /PA7)
  (net 24 /PB0)
  (net 25 /PB1)
  (net 26 /PB2)
  (net 27 /INT)
  (net 28 "Net-(TP1-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.25)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /INT)
    (add_net /MISO)
    (add_net /MOSI)
    (add_net /PA0)
    (add_net /PA1)
    (add_net /PA2)
    (add_net /PA7)
    (add_net /PB0)
    (add_net /PB1)
    (add_net /PB2)
    (add_net /Reset)
    (add_net /SCL)
    (add_net GND)
    (add_net "Net-(D1-Pad1)")
    (add_net "Net-(D2-Pad1)")
    (add_net "Net-(D3-Pad1)")
    (add_net "Net-(D4-Pad1)")
    (add_net "Net-(D5-Pad1)")
    (add_net "Net-(D6-Pad1)")
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(TP1-Pad1)")
    (add_net "Net-(U1-Pad10)")
    (add_net "Net-(U1-Pad17)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net VCC)
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 186.8932 101.7524)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1 0) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58AA844E)
    (at 190.9064 101.4222)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C2 (at 0 -1.5) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.5) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.75 0) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805 (layer F.Cu) (tedit 58AA8463)
    (at 196.0372 105.8672 270)
    (descr "Capacitor SMD 0805, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 -1.5 270) (layer F.SilkS))
    (fp_text value 10uF (at 0 1.75 270) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 270) (layer F.Fab))
    (pad 1 smd rect (at -1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 1 0 270) (size 1 1.25) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0603 (layer F.Cu) (tedit 58AA844E)
    (at 191.8462 112.014 180)
    (descr "Capacitor SMD 0603, reflow soldering, AVX (see smccp.pdf)")
    (tags "capacitor 0603")
    (attr smd)
    (fp_text reference C4 (at 0 -1.5 180) (layer F.SilkS))
    (fp_text value 100nF (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.5 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.75 0 180) (size 0.8 0.75) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (model Capacitors_SMD.3dshapes/C_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 186.0042 107.0864)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D1 (at 0 -1.25) (layer F.SilkS))
    (fp_text value red (at 0 1.35) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 20 /PA0))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 185.9534 105.4862)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D2 (at 0 -1.25) (layer F.SilkS))
    (fp_text value red (at 0 1.35) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 21 /PA1))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 186.0296 103.8098)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D3 (at 0 -1.25) (layer F.SilkS))
    (fp_text value red (at 0 1.35) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 22 /PA2))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D3-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 185.9534 113.6904)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D4 (at 0 -1.25) (layer F.SilkS))
    (fp_text value red (at 0 1.35) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 23 /PA7))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D4-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 186.0296 108.6612)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D5 (at 0 -1.25) (layer F.SilkS))
    (fp_text value red (at 0 1.35) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 24 /PB0))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D5-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 186.0042 110.3376)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D6 (at 0 -1.25) (layer F.SilkS))
    (fp_text value red (at 0 1.35) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 25 /PB1))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D6-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module LEDs:LED_0603 (layer F.Cu) (tedit 57FE93A5)
    (at 186.0296 112.014)
    (descr "LED 0603 smd package")
    (tags "LED led 0603 SMD smd SMT smt smdled SMDLED smtled SMTLED")
    (attr smd)
    (fp_text reference D7 (at 0 -1.25) (layer F.SilkS))
    (fp_text value red (at 0 1.35) (layer F.Fab))
    (pad 2 smd rect (at 0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 26 /PB2))
    (pad 1 smd rect (at -0.8 0 180) (size 0.8 0.8) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D7-Pad1)"))
    (model LEDs.3dshapes/LED_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58AAD9CA)
    (at 192.6844 105.7148 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R1 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 4K7 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 19 /SCL))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58AAD9CA)
    (at 193.548 103.7082 180)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R2 (at 0 -1.45 180) (layer F.SilkS))
    (fp_text value 4K7 (at 0 1.5 180) (layer F.Fab))
    (fp_text user %R (at 0 -1.45 180) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC))
    (pad 2 smd rect (at 0.75 0 180) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 17 /MOSI))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58AAD9CA)
    (at 182.2958 107.1372)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R3 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 50R (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 3 "Net-(D1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58AAD9CA)
    (at 182.3466 105.4862)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R4 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 50R (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 4 "Net-(D2-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58AAD9CA)
    (at 182.4228 103.8606)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R5 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 50R (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(D3-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58AAD9CA)
    (at 182.3466 113.411)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R6 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 50R (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(D4-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58AAD9CA)
    (at 182.2958 108.7374)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R7 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 50R (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(D5-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58AAD9CA)
    (at 182.2958 110.2868)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R8 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 50R (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 8 "Net-(D6-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0603 (layer F.Cu) (tedit 58AAD9CA)
    (at 182.3212 111.8362)
    (descr "Resistor SMD 0603, reflow soldering, Vishay (see dcrcw.pdf)")
    (tags "resistor 0603")
    (attr smd)
    (fp_text reference R9 (at 0 -1.45) (layer F.SilkS))
    (fp_text value 50R (at 0 1.5) (layer F.Fab))
    (fp_text user %R (at 0 -1.45) (layer F.Fab))
    (pad 1 smd rect (at -0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 2 GND))
    (pad 2 smd rect (at 0.75 0) (size 0.5 0.9) (layers F.Cu F.Paste F.Mask)
      (net 9 "Net-(D7-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0603.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module POV_lib:Molex_2x3_Contact (layer B.Cu) (tedit 59513E8F)
    (at 186.7154 111.2266)
    (fp_text reference J3 (at 0 4.4) (layer B.SilkS))
    (fp_text value CONN_02X03 (at -0.05 -4.15) (layer B.Fab))
    (pad 1 smd rect (at -1.6 1.925) (size 1.3 1.85) (layers B.Cu B.Paste B.Mask)
      (net 16 /Reset) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 2 smd rect (at -1.6 -1.925) (size 1.3 1.85) (layers B.Cu B.Paste B.Mask)
      (net 17 /MOSI) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 3 smd rect (at 0 1.925) (size 1.3 1.85) (layers B.Cu B.Paste B.Mask)
      (net 2 GND) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 4 smd rect (at 0 -1.925) (size 1.3 1.85) (layers B.Cu B.Paste B.Mask)
      (net 18 /MISO) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 5 smd rect (at 1.6 1.925) (size 1.3 1.85) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 6 smd rect (at 1.6 -1.925) (size 1.3 1.85) (layers B.Cu B.Paste B.Mask)
      (net 19 /SCL) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
  )
  (module POV_lib:LGA_12_2x2 (layer F.Cu) (tedit 59513D97)
    (at 190.7032 103.7336 90)
    (fp_text reference U2 (at 0 -2.3 90) (layer F.SilkS))
    (fp_text value LIS2DE12 (at 0 2.7 90) (layer F.Fab))
    (pad 1 smd rect (at -0.875 -0.75 90) (size 0.5 0.24) (layers F.Cu F.Paste F.Mask)
      (net 19 /SCL) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 2 smd rect (at -0.875 -0.25 90) (size 0.5 0.24) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 3 smd rect (at -0.875 0.25 90) (size 0.5 0.24) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 4 smd rect (at -0.875 0.75 90) (size 0.5 0.24) (layers F.Cu F.Paste F.Mask)
      (net 17 /MOSI) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 5 smd rect (at -0.25 0.875 180) (size 0.5 0.24) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 6 smd rect (at 0.25 0.875 180) (size 0.5 0.24) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 7 smd rect (at 0.875 0.75 90) (size 0.5 0.24) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 8 smd rect (at 0.875 0.25 90) (size 0.5 0.24) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 9 smd rect (at 0.875 -0.25 90) (size 0.5 0.24) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 10 smd rect (at 0.875 -0.75 90) (size 0.5 0.24) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 11 smd rect (at 0.25 -0.875 180) (size 0.5 0.24) (layers F.Cu F.Paste F.Mask)
      (net 28 "Net-(TP1-Pad1)") (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 12 smd rect (at -0.25 -0.875 180) (size 0.5 0.24) (layers F.Cu F.Paste F.Mask)
      (net 27 /INT) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
  )
  (module POV_lib:Molex_1x6_Contact (layer B.Cu) (tedit 595186E4)
    (at 182.3974 104.394 90)
    (fp_text reference J2 (at -0.2 2.9 90) (layer B.SilkS))
    (fp_text value CONN_01X06 (at 0.05 -3.1 90) (layer B.Fab))
    (pad 1 smd rect (at -3 0.875 90) (size 0.7 1.25) (layers B.Cu B.Paste B.Mask)
      (net 16 /Reset) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 2 smd rect (at -2 -0.875 90) (size 0.7 1.25) (layers B.Cu B.Paste B.Mask)
      (net 17 /MOSI))
    (pad 3 smd rect (at -1 0.875 90) (size 0.7 1.25) (layers B.Cu B.Paste B.Mask)
      (net 2 GND))
    (pad 4 smd rect (at 1 -0.875 90) (size 0.7 1.25) (layers B.Cu B.Paste B.Mask)
      (net 18 /MISO))
    (pad 5 smd rect (at 2 0.875 90) (size 0.7 1.25) (layers B.Cu B.Paste B.Mask)
      (net 1 VCC))
    (pad 6 smd rect (at 3 -0.875 90) (size 0.7 1.25) (layers B.Cu B.Paste B.Mask)
      (net 19 /SCL))
  )
  (module POV_lib:Molex_PicoBlade_53047-0210_02x1.25mm_Straight (layer F.Cu) (tedit 595332B5)
    (at 195.8594 103.1494 90)
    (descr "Molex PicoBlade, single row, top entry type, through hole, PN:53047-0210")
    (tags "connector molex picoblade")
    (fp_text reference J1 (at 0 1.55 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -1.7 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 1 VCC))
    (pad 2 thru_hole circle (at 1.25 0 90) (size 0.85 0.85) (drill 0.5) (layers *.Cu *.Mask)
      (net 2 GND))
    (model Connectors_Molex.3dshapes/Molex_PicoBlade_53047-0210_02x1.25mm_Straight.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module POV_lib:TP_331u (layer F.Cu) (tedit 5953ECF5)
    (at 188.722 103.3018)
    (fp_text reference TP1 (at 0 -1.3) (layer F.SilkS))
    (fp_text value TEST (at 0.05 1.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.69 0.69) (drill 0.331) (layers *.Cu *.Mask)
      (net 28 "Net-(TP1-Pad1)") (solder_mask_margin 0.01))
  )
  (module POV_lib:TP_331u (layer F.Cu) (tedit 5953ECF5)
    (at 188.0616 104.0384)
    (fp_text reference TP2 (at 0 -1.3) (layer F.SilkS))
    (fp_text value TEST (at 0.05 1.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.69 0.69) (drill 0.331) (layers *.Cu *.Mask)
      (net 27 /INT) (solder_mask_margin 0.01))
  )
  (module POV_lib:TP_331u (layer F.Cu) (tedit 5953ECF5)
    (at 189.738 105.8418)
    (fp_text reference TP3 (at 0 -1.3) (layer F.SilkS))
    (fp_text value TEST (at 0.05 1.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.69 0.69) (drill 0.331) (layers *.Cu *.Mask)
      (net 18 /MISO) (solder_mask_margin 0.01))
  )
  (module POV_lib:TP_331u (layer F.Cu) (tedit 5953ECF5)
    (at 194.2592 106.8578)
    (fp_text reference TP4 (at 0 -1.3) (layer F.SilkS))
    (fp_text value TEST (at 0.05 1.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.69 0.69) (drill 0.331) (layers *.Cu *.Mask)
      (net 17 /MOSI) (solder_mask_margin 0.01))
  )
  (module POV_lib:TP_331u (layer F.Cu) (tedit 5953ECF5)
    (at 190.8048 105.6894)
    (fp_text reference TP5 (at 0 -1.3) (layer F.SilkS))
    (fp_text value TEST (at 0.05 1.4) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 0.69 0.69) (drill 0.331) (layers *.Cu *.Mask)
      (net 19 /SCL) (solder_mask_margin 0.01))
  )
  (module POV_lib:20Pin_4x4_QFN (layer F.Cu) (tedit 5975146C)
    (at 191.6938 108.7628)
    (fp_text reference U1 (at 0 -3.3) (layer F.SilkS))
    (fp_text value ATTINY84 (at 0.15 3.25) (layer F.Fab))
    (pad 1 smd rect (at -1.9 -1) (size 0.6 0.24) (layers F.Cu F.Paste F.Mask)
      (net 19 /SCL) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 2 smd rect (at -1.9 -0.5) (size 0.6 0.24) (layers F.Cu F.Paste F.Mask)
      (net 27 /INT) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 3 smd rect (at -1.9 0) (size 0.6 0.24) (layers F.Cu F.Paste F.Mask)
      (net 22 /PA2) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 4 smd rect (at -1.9 0.5) (size 0.6 0.24) (layers F.Cu F.Paste F.Mask)
      (net 21 /PA1) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 5 smd rect (at -1.9 1) (size 0.6 0.24) (layers F.Cu F.Paste F.Mask)
      (net 20 /PA0) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 6 smd rect (at -1 1.9 90) (size 0.5 0.24) (layers F.Cu F.Paste F.Mask)
      (net 10 "Net-(U1-Pad6)") (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 7 smd rect (at -0.5 1.9 90) (size 0.5 0.24) (layers F.Cu F.Paste F.Mask)
      (net 11 "Net-(U1-Pad7)") (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 8 smd rect (at 0 1.9 90) (size 0.5 0.24) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 9 smd rect (at 0.5 1.9 90) (size 0.5 0.24) (layers F.Cu F.Paste F.Mask)
      (net 1 VCC) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 10 smd rect (at 1 1.9 90) (size 0.5 0.24) (layers F.Cu F.Paste F.Mask)
      (net 12 "Net-(U1-Pad10)") (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 11 smd rect (at 1.9 1) (size 0.6 0.24) (layers F.Cu F.Paste F.Mask)
      (net 24 /PB0) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 12 smd rect (at 1.9 0.5) (size 0.6 0.24) (layers F.Cu F.Paste F.Mask)
      (net 25 /PB1) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 13 smd rect (at 1.9 0) (size 0.6 0.24) (layers F.Cu F.Paste F.Mask)
      (net 16 /Reset) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 14 smd rect (at 1.9 -0.5) (size 0.6 0.24) (layers F.Cu F.Paste F.Mask)
      (net 26 /PB2) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 15 smd rect (at 1.9 -1) (size 0.6 0.24) (layers F.Cu F.Paste F.Mask)
      (net 23 /PA7) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 16 smd rect (at 1 -1.9 90) (size 0.5 0.24) (layers F.Cu F.Paste F.Mask)
      (net 17 /MOSI) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 17 smd rect (at 0.5 -1.9 90) (size 0.5 0.24) (layers F.Cu F.Paste F.Mask)
      (net 13 "Net-(U1-Pad17)") (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 18 smd rect (at 0 -1.9 90) (size 0.5 0.24) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(U1-Pad18)") (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 19 smd rect (at -0.5 -1.9 90) (size 0.5 0.24) (layers F.Cu F.Paste F.Mask)
      (net 15 "Net-(U1-Pad19)") (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 20 smd rect (at -1 -1.9 90) (size 0.5 0.24) (layers F.Cu F.Paste F.Mask)
      (net 18 /MISO) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 21 smd rect (at 0 0 90) (size 2.5 2.5) (layers F.Cu F.Paste F.Mask)
      (net 2 GND) (solder_mask_margin 0.01) (solder_paste_margin 0.01))
    (pad 21 thru_hole circle (at -0.75 0.75) (size 0.69 0.69) (drill 0.331) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 21 thru_hole circle (at 0.75 0.7) (size 0.69 0.69) (drill 0.331) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 21 thru_hole circle (at 0.75 -0.7) (size 0.69 0.69) (drill 0.331) (layers *.Cu *.Mask)
      (net 2 GND))
    (pad 21 thru_hole circle (at -0.75 -0.75) (size 0.69 0.69) (drill 0.331) (layers *.Cu *.Mask)
      (net 2 GND))
  )
  (gr_text 7/1/17 (at 193.1924 112.3696) (layer B.SilkS))
  (gr_text "POV\njkl" (at 192.4812 104.8766) (layer B.SilkS))
  (gr_line (start 180 100) (end 197.7 100) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 184.6154 114.5) (end 184.6154 115) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 188.8154 115) (end 188.8154 114.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 184.6154 114.5) (end 188.8154 114.5) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 180 100) (end 180 100.794) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 180 100.794) (end 180.5 100.794) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 180 115) (end 180 107.994) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 180.5 100.794) (end 180.5 107.994) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 180 115) (end 184.6154 115) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 180 107.994) (end 180.5 107.994) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 197.7 115) (end 188.8154 115) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 197.7 100) (end 197.7 115) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name GND) (layer B.Cu) (hatch edge 0.508)
    (connect_pads yes (clearance 0.154))
    (min_thickness 0.154)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 197.612 114.6302) (xy 180.3908 114.6302) (xy 180.3908 100.3808) (xy 197.612 100.3808)
      )
    )
  )
)
