<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="26.45798125" y1="29.96211875" x2="26.36058125" y2="29.962059375" width="0" layer="20"/>
<wire x1="26.36058125" y1="29.962059375" x2="26.26415" y2="29.9619" width="0" layer="20"/>
<wire x1="26.26415" y1="29.9619" x2="26.168740625" y2="29.96166875" width="0" layer="20"/>
<wire x1="26.168740625" y1="29.96166875" x2="26.07435" y2="29.961390625" width="0" layer="20"/>
<wire x1="26.07435" y1="29.961390625" x2="25.98103125" y2="29.96083125" width="0" layer="20"/>
<wire x1="25.98103125" y1="29.96083125" x2="25.888790625" y2="29.960259375" width="0" layer="20"/>
<wire x1="25.888790625" y1="29.960259375" x2="25.79768125" y2="29.959409375" width="0" layer="20"/>
<wire x1="25.79768125" y1="29.959409375" x2="25.7077" y2="29.95856875" width="0" layer="20"/>
<wire x1="25.7077" y1="29.95856875" x2="24.066940625" y2="29.926340625" width="0" layer="20"/>
<wire x1="24.066940625" y1="29.926340625" x2="22.23425" y2="29.8633" width="0" layer="20"/>
<wire x1="22.23425" y1="29.8633" x2="20.32533125" y2="29.77418125" width="0" layer="20"/>
<wire x1="20.32533125" y1="29.77418125" x2="18.45591875" y2="29.663690625" width="0" layer="20"/>
<wire x1="18.45591875" y1="29.663690625" x2="16.741740625" y2="29.53658125" width="0" layer="20"/>
<wire x1="16.741740625" y1="29.53658125" x2="15.298509375" y2="29.397559375" width="0" layer="20"/>
<wire x1="15.298509375" y1="29.397559375" x2="14.24195" y2="29.25138125" width="0" layer="20"/>
<wire x1="14.24195" y1="29.25138125" x2="13.68778125" y2="29.10275" width="0" layer="20"/>
<wire x1="13.68778125" y1="29.10275" x2="13.40298125" y2="28.889540625" width="0" layer="20"/>
<wire x1="13.40298125" y1="28.889540625" x2="12.980909375" y2="28.499940625" width="0" layer="20"/>
<wire x1="12.980909375" y1="28.499940625" x2="12.44945" y2="27.960940625" width="0" layer="20"/>
<wire x1="12.44945" y1="27.960940625" x2="11.836440625" y2="27.299509375" width="0" layer="20"/>
<wire x1="11.836440625" y1="27.299509375" x2="11.16975" y2="26.54265" width="0" layer="20"/>
<wire x1="11.16975" y1="26.54265" x2="10.47723125" y2="25.71733125" width="0" layer="20"/>
<wire x1="10.47723125" y1="25.71733125" x2="9.12615" y2="23.96926875" width="0" layer="20"/>
<wire x1="9.12615" y1="23.96926875" x2="8.936209375" y2="23.96286875" width="0" layer="20"/>
<wire x1="8.936209375" y1="23.96286875" x2="8.729959375" y2="23.95403125" width="0" layer="20"/>
<wire x1="8.729959375" y1="23.95403125" x2="8.52765" y2="23.942409375" width="0" layer="20"/>
<wire x1="8.52765" y1="23.942409375" x2="8.34953125" y2="23.92766875" width="0" layer="20"/>
<wire x1="8.34953125" y1="23.92766875" x2="7.720990625" y2="23.895290625" width="0" layer="20"/>
<wire x1="7.720990625" y1="23.895290625" x2="7.08333125" y2="23.87206875" width="0" layer="20"/>
<wire x1="7.08333125" y1="23.87206875" x2="6.47063125" y2="23.77935" width="0" layer="20"/>
<wire x1="6.47063125" y1="23.77935" x2="5.91696875" y2="23.53851875" width="0" layer="20"/>
<wire x1="5.91696875" y1="23.53851875" x2="5.6009" y2="23.26508125" width="0" layer="20"/>
<wire x1="5.6009" y1="23.26508125" x2="5.34678125" y2="22.921690625" width="0" layer="20"/>
<wire x1="5.34678125" y1="22.921690625" x2="5.158840625" y2="22.534" width="0" layer="20"/>
<wire x1="5.158840625" y1="22.534" x2="5.041290625" y2="22.12761875" width="0" layer="20"/>
<wire x1="5.041290625" y1="22.12761875" x2="5.03073125" y2="21.8568" width="0" layer="20"/>
<wire x1="5.03073125" y1="21.8568" x2="5.0734" y2="21.55073125" width="0" layer="20"/>
<wire x1="5.0734" y1="21.55073125" x2="5.14038125" y2="21.26313125" width="0" layer="20"/>
<wire x1="5.14038125" y1="21.26313125" x2="5.20278125" y2="21.0477" width="0" layer="20"/>
<wire x1="5.20278125" y1="21.0477" x2="4.9507" y2="20.91293125" width="0" layer="20"/>
<wire x1="4.9507" y1="20.91293125" x2="4.7157" y2="20.774159375" width="0" layer="20"/>
<wire x1="4.7157" y1="20.774159375" x2="4.502540625" y2="20.63211875" width="0" layer="20"/>
<wire x1="4.502540625" y1="20.63211875" x2="4.316009375" y2="20.487559375" width="0" layer="20"/>
<wire x1="4.316009375" y1="20.487559375" x2="3.441940625" y2="19.59296875" width="0" layer="20"/>
<wire x1="3.441940625" y1="19.59296875" x2="2.710309375" y2="18.564309375" width="0" layer="20"/>
<wire x1="2.710309375" y1="18.564309375" x2="2.08981875" y2="17.452240625" width="0" layer="20"/>
<wire x1="2.08981875" y1="17.452240625" x2="1.5492" y2="16.30745" width="0" layer="20"/>
<wire x1="1.5492" y1="16.30745" x2="0.97766875" y2="14.89638125" width="0" layer="20"/>
<wire x1="0.97766875" y1="14.89638125" x2="0.51555" y2="13.43955" width="0" layer="20"/>
<wire x1="0.51555" y1="13.43955" x2="0.18726875" y2="11.95035" width="0" layer="20"/>
<wire x1="0.18726875" y1="11.95035" x2="0.017240625" y2="10.442140625" width="0" layer="20"/>
<wire x1="0.017240625" y1="10.442140625" x2="0.091790625" y2="8.679940625" width="0" layer="20"/>
<wire x1="0.091790625" y1="8.679940625" x2="0.49228125" y2="7.10581875" width="0" layer="20"/>
<wire x1="0.49228125" y1="7.10581875" x2="1.12821875" y2="5.601509375" width="0" layer="20"/>
<wire x1="1.12821875" y1="5.601509375" x2="1.90916875" y2="4.0487" width="0" layer="20"/>
<wire x1="1.90916875" y1="4.0487" x2="2.01731875" y2="3.971259375" width="0" layer="20"/>
<wire x1="2.01731875" y1="3.971259375" x2="2.12546875" y2="3.893809375" width="0" layer="20"/>
<wire x1="2.12546875" y1="3.893809375" x2="2.23361875" y2="3.81636875" width="0" layer="20"/>
<wire x1="2.23361875" y1="3.81636875" x2="2.34178125" y2="3.73891875" width="0" layer="20"/>
<wire x1="2.34178125" y1="3.73891875" x2="2.43358125" y2="2.56258125" width="0" layer="20"/>
<wire x1="2.43358125" y1="2.56258125" x2="2.81461875" y2="1.349140625" width="0" layer="20"/>
<wire x1="2.81461875" y1="1.349140625" x2="3.403909375" y2="0.397559375" width="0" layer="20"/>
<wire x1="3.403909375" y1="0.397559375" x2="4.120459375" y2="0.00676875" width="0" layer="20"/>
<wire x1="4.120459375" y1="0.00676875" x2="5.18008125" y2="0.00041875" width="0" layer="20"/>
<wire x1="5.18008125" y1="0.00041875" x2="6.138409375" y2="0.01283125" width="0" layer="20"/>
<wire x1="6.138409375" y1="0.01283125" x2="7.21016875" y2="0.04058125" width="0" layer="20"/>
<wire x1="7.21016875" y1="0.04058125" x2="8.61008125" y2="0.080190625" width="0" layer="20"/>
<wire x1="8.61008125" y1="0.080190625" x2="9.19896875" y2="0.56986875" width="0" layer="20"/>
<wire x1="9.19896875" y1="0.56986875" x2="9.58438125" y2="1.0152" width="0" layer="20"/>
<wire x1="9.58438125" y1="1.0152" x2="9.86423125" y2="1.437509375" width="0" layer="20"/>
<wire x1="9.86423125" y1="1.437509375" x2="10.13645" y2="1.858159375" width="0" layer="20"/>
<wire x1="10.13645" y1="1.858159375" x2="13.876809375" y2="1.72796875" width="0" layer="20"/>
<wire x1="13.876809375" y1="1.72796875" x2="15.746990625" y2="1.66288125" width="0" layer="20"/>
<wire x1="15.746990625" y1="1.66288125" x2="17.61716875" y2="1.59778125" width="0" layer="20"/>
<wire x1="17.61716875" y1="1.59778125" x2="19.48735" y2="1.532690625" width="0" layer="20"/>
<wire x1="19.48735" y1="1.532690625" x2="21.35753125" y2="1.467590625" width="0" layer="20"/>
<wire x1="21.35753125" y1="1.467590625" x2="23.227709375" y2="1.4025" width="0" layer="20"/>
<wire x1="23.227709375" y1="1.4025" x2="25.097890625" y2="1.3374" width="0" layer="20"/>
<wire x1="25.097890625" y1="1.3374" x2="27.06681875" y2="1.4362" width="0" layer="20"/>
<wire x1="27.06681875" y1="1.4362" x2="29.035759375" y2="1.534990625" width="0" layer="20"/>
<wire x1="29.035759375" y1="1.534990625" x2="31.004690625" y2="1.633790625" width="0" layer="20"/>
<wire x1="31.004690625" y1="1.633790625" x2="32.97361875" y2="1.73258125" width="0" layer="20"/>
<wire x1="32.97361875" y1="1.73258125" x2="36.91148125" y2="1.93018125" width="0" layer="20"/>
<wire x1="36.91148125" y1="1.93018125" x2="40.84935" y2="2.12776875" width="0" layer="20"/>
<wire x1="40.84935" y1="2.12776875" x2="40.92558125" y2="1.875309375" width="0" layer="20"/>
<wire x1="40.92558125" y1="1.875309375" x2="41.14191875" y2="1.293890625" width="0" layer="20"/>
<wire x1="41.14191875" y1="1.293890625" x2="41.479809375" y2="0.64745" width="0" layer="20"/>
<wire x1="41.479809375" y1="0.64745" x2="41.92066875" y2="0.19991875" width="0" layer="20"/>
<wire x1="41.92066875" y1="0.19991875" x2="42.895990625" y2="0.06721875" width="0" layer="20"/>
<wire x1="42.895990625" y1="0.06721875" x2="44.626940625" y2="0.035590625" width="0" layer="20"/>
<wire x1="44.626940625" y1="0.035590625" x2="46.33905" y2="0.1101" width="0" layer="20"/>
<wire x1="46.33905" y1="0.1101" x2="47.257859375" y2="0.295790625" width="0" layer="20"/>
<wire x1="47.257859375" y1="0.295790625" x2="47.97776875" y2="1.275890625" width="0" layer="20"/>
<wire x1="47.97776875" y1="1.275890625" x2="48.358390625" y2="2.4506" width="0" layer="20"/>
<wire x1="48.358390625" y1="2.4506" x2="48.536290625" y2="3.753140625" width="0" layer="20"/>
<wire x1="48.536290625" y1="3.753140625" x2="48.648009375" y2="5.116740625" width="0" layer="20"/>
<wire x1="48.648009375" y1="5.116740625" x2="48.824009375" y2="5.64685" width="0" layer="20"/>
<wire x1="48.824009375" y1="5.64685" x2="49.22478125" y2="6.93916875" width="0" layer="20"/>
<wire x1="49.22478125" y1="6.93916875" x2="49.65941875" y2="8.546690625" width="0" layer="20"/>
<wire x1="49.65941875" y1="8.546690625" x2="49.93705" y2="10.02238125" width="0" layer="20"/>
<wire x1="49.93705" y1="10.02238125" x2="49.992009375" y2="10.7647" width="0" layer="20"/>
<wire x1="49.992009375" y1="10.7647" x2="49.9937" y2="11.51136875" width="0" layer="20"/>
<wire x1="49.9937" y1="11.51136875" x2="49.93531875" y2="12.25468125" width="0" layer="20"/>
<wire x1="49.93531875" y1="12.25468125" x2="49.80991875" y2="12.98688125" width="0" layer="20"/>
<wire x1="49.80991875" y1="12.98688125" x2="49.28933125" y2="14.89443125" width="0" layer="20"/>
<wire x1="49.28933125" y1="14.89443125" x2="48.59296875" y2="16.786490625" width="0" layer="20"/>
<wire x1="48.59296875" y1="16.786490625" x2="47.763609375" y2="18.555809375" width="0" layer="20"/>
<wire x1="47.763609375" y1="18.555809375" x2="46.844009375" y2="20.09511875" width="0" layer="20"/>
<wire x1="46.844009375" y1="20.09511875" x2="46.64155" y2="20.346040625" width="0" layer="20"/>
<wire x1="46.64155" y1="20.346040625" x2="46.38266875" y2="20.59668125" width="0" layer="20"/>
<wire x1="46.38266875" y1="20.59668125" x2="46.07751875" y2="20.84268125" width="0" layer="20"/>
<wire x1="46.07751875" y1="20.84268125" x2="45.736240625" y2="21.079709375" width="0" layer="20"/>
<wire x1="45.736240625" y1="21.079709375" x2="45.80431875" y2="21.35631875" width="0" layer="20"/>
<wire x1="45.80431875" y1="21.35631875" x2="45.87493125" y2="21.72263125" width="0" layer="20"/>
<wire x1="45.87493125" y1="21.72263125" x2="45.91551875" y2="22.11053125" width="0" layer="20"/>
<wire x1="45.91551875" y1="22.11053125" x2="45.89356875" y2="22.451940625" width="0" layer="20"/>
<wire x1="45.89356875" y1="22.451940625" x2="45.77205" y2="22.857490625" width="0" layer="20"/>
<wire x1="45.77205" y1="22.857490625" x2="45.58455" y2="23.24528125" width="0" layer="20"/>
<wire x1="45.58455" y1="23.24528125" x2="45.332640625" y2="23.58913125" width="0" layer="20"/>
<wire x1="45.332640625" y1="23.58913125" x2="45.017890625" y2="23.862840625" width="0" layer="20"/>
<wire x1="45.017890625" y1="23.862840625" x2="44.46421875" y2="24.10366875" width="0" layer="20"/>
<wire x1="44.46421875" y1="24.10366875" x2="43.85151875" y2="24.19638125" width="0" layer="20"/>
<wire x1="43.85151875" y1="24.19638125" x2="43.213859375" y2="24.219609375" width="0" layer="20"/>
<wire x1="43.213859375" y1="24.219609375" x2="42.58533125" y2="24.251990625" width="0" layer="20"/>
<wire x1="42.58533125" y1="24.251990625" x2="42.39518125" y2="24.267540625" width="0" layer="20"/>
<wire x1="42.39518125" y1="24.267540625" x2="42.17903125" y2="24.27961875" width="0" layer="20"/>
<wire x1="42.17903125" y1="24.27961875" x2="41.96155" y2="24.288590625" width="0" layer="20"/>
<wire x1="41.96155" y1="24.288590625" x2="41.76746875" y2="24.29483125" width="0" layer="20"/>
<wire x1="41.76746875" y1="24.29483125" x2="40.590459375" y2="25.81631875" width="0" layer="20"/>
<wire x1="40.590459375" y1="25.81631875" x2="39.94578125" y2="26.594690625" width="0" layer="20"/>
<wire x1="39.94578125" y1="26.594690625" x2="39.296159375" y2="27.34195" width="0" layer="20"/>
<wire x1="39.296159375" y1="27.34195" x2="38.665990625" y2="28.025959375" width="0" layer="20"/>
<wire x1="38.665990625" y1="28.025959375" x2="38.079659375" y2="28.614559375" width="0" layer="20"/>
<wire x1="38.079659375" y1="28.614559375" x2="37.56155" y2="29.075609375" width="0" layer="20"/>
<wire x1="37.56155" y1="29.075609375" x2="37.136040625" y2="29.376959375" width="0" layer="20"/>
<wire x1="37.136040625" y1="29.376959375" x2="36.67566875" y2="29.494209375" width="0" layer="20"/>
<wire x1="36.67566875" y1="29.494209375" x2="35.779940625" y2="29.60373125" width="0" layer="20"/>
<wire x1="35.779940625" y1="29.60373125" x2="34.541609375" y2="29.7031" width="0" layer="20"/>
<wire x1="34.541609375" y1="29.7031" x2="33.05346875" y2="29.78986875" width="0" layer="20"/>
<wire x1="33.05346875" y1="29.78986875" x2="31.408259375" y2="29.861609375" width="0" layer="20"/>
<wire x1="31.408259375" y1="29.861609375" x2="29.69875" y2="29.91586875" width="0" layer="20"/>
<wire x1="29.69875" y1="29.91586875" x2="28.01771875" y2="29.950209375" width="0" layer="20"/>
<wire x1="28.01771875" y1="29.950209375" x2="26.45793125" y2="29.9622" width="0" layer="20"/>
<wire x1="26.45793125" y1="29.9622" x2="26.45795" y2="29.962190625" width="0" layer="20"/>
<wire x1="26.45795" y1="29.962190625" x2="26.45798125" y2="29.96211875" width="0" layer="20"/>
<text>hackaday.io
/davedarko
/project/25944</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="CHIPLED-0603-TTW">
<description>&lt;b&gt;CHIPLED-0603&lt;/b&gt;&lt;p&gt;
Recommended Solder Pad useable for SmartLEDTM and Chipled - Package 0603&lt;br&gt;
Package able to withstand TTW-soldering heat&lt;br&gt;
Package suitable for TTW-soldering&lt;br&gt;
Source: http://www.osram.convergy.de/ ... LO_LS_LY L89K.pdf</description>
</package>
<package name="R0603">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08-EIAJ">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
</packages>
</library>
<library name="battery">
<description>&lt;b&gt;Lithium Batteries and NC Accus&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="CR2032SMD">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="KPS-1290">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3_SMD_PAD">
</package>
</packages>
</library>
<library name="testpad">
<description>&lt;b&gt;Test Pins/Pads&lt;/b&gt;&lt;p&gt;
Cream on SMD OFF.&lt;br&gt;
new: Attribute TP_SIGNAL_NAME&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="B1,27">
<description>&lt;b&gt;TEST PAD&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="LOGOS">
<packages>
<package name="HACKADAY_LOGO">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LED1" library="adafruit" package="CHIPLED-0603-TTW" value="">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="adafruit" package="CHIPLED-0603-TTW" value="">
<attribute name="VALUE"/>
</element>
<element name="LED3" library="adafruit" package="CHIPLED-0603-TTW" value="">
<attribute name="VALUE"/>
</element>
<element name="LED4" library="adafruit" package="CHIPLED-0603-TTW" value="">
<attribute name="VALUE"/>
</element>
<element name="LED5" library="adafruit" package="CHIPLED-0603-TTW" value="">
<attribute name="VALUE"/>
</element>
<element name="LED6" library="adafruit" package="CHIPLED-0603-TTW" value="">
<attribute name="VALUE"/>
</element>
<element name="LED7" library="adafruit" package="CHIPLED-0603-TTW" value="">
<attribute name="VALUE"/>
</element>
<element name="LED8" library="adafruit" package="CHIPLED-0603-TTW" value="">
<attribute name="VALUE"/>
</element>
<element name="U1" library="SparkFun-DigitalIC" package="SO08-EIAJ" value="Tiny85-20-SMT">
<attribute name="PROD_ID" value="IC-09092"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="SparkFun-Electromechanical" package="KPS-1290" value="SWITCH_SPDT">
<attribute name="PROD_ID" value="SWCH-10651"/>
</element>
<element name="U$2" library="battery" package="CR2032SMD" value="CR2032SMD"/>
<element name="JP1" library="SparkFun-Connectors" package="2X3_SMD_PAD" value="AVR_SPI_PRG_6"/>
<element name="R1" library="adafruit" package="R0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="adafruit" package="R0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="adafruit" package="R0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="adafruit" package="R0603" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="PB4" library="testpad" package="B1,27" value="PTR1B1,27">
<attribute name="TP_SIGNAL_NAME" value=""/>
<attribute name="NAME"/>
</element>
<element name="U$3" library="LOGOS" package="HACKADAY_LOGO" value="HACKADAY_1CM"/>
</elements>
<signals>
<signal name="N$6">
</signal>
<signal name="N$7">
</signal>
<signal name="N$8">
</signal>
<signal name="N$9">
<contactref element="LED1" pad="A@1"/>
<contactref element="LED2" pad="C@1"/>
<contactref element="LED7" pad="A@1"/>
<contactref element="LED8" pad="C@1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="LED5" pad="C@1"/>
<contactref element="LED6" pad="A@1"/>
<contactref element="LED7" pad="C@1"/>
<contactref element="LED8" pad="A@1"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="LED1" pad="C@1"/>
<contactref element="LED3" pad="A@1"/>
<contactref element="LED4" pad="C@1"/>
<contactref element="LED2" pad="A@1"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="LED3" pad="C@1"/>
<contactref element="LED4" pad="A@1"/>
<contactref element="LED6" pad="C@1"/>
<contactref element="LED5" pad="A@1"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$12222">
<contactref element="U$2" pad="-"/>
<contactref element="JP1" pad="P$6"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="MOSI">
<contactref element="R1" pad="1"/>
<contactref element="U1" pad="5"/>
<contactref element="JP1" pad="P$4"/>
</signal>
<signal name="MISO">
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="6"/>
<contactref element="JP1" pad="P$1"/>
</signal>
<signal name="SCK">
<contactref element="R3" pad="1"/>
<contactref element="U1" pad="7"/>
<contactref element="JP1" pad="P$3"/>
</signal>
<signal name="PB3">
<contactref element="R4" pad="1"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="U$2" pad="+"/>
<contactref element="U$1" pad="P"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="8"/>
<contactref element="JP1" pad="P$2"/>
<contactref element="U$1" pad="O"/>
</signal>
<signal name="RST">
<contactref element="JP1" pad="P$5"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U1" pad="3"/>
<contactref element="PB4" pad="TP"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
