<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.4.1">
<drawing>
<board>
<plain>
<wire x1="-23.2763" y1="34.7589" x2="-25.2763" y2="32.7589" width="0.1016" layer="20" curve="90"/>
<wire x1="-25.2763" y1="32.7589" x2="-25.2763" y2="-4.9911" width="0.0762" layer="20"/>
<wire x1="-25.2763" y1="-4.9911" x2="-23.2763" y2="-6.9911" width="0.0762" layer="20" curve="90"/>
<wire x1="-23.2763" y1="-6.9911" x2="35.2237" y2="-6.9911" width="0.0762" layer="20"/>
<wire x1="35.2237" y1="-6.9911" x2="37.2237" y2="-4.9911" width="0.0762" layer="20" curve="90"/>
<wire x1="37.2237" y1="-4.9911" x2="37.2237" y2="32.7589" width="0.0762" layer="20"/>
<wire x1="37.2237" y1="32.7589" x2="35.2237" y2="34.7589" width="0.0762" layer="20" curve="90"/>
<wire x1="35.2237" y1="34.7589" x2="15.7237" y2="34.7589" width="0.0762" layer="20"/>
<wire x1="15.7237" y1="34.7589" x2="14.2237" y2="36.2589" width="0.0762" layer="20" curve="-90"/>
<wire x1="14.2237" y1="36.2589" x2="14.2237" y2="48.7589" width="0.0762" layer="20"/>
<wire x1="14.2237" y1="48.7589" x2="7.6237" y2="48.7589" width="0.0762" layer="20" curve="180"/>
<wire x1="7.6237" y1="48.7589" x2="7.6237" y2="36.2589" width="0.0762" layer="20"/>
<wire x1="7.6237" y1="36.2589" x2="6.1237" y2="34.7589" width="0.0762" layer="20" curve="-90"/>
<wire x1="6.1237" y1="34.7589" x2="-23.2763" y2="34.7589" width="0.0762" layer="20"/>
<text>A0</text>
<text>A1</text>
<text>A2</text>
<text>A3</text>
<text>A4</text>
<text>A5</text>
<text>GND</text>
<text>VCC</text>
<text>SDA/D2</text>
<text>SCL/D3</text>
<text>D4</text>
<text>D5</text>
<text>D6</text>
<text>D7</text>
<text>GND</text>
<text>RX</text>
<text>TX</text>
<text>VCC</text>
<text>VCC</text>
<text>SCL</text>
<text>SDA</text>
<text>GND</text>
<text>VCC</text>
<text>RST</text>
<text>D+</text>
<text>D-</text>
<text>GND</text>
<text>GND</text>
<text>MISO</text>
<text>MOSI</text>
<text>SCK</text>
<text>RST</text>
<text>VCC</text>
<text>RGB_WS2812B</text>
<text>Ignite your full creativity.</text>
<text>DIY-shield for FP2</text>
<text>Rev. 1</text>
<text>news, information and more:</text>
<text>https://hackaday.io/project/28044-hacking-an-fairphone</text>
<text>DIY-shield for FP2</text>
<text>Rev. 1</text>
<text>Ready for hacking, making and much more !!</text>
<text>|</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="C0805K">
<description>&lt;b&gt;Ceramic Chip Capacitor KEMET 0805 Reflow solder&lt;/b&gt;&lt;p&gt;
Metric Code Size 2012</description>
</package>
<package name="1812">
<description>Multilayer SMD</description>
</package>
<package name="R0805W">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip, wave soldering</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X02_LOCK_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - Long Pads with Locking Footprint&lt;/h3&gt;
Pins are staggered by 0.005" from center to hold pins in place while soldering. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X06_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin with Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X06">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X06_LONGPADS_EXTRA_LONG">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin with extralong Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X04_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X08">
<description>&lt;h3&gt;Plated Through Hole -8 Pin&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
</packages>
</library>
<library name="jumper">
<description>&lt;b&gt;Jumpers&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SJ">
<description>&lt;b&gt;Solder jumper&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="connector_fairphone">
<packages>
<package name="BACKCONNECTOR">
</package>
</packages>
</library>
<library name="SparkFun-IC-Microcontroller">
<description>&lt;h3&gt;SparkFun Microcontrollers&lt;/h3&gt;
This library contains microcontrollers.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TQFP44">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X04_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - 4 Pin Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:4&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_04&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="crystal">
<description>&lt;b&gt;Crystals and Crystal Resonators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="CTS406">
<description>&lt;b&gt;Model 406 6.0x3.5mm Low Cost Surface Mount Crystal&lt;/b&gt;&lt;p&gt;
Source: 008-0260-0_E.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun LEDs&lt;/h3&gt;
This library contains discrete LEDs for illumination or indication, but no displays.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="WS2812BNEW">
<description>WS2812B (fat)

with larger pads; 
(Specifications: 
Pin count: 4
Size: 5.0 x 5.0 mm)</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="adafruit" package="C0805K" value="22pF">
<attribute name="NAME"/>
</element>
<element name="C2" library="adafruit" package="C0805K" value="22pF">
<attribute name="NAME"/>
</element>
<element name="C3" library="adafruit" package="C0805K" value="100nF">
<attribute name="NAME"/>
</element>
<element name="C5" library="adafruit" package="C0805K" value="1uF">
<attribute name="NAME"/>
</element>
<element name="C6" library="adafruit" package="C0805K" value="1uF">
<attribute name="NAME"/>
</element>
<element name="CHARGE_FP" library="SparkFun-Connectors" package="1X02_LOCK_LONGPADS" value=""/>
<element name="F1" library="adafruit" package="1812" value="1812_Fuse_PPTC">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ISP" library="SparkFun-Connectors" package="1X06_LONGPADS" value=""/>
<element name="J1" library="SparkFun-Connectors" package="1X06_LONGPADS_EXTRA_LONG" value="PROGRAMMING_PORT_USB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X04_LONGPADS" value="I2C">
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="D9" library="led" package="CHIP-LED0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D8" library="led" package="CHIP-LED0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D10" library="led" package="CHIP-LED0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="adafruit" package="R0805W" value="10k Ohm ">
<attribute name="NAME"/>
</element>
<element name="R10" library="adafruit" package="R0805W" value="350 Ohm"/>
<element name="R11" library="adafruit" package="R0805W" value="22 Ohm">
<attribute name="NAME"/>
</element>
<element name="R12" library="adafruit" package="R0805W" value="22 Ohm">
<attribute name="NAME"/>
</element>
<element name="R2" library="adafruit" package="R0805W" value="1kOhm">
<attribute name="NAME"/>
</element>
<element name="R3" library="adafruit" package="R0805W" value="22 Ohm">
<attribute name="NAME"/>
</element>
<element name="R4" library="adafruit" package="R0805W" value="22 Ohm">
<attribute name="NAME"/>
</element>
<element name="R8" library="adafruit" package="R0805W" value="350 Ohm"/>
<element name="R9" library="adafruit" package="R0805W" value="350 Ohm"/>
<element name="RST_J" library="jumper" package="SJ" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U$1" library="connector_fairphone" package="BACKCONNECTOR" value="FP2_Connector"/>
<element name="U$2" library="SparkFun-IC-Microcontroller" package="TQFP44" value="ATMEGA32U4">
<attribute name="PROD_ID" value="IC-11161"/>
</element>
<element name="Y1" library="crystal" package="CTS406" value="16MHz">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="VALUE"/>
</element>
<element name="SERIAL_PORT" library="SparkFun-Connectors" package="1X04_LONGPADS" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="PROD_ID" value="CONN-08438"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="1X08" value="">
<attribute name="PROD_ID" value="CONN-08438"/>
<attribute name="VALUE"/>
</element>
<element name="J7" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="J8" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="J9" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="J10" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="J11" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="J12" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="J13" library="SparkFun-Connectors" package="1X06" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="ANALOG_PORT" library="SparkFun-Connectors" package="1X04_LONGPADS" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-09696"/>
<attribute name="VALUE"/>
</element>
<element name="D11" library="led" package="CHIP-LED0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D12" library="led" package="CHIP-LED0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D13" library="led" package="CHIP-LED0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="adafruit" package="R0805W" value="350 Ohm"/>
<element name="R6" library="adafruit" package="R0805W" value="350 Ohm"/>
<element name="R7" library="adafruit" package="R0805W" value="350 Ohm"/>
<element name="D14" library="led" package="CHIP-LED0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D15" library="led" package="CHIP-LED0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R13" library="adafruit" package="R0805W" value="350 Ohm"/>
<element name="R14" library="adafruit" package="R0805W" value="350 Ohm"/>
<element name="R15" library="adafruit" package="R0805W" value="200 Ohm">
<attribute name="NAME"/>
</element>
<element name="RGB" library="SparkFun-LED" package="WS2812BNEW" value=""/>
<element name="R16" library="adafruit" package="R0805W" value="10 kOhm">
<attribute name="NAME"/>
</element>
<element name="R17" library="adafruit" package="R0805W" value="NTC">
<attribute name="VALUE"/>
</element>
<element name="TEMP_J2" library="jumper" package="SJ" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="U$2" pad="14"/>
<contactref element="U$2" pad="34"/>
<contactref element="U$2" pad="24"/>
<contactref element="U$2" pad="44"/>
<contactref element="R1" pad="1"/>
<contactref element="U$2" pad="2"/>
<contactref element="U$2" pad="7"/>
<contactref element="J1" pad="6"/>
<contactref element="J1" pad="12"/>
<contactref element="J1" pad="5"/>
<contactref element="J1" pad="11"/>
<contactref element="F1" pad="2"/>
<contactref element="J2" pad="4"/>
<contactref element="ISP" pad="6"/>
<contactref element="SERIAL_PORT" pad="1"/>
<contactref element="J5" pad="4"/>
<contactref element="J5" pad="3"/>
<contactref element="J5" pad="2"/>
<contactref element="J5" pad="1"/>
<contactref element="RGB" pad="1"/>
<contactref element="R16" pad="2"/>
</signal>
<signal name="GND">
<contactref element="U$1" pad="3"/>
<contactref element="U$2" pad="15"/>
<contactref element="U$2" pad="23"/>
<contactref element="U$2" pad="35"/>
<contactref element="U$2" pad="43"/>
<contactref element="U$2" pad="5"/>
<contactref element="C3" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="J1" pad="7"/>
<contactref element="J2" pad="1"/>
<contactref element="ISP" pad="1"/>
<contactref element="CHARGE_FP" pad="1"/>
<contactref element="D8" pad="C"/>
<contactref element="D9" pad="C"/>
<contactref element="D10" pad="C"/>
<contactref element="SERIAL_PORT" pad="4"/>
<contactref element="J5" pad="8"/>
<contactref element="J5" pad="7"/>
<contactref element="J5" pad="6"/>
<contactref element="J5" pad="5"/>
<contactref element="D12" pad="C"/>
<contactref element="D11" pad="C"/>
<contactref element="D13" pad="C"/>
<contactref element="D15" pad="C"/>
<contactref element="D14" pad="C"/>
<contactref element="RGB" pad="3"/>
<contactref element="R17" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="C3" pad="1"/>
<contactref element="U$2" pad="42"/>
</signal>
<signal name="D+">
<contactref element="U$2" pad="4"/>
<contactref element="R3" pad="2"/>
<contactref element="R12" pad="2"/>
</signal>
<signal name="D+_FP">
<contactref element="R3" pad="1"/>
<contactref element="U$1" pad="4"/>
</signal>
<signal name="D-_FP">
<contactref element="R4" pad="1"/>
<contactref element="U$1" pad="5"/>
</signal>
<signal name="RST">
<contactref element="RST_J" pad="1"/>
<contactref element="U$2" pad="13"/>
<contactref element="J1" pad="4"/>
<contactref element="J1" pad="10"/>
<contactref element="ISP" pad="5"/>
</signal>
<signal name="N$4">
<contactref element="RST_J" pad="2"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="C5" pad="1"/>
<contactref element="U$2" pad="6"/>
</signal>
<signal name="D-">
<contactref element="R4" pad="2"/>
<contactref element="U$2" pad="3"/>
<contactref element="R11" pad="2"/>
</signal>
<signal name="A2">
<contactref element="U$2" pad="38"/>
<contactref element="J8" pad="4"/>
<contactref element="ANALOG_PORT" pad="3"/>
</signal>
<signal name="D13">
<contactref element="U$2" pad="32"/>
<contactref element="J6" pad="3"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="A0">
<contactref element="U$2" pad="36"/>
<contactref element="J8" pad="6"/>
<contactref element="ANALOG_PORT" pad="1"/>
</signal>
<signal name="A1">
<contactref element="U$2" pad="37"/>
<contactref element="J8" pad="5"/>
<contactref element="ANALOG_PORT" pad="2"/>
</signal>
<signal name="D5">
<contactref element="U$2" pad="31"/>
<contactref element="J7" pad="3"/>
</signal>
<signal name="D10">
<contactref element="U$2" pad="30"/>
<contactref element="J6" pad="6"/>
<contactref element="R10" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="D10" pad="A"/>
<contactref element="R10" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="D8" pad="A"/>
<contactref element="R9" pad="2"/>
</signal>
<signal name="N$13">
<contactref element="D9" pad="A"/>
<contactref element="R8" pad="2"/>
</signal>
<signal name="D9">
<contactref element="U$2" pad="29"/>
<contactref element="R8" pad="1"/>
<contactref element="J6" pad="7"/>
</signal>
<signal name="D8">
<contactref element="U$2" pad="28"/>
<contactref element="R9" pad="1"/>
<contactref element="J6" pad="8"/>
</signal>
<signal name="D6">
<contactref element="U$2" pad="27"/>
<contactref element="J7" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="R2" pad="2"/>
<contactref element="U$2" pad="33"/>
</signal>
<signal name="N$14">
<contactref element="J1" pad="2"/>
<contactref element="J1" pad="8"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="J1" pad="3"/>
<contactref element="J1" pad="9"/>
<contactref element="R12" pad="1"/>
</signal>
<signal name="FP_VCC">
<contactref element="U$1" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="F1" pad="1"/>
</signal>
<signal name="SCL">
<contactref element="J2" pad="3"/>
<contactref element="U$2" pad="18"/>
<contactref element="J7" pad="5"/>
</signal>
<signal name="SDA">
<contactref element="J2" pad="2"/>
<contactref element="U$2" pad="19"/>
<contactref element="J7" pad="6"/>
</signal>
<signal name="SCK">
<contactref element="U$2" pad="9"/>
<contactref element="ISP" pad="4"/>
<contactref element="J6" pad="1"/>
<contactref element="R14" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="U$2" pad="10"/>
<contactref element="ISP" pad="3"/>
</signal>
<signal name="MISO">
<contactref element="U$2" pad="11"/>
<contactref element="ISP" pad="2"/>
<contactref element="J6" pad="2"/>
<contactref element="R13" pad="1"/>
</signal>
<signal name="CHRG">
<contactref element="U$1" pad="2"/>
<contactref element="CHARGE_FP" pad="2"/>
</signal>
<signal name="A3">
<contactref element="U$2" pad="39"/>
<contactref element="J8" pad="3"/>
<contactref element="ANALOG_PORT" pad="4"/>
</signal>
<signal name="A4">
<contactref element="U$2" pad="40"/>
<contactref element="J8" pad="2"/>
</signal>
<signal name="N$1">
<contactref element="U$2" pad="16"/>
<contactref element="Y1" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="U$2" pad="17"/>
<contactref element="Y1" pad="3"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="D4">
<contactref element="U$2" pad="25"/>
<contactref element="J7" pad="4"/>
</signal>
<signal name="D7">
<contactref element="U$2" pad="1"/>
<contactref element="J7" pad="1"/>
</signal>
<signal name="D11">
<contactref element="U$2" pad="12"/>
<contactref element="J6" pad="5"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="D12">
<contactref element="U$2" pad="26"/>
<contactref element="J6" pad="4"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="TX">
<contactref element="U$2" pad="21"/>
<contactref element="SERIAL_PORT" pad="2"/>
</signal>
<signal name="RX">
<contactref element="U$2" pad="20"/>
<contactref element="SERIAL_PORT" pad="3"/>
</signal>
<signal name="A5">
<contactref element="J8" pad="1"/>
<contactref element="U$2" pad="41"/>
<contactref element="TEMP_J2" pad="2"/>
</signal>
<signal name="N$5">
<contactref element="D13" pad="A"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="N$6">
<contactref element="D12" pad="A"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="D11" pad="A"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="D15" pad="A"/>
<contactref element="R14" pad="2"/>
</signal>
<signal name="N$17">
<contactref element="D14" pad="A"/>
<contactref element="R13" pad="2"/>
</signal>
<signal name="N$9">
<contactref element="U$2" pad="22"/>
</signal>
<signal name="DI1">
<contactref element="R15" pad="2"/>
<contactref element="RGB" pad="4"/>
</signal>
<signal name="N$18">
<contactref element="U$2" pad="8"/>
<contactref element="R15" pad="1"/>
</signal>
<signal name="N$19">
<contactref element="R16" pad="1"/>
<contactref element="R17" pad="2"/>
<contactref element="TEMP_J2" pad="1"/>
</signal>
<signal name="N$20">
</signal>
<signal name="N$21">
</signal>
</signals>
</board>
</drawing>
</eagle>
