<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="8.6.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="52.34" x2="0" y2="1" width="0" layer="20"/>
<wire x1="0" y1="1" x2="1" y2="0" width="0" layer="20" curve="90"/>
<wire x1="1" y1="0" x2="54.88" y2="0" width="0" layer="20"/>
<wire x1="54.88" y1="0" x2="55.88" y2="1" width="0" layer="20" curve="90"/>
<wire x1="55.88" y1="1" x2="55.88" y2="2.54" width="0" layer="20"/>
<wire x1="58.42" y1="5.08" x2="58.42" y2="37.846" width="0" layer="20"/>
<wire x1="54.356" y1="53.34" x2="1" y2="53.34" width="0" layer="20"/>
<wire x1="1" y1="53.34" x2="0" y2="52.34" width="0" layer="20" curve="90"/>
<hole x="3.81" y="2.54" drill="3.2"/>
<hole x="5.08" y="50.8" drill="3.2"/>
<hole x="55.88" y="35.56" drill="3.2"/>
<hole x="55.88" y="7.62" drill="3.2"/>
<wire x1="55.88" y1="2.54" x2="58.42" y2="5.08" width="0" layer="20"/>
<wire x1="54.356" y1="53.34" x2="55.88" y2="51.816" width="0" layer="20"/>
<wire x1="58.42" y1="37.846" x2="55.88" y2="40.386" width="0" layer="20"/>
<wire x1="55.88" y1="40.386" x2="55.88" y2="51.816" width="0" layer="20"/>
<text>IOREF</text>
<text>RESET</text>
<text>3V3</text>
<text>5V</text>
<text>GND</text>
<text>VIN</text>
<text>A0</text>
<text>A1</text>
<text>A2</text>
<text>A3</text>
<text>A4</text>
<text>A5</text>
<text>SCL</text>
<text>SDA</text>
<text>AREF</text>
<text>GND</text>
<text>13</text>
<text>12</text>
<text>11</text>
<text>10</text>
<text>9</text>
<text>8</text>
<text>7</text>
<text>6</text>
<text>5</text>
<text>4</text>
<text>3</text>
<text>2</text>
<text>1</text>
<text>0</text>
<text>TX</text>
<text>RX</text>
<text>NET</text>
<text>PWR</text>
<text>LTE</text>
<text>GPS</text>
<text>MICRO SIM</text>
<text>botletics</text>
<text>SIM7000 Shield</text>
<text>ALERT</text>
<text>Designed by Timothy Woo
Released under CC-BY-SA-4.0 license</text>
<text>SCL</text>
<text>SDA</text>
<text>GND</text>
<text>VCC</text>
<text>DTR</text>
<text>LED</text>
<text>v5</text>
<text>LOGIC</text>
<text>5V</text>
<text>GND</text>
<text>VCC</text>
<text>VCC</text>
<text>-VCC+</text>
<text>LOGIC</text>
<text>+</text>
<text>DONE</text>
<text>VBAT</text>
</plain>
<libraries>
<library name="TimWoo-Capacitors">
<packages>
<package name="0603-CAP-MARKED">
</package>
</packages>
</library>
<library name="TimWoo-Aesthetics">
<packages>
<package name="FIDUCIAL_1MM">
</package>
</packages>
</library>
<library name="TimWoo-IC">
<packages>
<package name="VQFN-14">
</package>
<package name="8-TSSOP">
</package>
</packages>
</library>
<library name="TimWoo-Resistors">
<packages>
<package name="0603-RES-MARKED">
</package>
<package name="RES_ARRAY_4X0603">
<description>&lt;b&gt;Chip Resistor Array&lt;/b&gt; size 4 × 0603&lt;p&gt;
convex termination - Phycomp Components&lt;br&gt;
Source: RS Components</description>
</package>
</packages>
</library>
<library name="TimWoo-Connectors">
<packages>
<package name="SMT-JUMPER_2_NO_SILK">
</package>
<package name="JST-2-SMD">
<description>2mm SMD side-entry connector. tDocu layer indicates the actual physical plastic housing. +/- indicate SparkFun standard batteries and wiring.</description>
</package>
</packages>
</library>
<library name="TimWoo-Diodes">
<packages>
<package name="SOD-323">
</package>
<package name="SOT-353">
</package>
</packages>
</library>
<library name="TimWoo-Capacitors">
<packages>
<package name="1210">
</package>
<package name="0603-CAP-MARKED">
</package>
</packages>
</library>
<library name="TimWoo-RF">
<packages>
<package name="SIM7000">
</package>
</packages>
</library>
<library name="TimWoo-LED">
<packages>
<package name="LED-0603-MARKED">
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-L">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo - Large - Silkscreen&lt;/h3&gt;
&lt;p&gt;Silkscreen logo for open-source hardware designs.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;OSHW_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="TimWoo-MOSFETs">
<packages>
<package name="SOT23-3">
</package>
</packages>
</library>
<library name="TimWoo-Connectors">
<packages>
<package name="1X10">
</package>
<package name="1X08">
</package>
<package name="1X06">
</package>
<package name="MICROSIM_SOCKET_PUSH-PULL">
</package>
<package name="USB-B-MICRO-SMD">
</package>
<package name="SMT-JUMPER_2_NC_TRACE_SILK">
</package>
<package name="1X04_ROUND">
</package>
<package name="U.FL">
</package>
<package name="SMT-JUMPER_3_1-NC_TRACE_SILK">
</package>
<package name="1X02">
</package>
</packages>
</library>
<library name="TimWoo-IC">
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt; - 5 Pin</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="FID2" library="TimWoo-Aesthetics" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="FID1" library="TimWoo-Aesthetics" package="FIDUCIAL_1MM" value="FIDUCIAL"/>
<element name="J8" library="TimWoo-Connectors" package="USB-B-MICRO-SMD" value="microUSB">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="U1" library="TimWoo-RF" package="SIM7000" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X1" library="TimWoo-Connectors" package="U.FL" value="LTE-uFL">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="X3" library="TimWoo-Connectors" package="MICROSIM_SOCKET_PUSH-PULL" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="TimWoo-Capacitors" package="0603-CAP-MARKED" value="0.22uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="TimWoo-Diodes" package="SOT-353" value="MSQA6V1W5T2G">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="TimWoo-Capacitors" package="0603-CAP-MARKED" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="TimWoo-Capacitors" package="0603-CAP-MARKED" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="TimWoo-Capacitors" package="1210" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="TimWoo-Capacitors" package="1210" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="TimWoo-Capacitors" package="0603-CAP-MARKED" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="TimWoo-Capacitors" package="0603-CAP-MARKED" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="TimWoo-IC" package="VQFN-14" value="TXB0104">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="TimWoo-Capacitors" package="0603-CAP-MARKED" value="33pF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="TimWoo-Diodes" package="SOD-323" value="250mA/100V">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-09646"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="TimWoo-Diodes" package="SOD-323" value="250mA/100V">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-09646"/>
<attribute name="VALUE"/>
</element>
<element name="X2" library="TimWoo-Connectors" package="U.FL" value="GNSS-uFL">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="TimWoo-Connectors" package="1X06" value="">
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="TimWoo-Connectors" package="1X08" value="">
<attribute name="PROD_ID" value="CONN-08438"/>
<attribute name="VALUE"/>
</element>
<element name="J5" library="TimWoo-Connectors" package="1X08" value="">
<attribute name="PROD_ID" value="CONN-08438"/>
<attribute name="VALUE"/>
</element>
<element name="J4" library="TimWoo-Connectors" package="1X10" value="">
<attribute name="PROD_ID" value="CONN-11563"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="TimWoo-Resistors" package="0603-RES-MARKED" value="2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="TimWoo-LED" package="LED-0603-MARKED" value="Green">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="TimWoo-Resistors" package="0603-RES-MARKED" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED3" library="TimWoo-LED" package="LED-0603-MARKED" value="Blue">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="TimWoo-IC" package="8-TSSOP" value="MCP9808">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="TimWoo-Resistors" package="0603-RES-MARKED" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="TimWoo-Resistors" package="0603-RES-MARKED" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="TimWoo-Resistors" package="0603-RES-MARKED" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="TimWoo-Capacitors" package="0603-CAP-MARKED" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="TimWoo-Resistors" package="RES_ARRAY_4X0603" value="10k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="TimWoo-Connectors" package="SMT-JUMPER_2_NO_SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-L" value="OSHW-LOGOL"/>
<element name="Q1" library="TimWoo-MOSFETs" package="SOT23-3" value="BSS138L"/>
<element name="Q2" library="TimWoo-MOSFETs" package="SOT23-3" value="BSS138L"/>
<element name="JP3" library="TimWoo-Connectors" package="SMT-JUMPER_2_NC_TRACE_SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J3" library="TimWoo-Connectors" package="1X04_ROUND" value="">
<attribute name="VALUE"/>
</element>
<element name="JP2" library="TimWoo-Connectors" package="SMT-JUMPER_2_NO_SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP4" library="TimWoo-Connectors" package="SMT-JUMPER_3_1-NC_TRACE_SILK" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J7" library="TimWoo-Connectors" package="1X02" value="V_logic">
<attribute name="VALUE"/>
</element>
<element name="IC1" library="TimWoo-IC" package="SOT23-5" value="MCP73831">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="IC-09995"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="TimWoo-Resistors" package="0603-RES-MARKED" value="2k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="TimWoo-Capacitors" package="0603-CAP-MARKED" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="TimWoo-Capacitors" package="0603-CAP-MARKED" value="4.7uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J6" library="TimWoo-Connectors" package="JST-2-SMD" value="LiPo">
<attribute name="PROD_ID" value="CONN-11443"/>
</element>
<element name="LED1" library="TimWoo-LED" package="LED-0603-MARKED" value="Green">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="TimWoo-Resistors" package="0603-RES-MARKED" value="1k">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="TimWoo-Capacitors" package="1210" value="100uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="J8" pad="GND"/>
<contactref element="J8" pad="SHIELD1"/>
<contactref element="J8" pad="SHIELD2"/>
<contactref element="J8" pad="SHIELD3"/>
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="17"/>
<contactref element="U1" pad="2"/>
<contactref element="U1" pad="39"/>
<contactref element="U1" pad="45"/>
<contactref element="U1" pad="46"/>
<contactref element="U1" pad="65"/>
<contactref element="U1" pad="64"/>
<contactref element="U1" pad="63"/>
<contactref element="U1" pad="62"/>
<contactref element="U1" pad="61"/>
<contactref element="U1" pad="59"/>
<contactref element="U1" pad="58"/>
<contactref element="U1" pad="54"/>
<contactref element="X1" pad="2"/>
<contactref element="X1" pad="1"/>
<contactref element="X3" pad="GND@4"/>
<contactref element="X3" pad="C5"/>
<contactref element="U1" pad="29"/>
<contactref element="D3" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C10" pad="2"/>
<contactref element="C11" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="IC2" pad="7"/>
<contactref element="IC2" pad="PAD"/>
<contactref element="X2" pad="2"/>
<contactref element="X2" pad="1"/>
<contactref element="J1" pad="3"/>
<contactref element="J1" pad="2"/>
<contactref element="J4" pad="7"/>
<contactref element="IC3" pad="4"/>
<contactref element="C5" pad="2"/>
<contactref element="R7" pad="1"/>
<contactref element="R7" pad="2"/>
<contactref element="R7" pad="3"/>
<contactref element="Q1" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="J3" pad="3"/>
<contactref element="J8" pad="SHIELD4"/>
<contactref element="X3" pad="GND@1"/>
<contactref element="X3" pad="GND@2"/>
<contactref element="X3" pad="GND@3"/>
<contactref element="X3" pad="GND@5"/>
<contactref element="X3" pad="GND@6"/>
<contactref element="J7" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="IC1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="J6" pad="1"/>
<contactref element="LED1" pad="C"/>
<contactref element="C12" pad="2"/>
</signal>
<signal name="VIN">
<contactref element="U1" pad="56"/>
<contactref element="U1" pad="57"/>
<contactref element="U1" pad="55"/>
<contactref element="C10" pad="1"/>
<contactref element="C11" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="C8" pad="1"/>
<contactref element="LED3" pad="A"/>
<contactref element="JP3" pad="1"/>
<contactref element="IC1" pad="3"/>
<contactref element="C2" pad="1"/>
<contactref element="J6" pad="2"/>
<contactref element="J1" pad="8"/>
<contactref element="C12" pad="1"/>
</signal>
<signal name="V_USB">
<contactref element="U1" pad="24"/>
<contactref element="J8" pad="VBUS"/>
</signal>
<signal name="D-">
<contactref element="J8" pad="D-"/>
<contactref element="U1" pad="28"/>
</signal>
<signal name="D+">
<contactref element="J8" pad="D+"/>
<contactref element="U1" pad="27"/>
</signal>
<signal name="1.8V">
<contactref element="U1" pad="15"/>
<contactref element="C3" pad="2"/>
<contactref element="IC2" pad="1"/>
<contactref element="IC2" pad="8"/>
</signal>
<signal name="RF_ANT">
<contactref element="U1" pad="60"/>
<contactref element="X1" pad="3"/>
</signal>
<signal name="SIM_VCC">
<contactref element="X3" pad="C1"/>
<contactref element="U1" pad="30"/>
<contactref element="D3" pad="1"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="SIM_RST">
<contactref element="X3" pad="C2"/>
<contactref element="U1" pad="33"/>
<contactref element="D3" pad="4"/>
</signal>
<signal name="SIM_CLK">
<contactref element="X3" pad="C3"/>
<contactref element="U1" pad="32"/>
<contactref element="D3" pad="3"/>
</signal>
<signal name="SIM_DATA">
<contactref element="X3" pad="C7"/>
<contactref element="U1" pad="31"/>
<contactref element="D3" pad="5"/>
</signal>
<signal name="PWR_STAT">
<contactref element="U1" pad="66"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="NRESET">
<contactref element="U1" pad="16"/>
<contactref element="D2" pad="A"/>
</signal>
<signal name="UC_RXD">
<contactref element="IC2" pad="12"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="UC_TXD">
<contactref element="IC2" pad="13"/>
<contactref element="J4" pad="4"/>
</signal>
<signal name="N$2">
<contactref element="D1" pad="A"/>
<contactref element="U1" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="C7" pad="2"/>
<contactref element="U1" pad="53"/>
</signal>
<signal name="N$3">
<contactref element="C7" pad="1"/>
<contactref element="X2" pad="3"/>
</signal>
<signal name="LTE_RST">
<contactref element="D2" pad="C"/>
<contactref element="J5" pad="8"/>
</signal>
<signal name="LTE_RI">
<contactref element="U1" pad="4"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="LTE_RXD">
<contactref element="IC2" pad="2"/>
<contactref element="U1" pad="10"/>
</signal>
<signal name="LTE_TXD">
<contactref element="IC2" pad="3"/>
<contactref element="U1" pad="9"/>
</signal>
<signal name="LTE_PWR">
<contactref element="D1" pad="C"/>
<contactref element="J5" pad="7"/>
</signal>
<signal name="NETLIGHT">
<contactref element="U1" pad="52"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="UC_RI">
<contactref element="IC2" pad="11"/>
<contactref element="J4" pad="2"/>
</signal>
<signal name="5V">
<contactref element="J1" pad="4"/>
<contactref element="JP4" pad="3"/>
<contactref element="IC1" pad="4"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="IC3" pad="1"/>
<contactref element="R6" pad="1"/>
<contactref element="J4" pad="9"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="SCL">
<contactref element="IC3" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="J4" pad="10"/>
<contactref element="J3" pad="1"/>
</signal>
<signal name="ALERT">
<contactref element="IC3" pad="3"/>
<contactref element="R3" pad="1"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="ADDR2">
<contactref element="IC3" pad="5"/>
<contactref element="R7" pad="8"/>
</signal>
<signal name="ADDR1">
<contactref element="IC3" pad="6"/>
<contactref element="R7" pad="7"/>
</signal>
<signal name="ADDR0">
<contactref element="IC3" pad="7"/>
<contactref element="R7" pad="6"/>
</signal>
<signal name="N$7">
<contactref element="J4" pad="5"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$4">
<contactref element="Q1" pad="3"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="R5" pad="2"/>
<contactref element="LED2" pad="C"/>
</signal>
<signal name="N$10">
<contactref element="Q2" pad="3"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="R8" pad="2"/>
<contactref element="LED3" pad="C"/>
</signal>
<signal name="LTE_DTR">
<contactref element="U1" pad="3"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="UC_DTR">
<contactref element="IC2" pad="10"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="JP3" pad="2"/>
<contactref element="LED2" pad="A"/>
</signal>
<signal name="N$8">
<contactref element="J4" pad="1"/>
<contactref element="JP2" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="R3" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="IC3" pad="8"/>
<contactref element="C5" pad="1"/>
<contactref element="J3" pad="4"/>
<contactref element="C4" pad="1"/>
<contactref element="IC2" pad="14"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="V_LOGIC">
<contactref element="JP4" pad="1"/>
<contactref element="J7" pad="2"/>
</signal>
<signal name="STAT">
<contactref element="IC1" pad="1"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="PROG">
<contactref element="IC1" pad="5"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$14">
<contactref element="R1" pad="2"/>
<contactref element="LED1" pad="A"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
