(kicad_pcb (version 4) (host pcbnew 4.0.6)
  (general
    (links 77)
    (no_connects 2)
    (area 55.804999 15.164999 166.445001 114.375001)
    (thickness 1.6)
    (drawings 4)
    (tracks 214)
    (zones 0)
    (modules 36)
    (nets 50)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (user_trace_width 0.25)
    (user_trace_width 0.5)
    (user_trace_width 0.75)
    (user_trace_width 1)
    (user_trace_width 2)
    (trace_clearance 0.2)
    (zone_clearance 0.508)
    (zone_45_only yes)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.15)
    (via_size 1.2)
    (via_drill 0.8)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (user_via 1.2 0.8)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.524 1.524)
    (pad_drill 0.762)
    (pad_to_mask_clearance 0.2)
    (aux_axis_origin 0 0)
    (visible_elements FFFFFF7F)
    (pcbplotparams
      (layerselection 0x00030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 1)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 /+5V)
  (net 2 /0v)
  (net 3 /+3.3V)
  (net 4 /Moisture)
  (net 5 /Temp_Humid)
  (net 6 /Water_level)
  (net 7 "Net-(D7-Pad1)")
  (net 8 /Fused_A)
  (net 9 /Water_Pump)
  (net 10 "Net-(D8-Pad1)")
  (net 11 /Exhaust)
  (net 12 "Net-(F1-Pad1)")
  (net 13 /Sense_active)
  (net 14 GNDPWR)
  (net 15 /Neutral)
  (net 16 /Mister)
  (net 17 /12V)
  (net 18 "Net-(R3-Pad1)")
  (net 19 "Net-(R3-Pad2)")
  (net 20 "Net-(R4-Pad1)")
  (net 21 "Net-(R4-Pad2)")
  (net 22 "Net-(R5-Pad1)")
  (net 23 "Net-(R5-Pad2)")
  (net 24 "Net-(R6-Pad2)")
  (net 25 "Net-(R7-Pad2)")
  (net 26 "Net-(R8-Pad2)")
  (net 27 "Net-(Q1-Pad1)")
  (net 28 "Net-(U1-Pad2)")
  (net 29 "Net-(U1-Pad3)")
  (net 30 "Net-(U1-Pad4)")
  (net 31 "Net-(U1-Pad5)")
  (net 32 "Net-(U1-Pad6)")
  (net 33 "Net-(U1-Pad7)")
  (net 34 "Net-(U1-Pad8)")
  (net 35 "Net-(U1-Pad9)")
  (net 36 "Net-(U1-Pad12)")
  (net 37 "Net-(U1-Pad13)")
  (net 38 "Net-(U1-Pad18)")
  (net 39 "Net-(U1-Pad19)")
  (net 40 "Net-(U1-Pad26)")
  (net 41 "Net-(U1-Pad27)")
  (net 42 "Net-(U1-Pad30)")
  (net 43 "Net-(U2-Pad5)")
  (net 44 "Net-(U2-Pad3)")
  (net 45 "Net-(U3-Pad5)")
  (net 46 "Net-(U3-Pad3)")
  (net 47 "Net-(U4-Pad2)")
  (net 48 "Net-(U4-Pad5)")
  (net 49 "Net-(J7-Pad2)")
  (net_class Default "This is the default net class."
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 1.2)
    (via_drill 0.8)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net /+3.3V)
    (add_net /+5V)
    (add_net /0v)
    (add_net /12V)
    (add_net /Exhaust)
    (add_net /Fused_A)
    (add_net /Mister)
    (add_net /Moisture)
    (add_net /Neutral)
    (add_net /Sense_active)
    (add_net /Temp_Humid)
    (add_net /Water_Pump)
    (add_net /Water_level)
    (add_net GNDPWR)
    (add_net "Net-(D7-Pad1)")
    (add_net "Net-(D8-Pad1)")
    (add_net "Net-(F1-Pad1)")
    (add_net "Net-(J7-Pad2)")
    (add_net "Net-(Q1-Pad1)")
    (add_net "Net-(R3-Pad1)")
    (add_net "Net-(R3-Pad2)")
    (add_net "Net-(R4-Pad1)")
    (add_net "Net-(R4-Pad2)")
    (add_net "Net-(R5-Pad1)")
    (add_net "Net-(R5-Pad2)")
    (add_net "Net-(R6-Pad2)")
    (add_net "Net-(R7-Pad2)")
    (add_net "Net-(R8-Pad2)")
    (add_net "Net-(U1-Pad12)")
    (add_net "Net-(U1-Pad13)")
    (add_net "Net-(U1-Pad18)")
    (add_net "Net-(U1-Pad19)")
    (add_net "Net-(U1-Pad2)")
    (add_net "Net-(U1-Pad26)")
    (add_net "Net-(U1-Pad27)")
    (add_net "Net-(U1-Pad3)")
    (add_net "Net-(U1-Pad30)")
    (add_net "Net-(U1-Pad4)")
    (add_net "Net-(U1-Pad5)")
    (add_net "Net-(U1-Pad6)")
    (add_net "Net-(U1-Pad7)")
    (add_net "Net-(U1-Pad8)")
    (add_net "Net-(U1-Pad9)")
    (add_net "Net-(U2-Pad3)")
    (add_net "Net-(U2-Pad5)")
    (add_net "Net-(U3-Pad3)")
    (add_net "Net-(U3-Pad5)")
    (add_net "Net-(U4-Pad2)")
    (add_net "Net-(U4-Pad5)")
  )
  (net_class bigger ""
    (clearance 0.2)
    (trace_width 0.5)
    (via_dia 1.2)
    (via_drill 0.8)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
  )
  (module Capacitors_THT:CP_Radial_D10.0mm_P5.00mm (layer F.Cu) (tedit 597BC7C2)
    (at 102.87 107.95 90)
    (descr "CP, Radial series, Radial, pin pitch=5.00mm, , diameter=10mm, Electrolytic Capacitor")
    (tags "CP Radial series Radial pin pitch 5.00mm  diameter 10mm Electrolytic Capacitor")
    (fp_text reference C1 (at 2.5 -6.31 90) (layer F.SilkS))
    (fp_text value 100uF (at 2.5 6.31 90) (layer F.Fab))
    (fp_text user %R (at 2.5 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 1 /+5V))
    (pad 2 thru_hole circle (at 5 0 90) (size 2 2) (drill 1) (layers *.Cu *.Mask)
      (net 2 /0v))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/CP_Radial_D10.0mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_THT:C_Disc_D5.0mm_W2.5mm_P5.00mm (layer F.Cu) (tedit 5AF83A06)
    (at 59.69 99.06 90)
    (descr "C, Disc series, Radial, pin pitch=5.00mm, , diameter*width=5*2.5mm^2, Capacitor, http://cdn-reichelt.de/documents/datenblatt/B300/DS_KERKO_TC.pdf")
    (tags "C Disc series Radial pin pitch 5.00mm  diameter 5mm width 2.5mm Capacitor")
    (fp_text reference C2 (at 2.5 -2.56 90) (layer F.SilkS))
    (fp_text value 100n (at 2.5 2.56 90) (layer F.Fab))
    (fp_text user %R (at 2.54 3.81 90) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 1 /+5V))
    (pad 2 thru_hole circle (at 5 0 90) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /0v))
    (model ${KISYS3DMOD}/Capacitors_THT.3dshapes/C_Disc_D5.0mm_W2.5mm_P5.00mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_MiniMELF_Handsoldering (layer B.Cu) (tedit 5905D919)
    (at 67.31 38.1)
    (descr "Diode Mini-MELF Handsoldering")
    (tags "Diode Mini-MELF Handsoldering")
    (attr smd)
    (fp_text reference D1 (at 0 1.75) (layer B.SilkS))
    (fp_text value D (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -2.75 0) (size 3.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 3 /+3.3V))
    (pad 2 smd rect (at 2.75 0) (size 3.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 /Moisture))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_MiniMELF_Handsoldering (layer B.Cu) (tedit 5905D919)
    (at 67.31 43.18 180)
    (descr "Diode Mini-MELF Handsoldering")
    (tags "Diode Mini-MELF Handsoldering")
    (attr smd)
    (fp_text reference D2 (at 0 1.75 180) (layer B.SilkS))
    (fp_text value D (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -2.75 0 180) (size 3.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 4 /Moisture))
    (pad 2 smd rect (at 2.75 0 180) (size 3.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 2 /0v))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_MiniMELF_Handsoldering (layer B.Cu) (tedit 5905D919)
    (at 80.01 38.1 180)
    (descr "Diode Mini-MELF Handsoldering")
    (tags "Diode Mini-MELF Handsoldering")
    (attr smd)
    (fp_text reference D3 (at 0 1.75 180) (layer B.SilkS))
    (fp_text value D (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -2.75 0 180) (size 3.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 3 /+3.3V))
    (pad 2 smd rect (at 2.75 0 180) (size 3.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 5 /Temp_Humid))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_MiniMELF_Handsoldering (layer B.Cu) (tedit 5905D919)
    (at 80.01 43.18)
    (descr "Diode Mini-MELF Handsoldering")
    (tags "Diode Mini-MELF Handsoldering")
    (attr smd)
    (fp_text reference D4 (at 0 1.75) (layer B.SilkS))
    (fp_text value D (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -2.75 0) (size 3.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 5 /Temp_Humid))
    (pad 2 smd rect (at 2.75 0) (size 3.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 2 /0v))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_MiniMELF_Handsoldering (layer B.Cu) (tedit 5AF6A131)
    (at 91.44 38.1)
    (descr "Diode Mini-MELF Handsoldering")
    (tags "Diode Mini-MELF Handsoldering")
    (attr smd)
    (fp_text reference D5 (at 0 1.75) (layer B.SilkS))
    (fp_text value D (at 0 -1.75 270) (layer B.Fab))
    (fp_text user %R (at 0 1.75) (layer B.Fab))
    (pad 1 smd rect (at -2.75 0) (size 3.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 3 /+3.3V))
    (pad 2 smd rect (at 2.75 0) (size 3.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 6 /Water_level))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Diodes_SMD:D_MiniMELF_Handsoldering (layer B.Cu) (tedit 5905D919)
    (at 91.44 43.18 180)
    (descr "Diode Mini-MELF Handsoldering")
    (tags "Diode Mini-MELF Handsoldering")
    (attr smd)
    (fp_text reference D6 (at 0 1.75 180) (layer B.SilkS))
    (fp_text value D (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 1.75 180) (layer B.Fab))
    (pad 1 smd rect (at -2.75 0 180) (size 3.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 6 /Water_level))
    (pad 2 smd rect (at 2.75 0 180) (size 3.3 1.7) (layers B.Cu B.Paste B.Mask)
      (net 2 /0v))
    (model ${KISYS3DMOD}/Diodes_SMD.3dshapes/D_MiniMELF.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 58CE52AD)
    (at 144.78 25.4 90)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference D7 (at 2.54 -3.62 90) (layer F.SilkS))
    (fp_text value T1235T-81 (at 2.54 3.92 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 7 "Net-(D7-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 8 /Fused_A))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 9 /Water_Pump))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 58CE52AD)
    (at 144.78 44.45 90)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference D8 (at 2.54 -3.62 90) (layer F.SilkS))
    (fp_text value T1235T-81 (at 2.54 3.92 90) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 10 "Net-(D8-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 8 /Fused_A))
    (pad 3 thru_hole oval (at 5.08 0 90) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 11 /Exhaust))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Fuse_Holders_and_Fuses:Fuseholder5x20_horiz_open_universal_Type-III (layer F.Cu) (tedit 0)
    (at 138.43 76.2 90)
    (descr "Fuseholder, 5x20, open, horizontal, Type-III, universal, inline, lateral,")
    (tags "Fuseholder 5x20 open horizontal Type-III universal inline lateral Sicherungshalter offen ")
    (fp_text reference F1 (at 10.2 -5.08 90) (layer F.SilkS))
    (fp_text value Fuse (at 12.74 6.35 90) (layer F.Fab))
    (pad 2 thru_hole circle (at 15.32 0 90) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 8 /Fused_A))
    (pad 2 thru_hole circle (at 20.4 0 90) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 8 /Fused_A))
    (pad 1 thru_hole circle (at 5.08 0 90) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 12 "Net-(F1-Pad1)"))
    (pad 1 thru_hole circle (at 0 0 90) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 12 "Net-(F1-Pad1)"))
    (pad 2 thru_hole circle (at 17.86 -2.54 90) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 8 /Fused_A))
    (pad 2 thru_hole circle (at 17.86 2.54 90) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 8 /Fused_A))
    (pad 1 thru_hole circle (at 2.54 -2.54 90) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 12 "Net-(F1-Pad1)"))
    (pad 1 thru_hole circle (at 2.54 2.54 90) (size 2.35 2.35) (drill 1.35) (layers *.Cu *.Mask)
      (net 12 "Net-(F1-Pad1)"))
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch1.27mm (layer F.Cu) (tedit 59650535)
    (at 64.77 20.32 90)
    (descr "Through hole straight pin header, 1x03, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x03 1.27mm single row")
    (fp_text reference J1 (at 0 -1.695 90) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 4.235 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 /0v))
    (pad 2 thru_hole oval (at 0 1.27 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 4 /Moisture))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 13 /Sense_active))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02_Pitch1.27mm (layer F.Cu) (tedit 5AF83A90)
    (at 91.44 20.32 90)
    (descr "Through hole straight pin header, 1x02, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x02 1.27mm single row")
    (fp_text reference J2 (at 0 -1.695 90) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 2.965 90) (layer F.Fab))
    (fp_text user %R (at -2.54 0 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 /0v))
    (pad 2 thru_hole oval (at 0 1.27 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 6 /Water_level))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x02_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x03_Pitch1.27mm (layer F.Cu) (tedit 59650535)
    (at 77.47 20.32 90)
    (descr "Through hole straight pin header, 1x03, 1.27mm pitch, single row")
    (tags "Through hole pin header THT 1x03 1.27mm single row")
    (fp_text reference J3 (at 0 -1.695 90) (layer F.SilkS))
    (fp_text value CONN_01X03 (at 0 4.235 90) (layer F.Fab))
    (fp_text user %R (at 0 1.27 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 2 /0v))
    (pad 2 thru_hole oval (at 0 1.27 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 5 /Temp_Humid))
    (pad 3 thru_hole oval (at 0 2.54 90) (size 1 1) (drill 0.65) (layers *.Cu *.Mask)
      (net 3 /+3.3V))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x03_Pitch1.27mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Phoenix:PhoenixContact_MC-G_03x5.08mm_Angled (layer F.Cu) (tedit 59566E61)
    (at 156.21 76.2 90)
    (descr "Generic Phoenix Contact connector footprint for series: MC-G; number of pins: 03; pin pitch: 5.08mm; Angled || order number: 1836192 8A 320V")
    (tags "phoenix_contact connector MC_01x03_G_5.08mm")
    (fp_text reference J4 (at 5.08 -2.8 90) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x03 (at 5.08 9 90) (layer F.Fab))
    (fp_text user %R (at 5.08 3 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 14 GNDPWR))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 15 /Neutral))
    (pad 3 thru_hole oval (at 10.16 0 90) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 12 "Net-(F1-Pad1)"))
    (model ${KISYS3DMOD}/Connectors_Phoenix.3dshapes/PhoenixContact_MC-G_03x5.08mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Phoenix:PhoenixContact_MSTBA-G_02x5.08mm_Angled (layer F.Cu) (tedit 59566E5C)
    (at 156.21 29.21 90)
    (descr "Generic Phoenix Contact connector footprint for series: MSTBA-G; number of pins: 02; pin pitch: 5.08mm; Angled || order number: 1757242 12A || order number: 1923869 16A (HC)")
    (tags "phoenix_contact connector MSTBA_01x02_G_5.08mm")
    (fp_text reference J5 (at 3.54 -3 90) (layer F.SilkS))
    (fp_text value Fan (at 2.54 11 90) (layer F.Fab))
    (fp_text user %R (at 3.54 3 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 /Neutral))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 9 /Water_Pump))
    (model ${KISYS3DMOD}/Connectors_Phoenix.3dshapes/PhoenixContact_MSTBA-G_02x5.08mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Phoenix:PhoenixContact_MSTBA-G_02x5.08mm_Angled (layer F.Cu) (tedit 59566E5C)
    (at 156.21 48.26 90)
    (descr "Generic Phoenix Contact connector footprint for series: MSTBA-G; number of pins: 02; pin pitch: 5.08mm; Angled || order number: 1757242 12A || order number: 1923869 16A (HC)")
    (tags "phoenix_contact connector MSTBA_01x02_G_5.08mm")
    (fp_text reference J6 (at 3.54 -3 90) (layer F.SilkS))
    (fp_text value Pump (at 2.54 11 90) (layer F.Fab))
    (fp_text user %R (at 3.54 3 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 15 /Neutral))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 2.08 3.6) (drill 1.4) (layers *.Cu *.Mask)
      (net 11 /Exhaust))
    (model ${KISYS3DMOD}/Connectors_Phoenix.3dshapes/PhoenixContact_MSTBA-G_02x5.08mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Connectors_Phoenix:PhoenixContact_MC-G_03x5.08mm_Angled (layer F.Cu) (tedit 59566E61)
    (at 156.21 107.95 90)
    (descr "Generic Phoenix Contact connector footprint for series: MC-G; number of pins: 03; pin pitch: 5.08mm; Angled || order number: 1836192 8A 320V")
    (tags "phoenix_contact connector MC_01x03_G_5.08mm")
    (fp_text reference J7 (at 5.08 -2.8 90) (layer F.SilkS))
    (fp_text value Screw_Terminal_1x03 (at 5.08 9 90) (layer F.Fab))
    (fp_text user %R (at 5.08 3 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 16 /Mister))
    (pad 2 thru_hole oval (at 5.08 0 90) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 49 "Net-(J7-Pad2)"))
    (pad 3 thru_hole oval (at 10.16 0 90) (size 1.8 3.6) (drill 1.2) (layers *.Cu *.Mask)
      (net 17 /12V))
    (model ${KISYS3DMOD}/Connectors_Phoenix.3dshapes/PhoenixContact_MC-G_03x5.08mm_Angled.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 91.44 25.4)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 1.7) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.75) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 /+3.3V))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 6 /Water_level))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 80.01 25.4 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 1.7 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 3 /+3.3V))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 5 /Temp_Humid))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5AF82AD8)
    (at 104.14 20.32 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 1.7 180) (layer B.SilkS))
    (fp_text value 270R (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at -1.27 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 18 "Net-(R3-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 19 "Net-(R3-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5AF82AEA)
    (at 104.14 39.37 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R4 (at 0 1.7 180) (layer B.SilkS))
    (fp_text value 270R (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at -3.81 -5.08 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 20 "Net-(R4-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 21 "Net-(R4-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 100.33 86.36 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R5 (at 0 1.7 180) (layer B.SilkS))
    (fp_text value 270R (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(R5-Pad1)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 23 "Net-(R5-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 130.81 21.59 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R6 (at 0 1.7 180) (layer B.SilkS))
    (fp_text value 330R (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 8 /Fused_A))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 24 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5AF82AFC)
    (at 129.54 39.37 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R7 (at 0 1.7 180) (layer B.SilkS))
    (fp_text value 330R (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 1.27 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 8 /Fused_A))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 25 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 135.89 97.79 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R8 (at 0 1.7 180) (layer B.SilkS))
    (fp_text value 1K8 (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 17 /12V))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(R8-Pad2)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 124.46 102.87 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R9 (at 0 1.7 180) (layer B.SilkS))
    (fp_text value 10K (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 49 "Net-(J7-Pad2)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(Q1-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 5AF82B11)
    (at 137.16 17.78 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R10 (at 0 1.7 180) (layer B.SilkS))
    (fp_text value 330R (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 9 /Water_Pump))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 7 "Net-(D7-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 58E0A804)
    (at 143.51 34.29 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R11 (at 0 1.7 180) (layer B.SilkS))
    (fp_text value 330R (at 0 -1.75 180) (layer B.Fab))
    (fp_text user %R (at 0 0 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 11 /Exhaust))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 10 "Net-(D8-Pad1)"))
    (model ${KISYS3DMOD}/Resistors_SMD.3dshapes/R_0805.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module "ESP8266:NodeMCU1.0(12-E)" (layer F.Cu) (tedit 58B08E61)
    (at 80.01 83.82)
    (fp_text reference U1 (at 0 0) (layer F.SilkS))
    (fp_text value "NodeMCU_1.0_(ESP-12E)" (at 0 -29.21) (layer F.Fab))
    (fp_text user VIN (at -11.43 15.24) (layer F.SilkS))
    (fp_text user G (at -11.43 12.7) (layer F.SilkS))
    (fp_text user RST (at -11.43 10.16) (layer F.SilkS))
    (fp_text user EN (at -11.43 7.62) (layer F.SilkS))
    (fp_text user 3V (at -11.43 5.08) (layer F.SilkS))
    (fp_text user G (at -11.43 2.54) (layer F.SilkS))
    (fp_text user SK (at -11.43 0) (layer F.SilkS))
    (fp_text user SO (at -11.43 -2.54) (layer F.SilkS))
    (fp_text user SC (at -11.43 -5.08) (layer F.SilkS))
    (fp_text user S1 (at -11.43 -7.62) (layer F.SilkS))
    (fp_text user S2 (at -11.43 -10.16) (layer F.SilkS))
    (fp_text user S3 (at -11.43 -12.7) (layer F.SilkS))
    (fp_text user VU (at -11.43 -15.24) (layer F.SilkS))
    (fp_text user G (at -11.43 -17.78) (layer F.SilkS))
    (fp_text user A0 (at -11.43 -20.32) (layer F.SilkS))
    (fp_text user 3V (at 11.43 15.24) (layer F.SilkS))
    (fp_text user G (at 11.43 12.7) (layer F.SilkS))
    (fp_text user TX (at 11.43 10.16) (layer F.SilkS))
    (fp_text user RX (at 11.43 7.62) (layer F.SilkS))
    (fp_text user D8 (at 11.43 5.08) (layer F.SilkS))
    (fp_text user D7 (at 11.43 2.54) (layer F.SilkS))
    (fp_text user D6 (at 11.43 0) (layer F.SilkS))
    (fp_text user D5 (at 11.43 -2.54) (layer F.SilkS))
    (fp_text user G (at 11.43 -5.08) (layer F.SilkS))
    (fp_text user 3V (at 11.43 -7.62) (layer F.SilkS))
    (fp_text user D4 (at 11.43 -10.16) (layer F.SilkS))
    (fp_text user D3 (at 11.43 -12.7) (layer F.SilkS))
    (fp_text user D2 (at 11.43 -15.24) (layer F.SilkS))
    (fp_text user D1 (at 11.43 -17.78) (layer F.SilkS))
    (fp_text user D0 (at 11.43 -20.32) (layer F.SilkS))
    (pad 1 thru_hole circle (at -13.97 -20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 4 /Moisture))
    (pad 2 thru_hole circle (at -13.97 -17.78) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 28 "Net-(U1-Pad2)"))
    (pad 3 thru_hole circle (at -13.97 -15.24) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 29 "Net-(U1-Pad3)"))
    (pad 4 thru_hole circle (at -13.97 -12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 30 "Net-(U1-Pad4)"))
    (pad 5 thru_hole circle (at -13.97 -10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 31 "Net-(U1-Pad5)"))
    (pad 6 thru_hole circle (at -13.97 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 32 "Net-(U1-Pad6)"))
    (pad 7 thru_hole circle (at -13.97 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 33 "Net-(U1-Pad7)"))
    (pad 8 thru_hole circle (at -13.97 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 34 "Net-(U1-Pad8)"))
    (pad 9 thru_hole circle (at -13.97 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 35 "Net-(U1-Pad9)"))
    (pad 10 thru_hole circle (at -13.97 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 /0v))
    (pad 11 thru_hole circle (at -13.97 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 3 /+3.3V))
    (pad 12 thru_hole circle (at -13.97 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 36 "Net-(U1-Pad12)"))
    (pad 13 thru_hole circle (at -13.97 10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 37 "Net-(U1-Pad13)"))
    (pad 14 thru_hole circle (at -13.97 12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 /0v))
    (pad 15 thru_hole circle (at -13.97 15.24) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 1 /+5V))
    (pad 16 thru_hole circle (at 13.97 15.24) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 3 /+3.3V))
    (pad 17 thru_hole circle (at 13.97 12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 /0v))
    (pad 18 thru_hole circle (at 13.97 10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 38 "Net-(U1-Pad18)"))
    (pad 19 thru_hole circle (at 13.97 7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 39 "Net-(U1-Pad19)"))
    (pad 20 thru_hole circle (at 13.97 5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 13 /Sense_active))
    (pad 21 thru_hole circle (at 13.97 2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 23 "Net-(R5-Pad2)"))
    (pad 22 thru_hole circle (at 13.97 0) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 21 "Net-(R4-Pad2)"))
    (pad 23 thru_hole circle (at 13.97 -2.54) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 19 "Net-(R3-Pad2)"))
    (pad 24 thru_hole circle (at 13.97 -5.08) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 2 /0v))
    (pad 25 thru_hole circle (at 13.97 -7.62) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 3 /+3.3V))
    (pad 26 thru_hole circle (at 13.97 -10.16) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 40 "Net-(U1-Pad26)"))
    (pad 27 thru_hole circle (at 13.97 -12.7) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 41 "Net-(U1-Pad27)"))
    (pad 28 thru_hole circle (at 13.97 -15.24) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 5 /Temp_Humid))
    (pad 29 thru_hole circle (at 13.97 -17.78) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 6 /Water_level))
    (pad 30 thru_hole circle (at 13.97 -20.32) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask F.SilkS)
      (net 42 "Net-(U1-Pad30)"))
  )
  (module Housings_DIP:DIP-6_W7.62mm (layer F.Cu) (tedit 59C78D6B)
    (at 110.49 20.32)
    (descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U2 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value MOC3042M (at 3.81 7.41) (layer F.Fab))
    (fp_text user %R (at 3.81 2.54) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 18 "Net-(R3-Pad1)"))
    (pad 4 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 7 "Net-(D7-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /0v))
    (pad 5 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 43 "Net-(U2-Pad5)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 44 "Net-(U2-Pad3)"))
    (pad 6 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 24 "Net-(R6-Pad2)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-6_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-6_W7.62mm (layer F.Cu) (tedit 5AF83382)
    (at 110.49 39.37)
    (descr "6-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils)")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil")
    (fp_text reference U3 (at 3.81 -2.33) (layer F.SilkS))
    (fp_text value MOC3042M (at 3.81 7.41) (layer F.Fab))
    (fp_text user %R (at 3.81 5.08) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 20 "Net-(R4-Pad1)"))
    (pad 4 thru_hole oval (at 7.62 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 10 "Net-(D8-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 2 /0v))
    (pad 5 thru_hole oval (at 7.62 2.54) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 45 "Net-(U3-Pad5)"))
    (pad 3 thru_hole oval (at 0 5.08) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 46 "Net-(U3-Pad3)"))
    (pad 6 thru_hole oval (at 7.62 0) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask)
      (net 25 "Net-(R7-Pad2)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-6_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Housings_DIP:DIP-6_W8.89mm_SMDSocket_LongPads (layer B.Cu) (tedit 59C78D6B)
    (at 121.92 95.25)
    (descr "6-lead though-hole mounted DIP package, row spacing 8.89 mm (350 mils), SMDSocket, LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 8.89mm 350mil SMDSocket LongPads")
    (attr smd)
    (fp_text reference U4 (at 0 4.87) (layer B.SilkS))
    (fp_text value TLP185 (at 0 -4.87) (layer B.Fab))
    (fp_text user %R (at 0 0) (layer B.Fab))
    (pad 1 smd rect (at -4.445 2.54) (size 3.1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 22 "Net-(R5-Pad1)"))
    (pad 4 smd rect (at 4.445 -2.54) (size 3.1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 27 "Net-(Q1-Pad1)"))
    (pad 2 smd rect (at -4.445 0) (size 3.1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 47 "Net-(U4-Pad2)"))
    (pad 5 smd rect (at 4.445 0) (size 3.1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 48 "Net-(U4-Pad5)"))
    (pad 3 smd rect (at -4.445 -2.54) (size 3.1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 2 /0v))
    (pad 6 smd rect (at 4.445 2.54) (size 3.1 1.6) (layers B.Cu B.Paste B.Mask)
      (net 26 "Net-(R8-Pad2)"))
    (model ${KISYS3DMOD}/Housings_DIP.3dshapes/DIP-6_W8.89mm_SMDSocket.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-220-3_Vertical (layer F.Cu) (tedit 58CE52AD)
    (at 134.62 107.95 180)
    (descr "TO-220-3, Vertical, RM 2.54mm")
    (tags "TO-220-3 Vertical RM 2.54mm")
    (fp_text reference Q1 (at 2.54 -3.62 180) (layer F.SilkS))
    (fp_text value IRF540N (at 2.54 3.92 180) (layer F.Fab))
    (fp_text user %R (at 2.54 -3.62 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 27 "Net-(Q1-Pad1)"))
    (pad 2 thru_hole oval (at 2.54 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 16 /Mister))
    (pad 3 thru_hole oval (at 5.08 0 180) (size 1.8 1.8) (drill 1) (layers *.Cu *.Mask)
      (net 49 "Net-(J7-Pad2)"))
    (model ${KISYS3DMOD}/TO_SOT_Packages_THT.3dshapes/TO-220-3_Vertical.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 0.393701 0.393701 0.393701))
      (rotate (xyz 0 0 0))
    )
  )
  (module Bernies:YS-12V450A (layer F.Cu) (tedit 5AF82722)
    (at 106.68 82.55)
    (fp_text reference PSU1 (at 7.62 1.27) (layer F.SilkS))
    (fp_text value 5VPSU (at 5.08 -30.48) (layer F.Fab))
    (fp_text user 0V (at 12.7 1.27) (layer F.SilkS))
    (fp_text user +5 (at 2.54 1.27) (layer F.SilkS))
    (fp_text user A (at 12.7 -30.48) (layer F.SilkS))
    (fp_text user N (at 17.78 -30.48) (layer F.SilkS))
    (pad 1 thru_hole circle (at 2.54 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 1 /+5V))
    (pad 2 thru_hole circle (at 12.7 -1.27) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 2 /0v))
    (pad 3 thru_hole circle (at 12.7 -27.94) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 8 /Fused_A))
    (pad 4 thru_hole circle (at 17.78 -27.94) (size 1.524 1.524) (drill 0.762) (layers *.Cu *.Mask)
      (net 15 /Neutral))
  )
  (module Pin_Headers:Pin_Header_Straight_1x01_Pitch2.54mm (layer F.Cu) (tedit 59650532)
    (at 160.02 83.82)
    (descr "Through hole straight pin header, 1x01, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x01 2.54mm single row")
    (fp_text reference J8 (at 0 -2.33) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 2.33) (layer F.Fab))
    (fp_text user %R (at 0 0 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask)
      (net 14 GNDPWR))
    (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Straight_1x01_Pitch2.54mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_line (start 55.88 15.24) (end 55.88 114.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166.37 15.24) (end 55.88 15.24) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 166.37 114.3) (end 166.37 15.24) (angle 90) (layer Edge.Cuts) (width 0.15))
  (gr_line (start 55.88 114.3) (end 166.37 114.3) (angle 90) (layer Edge.Cuts) (width 0.15))
  (zone (net 2) (net_name /0v) (layer B.Cu) (hatch edge 0.508)
    (connect_pads (clearance 0.508))
    (min_thickness 0.254)
    (fill yes (arc_segments 16) (thermal_gap 0.508) (thermal_bridge_width 0.508))
    (polygon
      (pts
        (xy 110.49 71.12) (xy 111.76 72.39) (xy 121.92 72.39) (xy 124.46 74.93) (xy 124.46 86.36)
        (xy 118.11 92.71) (xy 118.11 114.3) (xy 55.88 114.3) (xy 55.88 63.5) (xy 96.52 63.5)
        (xy 96.52 49.53) (xy 55.88 49.53) (xy 55.88 15.24) (xy 110.49 15.24)
      )
    )
  )
)
