(module Badgelife-Shitty-2x2 (layer F.Cu) (tedit 5AAC5583)
  (descr "Through hole angled pin header, 2x02, 2.54mm pitch, 6mm pin length, double rows")
  (tags "Through hole angled pin header THT 2x02 2.54mm double row")
  (fp_text reference J2 (at 0 0) (layer F.Fab))
  (fp_text value "#badgelife" (at 0 4.2) (layer F.Fab))
  (fp_text user SDA (at 2.54 -2.54) (layer B.SilkS))
  (fp_text user SCL (at 2.54 2.54) (layer B.SilkS))
  (fp_text user GND (at -2.54 2.54) (layer B.SilkS))
  (fp_text user VCC (at -2.54 -2.54) (layer B.SilkS))
  (pad 4 thru_hole circle (at 1.27 -1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 3 thru_hole oval (at 1.27 1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 1 thru_hole oval (at -1.27 -1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (pad 2 thru_hole oval (at -1.27 1.27) (size 1.7 1.7) (drill 1) (layers *.Cu *.Mask))
  (model ${KISYS3DMOD}/Pin_Headers.3dshapes/Pin_Header_Angled_2x02_Pitch2.54mm.wrl
    (at (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
