(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 32)
    (no_connects 0)
    (area 89.191667 96.175 152.008334 127.27626)
    (thickness 1.6)
    (drawings 17)
    (tracks 118)
    (zones 0)
    (modules 20)
    (nets 17)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.5)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.6 1.6)
    (pad_drill 0.8)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 100 125)
    (grid_origin 100 125)
    (visible_elements 7FFFF7FF)
    (pcbplotparams
      (layerselection 0x01030_80000001)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(P3-Pad1)")
  (net 2 "Net-(P4-Pad1)")
  (net 3 "Net-(P5-Pad1)")
  (net 4 "Net-(P6-Pad1)")
  (net 5 "Net-(6N136-Pad2)")
  (net 6 "Net-(6N136-Pad3)")
  (net 7 GND)
  (net 8 "Net-(6N136-Pad6)")
  (net 9 "Net-(6N136-Pad7)")
  (net 10 +5V)
  (net 11 "Net-(C1-Pad1)")
  (net 12 "Net-(D2-Pad2)")
  (net 13 "Net-(Q1-Pad2)")
  (net 14 "Net-(P1-Pad1)")
  (net 15 "Net-(P8-Pad1)")
  (net 16 "Net-(P2-Pad5)")
  (net_class Default "This is the default net class."
    (clearance 0.5)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(6N136-Pad2)")
    (add_net "Net-(6N136-Pad3)")
    (add_net "Net-(6N136-Pad6)")
    (add_net "Net-(6N136-Pad7)")
    (add_net "Net-(C1-Pad1)")
    (add_net "Net-(D2-Pad2)")
    (add_net "Net-(P1-Pad1)")
    (add_net "Net-(P2-Pad5)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P6-Pad1)")
    (add_net "Net-(P8-Pad1)")
    (add_net "Net-(Q1-Pad2)")
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 569681A0)
    (at 146 121)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference P3 (at 0.3 0.4) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0 5.00126) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers)
      (net 1 "Net-(P3-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 56968198)
    (at 104 121)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference P4 (at 0 -0.3) (layer F.SilkS))
    (fp_text value CONN_01X01 (at 0 5.00126) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers)
      (net 2 "Net-(P4-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 5696817B)
    (at 104 104)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference P5 (at 0 -4.50088) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at -9.4 3) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers)
      (net 3 "Net-(P5-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 5696816F)
    (at 146 104)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference P6 (at 0 -4.50088) (layer F.SilkS) hide)
    (fp_text value CONN_01X01 (at 0.6 -6) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers)
      (net 4 "Net-(P6-Pad1)"))
  )
  (module Housings_DIP:DIP-8_W7.62mm (layer F.Cu) (tedit 5697C026)
    (at 121 117.7 180)
    (descr "8-lead dip package, row spacing 7.62 mm (300 mils)")
    (tags "dil dip 2.54 300")
    (fp_text reference optoCpl (at 3.8 -1.3 180) (layer F.SilkS))
    (fp_text value optoCoupler (at 0 -3.72 180) (layer F.Fab))
    (pad 1 thru_hole oval (at 0 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 "Net-(6N136-Pad2)"))
    (pad 3 thru_hole oval (at 0 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(6N136-Pad3)"))
    (pad 4 thru_hole oval (at 0 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS))
    (pad 5 thru_hole oval (at 7.62 7.62 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad Vset thru_hole oval (at 7.62 5.08 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 8 "Net-(6N136-Pad6)"))
    (pad 7 thru_hole oval (at 7.62 2.54 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 9 "Net-(6N136-Pad7)"))
    (pad 8 thru_hole oval (at 7.62 0 180) (size 1.6 1.6) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 10 +5V))
    (model Housings_DIP.3dshapes/DIP-8_W7.62mm.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 541A9B8D)
    (at 111 121.7 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C1 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C1-Pad1)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 56968ABE)
    (at 123.5 121.8 90)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 2.1 90) (layer B.SilkS))
    (fp_text value 100nF (at 6.8 -0.4 90) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(6N136-Pad6)"))
    (pad 2 smd rect (at 1.25 0 90) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 541A9B8D)
    (at 108.9 112.8 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C3 (at 0 2.1 270) (layer B.SilkS))
    (fp_text value 100nF (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 10 +5V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer F.Cu) (tedit 54189DEE)
    (at 115.8 105.6)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R1 (at 0 -2.1) (layer F.SilkS))
    (fp_text value 180 (at 0 2.1) (layer F.Fab))
    (pad 1 smd rect (at -1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 14 "Net-(P1-Pad1)"))
    (pad 2 smd rect (at 1.35 0) (size 1.5 1.3) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(6N136-Pad2)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 54189DEE)
    (at 116.8 122.8 180)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R2 (at 0 2.1 180) (layer B.SilkS))
    (fp_text value 1k (at 0 -2.1 180) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(6N136-Pad6)"))
    (pad 2 smd rect (at 1.35 0 180) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 11 "Net-(C1-Pad1)"))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Resistors_SMD:R_0805_HandSoldering (layer B.Cu) (tedit 54189DEE)
    (at 132.4 120.1 270)
    (descr "Resistor SMD 0805, hand soldering")
    (tags "resistor 0805")
    (attr smd)
    (fp_text reference R3 (at 0 2.1 270) (layer B.SilkS))
    (fp_text value 100 (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(P8-Pad1)"))
    (pad 2 smd rect (at 1.35 0 270) (size 1.5 1.3) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (model Resistors_SMD.3dshapes/R_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5697DB70)
    (at 111.2 104.4 180)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P1 (at -0.1 0.2 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at -14.7 6.8 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 14 "Net-(P1-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 "Net-(6N136-Pad3)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5697DD91)
    (at 136.6 118.7)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P8 (at 1.05 -20.875) (layer Cmts.User))
    (fp_text value CONN_01X02 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(P8-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Diodes_SMD:SOD-123 (layer B.Cu) (tedit 5530FCB9)
    (at 139.1 104.2 270)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D2 (at 0 2 270) (layer B.SilkS))
    (fp_text value ZENER (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.635 0 270) (size 0.91 1.22) (layers B.Cu B.Paste B.Mask)
      (net 10 +5V))
    (pad 2 smd rect (at 1.635 0 270) (size 0.91 1.22) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(D2-Pad2)"))
  )
  (module Diodes_SMD:SOD-123 (layer B.Cu) (tedit 5530FCB9)
    (at 135.6 104.2 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D3 (at 0 2 90) (layer B.SilkS))
    (fp_text value ZENER (at 0 -2.1 90) (layer B.Fab))
    (pad 1 smd rect (at -1.635 0 90) (size 0.91 1.22) (layers B.Cu B.Paste B.Mask)
      (net 12 "Net-(D2-Pad2)"))
    (pad 2 smd rect (at 1.635 0 90) (size 0.91 1.22) (layers B.Cu B.Paste B.Mask)
      (net 10 +5V))
  )
  (module Diodes_SMD:SOD-123 (layer F.Cu) (tedit 5530FCB9)
    (at 119.8 103 90)
    (descr SOD-123)
    (tags SOD-123)
    (attr smd)
    (fp_text reference D1 (at 0 -2 90) (layer F.SilkS))
    (fp_text value D (at 0 2.1 90) (layer F.Fab))
    (pad 1 smd rect (at -1.635 0 90) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 5 "Net-(6N136-Pad2)"))
    (pad 2 smd rect (at 1.635 0 90) (size 0.91 1.22) (layers F.Cu F.Paste F.Mask)
      (net 6 "Net-(6N136-Pad3)"))
  )
  (module Pin_Headers:Pin_Header_Straight_2x03 (layer F.Cu) (tedit 5697DB88)
    (at 102 109.9)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P2 (at 2 -6) (layer F.SilkS))
    (fp_text value CONN_02X03 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 +5V))
    (pad 2 thru_hole oval (at 2.54 0) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 +5V))
    (pad 3 thru_hole oval (at 0 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 4 thru_hole oval (at 2.54 2.54) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 GND))
    (pad 5 thru_hole oval (at 0 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 16 "Net-(P2-Pad5)"))
    (pad 6 thru_hole oval (at 2.54 5.08) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 11 "Net-(C1-Pad1)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_2x03.wrl
      (at (xyz 0.05 -0.1 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Pin_Headers:Pin_Header_Straight_1x02 (layer F.Cu) (tedit 5697DB90)
    (at 144.4 110.9)
    (descr "Through hole pin header")
    (tags "pin header")
    (fp_text reference P7 (at 1.6 -6.8) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 10 +5V))
    (pad 2 thru_hole oval (at 0 2.54) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(D2-Pad2)"))
    (model Pin_Headers.3dshapes/Pin_Header_Straight_1x02.wrl
      (at (xyz 0 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module SMD_Packages:SOIC-8-N (layer B.Cu) (tedit 0)
    (at 130 111.6 180)
    (descr "Module Narrow CMS SOJ 8 pins large")
    (tags "CMS SOJ")
    (attr smd)
    (fp_text reference U1 (at 0 1.27 180) (layer B.SilkS))
    (fp_text value OpAmp (at 0 -1.27 180) (layer B.Fab))
    (pad 8 smd rect (at -1.905 3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 10 +5V))
    (pad 7 smd rect (at -0.635 3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask))
    (pad 6 smd rect (at 0.635 3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask))
    (pad 5 smd rect (at 1.905 3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask))
    (pad 4 smd rect (at 1.905 -3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 7 GND))
    (pad 3 smd rect (at 0.635 -3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 8 "Net-(6N136-Pad6)"))
    (pad 2 smd rect (at -0.635 -3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 15 "Net-(P8-Pad1)"))
    (pad 1 smd rect (at -1.905 -3.175 180) (size 0.508 1.143) (layers B.Cu B.Paste B.Mask)
      (net 13 "Net-(Q1-Pad2)"))
    (model SMD_Packages.3dshapes/SOIC-8-N.wrl
      (at (xyz 0 0 0))
      (scale (xyz 0.5 0.38 0.5))
      (rotate (xyz 0 0 0))
    )
  )
  (module TO_SOT_Packages_THT:TO-92_Molded_Wide_Oval (layer F.Cu) (tedit 5697DD96)
    (at 136.425 108.85 270)
    (descr "TO-92 leads molded, wide, oval pads, drill 0.8mm (see NXP sot054_po.pdf)")
    (tags "to-92 sc-43 sc-43a sot54 PA33 transistor")
    (fp_text reference Q1 (at -10.75 -2.825 270) (layer Cmts.User))
    (fp_text value BJT (at 0 3 270) (layer F.Fab))
    (pad 2 thru_hole oval (at 2.54 -2.54) (size 1.99898 1.50114) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 13 "Net-(Q1-Pad2)"))
    (pad 1 thru_hole oval (at 0 0) (size 1.50114 1.99898) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 12 "Net-(D2-Pad2)"))
    (pad 3 thru_hole oval (at 5.08 0) (size 1.50114 1.99898) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 15 "Net-(P8-Pad1)"))
    (model TO_SOT_Packages_THT.3dshapes/TO-92_Molded_Wide_Oval.wrl
      (at (xyz 0.1 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 -90))
    )
  )
  (gr_text fast (at 108.5 104 90) (layer F.SilkS))
  (gr_text c (at 138.125 107) (layer F.SilkS))
  (gr_text e (at 138.55 115.125) (layer F.SilkS))
  (gr_text b (at 141.275 111.2) (layer F.SilkS))
  (gr_text "Blu\n     BEAM" (at 126.6 103.4) (layer F.SilkS))
  (gr_text dV (at 139.85 119.725) (layer F.SilkS))
  (gr_text "+\nout\n-" (at 147.9 112.2) (layer F.SilkS))
  (gr_text gnd (at 108.2 110.8) (layer F.SilkS))
  (gr_text vset (at 108.5 115.5) (layer F.SilkS))
  (gr_text pwr (at 108.2 108.5) (layer F.SilkS))
  (gr_text "FAST_DRIVER_V1 \n14 Jan 2016" (at 126.4 122.8) (layer F.SilkS))
  (gr_line (start 100 100) (end 100 125) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 150 100) (end 100 100) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 150 125) (end 150 100) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100 125) (end 150 125) (angle 90) (layer Edge.Cuts) (width 0.1))
)
