(kicad_pcb (version 4) (host pcbnew 4.0.1-stable)
  (general
    (links 17)
    (no_connects 0)
    (area 98.591667 98.07412 151.408334 127.27626)
    (thickness 1.6)
    (drawings 10)
    (tracks 36)
    (zones 0)
    (modules 10)
    (nets 8)
  )
  (page A4)
  (layers
    (0 F.Cu signal)
    (31 B.Cu signal)
    (32 B.Adhes user)
    (33 F.Adhes user)
    (34 B.Paste user)
    (35 F.Paste user)
    (36 B.SilkS user)
    (37 F.SilkS user)
    (38 B.Mask user)
    (39 F.Mask user)
    (40 Dwgs.User user)
    (41 Cmts.User user)
    (42 Eco1.User user)
    (43 Eco2.User user)
    (44 Edge.Cuts user)
    (45 Margin user)
    (46 B.CrtYd user)
    (47 F.CrtYd user)
    (48 B.Fab user)
    (49 F.Fab user)
  )
  (setup
    (last_trace_width 0.5)
    (trace_clearance 0.5)
    (zone_clearance 0.508)
    (zone_45_only no)
    (trace_min 0.2)
    (segment_width 0.2)
    (edge_width 0.1)
    (via_size 0.6)
    (via_drill 0.4)
    (via_min_size 0.4)
    (via_min_drill 0.3)
    (uvia_size 0.3)
    (uvia_drill 0.1)
    (uvias_allowed no)
    (uvia_min_size 0.2)
    (uvia_min_drill 0.1)
    (pcb_text_width 0.3)
    (pcb_text_size 1.5 1.5)
    (mod_edge_width 0.15)
    (mod_text_size 1 1)
    (mod_text_width 0.15)
    (pad_size 1.5 1.5)
    (pad_drill 0.6)
    (pad_to_mask_clearance 0)
    (aux_axis_origin 100 125)
    (grid_origin 100 125)
    (visible_elements 7FFFFFFF)
    (pcbplotparams
      (layerselection 0x00080_00000000)
      (usegerberextensions false)
      (excludeedgelayer true)
      (linewidth 0.100000)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15)
      (hpglpenoverlay 2)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue true)
      (plotinvisibletext false)
      (padsonsilk false)
      (subtractmaskfromsilk false)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory ""))
  )
  (net 0 "")
  (net 1 "Net-(P3-Pad1)")
  (net 2 "Net-(P4-Pad1)")
  (net 3 "Net-(P5-Pad1)")
  (net 4 "Net-(P6-Pad1)")
  (net 5 +5V)
  (net 6 GND)
  (net 7 "Net-(C3-Pad1)")
  (net_class Default "This is the default net class."
    (clearance 0.5)
    (trace_width 0.5)
    (via_dia 0.6)
    (via_drill 0.4)
    (uvia_dia 0.3)
    (uvia_drill 0.1)
    (add_net +5V)
    (add_net GND)
    (add_net "Net-(C3-Pad1)")
    (add_net "Net-(P3-Pad1)")
    (add_net "Net-(P4-Pad1)")
    (add_net "Net-(P5-Pad1)")
    (add_net "Net-(P6-Pad1)")
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 568FDC31)
    (at 146 121)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference P3 (at 0 -4.50088) (layer Cmts.User) hide)
    (fp_text value CONN_01X01 (at 0 5.00126) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers)
      (net 1 "Net-(P3-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 568FDCC3)
    (at 104 121)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference P4 (at -1 -5) (layer Cmts.User) hide)
    (fp_text value CONN_01X01 (at 0 5.00126) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers)
      (net 2 "Net-(P4-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 568FDCB9)
    (at 104 104)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference P5 (at 0 -4.50088) (layer Cmts.User) hide)
    (fp_text value CONN_01X01 (at 0 5.00126) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers)
      (net 3 "Net-(P5-Pad1)"))
  )
  (module Mounting_Holes:MountingHole_3-5mm (layer F.Cu) (tedit 568FDC37)
    (at 146 104)
    (descr "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (tags "Mounting hole, Befestigungsbohrung, 3,5mm, No Annular, Kein Restring,")
    (fp_text reference P6 (at 0 -4.50088) (layer Cmts.User) hide)
    (fp_text value CONN_01X01 (at 0 5.00126) (layer F.Fab))
    (pad 1 thru_hole circle (at 0 0) (size 3.5 3.5) (drill 3.5) (layers)
      (net 4 "Net-(P6-Pad1)"))
  )
  (module Capacitors_ThroughHole:C_Radial_D10_L13_P5 (layer F.Cu) (tedit 568FD73A)
    (at 111 112 270)
    (descr "Radial Electrolytic Capacitor Diameter 10mm x Length 13mm, Pitch 5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C1 (at 1 2 270) (layer F.SilkS))
    (fp_text value 220uF (at 2.5 6.3 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 5 +5V))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D10_L13_P5.wrl
      (at (xyz 0.0984252 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Capacitors_SMD:C_0805_HandSoldering (layer B.Cu) (tedit 541A9B8D)
    (at 116 116 270)
    (descr "Capacitor SMD 0805, hand soldering")
    (tags "capacitor 0805")
    (attr smd)
    (fp_text reference C2 (at 0 2.1 270) (layer B.SilkS))
    (fp_text value 10uF (at 0 -2.1 270) (layer B.Fab))
    (pad 1 smd rect (at -1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 1.25 0 270) (size 1.5 1.25) (layers B.Cu B.Paste B.Mask)
      (net 6 GND))
    (model Capacitors_SMD.3dshapes/C_0805_HandSoldering.wrl
      (at (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (module Capacitors_ThroughHole:C_Radial_D10_L13_P5 (layer F.Cu) (tedit 568FDAA2)
    (at 138 112 270)
    (descr "Radial Electrolytic Capacitor Diameter 10mm x Length 13mm, Pitch 5mm")
    (tags "Electrolytic Capacitor")
    (fp_text reference C3 (at 1 2 270) (layer F.SilkS))
    (fp_text value 47uF (at 2.5 6.3 270) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C3-Pad1)"))
    (pad 2 thru_hole circle (at 5 0 270) (size 1.3 1.3) (drill 0.8) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (model Capacitors_ThroughHole.3dshapes/C_Radial_D10_L13_P5.wrl
      (at (xyz 0.0984252 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 90))
    )
  )
  (module Choke_SMD:Choke_SMD_10.4x10.4_H4.8 (layer F.Cu) (tedit 568FDAAA)
    (at 125 115)
    (descr "Choke, SMD, 10.4x10.4mm 4.8mm height")
    (tags "Choke, SMD")
    (attr smd)
    (fp_text reference L1 (at 0 -1) (layer F.SilkS))
    (fp_text value 100uH (at 0 6.35) (layer F.Fab))
    (pad 1 smd rect (at -4.15 0) (size 2.7 3.6) (layers F.Cu F.Paste F.Mask)
      (net 5 +5V))
    (pad 2 smd rect (at 4.15 0) (size 2.7 3.6) (layers F.Cu F.Paste F.Mask)
      (net 7 "Net-(C3-Pad1)"))
  )
  (module Socket_Strips:Socket_Strip_Straight_1x02 (layer F.Cu) (tedit 568FDD16)
    (at 120 105 90)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference in (at -3 0 180) (layer F.SilkS))
    (fp_text value CONN_01X02 (at 0 -3.1 90) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 5 +5V))
    (pad 2 thru_hole oval (at 2.54 0 90) (size 2.032 2.032) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_1x02.wrl
      (at (xyz 0.05 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (module Socket_Strips:Socket_Strip_Straight_2x05 (layer F.Cu) (tedit 568FDD28)
    (at 138 105 180)
    (descr "Through hole socket strip")
    (tags "socket strip")
    (fp_text reference out (at 6 -3 180) (layer F.SilkS))
    (fp_text value CONN_02X05 (at 0 -3.1 180) (layer F.Fab))
    (pad 1 thru_hole rect (at 0 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C3-Pad1)"))
    (pad 2 thru_hole oval (at 0 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 3 thru_hole oval (at 2.54 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C3-Pad1)"))
    (pad 4 thru_hole oval (at 2.54 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 5 thru_hole oval (at 5.08 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C3-Pad1)"))
    (pad 6 thru_hole oval (at 5.08 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 7 thru_hole oval (at 7.62 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C3-Pad1)"))
    (pad 8 thru_hole oval (at 7.62 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (pad 9 thru_hole oval (at 10.16 0 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 7 "Net-(C3-Pad1)"))
    (pad 10 thru_hole oval (at 10.16 2.54 180) (size 1.7272 1.7272) (drill 1.016) (layers *.Cu *.Mask F.SilkS)
      (net 6 GND))
    (model Socket_Strips.3dshapes/Socket_Strip_Straight_2x05.wrl
      (at (xyz 0.2 -0.05 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 180))
    )
  )
  (gr_text "Blu\n     BEAM" (at 111 103) (layer F.SilkS))
  (gr_text gnd (at 124 102) (layer F.SilkS))
  (gr_text pwr (at 124 105) (layer F.SilkS))
  (gr_text "PWR_FILTER_V1\n8 Jan 2016" (at 134 123) (layer F.SilkS))
  (gr_line (start 100 100) (end 100 125) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 150 100) (end 100 100) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 150 125) (end 150 100) (angle 90) (layer Edge.Cuts) (width 0.1))
  (gr_line (start 100 125) (end 150 125) (angle 90) (layer Edge.Cuts) (width 0.1))
)
