<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.5.0">
<drawing>
<library>
<packages>
<package name="IL-AG5-22P-D3L2">
</package>
<package name="RCJ_32XXX">
</package>
<package name="LM2596DC-DC">
</package>
<package name="USB-73725">
</package>
</packages>
<symbols>
<symbol name="IL-AG5-22P-D3L2">
<description>Automotive Connectors 22P Pin Header 2.5mm R/A
Manufacturer Part #: IL-AG5-22P-D3L2
Mouser Part #: 656-IL-AG5-22P-D3L2 

http://www.mouser.com/ProductDetail/JAE-Electronics/IL-AG5-22P-D3L2</description>
<pin name="+B"/>
<pin name="ACC"/>
<pin name="PWR_GND"/>
<pin name="ILL+"/>
<pin name="ILL-"/>
<pin name="AUD_RCH"/>
<pin name="AUD_LCH"/>
<pin name="AUD_SHIE"/>
<pin name="AUD_GND"/>
<pin name="RXD"/>
<pin name="N/C_1"/>
<pin name="N/C_3"/>
<pin name="N/C_4"/>
<pin name="IN"/>
<pin name="OUT"/>
<pin name="N/C_2"/>
<pin name="VIDEO"/>
<pin name="DVD_SHIE"/>
<pin name="DVD_GND"/>
<pin name="COM_GND"/>
<pin name="TXD"/>
<pin name="COM_SHIE"/>
</symbol>
<symbol name="RCJ-32234">
<pin name="X2_3"/>
<pin name="X2_4"/>
<pin name="X1_1"/>
<pin name="X1_2"/>
<pin name="X3_5"/>
<pin name="X3_6"/>
</symbol>
<symbol name="POWER_UNIT">
<pin name="VIN"/>
<pin name="VOUT"/>
<pin name="EN"/>
<pin name="GNDOUT"/>
<pin name="GND_IN"/>
</symbol>
<symbol name="USB-73725">
<pin name="USB_D+"/>
<pin name="USB_D-"/>
<pin name="USB_VDD"/>
<pin name="USB_GND"/>
<pin name="SHIELD@1"/>
<pin name="SHIELD@2"/>
<pin name="SHIELD@3"/>
<pin name="SHIELD@4"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="IL-AG5-22P-D3L2" uservalue="yes">
<gates>
<gate name="G$1" symbol="IL-AG5-22P-D3L2"/>
</gates>
<devices>
<device name="" package="IL-AG5-22P-D3L2">
<connects>
<connect gate="G$1" pin="+B" pad="2"/>
<connect gate="G$1" pin="ACC" pad="4"/>
<connect gate="G$1" pin="AUD_GND" pad="20"/>
<connect gate="G$1" pin="AUD_LCH" pad="8"/>
<connect gate="G$1" pin="AUD_RCH" pad="9"/>
<connect gate="G$1" pin="AUD_SHIE" pad="21"/>
<connect gate="G$1" pin="COM_GND" pad="7"/>
<connect gate="G$1" pin="COM_SHIE" pad="19"/>
<connect gate="G$1" pin="DVD_GND" pad="14"/>
<connect gate="G$1" pin="DVD_SHIE" pad="15"/>
<connect gate="G$1" pin="ILL+" pad="3"/>
<connect gate="G$1" pin="ILL-" pad="13"/>
<connect gate="G$1" pin="IN" pad="16"/>
<connect gate="G$1" pin="N/C_1" pad="1"/>
<connect gate="G$1" pin="N/C_2" pad="10"/>
<connect gate="G$1" pin="N/C_3" pad="11"/>
<connect gate="G$1" pin="N/C_4" pad="22"/>
<connect gate="G$1" pin="OUT" pad="17"/>
<connect gate="G$1" pin="PWR_GND" pad="12"/>
<connect gate="G$1" pin="RXD" pad="18"/>
<connect gate="G$1" pin="TXD" pad="6"/>
<connect gate="G$1" pin="VIDEO" pad="5"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RCJ_32XXX">
<gates>
<gate name="G$1" symbol="RCJ-32234"/>
</gates>
<devices>
<device name="" package="RCJ_32XXX">
<connects>
<connect gate="G$1" pin="X1_1" pad="P$1"/>
<connect gate="G$1" pin="X1_2" pad="P$2"/>
<connect gate="G$1" pin="X2_3" pad="P$3"/>
<connect gate="G$1" pin="X2_4" pad="P$4"/>
<connect gate="G$1" pin="X3_5" pad="P$5"/>
<connect gate="G$1" pin="X3_6" pad="P$6"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LM25966_EBAY">
<gates>
<gate name="G$1" symbol="POWER_UNIT"/>
</gates>
<devices>
<device name="" package="LM2596DC-DC">
<connects>
<connect gate="G$1" pin="EN" pad="EN"/>
<connect gate="G$1" pin="GNDOUT" pad="GND_OUT"/>
<connect gate="G$1" pin="GND_IN" pad="GND_IN"/>
<connect gate="G$1" pin="VIN" pad="VIN"/>
<connect gate="G$1" pin="VOUT" pad="VOUT"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="USB-73725">
<gates>
<gate name="G$1" symbol="USB-73725"/>
</gates>
<devices>
<device name="" package="USB-73725">
<connects>
<connect gate="G$1" pin="SHIELD@1" pad="SHIELD@1"/>
<connect gate="G$1" pin="SHIELD@2" pad="SHIELD@2"/>
<connect gate="G$1" pin="SHIELD@3" pad="SHIELD@3"/>
<connect gate="G$1" pin="SHIELD@4" pad="SHIELD@4"/>
<connect gate="G$1" pin="USB_D+" pad="USB_D+"/>
<connect gate="G$1" pin="USB_D-" pad="USB_D-"/>
<connect gate="G$1" pin="USB_GND" pad="USB_GND"/>
<connect gate="G$1" pin="USB_VDD" pad="USB_VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
