<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="30.714" y2="0" width="0" layer="20"/>
<wire x1="30.714" y1="0" x2="30.714" y2="12.624" width="0" layer="20"/>
<wire x1="30.714" y1="12.624" x2="0" y2="12.624" width="0" layer="20"/>
<wire x1="0" y1="12.624" x2="0" y2="0" width="0" layer="20"/>
<text>3.3V</text>
<text>GND</text>
<text>SCL</text>
<text>SDA</text>
<text>I2C: 0x40</text>
<text>SF2</text>
</plain>
<libraries>
<library name="Misenso">
<packages>
<package name="SEN-SENSIRION-SHT2X">
</package>
<package name="MISC-SENSIRION-SF2">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-CAP">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603-RES">
</package>
</packages>
</library>
<library name="pinhead">
<description>&lt;b&gt;Pin Header Connectors&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="1X04">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="Misenso" package="SEN-SENSIRION-SHT2X" value="SEN-SENSIRION-SHT2X"/>
<element name="U$2" library="Misenso" package="MISC-SENSIRION-SF2" value="MISC-SENSIRION-SF2"/>
<element name="C1" library="SparkFun-Capacitors" package="0603-CAP" value="0.1uF">
<attribute name="PROD_ID" value="CAP-00810"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603-RES" value="10K">
<attribute name="PROD_ID" value="RES-00824"/>
</element>
<element name="JP1" library="pinhead" package="1X04" value=""/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="JP1" pad="2"/>
</signal>
<signal name="SCL">
<contactref element="U$1" pad="6"/>
<contactref element="JP1" pad="3"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="U$1" pad="1"/>
<contactref element="JP1" pad="4"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="3.3V">
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="U$1" pad="5"/>
<contactref element="C1" pad="1"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$2">
</signal>
<signal name="N$3">
</signal>
</signals>
</board>
</drawing>
</eagle>
