<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.4.0">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="100" y2="0" width="0" layer="20"/>
<wire x1="100" y1="0" x2="100" y2="85" width="0" layer="20"/>
<wire x1="100" y1="85" x2="0" y2="85" width="0" layer="20"/>
<wire x1="0" y1="85" x2="0" y2="0" width="0" layer="20"/>
<text>power+

GND

load+

GND</text>
<text>power+

GND

load+

GND</text>
<text>power+

GND

load+

GND</text>
<text>3</text>
<text>2</text>
<text>1</text>
<wire x1="-1" y1="-1" x2="-1" y2="86" width="0.1778" layer="46"/>
<wire x1="-1" y1="86" x2="101" y2="86" width="0.1778" layer="46"/>
<wire x1="101" y1="86" x2="101" y2="-1" width="0.1778" layer="46"/>
<wire x1="101" y1="-1" x2="-1" y2="-1" width="0.1778" layer="46"/>
</plain>
<libraries>
<library name="tmb_boards">
<packages>
<package name="BANANA_PRO">
</package>
<package name="SWITCHDOC_INA3221">
</package>
<package name="ARDOKIT_DS1307_RIGHT">
</package>
</packages>
</library>
<library name="tmb_connectors">
<packages>
<package name="1X20_LONGPADS">
</package>
<package name="W237-132">
<description>&lt;b&gt;WAGO SREW CLAMP&lt;/b&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="JP1" library="tmb_connectors" package="1X20_LONGPADS" value=""/>
<element name="JP2" library="tmb_connectors" package="1X20_LONGPADS" value=""/>
<element name="U$2" library="tmb_boards" package="BANANA_PRO" value="BANANA_PRO"/>
<element name="X1" library="tmb_boards" package="SWITCHDOC_INA3221" value="SWITCHDOC_INA3221"/>
<element name="X3" library="tmb_connectors" package="W237-132" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="X4" library="tmb_connectors" package="W237-132" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="X2" library="tmb_connectors" package="W237-132" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="X5" library="tmb_connectors" package="W237-132" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="X6" library="tmb_connectors" package="W237-132" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="X7" library="tmb_connectors" package="W237-132" value="">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
<element name="X8" library="tmb_boards" package="ARDOKIT_DS1307_RIGHT" value="ARDOKIT_DS1307RIGHT"/>
</elements>
<signals>
<signal name="GND">
<contactref element="JP1" pad="5"/>
<contactref element="U$2" pad="9"/>
<contactref element="X1" pad="2"/>
<contactref element="X4" pad="2"/>
<contactref element="X3" pad="2"/>
<contactref element="X5" pad="2"/>
<contactref element="X2" pad="2"/>
<contactref element="X7" pad="2"/>
<contactref element="X6" pad="2"/>
<contactref element="X8" pad="GND"/>
</signal>
<signal name="N$21">
<contactref element="JP1" pad="2"/>
<contactref element="U$2" pad="3"/>
<contactref element="X1" pad="4"/>
<contactref element="X8" pad="SDA"/>
</signal>
<signal name="N$22">
<contactref element="JP1" pad="3"/>
<contactref element="U$2" pad="5"/>
<contactref element="X1" pad="3"/>
<contactref element="X8" pad="SCL"/>
</signal>
<signal name="N$31">
<contactref element="JP2" pad="3"/>
<contactref element="U$2" pad="6"/>
</signal>
<signal name="N$32">
<contactref element="JP2" pad="4"/>
<contactref element="U$2" pad="8"/>
</signal>
<signal name="N$33">
<contactref element="JP2" pad="5"/>
<contactref element="U$2" pad="10"/>
</signal>
<signal name="N$34">
<contactref element="JP2" pad="6"/>
<contactref element="U$2" pad="12"/>
</signal>
<signal name="N$35">
<contactref element="JP2" pad="7"/>
<contactref element="U$2" pad="14"/>
</signal>
<signal name="N$1">
<contactref element="U$2" pad="16"/>
<contactref element="JP2" pad="8"/>
</signal>
<signal name="N$2">
<contactref element="U$2" pad="18"/>
<contactref element="JP2" pad="9"/>
</signal>
<signal name="N$3">
<contactref element="U$2" pad="20"/>
<contactref element="JP2" pad="10"/>
</signal>
<signal name="N$13">
<contactref element="U$2" pad="22"/>
<contactref element="JP2" pad="11"/>
</signal>
<signal name="N$14">
<contactref element="U$2" pad="24"/>
<contactref element="JP2" pad="12"/>
</signal>
<signal name="N$15">
<contactref element="U$2" pad="26"/>
<contactref element="JP2" pad="13"/>
</signal>
<signal name="N$16">
<contactref element="U$2" pad="28"/>
<contactref element="JP2" pad="14"/>
</signal>
<signal name="N$17">
<contactref element="U$2" pad="30"/>
<contactref element="JP2" pad="15"/>
</signal>
<signal name="N$18">
<contactref element="U$2" pad="32"/>
<contactref element="JP2" pad="16"/>
</signal>
<signal name="N$19">
<contactref element="U$2" pad="34"/>
<contactref element="JP2" pad="17"/>
</signal>
<signal name="N$20">
<contactref element="U$2" pad="36"/>
<contactref element="JP2" pad="18"/>
</signal>
<signal name="N$23">
<contactref element="U$2" pad="38"/>
<contactref element="JP2" pad="19"/>
</signal>
<signal name="N$24">
<contactref element="U$2" pad="40"/>
<contactref element="JP2" pad="20"/>
</signal>
<signal name="N$26">
<contactref element="JP1" pad="4"/>
<contactref element="U$2" pad="7"/>
</signal>
<signal name="N$28">
<contactref element="JP1" pad="6"/>
<contactref element="U$2" pad="11"/>
</signal>
<signal name="N$29">
<contactref element="JP1" pad="7"/>
<contactref element="U$2" pad="13"/>
</signal>
<signal name="N$36">
<contactref element="JP1" pad="8"/>
<contactref element="U$2" pad="15"/>
</signal>
<signal name="N$38">
<contactref element="JP1" pad="10"/>
<contactref element="U$2" pad="19"/>
</signal>
<signal name="N$39">
<contactref element="JP1" pad="11"/>
<contactref element="U$2" pad="21"/>
</signal>
<signal name="N$40">
<contactref element="JP1" pad="12"/>
<contactref element="U$2" pad="23"/>
</signal>
<signal name="N$41">
<contactref element="JP1" pad="13"/>
<contactref element="U$2" pad="25"/>
</signal>
<signal name="N$42">
<contactref element="JP1" pad="14"/>
<contactref element="U$2" pad="27"/>
</signal>
<signal name="N$43">
<contactref element="JP1" pad="15"/>
<contactref element="U$2" pad="29"/>
</signal>
<signal name="N$44">
<contactref element="JP1" pad="16"/>
<contactref element="U$2" pad="31"/>
</signal>
<signal name="N$45">
<contactref element="JP1" pad="17"/>
<contactref element="U$2" pad="33"/>
</signal>
<signal name="N$46">
<contactref element="JP1" pad="18"/>
<contactref element="U$2" pad="35"/>
</signal>
<signal name="N$47">
<contactref element="JP1" pad="19"/>
<contactref element="U$2" pad="37"/>
</signal>
<signal name="N$48">
<contactref element="JP1" pad="20"/>
<contactref element="U$2" pad="39"/>
</signal>
<signal name="3.3V">
<contactref element="X1" pad="1"/>
<contactref element="JP1" pad="9"/>
<contactref element="U$2" pad="17"/>
</signal>
<signal name="N$5">
<contactref element="X1" pad="9"/>
<contactref element="X4" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="X6" pad="1"/>
<contactref element="X1" pad="14"/>
</signal>
<signal name="N$7">
<contactref element="X7" pad="1"/>
<contactref element="X1" pad="13"/>
</signal>
<signal name="N$8">
<contactref element="X2" pad="1"/>
<contactref element="X1" pad="12"/>
</signal>
<signal name="N$9">
<contactref element="X5" pad="1"/>
<contactref element="X1" pad="11"/>
</signal>
<signal name="N$10">
<contactref element="X3" pad="1"/>
<contactref element="X1" pad="10"/>
</signal>
<signal name="5V">
<contactref element="JP2" pad="1"/>
<contactref element="U$2" pad="2"/>
<contactref element="X8" pad="VCC"/>
</signal>
<signal name="N$4">
<contactref element="U$2" pad="4"/>
<contactref element="JP2" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="JP1" pad="1"/>
<contactref element="U$2" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
