<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="35.54" y2="0" width="0" layer="20"/>
<wire x1="35.54" y1="0" x2="35.56" y2="25.4" width="0" layer="20"/>
<wire x1="35.56" y1="25.4" x2="0" y2="25.4" width="0" layer="20"/>
<wire x1="0" y1="25.4" x2="0" y2="0" width="0" layer="20"/>
<text>Geppetto
Electronics
GPS PI Hat
v0.2</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="PANASONIC_H13">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="SOD-323F">
</package>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="U.FL">
</package>
<package name="2X10">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="2PT_GND_TIE">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SkyTraqGPS">
<packages>
<package name="LGA69">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0402TVS">
</package>
</packages>
</library>
<library name="AP2331">
<packages>
<package name="SOT23-3">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="1µF">
<attribute name="NAME"/>
</element>
<element name="L1" library="SparkFun-Passives" package="0805" value="0.033µH">
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="10kΩ">
<attribute name="NAME"/>
</element>
<element name="JP2" library="SparkFun-Connectors" package="U.FL" value="U.FL">
<attribute name="NAME"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="1µF">
<attribute name="NAME"/>
</element>
<element name="PT1" library="SparkFun-Passives" package="2PT_GND_TIE" value="2PT_GND_TIE"/>
<element name="LED1" library="adafruit" package="CHIP-LED0805" value="GPS"/>
<element name="R1" library="SparkFun-Resistors" package="0805" value="330Ω">
<attribute name="NAME"/>
</element>
<element name="U1" library="SkyTraqGPS" package="LGA69" value="VENUS838LPX-T">
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="1kΩ">
<attribute name="NAME"/>
</element>
<element name="D2" library="adafruit" package="SOD-323F" value="BAT54">
<attribute name="NAME"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="330Ω">
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="1µF">
<attribute name="NAME"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="PANASONIC_H13" value="100mF">
<attribute name="NAME"/>
</element>
<element name="D1" library="SparkFun-DiscreteSemi" package="0402TVS" value="0402TVS">
<attribute name="NAME"/>
</element>
<element name="JP1" library="SparkFun-Connectors" package="2X10" value="M10X2"/>
<element name="IC1" library="AP2331" package="SOT23-3" value="AP2331-SOT23">
<attribute name="NAME"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="0.1µF">
<attribute name="NAME"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0805" value="0.1µF">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="C1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="PT1" pad="P$1"/>
<contactref element="U1" pad="P$60"/>
<contactref element="U1" pad="P$19"/>
<contactref element="U1" pad="P$11"/>
<contactref element="U1" pad="P$10"/>
<contactref element="U1" pad="P$49"/>
<contactref element="U1" pad="P$64"/>
<contactref element="U1" pad="P$15"/>
<contactref element="C4" pad="-"/>
<contactref element="C3" pad="1"/>
<contactref element="JP1" pad="6"/>
<contactref element="IC1" pad="1"/>
<contactref element="JP1" pad="9"/>
<contactref element="JP1" pad="14"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="R2" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="P$2"/>
<contactref element="U1" pad="P$58"/>
<contactref element="R3" pad="2"/>
<contactref element="D2" pad="A"/>
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="C1" pad="2"/>
<contactref element="R2" pad="1"/>
<contactref element="U1" pad="P$1"/>
</signal>
<signal name="AGND">
<contactref element="JP2" pad="P$1"/>
<contactref element="JP2" pad="P$2"/>
<contactref element="PT1" pad="P$2"/>
<contactref element="U1" pad="P$24"/>
<contactref element="U1" pad="P$28"/>
<contactref element="U1" pad="P$29"/>
<contactref element="U1" pad="P$33"/>
<contactref element="U1" pad="P$21"/>
<contactref element="U1" pad="P$25"/>
<contactref element="U1" pad="P$31"/>
<contactref element="U1" pad="P$65"/>
<contactref element="U1" pad="P$27"/>
<contactref element="U1" pad="P$62"/>
<contactref element="U1" pad="P$61"/>
<contactref element="U1" pad="P$69"/>
<contactref element="U1" pad="P$22"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$7">
<contactref element="JP2" pad="P$3"/>
<contactref element="L1" pad="2"/>
<contactref element="U1" pad="P$32"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="PPS">
<contactref element="U1" pad="P$40"/>
<contactref element="JP1" pad="12"/>
</signal>
<signal name="RXD">
<contactref element="U1" pad="P$42"/>
<contactref element="JP1" pad="8"/>
</signal>
<signal name="TXD">
<contactref element="U1" pad="P$44"/>
<contactref element="JP1" pad="10"/>
</signal>
<signal name="LED">
<contactref element="LED1" pad="C"/>
<contactref element="U1" pad="P$7"/>
</signal>
<signal name="N$1">
<contactref element="R1" pad="1"/>
<contactref element="LED1" pad="A"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="P$9"/>
<contactref element="R3" pad="1"/>
</signal>
<signal name="VBATT">
<contactref element="D2" pad="C"/>
<contactref element="R4" pad="2"/>
<contactref element="U1" pad="P$18"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="C4" pad="+"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="L1" pad="1"/>
<contactref element="IC1" pad="2"/>
<contactref element="C6" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="IC1" pad="3"/>
<contactref element="JP1" pad="4"/>
<contactref element="JP1" pad="2"/>
<contactref element="C5" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
