<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.0">
<drawing>
<board>
<plain>
<wire x1="100" y1="0" x2="100" y2="80" width="0" layer="20"/>
<wire x1="100" y1="80" x2="0" y2="80" width="0" layer="20"/>
<wire x1="0" y1="80" x2="0" y2="0" width="0" layer="20"/>
<text>Power BLough-R</text>
<hole x="38.608" y="36.83" drill="3.048"/>
<hole x="38.608" y="49.53" drill="3.048"/>
<text>By Brian Lough</text>
<text>blough.ie/bloughr</text>
<text>V1.0.0</text>
<text>Top Side!</text>
<wire x1="27.686" y1="34.29" x2="49.53" y2="34.29" width="0.1524" layer="20"/>
<wire x1="49.53" y1="34.29" x2="49.53" y2="52.07" width="0.1524" layer="20"/>
<text>Male</text>
<text>Female</text>
<wire x1="27.686" y1="34.29" x2="27.686" y2="52.07" width="0.1524" layer="20"/>
<wire x1="27.686" y1="52.07" x2="49.53" y2="52.07" width="0.1524" layer="20"/>
<text>The name only makes sense 
if you know Lough is 
pronounced "lock" 
:)</text>
<text>Designed in
Ireland
</text>
<text>Probably Made 
in China</text>
</plain>
<libraries>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-A-H">
<description>&lt;h3&gt;USB Type 'A' Male Connector - PTH&lt;/h3&gt;
Shield pins may be grounded.
&lt;br&gt; tDocu shows plug end. 
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=�http://www.4uconnector.com/online/object/4udrawing/10016.pdf�&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;USB_A&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="con-berg">
<description>&lt;b&gt;Berg Connectors&lt;/b&gt;&lt;p&gt;
Based on  the following source:
&lt;ul&gt;
&lt;li&gt;http://catalog.fciconnect.com
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="PN87520-S">
<description>&lt;b&gt;USB connector&lt;/b&gt; with shield&lt;p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="MALE" library="SparkFun-Connectors" package="USB-A-H" value="USB_A_PTH_MALE">
<attribute name="PROD_ID" value="CONN-08367"/>
<attribute name="SF_ID" value="PRT-00437"/>
</element>
<element name="FEMALE" library="con-berg" package="PN87520-S" value="PN87520-S">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
</element>
</elements>
<signals>
<signal name="VBUS">
<contactref element="MALE" pad="VBUS"/>
</signal>
<signal name="SHIELD">
<contactref element="MALE" pad="SHLD1"/>
<contactref element="MALE" pad="SHLD2"/>
<contactref element="FEMALE" pad="S2"/>
<contactref element="FEMALE" pad="S1"/>
</signal>
<signal name="GND">
<contactref element="MALE" pad="GND"/>
<contactref element="FEMALE" pad="4"/>
</signal>
<signal name="D+">
<contactref element="MALE" pad="D+"/>
<contactref element="FEMALE" pad="3"/>
</signal>
<signal name="D-">
<contactref element="MALE" pad="D-"/>
<contactref element="FEMALE" pad="2"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
