<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<text>Remoteduino</text>
<text>sjm4306</text>
<text>041219</text>
<wire x1="3.175" y1="0" x2="60.325" y2="0" width="0" layer="20"/>
<wire x1="63.5" y1="3.175" x2="63.5" y2="81.5975" width="0" layer="20"/>
<wire x1="60.325" y1="84.7725" x2="3.175" y2="84.7725" width="0" layer="20"/>
<wire x1="0" y1="81.5975" x2="0" y2="3.175" width="0" layer="20"/>
<wire x1="3.175" y1="84.7725" x2="0" y2="81.5975" width="0" layer="20" curve="90"/>
<wire x1="60.325" y1="84.7725" x2="63.5" y2="81.5975" width="0" layer="20" curve="-90"/>
<wire x1="60.325" y1="0" x2="63.5" y2="3.175" width="0" layer="20" curve="90"/>
<wire x1="3.175" y1="0" x2="0" y2="3.175" width="0" layer="20" curve="-90"/>
<text>TD</text>
<text>PD</text>
</plain>
<libraries>
<library name="adafruit">
<packages>
<package name="C0805">
<description>&lt;b&gt;CAPACITOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
<package name="CHIP-LED0805">
<description>&lt;b&gt;Hyper CHIPLED Hyper-Bright LED&lt;/b&gt;&lt;p&gt;
LB R99A&lt;br&gt;
Source: http://www.osram.convergy.de/ ... lb_r99a.pdf</description>
</package>
<package name="M0805">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
MELF 0.10 W</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="2X3">
<description>&lt;h3&gt;Plated Through Hole - 2x3&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X01">
<description>&lt;h3&gt;Plated Through Hole&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:1&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-IC-Microcontroller">
<description>&lt;h3&gt;SparkFun Microcontrollers&lt;/h3&gt;
This library contains microcontrollers.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TQFP32-08">
<description>&lt;B&gt;Thin Plasic Quad Flat Package&lt;/B&gt; Grid 0.8 mm</description>
</package>
</packages>
</library>
<library name="SparkFun-Clocks">
<description>&lt;h3&gt;SparkFun Clocks, Oscillators and Resonators&lt;/h3&gt;
This library contains the real-time clocks, oscillators, resonators, and crystals we use. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="CRYSTAL-SMD-5X3.2-2PAD">
<description>&lt;h3&gt;5x3.2mm 2-pad SMD Crystal&lt;/h3&gt;
&lt;p&gt;&lt;a href="http://www.txccrystal.com/images/pdf/7a.pdf"&gt;Example Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="LED2X5">
<description>&lt;B&gt;LED&lt;/B&gt;&lt;p&gt;
2 x 5 mm, rectangle</description>
</package>
</packages>
</library>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH_SMD_6.2MM_TALL">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - SMD, 6.2mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.apem.com/files/apem/brochures/ADTS6-ADTSM-KTSC6.pdf"&gt;Datasheet&lt;/a&gt; (ADTSM63NVTR)&lt;/p&gt;</description>
</package>
<package name="SWITCH_SPST_SMD_A">
<description>&lt;h3&gt;SPDT Slide Switch - SMD&lt;/h3&gt;
&lt;p&gt;Single-pole, double-throw (SPDT) switch.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Components/Switches/SLIDE.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Discrete Semiconductors&lt;/h3&gt;
This library contains diodes, optoisolators, TRIACs, MOSFETs, transistors, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
<description>SOT23-3</description>
</package>
</packages>
</library>
<library name="sjm4306_LOGO">
<packages>
<package name="SJM4306_MEDIUM_NO_COPPER">
</package>
<package name="SJM4306_LARGE_NO_COPPER">
</package>
</packages>
</library>
<library name="SparkFun-Batteries">
<description>&lt;h3&gt;SparkFun Batteries&lt;/h3&gt;
This library contains battery clips, connectors, and appropriately sized silk outlines for LiPo batteries. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BATTCOM_20MM_PTH">
<description>&lt;h3&gt;20mm (CR2032) Coin Cell Battery Holder - PTH&lt;/h3&gt;
&lt;p&gt;Basic 20mm coin cell holder. Posts can be inserted into 0.1" perf board! Holds the common CR2032 type batteries.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://www.sparkfun.com/datasheets/Prototyping/CoinCellHolder-20mm.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="jump-0r-smd">
<description>Soldering jumper and bridges</description>
<packages>
<package name="C0R-JMP">
<description>&lt;b&gt;0R Jumper Variant C&lt;/b&gt;&lt;p&gt;
Solder type</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="adafruit" package="C0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C2" library="adafruit" package="C0805" value="22pF">
<attribute name="NAME"/>
</element>
<element name="C3" library="adafruit" package="C0805" value="22pF">
<attribute name="NAME"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="2X3" value="ICSP">
<attribute name="PROD_ID" value="CONN-09701"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="1X01" value="Vcc">
<attribute name="VALUE"/>
</element>
<element name="J7" library="SparkFun-Connectors" package="1X01" value="Gnd">
<attribute name="VALUE"/>
</element>
<element name="L" library="adafruit" package="CHIP-LED0805" value="Red">
<attribute name="NAME"/>
</element>
<element name="R1" library="adafruit" package="M0805" value="10K">
<attribute name="NAME"/>
</element>
<element name="R2" library="adafruit" package="M0805" value="100">
<attribute name="NAME"/>
</element>
<element name="R3" library="adafruit" package="M0805" value="1K">
<attribute name="NAME"/>
</element>
<element name="U1" library="SparkFun-IC-Microcontroller" package="TQFP32-08" value="ATMEGA328P_TQFP">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="IC-09069"/>
<attribute name="VALUE"/>
</element>
<element name="Y1" library="SparkFun-Clocks" package="CRYSTAL-SMD-5X3.2-2PAD" value="16MHz"/>
<element name="IRLED" library="led" package="LED2X5" value=""/>
<element name="PWR" library="SparkFun-Switches" package="TACTILE_SWITCH_SMD_6.2MM_TALL" value="MOMENTARY-SWITCH-SPST-SMD-6.2MM-TALL">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="SWCH-11966"/>
<attribute name="SF_SKU" value="COM-12992"/>
</element>
<element name="PLAY" library="SparkFun-Switches" package="TACTILE_SWITCH_SMD_6.2MM_TALL" value="MOMENTARY-SWITCH-SPST-SMD-6.2MM-TALL">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="SWCH-11966"/>
<attribute name="SF_SKU" value="COM-12992"/>
</element>
<element name="FFW" library="SparkFun-Switches" package="TACTILE_SWITCH_SMD_6.2MM_TALL" value="MOMENTARY-SWITCH-SPST-SMD-6.2MM-TALL">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="SWCH-11966"/>
<attribute name="SF_SKU" value="COM-12992"/>
</element>
<element name="REW" library="SparkFun-Switches" package="TACTILE_SWITCH_SMD_6.2MM_TALL" value="MOMENTARY-SWITCH-SPST-SMD-6.2MM-TALL">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="SWCH-11966"/>
<attribute name="SF_SKU" value="COM-12992"/>
</element>
<element name="VOLUP" library="SparkFun-Switches" package="TACTILE_SWITCH_SMD_6.2MM_TALL" value="MOMENTARY-SWITCH-SPST-SMD-6.2MM-TALL">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="SWCH-11966"/>
<attribute name="SF_SKU" value="COM-12992"/>
</element>
<element name="VOLDN" library="SparkFun-Switches" package="TACTILE_SWITCH_SMD_6.2MM_TALL" value="MOMENTARY-SWITCH-SPST-SMD-6.2MM-TALL">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="SWCH-11966"/>
<attribute name="SF_SKU" value="COM-12992"/>
</element>
<element name="STOP" library="SparkFun-Switches" package="TACTILE_SWITCH_SMD_6.2MM_TALL" value="MOMENTARY-SWITCH-SPST-SMD-6.2MM-TALL">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="SWCH-11966"/>
<attribute name="SF_SKU" value="COM-12992"/>
</element>
<element name="Q1" library="SparkFun-DiscreteSemi" package="SOT23-3" value="600mA/40V">
<attribute name="PROD_ID" value="TRANS-08049"/>
</element>
<element name="R4" library="adafruit" package="M0805" value="1K">
<attribute name="NAME"/>
</element>
<element name="MODE" library="SparkFun-Switches" package="TACTILE_SWITCH_SMD_6.2MM_TALL" value="MOMENTARY-SWITCH-SPST-SMD-6.2MM-TALL">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="SWCH-11966"/>
<attribute name="SF_SKU" value="COM-12992"/>
</element>
<element name="RX" library="SparkFun-Connectors" package="1X01" value=""/>
<element name="TX" library="SparkFun-Connectors" package="1X01" value=""/>
<element name="PAUSE" library="SparkFun-Switches" package="TACTILE_SWITCH_SMD_6.2MM_TALL" value="MOMENTARY-SWITCH-SPST-SMD-6.2MM-TALL">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="SWCH-11966"/>
<attribute name="SF_SKU" value="COM-12992"/>
</element>
<element name="A" library="SparkFun-Switches" package="TACTILE_SWITCH_SMD_6.2MM_TALL" value="MOMENTARY-SWITCH-SPST-SMD-6.2MM-TALL">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="SWCH-11966"/>
<attribute name="SF_SKU" value="COM-12992"/>
</element>
<element name="B" library="SparkFun-Switches" package="TACTILE_SWITCH_SMD_6.2MM_TALL" value="MOMENTARY-SWITCH-SPST-SMD-6.2MM-TALL">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="SWCH-11966"/>
<attribute name="SF_SKU" value="COM-12992"/>
</element>
<element name="C" library="SparkFun-Switches" package="TACTILE_SWITCH_SMD_6.2MM_TALL" value="MOMENTARY-SWITCH-SPST-SMD-6.2MM-TALL">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="SWCH-11966"/>
<attribute name="SF_SKU" value="COM-12992"/>
</element>
<element name="D" library="SparkFun-Switches" package="TACTILE_SWITCH_SMD_6.2MM_TALL" value="MOMENTARY-SWITCH-SPST-SMD-6.2MM-TALL">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="SWCH-11966"/>
<attribute name="SF_SKU" value="COM-12992"/>
</element>
<element name="E" library="SparkFun-Switches" package="TACTILE_SWITCH_SMD_6.2MM_TALL" value="MOMENTARY-SWITCH-SPST-SMD-6.2MM-TALL">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="SWCH-11966"/>
<attribute name="SF_SKU" value="COM-12992"/>
</element>
<element name="F" library="SparkFun-Switches" package="TACTILE_SWITCH_SMD_6.2MM_TALL" value="MOMENTARY-SWITCH-SPST-SMD-6.2MM-TALL">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="SWCH-11966"/>
<attribute name="SF_SKU" value="COM-12992"/>
</element>
<element name="U$1" library="sjm4306_LOGO" package="SJM4306_MEDIUM_NO_COPPER" value=""/>
<element name="U$2" library="sjm4306_LOGO" package="SJM4306_LARGE_NO_COPPER" value=""/>
<element name="S1" library="SparkFun-Switches" package="SWITCH_SPST_SMD_A" value="">
<attribute name="PROD_ID" value="SWCH-10651"/>
<attribute name="SF_SKU" value="COM-10860"/>
</element>
<element name="REC" library="SparkFun-Connectors" package="1X01" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="BT1" library="SparkFun-Batteries" package="BATTCOM_20MM_PTH" value="">
<attribute name="PROD_ID" value="BATT-09031"/>
<attribute name="SF_SKU" value="PRT-00783"/>
</element>
<element name="JMP1" library="jump-0r-smd" package="C0R-JMP" value="0R-JUMPC">
<attribute name="VALUE"/>
</element>
<element name="JMP2" library="jump-0r-smd" package="C0R-JMP" value="0R-JUMPC">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="21"/>
<contactref element="U1" pad="3"/>
<contactref element="U1" pad="5"/>
<contactref element="C1" pad="2"/>
<contactref element="J1" pad="6"/>
<contactref element="R3" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="J7" pad="1"/>
<contactref element="PWR" pad="B2"/>
<contactref element="PLAY" pad="B2"/>
<contactref element="FFW" pad="B2"/>
<contactref element="REW" pad="B2"/>
<contactref element="VOLUP" pad="B2"/>
<contactref element="VOLDN" pad="B2"/>
<contactref element="Q1" pad="2"/>
<contactref element="PAUSE" pad="B2"/>
<contactref element="STOP" pad="B2"/>
<contactref element="MODE" pad="B2"/>
<contactref element="A" pad="B2"/>
<contactref element="B" pad="B2"/>
<contactref element="C" pad="B2"/>
<contactref element="D" pad="B2"/>
<contactref element="E" pad="B2"/>
<contactref element="F" pad="B2"/>
<contactref element="JMP1" pad="3"/>
<contactref element="BT1" pad="2"/>
</signal>
<signal name="VCC">
<contactref element="U1" pad="18"/>
<contactref element="U1" pad="6"/>
<contactref element="U1" pad="4"/>
<contactref element="R1" pad="2"/>
<contactref element="U1" pad="20"/>
<contactref element="C1" pad="1"/>
<contactref element="J1" pad="2"/>
<contactref element="J5" pad="1"/>
<contactref element="S1" pad="2"/>
<contactref element="JMP2" pad="1"/>
</signal>
<signal name="RST">
<contactref element="U1" pad="29"/>
<contactref element="R1" pad="1"/>
<contactref element="J1" pad="5"/>
</signal>
<signal name="N$2">
<contactref element="U1" pad="8"/>
<contactref element="Y1" pad="P$1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U1" pad="7"/>
<contactref element="Y1" pad="P$2"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="MOSI">
<contactref element="J1" pad="4"/>
<contactref element="U1" pad="15"/>
<contactref element="REC" pad="1"/>
</signal>
<signal name="MISO">
<contactref element="J1" pad="1"/>
<contactref element="U1" pad="16"/>
<contactref element="MODE" pad="A2"/>
</signal>
<signal name="SCK">
<contactref element="J1" pad="3"/>
<contactref element="U1" pad="17"/>
<contactref element="L" pad="A"/>
</signal>
<signal name="A0">
<contactref element="U1" pad="23"/>
<contactref element="F" pad="A2"/>
</signal>
<signal name="A1">
<contactref element="U1" pad="24"/>
<contactref element="E" pad="A2"/>
</signal>
<signal name="A2">
<contactref element="U1" pad="25"/>
<contactref element="D" pad="A2"/>
</signal>
<signal name="A3">
<contactref element="U1" pad="26"/>
<contactref element="C" pad="A2"/>
</signal>
<signal name="A4">
<contactref element="U1" pad="27"/>
<contactref element="B" pad="A2"/>
</signal>
<signal name="A5">
<contactref element="U1" pad="28"/>
<contactref element="A" pad="A2"/>
</signal>
<signal name="A6">
<contactref element="U1" pad="19"/>
</signal>
<signal name="A7">
<contactref element="U1" pad="22"/>
</signal>
<signal name="D0">
<contactref element="U1" pad="30"/>
<contactref element="RX" pad="1"/>
</signal>
<signal name="D1">
<contactref element="U1" pad="31"/>
<contactref element="TX" pad="1"/>
</signal>
<signal name="D2">
<contactref element="U1" pad="32"/>
<contactref element="PWR" pad="A2"/>
</signal>
<signal name="D3">
<contactref element="U1" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="JMP2" pad="3"/>
</signal>
<signal name="D4">
<contactref element="U1" pad="2"/>
<contactref element="PLAY" pad="A2"/>
</signal>
<signal name="D5">
<contactref element="U1" pad="9"/>
<contactref element="PAUSE" pad="A2"/>
</signal>
<signal name="D6">
<contactref element="U1" pad="10"/>
<contactref element="FFW" pad="A2"/>
</signal>
<signal name="D7">
<contactref element="U1" pad="11"/>
<contactref element="REW" pad="A2"/>
</signal>
<signal name="D8">
<contactref element="U1" pad="12"/>
<contactref element="VOLUP" pad="A2"/>
</signal>
<signal name="D9">
<contactref element="U1" pad="13"/>
<contactref element="VOLDN" pad="A2"/>
</signal>
<signal name="D10">
<contactref element="U1" pad="14"/>
<contactref element="STOP" pad="A2"/>
</signal>
<signal name="N$1">
<contactref element="L" pad="C"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="R2" pad="2"/>
<contactref element="IRLED" pad="K"/>
</signal>
<signal name="N$5">
<contactref element="Q1" pad="1"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="JMP2" pad="2"/>
<contactref element="IRLED" pad="A"/>
</signal>
<signal name="N$6">
<contactref element="JMP1" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="JMP1" pad="1"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$7">
<contactref element="S1" pad="1"/>
<contactref element="BT1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
