<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0.75" y1="0" x2="16" y2="0" width="0" layer="20"/>
<wire x1="16" y1="0" x2="16" y2="16.125" width="0" layer="20"/>
<wire x1="16" y1="16.125" x2="0.75" y2="16.125" width="0" layer="20"/>
<wire x1="0.75" y1="16.125" x2="0.75" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="led">
<description>&lt;b&gt;LEDs&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;&lt;br&gt;
Extended by Federico Battaglin &lt;author&gt;&amp;lt;federico.rd@fdpinternational.com&amp;gt;&lt;/author&gt; with DUOLED</description>
<packages>
<package name="SML0603">
<description>&lt;b&gt;SML0603-XXX (HIGH INTENSITY) LED&lt;/b&gt;&lt;p&gt;
&lt;table&gt;
&lt;tr&gt;&lt;td&gt;AG3K&lt;/td&gt;&lt;td&gt;AQUA GREEN&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;B1K&lt;/td&gt;&lt;td&gt;SUPER BLUE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;R1K&lt;/td&gt;&lt;td&gt;SUPER RED&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;R3K&lt;/td&gt;&lt;td&gt;ULTRA RED&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;O3K&lt;/td&gt;&lt;td&gt;SUPER ORANGE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;O3KH&lt;/td&gt;&lt;td&gt;SOFT ORANGE&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;Y3KH&lt;/td&gt;&lt;td&gt;SUPER YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;Y3K&lt;/td&gt;&lt;td&gt;SUPER YELLOW&lt;/td&gt;&lt;/tr&gt;
&lt;tr&gt;&lt;td&gt;2CW&lt;/td&gt;&lt;td&gt;WHITE&lt;/td&gt;&lt;/tr&gt;
&lt;/table&gt;
Source: http://www.ledtronics.com/ds/smd-0603/Dstr0092.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-IC-Microcontroller">
<description>&lt;h3&gt;SparkFun Microcontrollers&lt;/h3&gt;
This library contains microcontrollers.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SSOP20">
<description>&lt;b&gt;Shrink Small Outline Package&lt;/b&gt;&lt;p&gt;
package type SS</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X01NS_KIT">
<description>&lt;h3&gt;Plated Through Hole - No Silk Outline Kit Version&lt;/h3&gt;
&lt;p&gt; Mask on only one side to make soldering in kits easier.
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:1&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_01&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LED1" library="led" package="SML0603" value="A"/>
<element name="LED10" library="led" package="SML0603" value="J"/>
<element name="LED11" library="led" package="SML0603" value="K"/>
<element name="LED12" library="led" package="SML0603" value="L"/>
<element name="LED13" library="led" package="SML0603" value="M"/>
<element name="LED14" library="led" package="SML0603" value="N"/>
<element name="LED15" library="led" package="SML0603" value="O"/>
<element name="LED16" library="led" package="SML0603" value="P"/>
<element name="LED17" library="led" package="SML0603" value="Q"/>
<element name="LED18" library="led" package="SML0603" value="R"/>
<element name="LED19" library="led" package="SML0603" value="S"/>
<element name="LED2" library="led" package="SML0603" value="B"/>
<element name="LED20" library="led" package="SML0603" value="T"/>
<element name="LED3" library="led" package="SML0603" value="C"/>
<element name="LED4" library="led" package="SML0603" value="D"/>
<element name="LED5" library="led" package="SML0603" value="E"/>
<element name="LED6" library="led" package="SML0603" value="F"/>
<element name="LED7" library="led" package="SML0603" value="G"/>
<element name="LED8" library="led" package="SML0603" value="H"/>
<element name="LED9" library="led" package="SML0603" value="I"/>
<element name="IC1" library="SparkFun-IC-Microcontroller" package="SSOP20" value="PIC16F88-SSOP">
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X01NS_KIT" value="">
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="1X01NS_KIT" value="">
<attribute name="VALUE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X01NS_KIT" value="">
<attribute name="VALUE"/>
</element>
<element name="J4" library="SparkFun-Connectors" package="1X01NS_KIT" value="">
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="1X01NS_KIT" value="">
<attribute name="VALUE"/>
</element>
<element name="J6" library="SparkFun-Connectors" package="1X01NS_KIT" value="">
<attribute name="VALUE"/>
</element>
<element name="J7" library="SparkFun-Connectors" package="1X01NS_KIT" value="">
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="A0">
<contactref element="LED1" pad="A"/>
<contactref element="LED18" pad="A"/>
<contactref element="LED13" pad="A"/>
<contactref element="LED14" pad="A"/>
<contactref element="LED15" pad="A"/>
<contactref element="LED16" pad="A"/>
<contactref element="LED17" pad="A"/>
<contactref element="IC1" pad="18"/>
</signal>
<signal name="A1">
<contactref element="LED2" pad="A"/>
<contactref element="LED12" pad="A"/>
<contactref element="LED19" pad="A"/>
<contactref element="IC1" pad="17"/>
</signal>
<signal name="A2">
<contactref element="LED3" pad="A"/>
<contactref element="LED11" pad="A"/>
<contactref element="LED20" pad="A"/>
<contactref element="IC1" pad="12"/>
</signal>
<signal name="A3">
<contactref element="LED4" pad="A"/>
<contactref element="LED5" pad="A"/>
<contactref element="LED10" pad="A"/>
<contactref element="LED9" pad="A"/>
<contactref element="LED8" pad="A"/>
<contactref element="LED7" pad="A"/>
<contactref element="LED6" pad="A"/>
<contactref element="IC1" pad="11"/>
</signal>
<signal name="C0">
<contactref element="LED4" pad="C"/>
<contactref element="LED1" pad="C"/>
<contactref element="LED2" pad="C"/>
<contactref element="LED3" pad="C"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="C1">
<contactref element="LED5" pad="C"/>
<contactref element="LED18" pad="C"/>
<contactref element="IC1" pad="2"/>
</signal>
<signal name="C2">
<contactref element="LED6" pad="C"/>
<contactref element="LED17" pad="C"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="C3">
<contactref element="LED7" pad="C"/>
<contactref element="LED16" pad="C"/>
<contactref element="LED19" pad="C"/>
<contactref element="LED20" pad="C"/>
<contactref element="IC1" pad="7"/>
</signal>
<signal name="C4">
<contactref element="LED8" pad="C"/>
<contactref element="LED15" pad="C"/>
<contactref element="IC1" pad="8"/>
</signal>
<signal name="C5">
<contactref element="LED9" pad="C"/>
<contactref element="LED14" pad="C"/>
<contactref element="IC1" pad="9"/>
</signal>
<signal name="C6">
<contactref element="LED10" pad="C"/>
<contactref element="LED13" pad="C"/>
<contactref element="LED12" pad="C"/>
<contactref element="LED11" pad="C"/>
<contactref element="IC1" pad="10"/>
</signal>
<signal name="MCLR">
<contactref element="IC1" pad="4"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="SDA">
<contactref element="J6" pad="1"/>
<contactref element="IC1" pad="20"/>
</signal>
<signal name="SCL">
<contactref element="J7" pad="1"/>
<contactref element="IC1" pad="19"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="6"/>
<contactref element="IC1" pad="5"/>
<contactref element="J3" pad="1"/>
<contactref element="J4" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="IC1" pad="15"/>
<contactref element="IC1" pad="16"/>
<contactref element="J2" pad="1"/>
<contactref element="J1" pad="1"/>
</signal>
<signal name="PGC">
<contactref element="IC1" pad="13"/>
</signal>
<signal name="PGD">
<contactref element="IC1" pad="14"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
