<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.1">
<drawing>
<board>
<plain>
<wire x1="58.42" y1="35.56" x2="93.96" y2="35.56" width="0" layer="20"/>
<wire x1="93.96" y1="35.56" x2="93.96" y2="63.17" width="0" layer="20"/>
<wire x1="93.96" y1="63.17" x2="58.42" y2="63.17" width="0" layer="20"/>
<wire x1="58.42" y1="63.17" x2="58.42" y2="35.56" width="0" layer="20"/>
</plain>
<libraries>
<library name="FAB_Hello">
<packages>
<package name="1206">
<description>&lt;b&gt;RESISTOR&lt;/b&gt;&lt;p&gt;
chip</description>
</package>
</packages>
</library>
<library name="fab">
<packages>
<package name="R1206FAB">
</package>
</packages>
</library>
<library name="WEIDMULLER-PM5.08_2_90BLK">
<description>&lt;b&gt; Developed By element14 &lt;/b&gt;&lt;p&gt; 

For feedback and Technical support please contact reach from below:
&lt;br&gt; Tech Support e-mail  : &lt;a href="mailto:CAD_Tech@element14.com"&gt;CAD_Tech@element14.com&lt;/a&gt;
&lt;br&gt;Community website: &lt;a href=http://www.element14.com/community/community/knode/cad_tools/cadsoft_eagle/eagle_cad_libraries&gt;
EAGLE CAD Libraries on element14&lt;/a&gt;</description>
<packages>
<package name="WEIDMULLER_PM5.08_2">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="FAB_Hello" package="1206" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="FAB_Hello" package="1206" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="FAB_Hello" package="1206" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="fab" package="R1206FAB" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="fab" package="R1206FAB" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="fab" package="R1206FAB" value="4.7K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T1" library="WEIDMULLER-PM5.08_2_90BLK" package="WEIDMULLER_PM5.08_2" value="">
<attribute name="MPN" value="PM5.08/2/90 BLK"/>
<attribute name="OC_FARNELL" value="1131855 "/>
<attribute name="OC_NEWARK" value="26M1980 "/>
<attribute name="PACKAGE" value="TH-R/A"/>
<attribute name="SUPPLIER" value="WEIDMULLER "/>
</element>
<element name="T2" library="WEIDMULLER-PM5.08_2_90BLK" package="WEIDMULLER_PM5.08_2" value="">
<attribute name="MPN" value="PM5.08/2/90 BLK"/>
<attribute name="OC_FARNELL" value="1131855 "/>
<attribute name="OC_NEWARK" value="26M1980 "/>
<attribute name="PACKAGE" value="TH-R/A"/>
<attribute name="SUPPLIER" value="WEIDMULLER "/>
</element>
<element name="T3" library="WEIDMULLER-PM5.08_2_90BLK" package="WEIDMULLER_PM5.08_2" value="">
<attribute name="MPN" value="PM5.08/2/90 BLK"/>
<attribute name="OC_FARNELL" value="1131855 "/>
<attribute name="OC_NEWARK" value="26M1980 "/>
<attribute name="PACKAGE" value="TH-R/A"/>
<attribute name="SUPPLIER" value="WEIDMULLER "/>
</element>
<element name="POWER" library="WEIDMULLER-PM5.08_2_90BLK" package="WEIDMULLER_PM5.08_2" value="">
<attribute name="MPN" value="PM5.08/2/90 BLK"/>
<attribute name="OC_FARNELL" value="1131855 "/>
<attribute name="OC_NEWARK" value="26M1980 "/>
<attribute name="PACKAGE" value="TH-R/A"/>
<attribute name="SUPPLIER" value="WEIDMULLER "/>
</element>
</elements>
<signals>
<signal name="VCC">
<contactref element="R1" pad="1"/>
<contactref element="R3" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="POWER" pad="2"/>
</signal>
<signal name="T1">
<contactref element="R1" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="T1" pad="2"/>
</signal>
<signal name="T2">
<contactref element="R2" pad="2"/>
<contactref element="C2" pad="1"/>
<contactref element="T2" pad="2"/>
</signal>
<signal name="T3">
<contactref element="R3" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="T3" pad="2"/>
</signal>
<signal name="GND">
<contactref element="C1" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="T1" pad="1"/>
<contactref element="T2" pad="1"/>
<contactref element="POWER" pad="1"/>
<contactref element="T3" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
