<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<text>Geppetto Electronics
Pi EVSE Hat
v4.1.1</text>
<text>Pilot</text>
<text>GFI</text>
<text>GFI
Test</text>
<text>Cur
Sense</text>
<text>HV Board</text>
<text>+5V</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="1210">
</package>
<package name="PANASONIC_D">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="SOD-323F">
</package>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMA-DIODE">
<description>&lt;B&gt;Diode&lt;/B&gt;&lt;p&gt;
Basic SMA packaged diode. Good for reverse polarization protection. Common part #: MBRA140</description>
</package>
<package name="SOT23-3">
</package>
</packages>
</library>
<library name="TC1044S">
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; Fits JEDEC packages (narrow SOIC-8)</description>
</package>
</packages>
</library>
<library name="AP2331">
<packages>
<package name="SOT23-5">
</package>
<package name="SOT23-6">
</package>
</packages>
</library>
<library name="AD5680">
<packages>
<package name="SO014">
</package>
</packages>
</library>
<library name="SparkFun-Connectors-new">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-3.5MM-3">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SCREWTERMINAL-5MM-2">
</package>
<package name="SCREWTERMINAL-3.5MM-2">
</package>
</packages>
</library>
<library name="dcx(xxxx)u">
<packages>
<package name="SOT23-6">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="AXIAL-0.3">
</package>
</packages>
</library>
<library name="con-hirose">
<description>&lt;b&gt;Hirose Connectors&lt;/b&gt;&lt;p&gt;
www.hirose.co.jp&lt;p&gt;
Include : &lt;br&gt;
con-hirose-df12d(3.0)60dp0.5v80.lbr from Bob Starr &amp;lt;rtzaudio@mindspring.com&amp;gt;&lt;br&gt;
con-hirose.lbr from Bob Starr &amp;lt;rtzaudio@mindspring.com&amp;gt;&lt;br&gt;</description>
<packages>
<package name="FH21-10S-1DSA">
<description>&lt;b&gt;FPC Connector&lt;/b&gt;&lt;p&gt;
1 MM, vertical</description>
</package>
</packages>
</library>
<library name="raspberrypi_bastelstube_v13">
<description>&lt;b&gt;Raspberry Pi&lt;/b&gt; by &lt;b&gt;Martin's Bastelstube&lt;/b&gt;
&lt;p&gt;
Different shapes of piggyback boards for the famous &amp;amp; fabulous
&lt;a href="http://www.raspberrypi.org/"&gt;Raspberry Pi&lt;/a&gt; computer.
&lt;p&gt;
The outline of the Raspberry Pi board is drawn on layer 52 bDocu, so you can make it invisible if necessary.&lt;br/&gt;
Recommendation: Start your design with RASPI_BOARD_*_FULL, so you are aware of all the big components and
connectors when you're drawing the dimensions of your board and placing your own components.&lt;br/&gt;
Later, you can simply change the package of your Raspberry Pi connector to the RASPI_BOARD_*_EDGES type,
so you can concentrate on your own design.
&lt;p&gt;
Most of my board packages don't have the outline drawn in layer 20 Dimension (except the HATs). This allows you to deviate from the original Raspberry Pi board shape, e.g. when you need more space behind the GPIO connector for the routing of the power supply lines. If you want to stick exactly to the Raspberry Pi board shape, then just draw the Dimension layer right on the lines in layer bDocu.

&lt;hr&gt;&lt;br/&gt;

Version 1.3
&lt;ul&gt;
&lt;li&gt;Added the shape and dimensions of the HAT board with &amp;amp; without the camera and display flex cutout&lt;/li&gt;
&lt;li&gt;New GPIO connector version (suffix &amp;quot;#&amp;quot;) with all pins connected (no more &amp;quot;n.c.&amp;quot; pins)&lt;/li&gt;
&lt;li&gt;Two more &amp;quot;AB-&amp;quot; boards with 5 and 6 drill holes / pads, mechanically compatible with all RasPi versions&lt;/li&gt;
&lt;/ul&gt;

Version 1.2
&lt;ul&gt;
&lt;li&gt;Added a 26-pin GPIO connector with board dimensions of model B+&lt;br/&gt;
       for backwards compatibility with models A and B, named &amp;quot;B-&amp;quot;&lt;/li&gt;
&lt;/ul&gt;

Version 1.1
&lt;ul&gt;
&lt;li&gt;New GPIO connector and board dimensions of model B+&lt;/li&gt;
&lt;li&gt;Old connector and board (for models A and B) renamed to AB&lt;/li&gt;
&lt;li&gt;GPIO pin numbers on connector changed to match Rev2 board design&lt;/li&gt;
&lt;/ul&gt;

Version 1.0
&lt;ul&gt;
&lt;li&gt;More detailed descriptions for all components&lt;/li&gt;
&lt;li&gt;Published on Cadsoft webpage&lt;/li&gt;
&lt;/ul&gt;

&lt;hr&gt;&lt;br/&gt;

Designed by &lt;a href="http://bastelstube.rocci.net/"&gt;Martin's Bastelstube&lt;/a&gt;&lt;br&gt;
Comments / complaints / bug reports / suggestions to &lt;author&gt;eightbit@web.de&lt;/author&gt;</description>
<packages>
<package name="RASPI_BOARD_B+HAT_DF_CF">
<description>Raspberry Pi board model B+ HAT board&lt;br/&gt;
Official outline with cutouts for display &amp;amp; camera flex connector</description>
</package>
</packages>
</library>
<library name="diode">
<description>&lt;b&gt;Diodes&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola : www.onsemi.com
&lt;li&gt;Fairchild : www.fairchildsemi.com
&lt;li&gt;Philips : www.semiconductors.com
&lt;li&gt;Vishay : www.vishay.de
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SOD123">
<description>&lt;b&gt;Diode&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="74xx-little-us">
<description>&lt;b&gt;Single and Dual Gates Family, US symbols&lt;/b&gt;&lt;p&gt;
Little logic devices from Texas Instruments&lt;br&gt;
TinyLogic(R) from FAIRCHILD Semiconductor TM
&lt;p&gt;
&lt;author&gt;Created by evgeni@eniks.com&lt;/author&gt;&lt;br&gt;
&lt;author&gt;Extended by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SSOP08">
<description>&lt;b&gt;SMT SSOP 08&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="74xx-us">
<description>&lt;b&gt;TTL Devices, 74xx Series with US Symbols&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Texas Instruments &lt;i&gt;TTL Data Book&lt;/i&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;Volume 1, 1996.
&lt;li&gt;TTL Data Book, Volume 2 , 1993
&lt;li&gt;National Seminconductor Databook 1990, ALS/LS Logic
&lt;li&gt;ttl 74er digital data dictionary, ECA Electronic + Acustic GmbH, ISBN 3-88109-032-0
&lt;li&gt;http://icmaster.com/ViewCompare.asp
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO14">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package 8&lt;/b&gt;&lt;br&gt;
NS Package M08A</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SRN6045">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="10µF">
<attribute name="NAME"/>
</element>
<element name="C10" library="SparkFun-Capacitors" package="0805" value="10µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="SparkFun-Capacitors" package="0805" value="0.1µF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="0.022µF">
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="1210" value="10µF">
<attribute name="NAME"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="1210" value="10µF">
<attribute name="NAME"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="0.1µF">
<attribute name="NAME"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0805" value="0.1µF">
<attribute name="NAME"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="0805" value="0.1µF">
<attribute name="NAME"/>
</element>
<element name="C9" library="SparkFun-Capacitors" package="0805" value="0.1µF">
<attribute name="NAME"/>
</element>
<element name="D1" library="adafruit" package="SOD-323F" value="1N4148">
<attribute name="NAME"/>
</element>
<element name="D5" library="diode" package="SOD123" value="MMSZ5222B">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="22"/>
</element>
<element name="D2" library="SparkFun-DiscreteSemi" package="SMA-DIODE" value="P6KE16CA">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-08053"/>
</element>
<element name="D4" library="diode" package="SOD123" value="MMSZ5222B">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="22"/>
</element>
<element name="D3" library="diode" package="SOD123" value="MMSZ5222B">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="22"/>
</element>
<element name="D6" library="diode" package="SOD123" value="MMSZ5222B">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="22"/>
</element>
<element name="IC1" library="linear" package="SO08" value="LM358D">
<attribute name="NAME"/>
</element>
<element name="IC5" library="TC1044S" package="SO08" value="TC1044S_OA">
<attribute name="NAME"/>
</element>
<element name="IC7" library="AP2331" package="SOT23-5" value="STWD100NYWY3F">
<attribute name="NAME"/>
</element>
<element name="IC8" library="AD5680" package="SO014" value="MCP3004-I/SL">
<attribute name="NAME"/>
</element>
<element name="JP3" library="SparkFun-Connectors-new" package="SCREWTERMINAL-3.5MM-3" value="M03SCREW">
<attribute name="NAME"/>
</element>
<element name="JP4" library="SparkFun-Connectors" package="SCREWTERMINAL-5MM-2" value="PILOT">
<attribute name="NAME"/>
</element>
<element name="JP5" library="SparkFun-Connectors" package="SCREWTERMINAL-3.5MM-2" value="CURRENT">
<attribute name="NAME"/>
</element>
<element name="Q2" library="dcx(xxxx)u" package="SOT23-6" value="DMG6602SVTQ">
<attribute name="NAME"/>
</element>
<element name="Q1" library="dcx(xxxx)u" package="SOT23-6" value="DMG6602SVTQ">
<attribute name="NAME"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="330Ω">
<attribute name="NAME"/>
</element>
<element name="R10" library="SparkFun-Resistors" package="0805" value="200kΩ">
<attribute name="NAME"/>
</element>
<element name="R13" library="SparkFun-Resistors" package="0805" value="100kΩ">
<attribute name="NAME"/>
</element>
<element name="R14" library="SparkFun-Resistors" package="0805" value="56kΩ">
<attribute name="NAME"/>
</element>
<element name="R15" library="SparkFun-Resistors" package="0805" value="10kΩ">
<attribute name="NAME"/>
</element>
<element name="R16" library="SparkFun-Resistors" package="0805" value="1kΩ">
<attribute name="NAME"/>
</element>
<element name="R17" library="SparkFun-Resistors" package="0805" value="1kΩ">
<attribute name="NAME"/>
</element>
<element name="R18" library="SparkFun-Resistors" package="0805" value="4.7kΩ">
<attribute name="NAME"/>
</element>
<element name="R19" library="SparkFun-Resistors" package="0805" value="4.7kΩ">
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="330Ω">
<attribute name="NAME"/>
</element>
<element name="R22" library="SparkFun-Resistors" package="0805" value="10kΩ">
<attribute name="NAME"/>
</element>
<element name="R24" library="SparkFun-Resistors" package="0805" value="100kΩ">
<attribute name="NAME"/>
</element>
<element name="R25" library="SparkFun-Resistors" package="0805" value="20kΩ">
<attribute name="NAME"/>
</element>
<element name="R26" library="SparkFun-Resistors" package="0805" value="10kΩ">
<attribute name="NAME"/>
</element>
<element name="R12" library="SparkFun-Resistors" package="0805" value="10kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R23" library="SparkFun-Resistors" package="AXIAL-0.3" value="Rb">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R21" library="SparkFun-Resistors" package="0805" value="560Ω">
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="1kΩ">
<attribute name="NAME"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="100kΩ">
<attribute name="NAME"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0805" value="150Ω">
<attribute name="NAME"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0805" value="10kΩ">
<attribute name="NAME"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0805" value="10kΩ">
<attribute name="NAME"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0805" value="10kΩ">
<attribute name="NAME"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0805" value="1kΩ 1%">
<attribute name="NAME"/>
</element>
<element name="JP2" library="con-hirose" package="FH21-10S-1DSA" value="FH21-10S-1DSA">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="0"/>
</element>
<element name="JP1" library="raspberrypi_bastelstube_v13" package="RASPI_BOARD_B+HAT_DF_CF" value="RASPI_BOARD_B+#_HDC"/>
<element name="R20" library="SparkFun-Resistors" package="0805" value="10kΩ">
<attribute name="NAME"/>
</element>
<element name="R31" library="SparkFun-Resistors" package="0805" value="10kΩ">
<attribute name="NAME"/>
</element>
<element name="IC4" library="74xx-little-us" package="SSOP08" value="74HC3G16">
<attribute name="NAME"/>
</element>
<element name="C15" library="SparkFun-Capacitors" package="0805" value="0.1µF">
<attribute name="NAME"/>
</element>
<element name="IC3" library="74xx-little-us" package="SSOP08" value="741G74">
<attribute name="NAME"/>
</element>
<element name="IC2" library="74xx-us" package="SO14" value="74LS00D">
<attribute name="NAME"/>
</element>
<element name="R23B" library="SparkFun-Resistors" package="0805" value="Rb"/>
<element name="R11" library="SparkFun-Resistors" package="0805" value="10kΩ">
<attribute name="NAME"/>
</element>
<element name="L1" library="SparkFun-Passives" package="SRN6045" value="4.7µH">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="NDUC-11627"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="1210" value="10µF">
<attribute name="NAME"/>
</element>
<element name="IC6" library="AP2331" package="SOT23-6" value="AP6320XWU">
<attribute name="NAME"/>
</element>
<element name="C14" library="SparkFun-Capacitors" package="0805" value="0.1uF">
<attribute name="NAME"/>
</element>
<element name="C11" library="SparkFun-Capacitors" package="PANASONIC_D" value="47µF">
<attribute name="NAME"/>
</element>
<element name="Q4" library="SparkFun-DiscreteSemi" package="SOT23-3" value="BSS84">
<attribute name="NAME"/>
</element>
<element name="R27" library="SparkFun-Resistors" package="0805" value="10kΩ">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q5" library="SparkFun-DiscreteSemi" package="SOT23-3" value="BSS84">
<attribute name="NAME"/>
</element>
<element name="R28" library="SparkFun-Resistors" package="0805" value="330Ω">
<attribute name="NAME"/>
</element>
<element name="LED1" library="adafruit" package="CHIPLED_0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q6" library="SparkFun-DiscreteSemi" package="SOT23-3" value="BSS84">
<attribute name="NAME"/>
</element>
<element name="R29" library="SparkFun-Resistors" package="0805" value="330Ω">
<attribute name="NAME"/>
</element>
<element name="LED2" library="adafruit" package="CHIPLED_0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="Q3" library="dcx(xxxx)u" package="SOT23-6" value="DMG6602SVTQ">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="N$3">
<contactref element="IC3" pad="3"/>
<contactref element="IC2" pad="2"/>
<contactref element="Q6" pad="1"/>
</signal>
<signal name="RELAY_OUT">
<contactref element="JP2" pad="9"/>
<contactref element="Q4" pad="3"/>
<contactref element="R27" pad="1"/>
</signal>
<signal name="N$5">
<contactref element="IC7" pad="3"/>
<contactref element="IC2" pad="8"/>
<contactref element="IC2" pad="12"/>
</signal>
<signal name="PI_RELAY">
<contactref element="JP1" pad="11"/>
<contactref element="R20" pad="2"/>
<contactref element="IC2" pad="1"/>
<contactref element="IC2" pad="9"/>
<contactref element="IC2" pad="10"/>
</signal>
<signal name="N$2">
<contactref element="IC3" pad="6"/>
<contactref element="IC2" pad="11"/>
</signal>
<signal name="GND">
<contactref element="IC1" pad="3"/>
<contactref element="R2" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="D6" pad="C"/>
<contactref element="R7" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="IC7" pad="2"/>
<contactref element="C9" pad="2"/>
<contactref element="R25" pad="1"/>
<contactref element="IC1" pad="4"/>
<contactref element="C7" pad="2"/>
<contactref element="C6" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="IC5" pad="3"/>
<contactref element="C4" pad="1"/>
<contactref element="JP2" pad="1"/>
<contactref element="JP2" pad="10"/>
<contactref element="JP1" pad="6"/>
<contactref element="JP1" pad="39"/>
<contactref element="JP1" pad="34"/>
<contactref element="JP1" pad="30"/>
<contactref element="JP1" pad="25"/>
<contactref element="JP1" pad="20"/>
<contactref element="JP1" pad="9"/>
<contactref element="JP1" pad="14"/>
<contactref element="R13" pad="1"/>
<contactref element="D2" pad="A"/>
<contactref element="Q2" pad="5"/>
<contactref element="IC8" pad="7"/>
<contactref element="IC8" pad="12"/>
<contactref element="C10" pad="2"/>
<contactref element="C12" pad="2"/>
<contactref element="R12" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="R20" pad="1"/>
<contactref element="R31" pad="1"/>
<contactref element="IC4" pad="4"/>
<contactref element="C15" pad="2"/>
<contactref element="IC3" pad="1"/>
<contactref element="IC3" pad="2"/>
<contactref element="IC3" pad="4"/>
<contactref element="IC2" pad="7"/>
<contactref element="JP3" pad="3"/>
<contactref element="C8" pad="2"/>
<contactref element="IC6" pad="4"/>
<contactref element="C11" pad="-"/>
<contactref element="R15" pad="2"/>
<contactref element="R27" pad="2"/>
<contactref element="R28" pad="2"/>
<contactref element="R29" pad="2"/>
<contactref element="Q3" pad="5"/>
</signal>
<signal name="PI_GFI_CLR">
<contactref element="JP1" pad="13"/>
<contactref element="R31" pad="2"/>
<contactref element="IC2" pad="13"/>
</signal>
<signal name="GFI_LOCK">
<contactref element="IC4" pad="6"/>
<contactref element="IC3" pad="5"/>
</signal>
<signal name="N$4">
<contactref element="R1" pad="1"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="N$6">
<contactref element="R3" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="JP3" pad="2"/>
<contactref element="D5" pad="C"/>
</signal>
<signal name="N$7">
<contactref element="R3" pad="1"/>
<contactref element="IC1" pad="2"/>
<contactref element="R4" pad="2"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="1"/>
<contactref element="D1" pad="A"/>
</signal>
<signal name="N$9">
<contactref element="D1" pad="C"/>
<contactref element="R4" pad="1"/>
<contactref element="C2" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="R5" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="R5" pad="1"/>
<contactref element="IC1" pad="5"/>
</signal>
<signal name="GFI">
<contactref element="IC1" pad="7"/>
<contactref element="R6" pad="1"/>
<contactref element="IC2" pad="4"/>
<contactref element="IC2" pad="5"/>
</signal>
<signal name="GFI_TEST">
<contactref element="R7" pad="2"/>
<contactref element="JP1" pad="18"/>
<contactref element="Q3" pad="1"/>
</signal>
<signal name="N$13">
<contactref element="R8" pad="2"/>
<contactref element="Q3" pad="3"/>
<contactref element="Q3" pad="6"/>
</signal>
<signal name="N$14">
<contactref element="R1" pad="2"/>
<contactref element="Q3" pad="4"/>
</signal>
<signal name="+5V">
<contactref element="R8" pad="1"/>
<contactref element="R24" pad="2"/>
<contactref element="IC1" pad="8"/>
<contactref element="C7" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="JP1" pad="4"/>
<contactref element="JP1" pad="2"/>
<contactref element="R14" pad="1"/>
<contactref element="IC8" pad="13"/>
<contactref element="IC8" pad="14"/>
<contactref element="C10" pad="1"/>
<contactref element="C12" pad="1"/>
<contactref element="R26" pad="1"/>
<contactref element="IC3" pad="8"/>
<contactref element="IC2" pad="14"/>
<contactref element="IC7" pad="5"/>
<contactref element="C9" pad="1"/>
<contactref element="JP2" pad="3"/>
<contactref element="IC6" pad="1"/>
<contactref element="L1" pad="2"/>
<contactref element="C11" pad="+"/>
<contactref element="JP4" pad="1"/>
<contactref element="Q4" pad="2"/>
<contactref element="Q5" pad="2"/>
<contactref element="Q6" pad="2"/>
<contactref element="Q3" pad="2"/>
</signal>
<signal name="+3V3">
<contactref element="JP1" pad="17"/>
<contactref element="Q2" pad="2"/>
<contactref element="IC4" pad="8"/>
<contactref element="C15" pad="1"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="PI_WD">
<contactref element="JP1" pad="7"/>
<contactref element="R11" pad="2"/>
<contactref element="IC7" pad="4"/>
</signal>
<signal name="N$23">
<contactref element="R24" pad="1"/>
<contactref element="R25" pad="2"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="N$29">
<contactref element="D6" pad="A"/>
<contactref element="D5" pad="A"/>
</signal>
<signal name="-12V">
<contactref element="IC5" pad="5"/>
<contactref element="C4" pad="2"/>
<contactref element="R17" pad="1"/>
<contactref element="Q1" pad="5"/>
</signal>
<signal name="+12V">
<contactref element="IC5" pad="1"/>
<contactref element="IC5" pad="8"/>
<contactref element="R16" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="JP2" pad="2"/>
<contactref element="C8" pad="1"/>
<contactref element="IC6" pad="3"/>
<contactref element="IC6" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="IC5" pad="2"/>
<contactref element="C3" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="C3" pad="2"/>
<contactref element="IC5" pad="4"/>
</signal>
<signal name="RELAY_TEST">
<contactref element="JP2" pad="5"/>
<contactref element="IC4" pad="3"/>
</signal>
<signal name="PILOT_TTL">
<contactref element="JP1" pad="12"/>
<contactref element="R15" pad="1"/>
<contactref element="Q2" pad="3"/>
<contactref element="Q2" pad="1"/>
</signal>
<signal name="PI_RLY_TST">
<contactref element="JP1" pad="16"/>
<contactref element="IC4" pad="5"/>
</signal>
<signal name="MOSI">
<contactref element="JP1" pad="19"/>
<contactref element="IC8" pad="9"/>
</signal>
<signal name="MISO">
<contactref element="IC8" pad="10"/>
<contactref element="IC4" pad="1"/>
</signal>
<signal name="SCK">
<contactref element="JP1" pad="23"/>
<contactref element="IC8" pad="11"/>
</signal>
<signal name="!CS0">
<contactref element="JP1" pad="24"/>
<contactref element="IC8" pad="8"/>
</signal>
<signal name="PI_GFI">
<contactref element="JP1" pad="15"/>
<contactref element="IC4" pad="2"/>
</signal>
<signal name="AC_VOLTS">
<contactref element="JP2" pad="4"/>
<contactref element="IC8" pad="3"/>
</signal>
<signal name="PILOT_RD">
<contactref element="R10" pad="2"/>
<contactref element="R13" pad="2"/>
<contactref element="R14" pad="2"/>
<contactref element="IC8" pad="1"/>
</signal>
<signal name="PILOT_B">
<contactref element="R9" pad="2"/>
<contactref element="R10" pad="1"/>
<contactref element="D2" pad="C"/>
<contactref element="JP4" pad="2"/>
</signal>
<signal name="N$15">
<contactref element="R19" pad="2"/>
<contactref element="Q2" pad="4"/>
</signal>
<signal name="N$19">
<contactref element="R18" pad="2"/>
<contactref element="Q2" pad="6"/>
</signal>
<signal name="N$20">
<contactref element="R9" pad="1"/>
<contactref element="Q1" pad="4"/>
<contactref element="Q1" pad="6"/>
</signal>
<signal name="N$21">
<contactref element="R16" pad="1"/>
<contactref element="R18" pad="1"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$22">
<contactref element="R17" pad="2"/>
<contactref element="R19" pad="1"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="CURRENT_RD">
<contactref element="D3" pad="C"/>
<contactref element="R21" pad="1"/>
<contactref element="IC8" pad="2"/>
</signal>
<signal name="N$24">
<contactref element="R26" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="R23" pad="P$1"/>
<contactref element="D4" pad="C"/>
<contactref element="C13" pad="2"/>
<contactref element="R23B" pad="1"/>
<contactref element="JP5" pad="1"/>
</signal>
<signal name="N$25">
<contactref element="D4" pad="A"/>
<contactref element="D3" pad="A"/>
</signal>
<signal name="N$26">
<contactref element="R21" pad="2"/>
<contactref element="R23" pad="P$2"/>
<contactref element="R23B" pad="2"/>
<contactref element="JP5" pad="2"/>
</signal>
<signal name="N$27">
<contactref element="IC7" pad="1"/>
<contactref element="R22" pad="2"/>
<contactref element="IC3" pad="7"/>
</signal>
<signal name="PI_MISO">
<contactref element="JP1" pad="21"/>
<contactref element="IC4" pad="7"/>
</signal>
<signal name="N$30">
<contactref element="IC2" pad="6"/>
<contactref element="R22" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="L1" pad="1"/>
<contactref element="IC6" pad="5"/>
<contactref element="C14" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="IC6" pad="6"/>
<contactref element="C14" pad="1"/>
</signal>
<signal name="3V3A">
<contactref element="JP1" pad="1"/>
</signal>
<signal name="N$18">
<contactref element="Q5" pad="1"/>
<contactref element="IC2" pad="3"/>
<contactref element="Q4" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="LED1" pad="A"/>
<contactref element="Q5" pad="3"/>
</signal>
<signal name="N$28">
<contactref element="R28" pad="1"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="N$32">
<contactref element="LED2" pad="A"/>
<contactref element="Q6" pad="3"/>
</signal>
<signal name="N$33">
<contactref element="R29" pad="1"/>
<contactref element="LED2" pad="C"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
