<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="26.194" y1="30.48" x2="2" y2="30.48" width="0" layer="20"/>
<wire x1="2" y1="30.48" x2="0" y2="28.48" width="0" layer="20" curve="90"/>
<wire x1="0" y1="28.48" x2="0" y2="2" width="0" layer="20"/>
<wire x1="0" y1="2" x2="2" y2="0" width="0" layer="20" curve="90"/>
<wire x1="2" y1="0" x2="26.194" y2="0" width="0" layer="20"/>
<wire x1="26.194" y1="0" x2="28.194" y2="2" width="0" layer="20" curve="90"/>
<wire x1="28.194" y1="2" x2="28.194" y2="28.48" width="0" layer="20"/>
<wire x1="28.194" y1="28.48" x2="26.194" y2="30.48" width="0" layer="20" curve="90"/>
<text>MOUSE HAT AUG 2020</text>
<text>MOUSE OUT</text>
<text>+</text>
<text>GND</text>
<text>GND</text>
<text>GND</text>
<text>VBATT</text>
<text>VBATT</text>
<text>MCLR</text>
<text>GND</text>
<text>DATA</text>
<text>CLK</text>
<text>TX</text>
<text>RX</text>
<text>IR</text>
<text>GND</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SophiEaglev9">
<packages>
<package name="SOIC20">
</package>
<package name="TAG_CONNECT_MCP">
</package>
<package name="10MM_BATT_HOLDER">
</package>
<package name="TSOP6238">
</package>
<package name="LED_RGB_SUN">
</package>
<package name="TEST_POINT_LARGE">
</package>
<package name="SOT-363">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="0603" value="10uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-11015"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0603" value="10uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-11015"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="1X06_NO_SILK" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603" value="10k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07857"/>
</element>
<element name="U1" library="SophiEaglev9" package="SOIC20" value="PIC16LF1708">
<attribute name="NAME"/>
</element>
<element name="TC" library="SophiEaglev9" package="TAG_CONNECT_MCP" value="MCP_TAG_CONNECT"/>
<element name="J2" library="SparkFun-Connectors" package="1X06_NO_SILK" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CONN-08437"/>
<attribute name="VALUE"/>
</element>
<element name="U$2" library="SophiEaglev9" package="10MM_BATT_HOLDER" value="10MM_BATT_HOLDER"/>
<element name="U3" library="SophiEaglev9" package="TSOP6238" value="IR RECEIVER">
<attribute name="NAME"/>
</element>
<element name="U$6" library="SophiEaglev9" package="LED_RGB_SUN" value="SUN">
<attribute name="VALUE"/>
</element>
<element name="U$5" library="SophiEaglev9" package="TEST_POINT_LARGE" value="TEST_POINT"/>
<element name="U$7" library="SophiEaglev9" package="TEST_POINT_LARGE" value="TEST_POINT"/>
<element name="U$8" library="SophiEaglev9" package="TEST_POINT_LARGE" value="TEST_POINT"/>
<element name="U$9" library="SophiEaglev9" package="TEST_POINT_LARGE" value="TEST_POINT"/>
<element name="R11" library="SparkFun-Resistors" package="0603" value="0">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-08787"/>
</element>
<element name="U$10" library="SophiEaglev9" package="TEST_POINT_LARGE" value="TEST_POINT"/>
<element name="U$12" library="SophiEaglev9" package="TEST_POINT_LARGE" value="TEST_POINT"/>
<element name="U$13" library="SophiEaglev9" package="TEST_POINT_LARGE" value="TEST_POINT"/>
<element name="U2" library="SophiEaglev9" package="SOT-363" value="SSM6P35AFU">
<attribute name="NAME"/>
<attribute name="U5" value="SSM6P35AFU"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0603" value="4.7k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="4.7k"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0603" value="4.7k">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="4.7k"/>
</element>
<element name="U$14" library="SophiEaglev9" package="TEST_POINT_LARGE" value="TEST_POINT"/>
</elements>
<signals>
<signal name="RC5">
<contactref element="U1" pad="5"/>
<contactref element="U$6" pad="4"/>
</signal>
<signal name="VBATT">
<contactref element="U1" pad="1"/>
<contactref element="C2" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="J1" pad="2"/>
<contactref element="TC" pad="2"/>
<contactref element="U3" pad="3"/>
<contactref element="U$7" pad="P$1"/>
<contactref element="U$9" pad="P$1"/>
<contactref element="R11" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="R2" pad="2"/>
<contactref element="U$2" pad="3"/>
<contactref element="U$2" pad="1"/>
</signal>
<signal name="GND">
<contactref element="C2" pad="2"/>
<contactref element="U1" pad="20"/>
<contactref element="C1" pad="2"/>
<contactref element="J1" pad="3"/>
<contactref element="TC" pad="3"/>
<contactref element="U$5" pad="P$1"/>
<contactref element="U$8" pad="P$1"/>
<contactref element="U3" pad="1"/>
<contactref element="U$12" pad="P$1"/>
<contactref element="U$14" pad="P$1"/>
<contactref element="J2" pad="6"/>
<contactref element="U$2" pad="2"/>
</signal>
<signal name="MCLR">
<contactref element="J1" pad="1"/>
<contactref element="TC" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="C1" pad="1"/>
<contactref element="U1" pad="4"/>
</signal>
<signal name="RX">
<contactref element="U1" pad="12"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="TX">
<contactref element="U1" pad="10"/>
<contactref element="J2" pad="1"/>
</signal>
<signal name="RC6">
<contactref element="U1" pad="8"/>
<contactref element="R4" pad="2"/>
<contactref element="U2" pad="1"/>
</signal>
<signal name="RC7">
<contactref element="U1" pad="9"/>
</signal>
<signal name="RC4">
<contactref element="U1" pad="6"/>
<contactref element="U$6" pad="2"/>
</signal>
<signal name="RC3">
<contactref element="U1" pad="7"/>
<contactref element="J2" pad="4"/>
<contactref element="U2" pad="2"/>
</signal>
<signal name="RC0">
<contactref element="U1" pad="16"/>
</signal>
<signal name="IR_IN">
<contactref element="U1" pad="17"/>
<contactref element="U3" pad="4"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="RA4">
<contactref element="U1" pad="3"/>
</signal>
<signal name="RA5">
<contactref element="U1" pad="2"/>
<contactref element="U$6" pad="3"/>
</signal>
<signal name="ICSPDAT">
<contactref element="U1" pad="19"/>
<contactref element="J1" pad="4"/>
<contactref element="TC" pad="4"/>
</signal>
<signal name="RC1">
<contactref element="U1" pad="15"/>
</signal>
<signal name="RB4">
<contactref element="U1" pad="13"/>
<contactref element="R2" pad="1"/>
<contactref element="U2" pad="4"/>
</signal>
<signal name="ICSPCLK">
<contactref element="U1" pad="18"/>
<contactref element="J1" pad="5"/>
<contactref element="TC" pad="5"/>
</signal>
<signal name="RC2">
<contactref element="U1" pad="14"/>
<contactref element="J2" pad="5"/>
<contactref element="U2" pad="5"/>
</signal>
<signal name="RB6">
<contactref element="U1" pad="11"/>
</signal>
<signal name="N$3">
<contactref element="U$6" pad="1"/>
<contactref element="R11" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="U2" pad="3"/>
<contactref element="U$10" pad="P$1"/>
</signal>
<signal name="N$2">
<contactref element="U2" pad="6"/>
<contactref element="U$13" pad="P$1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
