(export (version D)
  (design
    (source C:\Users\Standa\Desktop\Projects\LCR\HW\Dev\LCR.sch)
    (date "23-Oct-19 9:37:34 PM")
    (tool "Eeschema (5.1.4)-1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source LCR.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref J1)
      (value USB_B_Micro)
      (footprint Connector_USB:USB_Micro-B_Molex_47346-0001)
      (datasheet ~)
      (libsource (lib Connector) (part USB_B_Micro) (description "USB Micro Type B connector"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA4A662))
    (comp (ref U2)
      (value STM32F030F4Px)
      (footprint Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm)
      (datasheet http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/DM00088500.pdf)
      (libsource (lib MCU_ST_STM32F0) (part STM32F030F4Px) (description "ARM Cortex-M0 MCU, 16KB flash, 4KB RAM, 48MHz, 2.4-3.6V, 15 GPIO, TSSOP-20"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA4D175))
    (comp (ref C6)
      (value 100n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA5044D))
    (comp (ref C8)
      (value 100n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA51045))
    (comp (ref C2)
      (value 100n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA61328))
    (comp (ref R7)
      (value 10K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA6330E))
    (comp (ref R5)
      (value 10K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA6645D))
    (comp (ref Q1)
      (value DMP3098L)
      (footprint Package_TO_SOT_SMD:SOT-23)
      (datasheet http://www.farnell.com/datasheets/1915664.pdf)
      (libsource (lib 00_Mix) (part DMP3098L) (description "DMP3098L-7 -  MOSFET Transistor, P Channel, 3.8 A, -30 V, 0.056 ohm, -10 V, -1.8 V"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA6F456))
    (comp (ref R1)
      (value 0R)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA7237E))
    (comp (ref C1)
      (value 4u7)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA76311))
    (comp (ref C5)
      (value 4u7)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA775A3))
    (comp (ref R6)
      (value 4K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA7D379))
    (comp (ref R2)
      (value 1K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA51DF3))
    (comp (ref D2)
      (value RED)
      (footprint Diode_SMD:D_1206_3216Metric)
      (datasheet ~)
      (libsource (lib Device) (part LED_Small) (description "Light emitting diode, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA52B7B))
    (comp (ref U1)
      (value MCP73831-2-OT)
      (footprint Package_TO_SOT_SMD:SOT-23-5)
      (datasheet http://ww1.microchip.com/downloads/en/DeviceDoc/20001984g.pdf)
      (libsource (lib 00_Mix) (part MCP73831-2-OT) (description "Single cell, Li-Ion/Li-Po charge management controller, 4.20V, Tri-State Status Output, in SOT23-5 package"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA4C57F))
    (comp (ref R25)
      (value 150R)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DAD4CC5))
    (comp (ref R18)
      (value 150R)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DAD9E42))
    (comp (ref R19)
      (value 150R)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DADA221))
    (comp (ref R20)
      (value 150R)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DADA6DF))
    (comp (ref R21)
      (value 150R)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DADAB74))
    (comp (ref C11)
      (value 10n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DB10EA8))
    (comp (ref R17)
      (value 1K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DBE3D5D))
    (comp (ref C13)
      (value 10n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DBED62E))
    (comp (ref SW2)
      (value SW_Push)
      (footprint Button_Switch_THT:SW_PUSH_6mm)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push) (description "Push button switch, generic, two pins"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DB57124))
    (comp (ref U4)
      (value MCP6022-I_SN)
      (footprint Package_SO:SOIC-8_3.9x4.9mm_P1.27mm)
      (datasheet https://www.tme.eu/Document/e53df4b1836c376b19d8bc3b9f170709/mcp6021.pdf)
      (libsource (lib 00_Mix) (part MCP6022-I_SN) (description "Rail-to-Rail Input/Output, 10 MHz Op Amps"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DB9B476))
    (comp (ref R29)
      (value 33K/.1%)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DBA3FEE))
    (comp (ref R23)
      (value 0R)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DBA5B59))
    (comp (ref R26)
      (value 330K/.1%)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DBA5B5F))
    (comp (ref R15)
      (value 100R)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DBD34D2))
    (comp (ref C10)
      (value 10n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DBD3A5C))
    (comp (ref C14)
      (value 100n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DBF27D1))
    (comp (ref R32)
      (value 330K/.1%)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DC4B45D))
    (comp (ref R33)
      (value 330K/.1%)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DC4B463))
    (comp (ref R28)
      (value 100R)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DC8CA68))
    (comp (ref C15)
      (value 10n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DC8CA6E))
    (comp (ref D7)
      (value S1G)
      (footprint Diode_SMD:D_SMA)
      (datasheet ~)
      (libsource (lib Device) (part D_Small) (description "Diode, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DADDE9F))
    (comp (ref D4)
      (value S1G)
      (footprint Diode_SMD:D_SMA)
      (datasheet ~)
      (libsource (lib Device) (part D_Small) (description "Diode, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DADDB1F))
    (comp (ref R34)
      (value 50R)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DC6F847))
    (comp (ref C12)
      (value 10n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DC24198))
    (comp (ref C18)
      (value DNP)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DC13E91))
    (comp (ref R30)
      (value 150R/.1%)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DBDA8F5))
    (comp (ref D8)
      (value S1G)
      (footprint Diode_SMD:D_SMA)
      (datasheet ~)
      (libsource (lib Device) (part D_Small) (description "Diode, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DB71B76))
    (comp (ref D5)
      (value S1G)
      (footprint Diode_SMD:D_SMA)
      (datasheet ~)
      (libsource (lib Device) (part D_Small) (description "Diode, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DB71715))
    (comp (ref D6)
      (value S1G)
      (footprint Diode_SMD:D_SMA)
      (datasheet ~)
      (libsource (lib Device) (part D_Small) (description "Diode, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DB5DBF8))
    (comp (ref D3)
      (value S1G)
      (footprint Diode_SMD:D_SMA)
      (datasheet ~)
      (libsource (lib Device) (part D_Small) (description "Diode, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DB5CBDA))
    (comp (ref R24)
      (value 33K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DB4C4BF))
    (comp (ref R27)
      (value 10K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DB4C10C))
    (comp (ref C16)
      (value 100n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DAA62C9))
    (comp (ref U5)
      (value MCP6022-I_SN)
      (footprint Package_SO:SOIC-8_3.9x4.9mm_P1.27mm)
      (datasheet https://www.tme.eu/Document/e53df4b1836c376b19d8bc3b9f170709/mcp6021.pdf)
      (libsource (lib 00_Mix) (part MCP6022-I_SN) (description "Rail-to-Rail Input/Output, 10 MHz Op Amps"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA967D3))
    (comp (ref C17)
      (value DNP)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DC0985C))
    (comp (ref J5)
      (value DUT)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DB58A4A))
    (comp (ref R31)
      (value 33K/.1%)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DBA4B25))
    (comp (ref R35)
      (value 0R)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DC42F94))
    (comp (ref R36)
      (value 33K/.1%)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DC42F9A))
    (comp (ref R16)
      (value 1K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DBE34CA))
    (comp (ref R22)
      (value 100R)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DC2514A))
    (comp (ref R14)
      (value 300R)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DAB55C0))
    (comp (ref R9)
      (value 300R)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DAB50D0))
    (comp (ref R13)
      (value 300R)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DAB4DBB))
    (comp (ref R8)
      (value 300R)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DAB4932))
    (comp (ref R12)
      (value 300R)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DAA82CF))
    (comp (ref Y1)
      (value 8MHz)
      (footprint Crystal:Crystal_SMD_HC49-SD)
      (datasheet ~)
      (libsource (lib Device) (part Crystal_Small) (description "Two pin crystal, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E3ED6B3))
    (comp (ref C3)
      (value 10n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E3F006E))
    (comp (ref C4)
      (value 10n)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E3F12DE))
    (comp (ref U3)
      (value LM1117-3.3)
      (footprint Package_TO_SOT_SMD:SOT-223-3_TabPin2)
      (datasheet http://www.ti.com/lit/ds/symlink/lm1117.pdf)
      (libsource (lib Regulator_Linear) (part LM1117-3.3) (description "800mA Low-Dropout Linear Regulator, 3.3V fixed output, TO-220/TO-252/TO-263/SOT-223"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E4D375F))
    (comp (ref J3)
      (value Display)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x04_Male) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA54FB6))
    (comp (ref J4)
      (value SWD)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x04_Male) (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA53C45))
    (comp (ref R10)
      (value 2K2)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E5B1A6C))
    (comp (ref R11)
      (value 2K2)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E5B215F))
    (comp (ref C7)
      (value 10u)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E73A5DE))
    (comp (ref C9)
      (value 10u)
      (footprint Capacitor_SMD:C_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E73B161))
    (comp (ref R3)
      (value 10K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E959806))
    (comp (ref R4)
      (value 1K)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E95A6A3))
    (comp (ref D1)
      (value 7V)
      (footprint Diode_SMD:D_SMA)
      (datasheet ~)
      (libsource (lib Device) (part D_TVS) (description "Bidirectional transient-voltage-suppression diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5E96E699))
    (comp (ref BZ1)
      (value Buzzer)
      (footprint Buzzer_Beeper:Buzzer_12x9.5RM7.6)
      (datasheet ~)
      (libsource (lib Device) (part Buzzer) (description "Buzzer, polarized"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5EA072FD))
    (comp (ref SW1)
      (value SW_Push)
      (footprint Button_Switch_THT:SW_PUSH_6mm)
      (datasheet ~)
      (libsource (lib Switch) (part SW_Push) (description "Push button switch, generic, two pins"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5EA920A2))
    (comp (ref J2)
      (value "Battery terminal")
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5DA781AE))
    (comp (ref R37)
      (value 300R)
      (footprint Resistor_SMD:R_0805_2012Metric)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ED6804E)))
  (libparts
    (libpart (lib 00_Mix) (part DMP3098L)
      (aliases
        (alias SQ2361ES))
      (description "DMP3098L-7 -  MOSFET Transistor, P Channel, 3.8 A, -30 V, 0.056 ohm, -10 V, -1.8 V")
      (docs http://www.farnell.com/datasheets/1915664.pdf)
      (fields
        (field (name Reference) Q)
        (field (name Value) DMP3098L)
        (field (name Footprint) TO_SOT_Packages_SMD:SOT-23))
      (pins
        (pin (num 1) (name G) (type input))
        (pin (num 2) (name S) (type passive))
        (pin (num 3) (name D) (type passive))))
    (libpart (lib 00_Mix) (part MCP6022-I_SN)
      (description "Rail-to-Rail Input/Output, 10 MHz Op Amps")
      (docs https://www.tme.eu/Document/e53df4b1836c376b19d8bc3b9f170709/mcp6021.pdf)
      (footprints
        (fp SOIC*3.9x4.9mm*P1.27mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) MCP6022-I_SN))
      (pins
        (pin (num 1) (name ~) (type output))
        (pin (num 2) (name -) (type input))
        (pin (num 3) (name +) (type input))
        (pin (num 4) (name V-) (type power_in))
        (pin (num 5) (name +) (type input))
        (pin (num 6) (name -) (type input))
        (pin (num 7) (name ~) (type output))
        (pin (num 8) (name V+) (type power_in))))
    (libpart (lib 00_Mix) (part MCP73832-2-OT)
      (aliases
        (alias MCP73832-5-OT)
        (alias MCP73832-4-OT)
        (alias MCP73832-3-OT)
        (alias MCP73831-2-OT)
        (alias MCP73831-5-OT)
        (alias MCP73831-4-OT)
        (alias MCP73831-3-OT))
      (description "Single cell, Li-Ion/Li-Po charge management controller, 4.20V, Open-Drain Status Output, in SOT23-5 package")
      (docs http://ww1.microchip.com/downloads/en/DeviceDoc/20001984g.pdf)
      (footprints
        (fp SOT?23*))
      (fields
        (field (name Reference) U)
        (field (name Value) MCP73832-2-OT)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-23-5))
      (pins
        (pin (num 1) (name STAT) (type output))
        (pin (num 2) (name VSS) (type power_in))
        (pin (num 3) (name VBAT) (type power_out))
        (pin (num 4) (name VDD) (type power_in))
        (pin (num 5) (name PROG) (type input))))
    (libpart (lib Connector) (part Conn_01x02_Male)
      (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib Connector) (part Conn_01x04_Male)
      (description "Generic connector, single row, 01x04, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x04_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))
        (pin (num 3) (name Pin_3) (type passive))
        (pin (num 4) (name Pin_4) (type passive))))
    (libpart (lib Connector) (part USB_B_Micro)
      (aliases
        (alias USB_B_Mini))
      (description "USB Micro Type B connector")
      (docs ~)
      (footprints
        (fp USB*))
      (fields
        (field (name Reference) J)
        (field (name Value) USB_B_Micro))
      (pins
        (pin (num 1) (name VBUS) (type power_out))
        (pin (num 2) (name D-) (type passive))
        (pin (num 3) (name D+) (type passive))
        (pin (num 4) (name ID) (type passive))
        (pin (num 5) (name GND) (type power_out))
        (pin (num 6) (name Shield) (type passive))))
    (libpart (lib Device) (part Buzzer)
      (description "Buzzer, polarized")
      (docs ~)
      (footprints
        (fp *Buzzer*))
      (fields
        (field (name Reference) BZ)
        (field (name Value) Buzzer))
      (pins
        (pin (num 1) (name -) (type passive))
        (pin (num 2) (name +) (type passive))))
    (libpart (lib Device) (part C_Small)
      (description "Unpolarized capacitor, small symbol")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part Crystal_Small)
      (description "Two pin crystal, small symbol")
      (docs ~)
      (footprints
        (fp Crystal*))
      (fields
        (field (name Reference) Y)
        (field (name Value) Crystal_Small))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive))))
    (libpart (lib Device) (part D_Small)
      (description "Diode, small symbol")
      (docs ~)
      (footprints
        (fp TO-???*)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_Small))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part D_TVS)
      (description "Bidirectional transient-voltage-suppression diode")
      (docs ~)
      (footprints
        (fp TO-???*)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_TVS))
      (pins
        (pin (num 1) (name A1) (type passive))
        (pin (num 2) (name A2) (type passive))))
    (libpart (lib Device) (part LED_Small)
      (description "Light emitting diode, small symbol")
      (docs ~)
      (footprints
        (fp LED*)
        (fp LED_SMD:*)
        (fp LED_THT:*))
      (fields
        (field (name Reference) D)
        (field (name Value) LED_Small))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part R_Small)
      (description "Resistor, small symbol")
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib MCU_ST_STM32F0) (part STM32F030F4Px)
      (description "ARM Cortex-M0 MCU, 16KB flash, 4KB RAM, 48MHz, 2.4-3.6V, 15 GPIO, TSSOP-20")
      (docs http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/DM00088500.pdf)
      (footprints
        (fp TSSOP*4.4x6.5mm*P0.65mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) STM32F030F4Px)
        (field (name Footprint) Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm))
      (pins
        (pin (num 1) (name BOOT0) (type input))
        (pin (num 2) (name PF0) (type input))
        (pin (num 3) (name PF1) (type input))
        (pin (num 4) (name NRST) (type input))
        (pin (num 5) (name VDDA) (type power_in))
        (pin (num 6) (name PA0) (type BiDi))
        (pin (num 7) (name PA1) (type BiDi))
        (pin (num 8) (name PA2) (type BiDi))
        (pin (num 9) (name PA3) (type BiDi))
        (pin (num 10) (name PA4) (type BiDi))
        (pin (num 11) (name PA5) (type BiDi))
        (pin (num 12) (name PA6) (type BiDi))
        (pin (num 13) (name PA7) (type BiDi))
        (pin (num 14) (name PB1) (type BiDi))
        (pin (num 15) (name VSS) (type power_in))
        (pin (num 16) (name VDD) (type power_in))
        (pin (num 17) (name PA9) (type BiDi))
        (pin (num 18) (name PA10) (type BiDi))
        (pin (num 19) (name PA13) (type BiDi))
        (pin (num 20) (name PA14) (type BiDi))))
    (libpart (lib Regulator_Linear) (part LM1117-1.8)
      (aliases
        (alias LM1117-2.5)
        (alias LM1117-3.3)
        (alias LM1117-5.0)
        (alias TLV1117-15)
        (alias TLV1117-18)
        (alias TLV1117-25)
        (alias TLV1117-33)
        (alias TLV1117-50))
      (description "800mA Low-Dropout Linear Regulator, 1.8V fixed output, TO-220/TO-252/TO-263/SOT-223")
      (docs http://www.ti.com/lit/ds/symlink/lm1117.pdf)
      (footprints
        (fp SOT?223*)
        (fp TO?263*)
        (fp TO?252*)
        (fp TO?220*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM1117-1.8))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name VO) (type power_out))
        (pin (num 3) (name VI) (type power_in))))
    (libpart (lib Switch) (part SW_Push)
      (description "Push button switch, generic, two pins")
      (docs ~)
      (fields
        (field (name Reference) SW)
        (field (name Value) SW_Push))
      (pins
        (pin (num 1) (name 1) (type passive))
        (pin (num 2) (name 2) (type passive)))))
  (libraries
    (library (logical 00_Mix)
      (uri C:/Users/Standa/Desktop/Projects/aaaKicadLibs/aaaStandaLib/00_Mix.lib))
    (library (logical Connector)
      (uri C:\Programs\KiCad\share\kicad\library/Connector.lib))
    (library (logical Device)
      (uri C:\Programs\KiCad\share\kicad\library/Device.lib))
    (library (logical MCU_ST_STM32F0)
      (uri C:\Programs\KiCad\share\kicad\library/MCU_ST_STM32F0.lib))
    (library (logical Regulator_Linear)
      (uri C:\Programs\KiCad\share\kicad\library/Regulator_Linear.lib))
    (library (logical Switch)
      (uri C:\Programs\KiCad\share\kicad\library/Switch.lib)))
  (nets
    (net (code 1) (name "Net-(R33-Pad2)")
      (node (ref R33) (pin 2))
      (node (ref U4) (pin 6))
      (node (ref R35) (pin 1)))
    (net (code 2) (name "Net-(R29-Pad2)")
      (node (ref R29) (pin 2))
      (node (ref R31) (pin 1)))
    (net (code 3) (name "Net-(R35-Pad2)")
      (node (ref R35) (pin 2))
      (node (ref R36) (pin 1)))
    (net (code 4) (name /VM10R)
      (node (ref U2) (pin 8))
      (node (ref C15) (pin 2))
      (node (ref R28) (pin 1)))
    (net (code 5) (name /IM)
      (node (ref R22) (pin 1))
      (node (ref U2) (pin 7))
      (node (ref C12) (pin 2)))
    (net (code 6) (name "Net-(R14-Pad1)")
      (node (ref U2) (pin 13))
      (node (ref R14) (pin 1)))
    (net (code 7) (name "Net-(R18-Pad2)")
      (node (ref R8) (pin 2))
      (node (ref R19) (pin 1))
      (node (ref R18) (pin 2)))
    (net (code 8) (name "Net-(C11-Pad1)")
      (node (ref R14) (pin 2))
      (node (ref C11) (pin 1))
      (node (ref R21) (pin 2))
      (node (ref R24) (pin 2)))
    (net (code 9) (name "Net-(R9-Pad1)")
      (node (ref R9) (pin 1))
      (node (ref U2) (pin 12)))
    (net (code 10) (name "Net-(R20-Pad2)")
      (node (ref R20) (pin 2))
      (node (ref R9) (pin 2))
      (node (ref R21) (pin 1)))
    (net (code 11) (name "Net-(R13-Pad1)")
      (node (ref U2) (pin 11))
      (node (ref R13) (pin 1)))
    (net (code 12) (name "Net-(R13-Pad2)")
      (node (ref R19) (pin 2))
      (node (ref R20) (pin 1))
      (node (ref R13) (pin 2)))
    (net (code 13) (name "Net-(R8-Pad1)")
      (node (ref R8) (pin 1))
      (node (ref U2) (pin 10)))
    (net (code 14) (name "Net-(R12-Pad1)")
      (node (ref U2) (pin 9))
      (node (ref R12) (pin 1)))
    (net (code 15) (name GND)
      (node (ref U2) (pin 15))
      (node (ref U3) (pin 1))
      (node (ref R7) (pin 2))
      (node (ref J3) (pin 1))
      (node (ref U1) (pin 2))
      (node (ref C11) (pin 2))
      (node (ref BZ1) (pin 2))
      (node (ref C8) (pin 2))
      (node (ref J1) (pin 5))
      (node (ref C6) (pin 2))
      (node (ref J2) (pin 1))
      (node (ref C7) (pin 1))
      (node (ref C9) (pin 1))
      (node (ref R6) (pin 1))
      (node (ref J4) (pin 2))
      (node (ref C5) (pin 1))
      (node (ref C1) (pin 1))
      (node (ref C12) (pin 1))
      (node (ref C13) (pin 1))
      (node (ref Q1) (pin 1))
      (node (ref R17) (pin 1))
      (node (ref R25) (pin 2))
      (node (ref R4) (pin 1))
      (node (ref C15) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref U5) (pin 4))
      (node (ref C16) (pin 2))
      (node (ref C14) (pin 2))
      (node (ref D8) (pin 2))
      (node (ref C3) (pin 1))
      (node (ref D1) (pin 2))
      (node (ref U4) (pin 4))
      (node (ref C10) (pin 1))
      (node (ref C2) (pin 2)))
    (net (code 16) (name "Net-(D6-Pad1)")
      (node (ref D6) (pin 1))
      (node (ref D7) (pin 2)))
    (net (code 17) (name "Net-(D3-Pad1)")
      (node (ref D6) (pin 2))
      (node (ref D5) (pin 2))
      (node (ref R31) (pin 2))
      (node (ref R36) (pin 2))
      (node (ref D3) (pin 1))
      (node (ref J5) (pin 2))
      (node (ref R34) (pin 1)))
    (net (code 18) (name "Net-(D3-Pad2)")
      (node (ref D4) (pin 1))
      (node (ref D3) (pin 2)))
    (net (code 19) (name "Net-(C17-Pad2)")
      (node (ref R34) (pin 2))
      (node (ref U5) (pin 1))
      (node (ref C17) (pin 2))
      (node (ref R27) (pin 1)))
    (net (code 20) (name "Net-(C17-Pad1)")
      (node (ref R27) (pin 2))
      (node (ref R24) (pin 1))
      (node (ref U5) (pin 2))
      (node (ref C17) (pin 1)))
    (net (code 21) (name /1V65)
      (node (ref U5) (pin 5))
      (node (ref U4) (pin 5))
      (node (ref R16) (pin 1))
      (node (ref C13) (pin 2))
      (node (ref U4) (pin 3))
      (node (ref R17) (pin 2))
      (node (ref U5) (pin 3)))
    (net (code 22) (name "Net-(C18-Pad1)")
      (node (ref D7) (pin 1))
      (node (ref D4) (pin 2))
      (node (ref C18) (pin 1))
      (node (ref U5) (pin 6))
      (node (ref R30) (pin 2))
      (node (ref D8) (pin 1))
      (node (ref J5) (pin 1)))
    (net (code 23) (name +BATT)
      (node (ref U3) (pin 3))
      (node (ref SW2) (pin 2))
      (node (ref U5) (pin 8))
      (node (ref R3) (pin 2))
      (node (ref C16) (pin 1))
      (node (ref D5) (pin 1))
      (node (ref C7) (pin 2)))
    (net (code 24) (name "Net-(BZ1-Pad1)")
      (node (ref U2) (pin 14))
      (node (ref SW1) (pin 2))
      (node (ref R4) (pin 2))
      (node (ref R3) (pin 1))
      (node (ref BZ1) (pin 1)))
    (net (code 25) (name +3V3)
      (node (ref R37) (pin 2))
      (node (ref C6) (pin 1))
      (node (ref C14) (pin 1))
      (node (ref U4) (pin 8))
      (node (ref C8) (pin 1))
      (node (ref R5) (pin 2))
      (node (ref U2) (pin 16))
      (node (ref R11) (pin 1))
      (node (ref R16) (pin 2))
      (node (ref U3) (pin 2))
      (node (ref R10) (pin 1))
      (node (ref C9) (pin 2))
      (node (ref U2) (pin 5))
      (node (ref J3) (pin 2)))
    (net (code 26) (name "Net-(C5-Pad2)")
      (node (ref U1) (pin 3))
      (node (ref C5) (pin 2))
      (node (ref SW2) (pin 1))
      (node (ref J2) (pin 2)))
    (net (code 27) (name "Net-(J1-Pad1)")
      (node (ref Q1) (pin 3))
      (node (ref J1) (pin 1)))
    (net (code 28) (name "Net-(R37-Pad1)")
      (node (ref SW1) (pin 1))
      (node (ref R37) (pin 1)))
    (net (code 29) (name /NRST)
      (node (ref C2) (pin 1))
      (node (ref J4) (pin 4))
      (node (ref U2) (pin 4))
      (node (ref R5) (pin 1)))
    (net (code 30) (name "Net-(C4-Pad2)")
      (node (ref Y1) (pin 2))
      (node (ref U2) (pin 3))
      (node (ref C4) (pin 2)))
    (net (code 31) (name "Net-(C3-Pad2)")
      (node (ref Y1) (pin 1))
      (node (ref C3) (pin 2))
      (node (ref U2) (pin 2)))
    (net (code 32) (name /SWD)
      (node (ref J4) (pin 3))
      (node (ref U2) (pin 20)))
    (net (code 33) (name "Net-(D2-Pad1)")
      (node (ref R2) (pin 1))
      (node (ref D2) (pin 1)))
    (net (code 34) (name "Net-(R2-Pad2)")
      (node (ref U1) (pin 1))
      (node (ref R2) (pin 2)))
    (net (code 35) (name "Net-(C1-Pad2)")
      (node (ref Q1) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref U1) (pin 4))
      (node (ref D1) (pin 1))
      (node (ref D2) (pin 2)))
    (net (code 36) (name "Net-(R6-Pad2)")
      (node (ref U1) (pin 5))
      (node (ref R6) (pin 2)))
    (net (code 37) (name "Net-(J1-Pad3)")
      (node (ref R1) (pin 1))
      (node (ref J1) (pin 3)))
    (net (code 38) (name "Net-(J1-Pad2)")
      (node (ref R1) (pin 2))
      (node (ref J1) (pin 2)))
    (net (code 39) (name "Net-(R12-Pad2)")
      (node (ref R25) (pin 1))
      (node (ref R18) (pin 1))
      (node (ref R12) (pin 2)))
    (net (code 40) (name "Net-(J1-Pad6)")
      (node (ref J1) (pin 6)))
    (net (code 41) (name "Net-(J1-Pad4)")
      (node (ref J1) (pin 4)))
    (net (code 42) (name "Net-(R7-Pad1)")
      (node (ref U2) (pin 1))
      (node (ref R7) (pin 1)))
    (net (code 43) (name /SDA)
      (node (ref U2) (pin 18))
      (node (ref R10) (pin 2))
      (node (ref J3) (pin 4)))
    (net (code 44) (name /SCL)
      (node (ref R11) (pin 2))
      (node (ref J3) (pin 3))
      (node (ref U2) (pin 17)))
    (net (code 45) (name "Net-(R32-Pad2)")
      (node (ref R33) (pin 1))
      (node (ref R32) (pin 2)))
    (net (code 46) (name "Net-(R28-Pad2)")
      (node (ref R32) (pin 1))
      (node (ref U4) (pin 7))
      (node (ref R28) (pin 2)))
    (net (code 47) (name "Net-(C18-Pad2)")
      (node (ref U5) (pin 7))
      (node (ref R22) (pin 2))
      (node (ref C18) (pin 2))
      (node (ref R30) (pin 1)))
    (net (code 48) (name /SWCLK)
      (node (ref J4) (pin 1))
      (node (ref U2) (pin 19)))
    (net (code 49) (name /VM100R)
      (node (ref U2) (pin 6))
      (node (ref C10) (pin 2))
      (node (ref R15) (pin 1)))
    (net (code 50) (name "Net-(R15-Pad2)")
      (node (ref R23) (pin 1))
      (node (ref R15) (pin 2))
      (node (ref U4) (pin 1)))
    (net (code 51) (name "Net-(R26-Pad2)")
      (node (ref U4) (pin 2))
      (node (ref R29) (pin 1))
      (node (ref R26) (pin 2)))
    (net (code 52) (name "Net-(R23-Pad2)")
      (node (ref R23) (pin 2))
      (node (ref R26) (pin 1)))))