<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.3.0">
<drawing>
<schematic>
<libraries>
<library name="frames">
<description>&lt;b&gt;Frames for Sheet and Layout&lt;/b&gt;</description>
<packages>
</packages>
<symbols>
<symbol name="A4L-LOC">
</symbol>
</symbols>
<devicesets>
<deviceset name="A4L-LOC" prefix="FRAME" uservalue="yes">
<description>&lt;b&gt;FRAME&lt;/b&gt;&lt;p&gt;
DIN A4, landscape with location and doc. field</description>
<gates>
<gate name="G$1" symbol="A4L-LOC"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="ixys">
<packages>
<package name="KXOB25-01X8F">
<description>KXOB25-01X8F
Solar Cell</description>
</package>
</packages>
<symbols>
<symbol name="KXOB25-01X8F">
<pin name="+"/>
<pin name="-"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="KXOB25-01X8F">
<gates>
<gate name="G$1" symbol="KXOB25-01X8F"/>
</gates>
<devices>
<device name="" package="KXOB25-01X8F">
<connects>
<connect gate="G$1" pin="+" pad="P$1"/>
<connect gate="G$1" pin="-" pad="P$2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="supply1">
<description>&lt;b&gt;Supply Symbols&lt;/b&gt;&lt;p&gt;
 GND, VCC, 0V, +5V, -5V, etc.&lt;p&gt;
 Please keep in mind, that these devices are necessary for the
 automatic wiring of the supply signals.&lt;p&gt;
 The pin name defined in the symbol is identical to the net which is to be wired automatically.&lt;p&gt;
 In this library the device names are the same as the pin names of the symbols, therefore the correct signal names appear next to the supply symbols in the schematic.&lt;p&gt;
 &lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
</packages>
<symbols>
<symbol name="+3V3">
<pin name="+3V3" direction="sup"/>
</symbol>
<symbol name="GND">
<pin name="GND" direction="sup"/>
</symbol>
<symbol name="+5V">
<pin name="+5V" direction="sup"/>
</symbol>
<symbol name="V+">
<pin name="V+" direction="sup"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="+3V3" prefix="+3V3">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="G$1" symbol="+3V3"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="GND" prefix="GND">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="GND"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="+5V" prefix="P+">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="+5V"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="V+" prefix="P+">
<description>&lt;b&gt;SUPPLY SYMBOL&lt;/b&gt;</description>
<gates>
<gate name="1" symbol="V+"/>
</gates>
<devices>
<device name="">
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="samacsys">
<description>&lt;b&gt;https://eagle.componentsearchengine.com&lt;/b&gt;&lt;p&gt;&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="QFP50P1200X1200X120-64N">
<description>&lt;b&gt;(PT)64-Lead(TQFP)&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="ECS327516TR">
<description>&lt;b&gt;ECS-.327-5-16-TR-1&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="SON50P200X200X90-9N">
<description>&lt;b&gt;VDFN&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="PQFN50P300X300X100-16N">
<description>&lt;b&gt;LGA-16_2&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="8-PIN-METAL-LID-LGA">
<description>&lt;b&gt;8-pin metal-lid LGA&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="SOD2713X115N">
<description>&lt;b&gt;SOD-323&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="KSDELLS122JHKI1">
<description>&lt;b&gt;KS DELLS1.22-JHKI-1-1&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="SON65P200X200X65-7N">
<description>&lt;b&gt;OPT3004DNPR&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="EDC334Z5R5V">
<description>&lt;b&gt;EDC334Z5R5V-3&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
<symbols>
<symbol name="ATSAML21J18B-AUT">
<pin name="PA00"/>
<pin name="PA01"/>
<pin name="PA02"/>
<pin name="PA03"/>
<pin name="PB04"/>
<pin name="PB05"/>
<pin name="GNDANA"/>
<pin name="VDDANA"/>
<pin name="PB06"/>
<pin name="PB07"/>
<pin name="PB08"/>
<pin name="PB09"/>
<pin name="PA04"/>
<pin name="PA05"/>
<pin name="PA06"/>
<pin name="PA07"/>
<pin name="PA08"/>
<pin name="PA09"/>
<pin name="PA10"/>
<pin name="PA11"/>
<pin name="VDDIO_1"/>
<pin name="GND_1"/>
<pin name="PB10"/>
<pin name="PB11"/>
<pin name="PB12"/>
<pin name="PB13"/>
<pin name="PB14"/>
<pin name="PB15"/>
<pin name="PA12"/>
<pin name="PA13"/>
<pin name="PA14"/>
<pin name="PA15"/>
<pin name="VDDIO_3"/>
<pin name="GND_3"/>
<pin name="PA25"/>
<pin name="PA24"/>
<pin name="PA23"/>
<pin name="PA22"/>
<pin name="PA21"/>
<pin name="PA20"/>
<pin name="PB17"/>
<pin name="PB16"/>
<pin name="PA19"/>
<pin name="PA18"/>
<pin name="PA17"/>
<pin name="PA16"/>
<pin name="VDDIO_2"/>
<pin name="GND_2"/>
<pin name="PB03"/>
<pin name="PB02"/>
<pin name="PB01"/>
<pin name="PB00"/>
<pin name="PB31"/>
<pin name="PB30"/>
<pin name="PA31"/>
<pin name="PA30"/>
<pin name="VDDIN"/>
<pin name="VSW"/>
<pin name="GND_4"/>
<pin name="VDDCORE"/>
<pin name="!RESET"/>
<pin name="PA27"/>
<pin name="PB23"/>
<pin name="PB22"/>
</symbol>
<symbol name="ECS-.327-7-16-C-TR">
<pin name="IN/OUT"/>
<pin name="OUT/IN"/>
</symbol>
<symbol name="MCP1810T-33I_J8A">
<pin name="GND" direction="pwr"/>
<pin name="VOUT" direction="out"/>
<pin name="NC_1"/>
<pin name="NC_2"/>
<pin name="EP" direction="pwr"/>
<pin name="!SHDN" direction="in"/>
<pin name="VIN" direction="in"/>
<pin name="FB" direction="in"/>
<pin name="NC_3"/>
</symbol>
<symbol name="LIS3DHTR">
<pin name="VDDIO" direction="pwr"/>
<pin name="NC_1"/>
<pin name="NC_2"/>
<pin name="SCL/SPC"/>
<pin name="GND_1" direction="pwr"/>
<pin name="SDA/SDI/SDO"/>
<pin name="SDO/SA0"/>
<pin name="CS" direction="in"/>
<pin name="INT2" direction="in"/>
<pin name="RES"/>
<pin name="INT1" direction="in"/>
<pin name="GND_2" direction="pwr"/>
<pin name="ADC3"/>
<pin name="VDD" direction="pwr"/>
<pin name="ADC2"/>
<pin name="ADC1"/>
</symbol>
<symbol name="BMP280">
<pin name="GND_1" direction="pwr"/>
<pin name="CSB" direction="in"/>
<pin name="SDI"/>
<pin name="SCK"/>
<pin name="SDO"/>
<pin name="VDDIO_1" direction="pwr"/>
<pin name="GND_2" direction="pwr"/>
<pin name="VDDIO_2" direction="pwr"/>
</symbol>
<symbol name="BZX384C5V6-HG3-08">
<pin name="K"/>
<pin name="A"/>
</symbol>
<symbol name="KS_DELLS1.22-JHKI-1">
<pin name="K"/>
<pin name="A"/>
</symbol>
<symbol name="OPT3004DNPR">
<pin name="VDD"/>
<pin name="ADDR"/>
<pin name="GND"/>
<pin name="EP"/>
<pin name="SDA"/>
<pin name="INT"/>
<pin name="SCL"/>
</symbol>
<symbol name="EDC334Z5R5V">
<pin name="+"/>
<pin name="-"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="ATSAML21J18B-AUT" prefix="IC">
<description>&lt;b&gt;MICROCHIP - ATSAML21J18B-AUT. - Cortex-MO+,256KBFLASH, 32 KBSRAM, USB, U&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://ww1.microchip.com/downloads/en/DeviceDoc/60001477A.pdf"&gt; Datasheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="ATSAML21J18B-AUT"/>
</gates>
<devices>
<device name="" package="QFP50P1200X1200X120-64N">
<connects>
<connect gate="G$1" pin="!RESET" pad="52"/>
<connect gate="G$1" pin="GNDANA" pad="7"/>
<connect gate="G$1" pin="GND_1" pad="22"/>
<connect gate="G$1" pin="GND_2" pad="33"/>
<connect gate="G$1" pin="GND_3" pad="47"/>
<connect gate="G$1" pin="GND_4" pad="54"/>
<connect gate="G$1" pin="PA00" pad="1"/>
<connect gate="G$1" pin="PA01" pad="2"/>
<connect gate="G$1" pin="PA02" pad="3"/>
<connect gate="G$1" pin="PA03" pad="4"/>
<connect gate="G$1" pin="PA04" pad="13"/>
<connect gate="G$1" pin="PA05" pad="14"/>
<connect gate="G$1" pin="PA06" pad="15"/>
<connect gate="G$1" pin="PA07" pad="16"/>
<connect gate="G$1" pin="PA08" pad="17"/>
<connect gate="G$1" pin="PA09" pad="18"/>
<connect gate="G$1" pin="PA10" pad="19"/>
<connect gate="G$1" pin="PA11" pad="20"/>
<connect gate="G$1" pin="PA12" pad="29"/>
<connect gate="G$1" pin="PA13" pad="30"/>
<connect gate="G$1" pin="PA14" pad="31"/>
<connect gate="G$1" pin="PA15" pad="32"/>
<connect gate="G$1" pin="PA16" pad="35"/>
<connect gate="G$1" pin="PA17" pad="36"/>
<connect gate="G$1" pin="PA18" pad="37"/>
<connect gate="G$1" pin="PA19" pad="38"/>
<connect gate="G$1" pin="PA20" pad="41"/>
<connect gate="G$1" pin="PA21" pad="42"/>
<connect gate="G$1" pin="PA22" pad="43"/>
<connect gate="G$1" pin="PA23" pad="44"/>
<connect gate="G$1" pin="PA24" pad="45"/>
<connect gate="G$1" pin="PA25" pad="46"/>
<connect gate="G$1" pin="PA27" pad="51"/>
<connect gate="G$1" pin="PA30" pad="57"/>
<connect gate="G$1" pin="PA31" pad="58"/>
<connect gate="G$1" pin="PB00" pad="61"/>
<connect gate="G$1" pin="PB01" pad="62"/>
<connect gate="G$1" pin="PB02" pad="63"/>
<connect gate="G$1" pin="PB03" pad="64"/>
<connect gate="G$1" pin="PB04" pad="5"/>
<connect gate="G$1" pin="PB05" pad="6"/>
<connect gate="G$1" pin="PB06" pad="9"/>
<connect gate="G$1" pin="PB07" pad="10"/>
<connect gate="G$1" pin="PB08" pad="11"/>
<connect gate="G$1" pin="PB09" pad="12"/>
<connect gate="G$1" pin="PB10" pad="23"/>
<connect gate="G$1" pin="PB11" pad="24"/>
<connect gate="G$1" pin="PB12" pad="25"/>
<connect gate="G$1" pin="PB13" pad="26"/>
<connect gate="G$1" pin="PB14" pad="27"/>
<connect gate="G$1" pin="PB15" pad="28"/>
<connect gate="G$1" pin="PB16" pad="39"/>
<connect gate="G$1" pin="PB17" pad="40"/>
<connect gate="G$1" pin="PB22" pad="49"/>
<connect gate="G$1" pin="PB23" pad="50"/>
<connect gate="G$1" pin="PB30" pad="59"/>
<connect gate="G$1" pin="PB31" pad="60"/>
<connect gate="G$1" pin="VDDANA" pad="8"/>
<connect gate="G$1" pin="VDDCORE" pad="53"/>
<connect gate="G$1" pin="VDDIN" pad="56"/>
<connect gate="G$1" pin="VDDIO_1" pad="21"/>
<connect gate="G$1" pin="VDDIO_2" pad="34"/>
<connect gate="G$1" pin="VDDIO_3" pad="48"/>
<connect gate="G$1" pin="VSW" pad="55"/>
</connects>
<technologies>
<technology name="">
<attribute name="DESCRIPTION" value="MICROCHIP - ATSAML21J18B-AUT. - Cortex-MO+,256KBFLASH, 32 KBSRAM, USB, U"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ATSAML21J18B-AUT"/>
<attribute name="MOUSER_PART_NUMBER" value="556-ATSAML21J18B-AUT"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=556-ATSAML21J18B-AUT"/>
<attribute name="RS_PART_NUMBER" value=""/>
<attribute name="RS_PRICE-STOCK" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="ECS-.327-7-16-C-TR" prefix="Y">
<description>&lt;b&gt;Crystals 32.768kHz 7pF 10ppm -40C +85C&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="https://www.mouser.com/datasheet/2/122/ECX-16-845175.pdf"&gt; Datasheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="ECS-.327-7-16-C-TR"/>
</gates>
<devices>
<device name="" package="ECS327516TR">
<connects>
<connect gate="G$1" pin="IN/OUT" pad="1"/>
<connect gate="G$1" pin="OUT/IN" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DESCRIPTION" value="Crystals 32.768kHz 7pF 10ppm -40C +85C"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="MANUFACTURER_NAME" value="ECS"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="ECS-.327-7-16-C-TR"/>
<attribute name="MOUSER_PART_NUMBER" value="520-.327-7-16-CT"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=520-.327-7-16-CT"/>
<attribute name="RS_PART_NUMBER" value=""/>
<attribute name="RS_PRICE-STOCK" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="MCP1810T-33I_J8A" prefix="PS">
<description>&lt;b&gt;LDO Regulator 150mA 3.3V Low IQ VDFN8&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="https://componentsearchengine.com/Datasheets/2/MCP1810T-33I_J8A.pdf"&gt; Datasheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="MCP1810T-33I_J8A"/>
</gates>
<devices>
<device name="" package="SON50P200X200X90-9N">
<connects>
<connect gate="G$1" pin="!SHDN" pad="8"/>
<connect gate="G$1" pin="EP" pad="9"/>
<connect gate="G$1" pin="FB" pad="6"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="NC_1" pad="3"/>
<connect gate="G$1" pin="NC_2" pad="4"/>
<connect gate="G$1" pin="NC_3" pad="5"/>
<connect gate="G$1" pin="VIN" pad="7"/>
<connect gate="G$1" pin="VOUT" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DESCRIPTION" value="LDO Regulator 150mA 3.3V Low IQ VDFN8"/>
<attribute name="HEIGHT" value="0.9mm"/>
<attribute name="MANUFACTURER_NAME" value="Microchip"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="MCP1810T-33I/J8A"/>
<attribute name="MOUSER_PART_NUMBER" value="579-MCP1810T-33I/J8A"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=579-MCP1810T-33I%2FJ8A"/>
<attribute name="RS_PART_NUMBER" value="1468894P"/>
<attribute name="RS_PRICE-STOCK" value="http://uk.rs-online.com/web/p/products/1468894P"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="LIS3DHTR" prefix="AC">
<description>&lt;b&gt;Accelerometer 3-Axis 2g/16g 1.8V LGA16 STMicroelectronics LIS3DHTR Accelerometer IC, 3-axis, I2C, SPI 1.71  3.6 V, 16-Pin LGA&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.st.com/web/en/resource/technical/document/datasheet/CD00274221.pdf"&gt; Datasheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="LIS3DHTR"/>
</gates>
<devices>
<device name="" package="PQFN50P300X300X100-16N">
<connects>
<connect gate="G$1" pin="ADC1" pad="16"/>
<connect gate="G$1" pin="ADC2" pad="15"/>
<connect gate="G$1" pin="ADC3" pad="13"/>
<connect gate="G$1" pin="CS" pad="8"/>
<connect gate="G$1" pin="GND_1" pad="5"/>
<connect gate="G$1" pin="GND_2" pad="12"/>
<connect gate="G$1" pin="INT1" pad="11"/>
<connect gate="G$1" pin="INT2" pad="9"/>
<connect gate="G$1" pin="NC_1" pad="2"/>
<connect gate="G$1" pin="NC_2" pad="3"/>
<connect gate="G$1" pin="RES" pad="10"/>
<connect gate="G$1" pin="SCL/SPC" pad="4"/>
<connect gate="G$1" pin="SDA/SDI/SDO" pad="6"/>
<connect gate="G$1" pin="SDO/SA0" pad="7"/>
<connect gate="G$1" pin="VDD" pad="14"/>
<connect gate="G$1" pin="VDDIO" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="ALLIED_NUMBER" value="70521157"/>
<attribute name="ALLIED_PRICE-STOCK" value="http://www.alliedelec.com/stmicroelectronics-lis3dhtr/70521157/"/>
<attribute name="DESCRIPTION" value="Accelerometer 3-Axis 2g/16g 1.8V LGA16 STMicroelectronics LIS3DHTR Accelerometer IC, 3-axis, I2C, SPI 1.71  3.6 V, 16-Pin LGA"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="MANUFACTURER_NAME" value="STMicroelectronics"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="LIS3DHTR"/>
<attribute name="MOUSER_PART_NUMBER" value="511-LIS3DHTR"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=511-LIS3DHTR"/>
<attribute name="RS_PART_NUMBER" value="7931364P"/>
<attribute name="RS_PRICE-STOCK" value="http://uk.rs-online.com/web/p/products/7931364P"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BMP280" prefix="IC">
<description>&lt;b&gt;Digital Pressure Sensor&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="https://ae-bst.resource.bosch.com/media/products/dokumente/bmp280/BST-BMP280-DS001-11.pdf"&gt; Datasheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="BMP280"/>
</gates>
<devices>
<device name="" package="8-PIN-METAL-LID-LGA">
<connects>
<connect gate="G$1" pin="CSB" pad="2"/>
<connect gate="G$1" pin="GND_1" pad="1"/>
<connect gate="G$1" pin="GND_2" pad="7"/>
<connect gate="G$1" pin="SCK" pad="4"/>
<connect gate="G$1" pin="SDI" pad="3"/>
<connect gate="G$1" pin="SDO" pad="5"/>
<connect gate="G$1" pin="VDDIO_1" pad="6"/>
<connect gate="G$1" pin="VDDIO_2" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DESCRIPTION" value="Digital Pressure Sensor"/>
<attribute name="HEIGHT" value="mm"/>
<attribute name="MANUFACTURER_NAME" value="Bosch Sensortec"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="bmp280"/>
<attribute name="MOUSER_PART_NUMBER" value="262-BMP280"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=262-BMP280"/>
<attribute name="RS_PART_NUMBER" value=""/>
<attribute name="RS_PRICE-STOCK" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="BZX384C5V6-HG3-08" prefix="Z">
<description>&lt;b&gt;Zener Diodes 5.6V Zener SOD-323&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="https://componentsearchengine.com/Datasheets/1/BZX384C5V6-HG3-08.pdf"&gt; Datasheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="BZX384C5V6-HG3-08"/>
</gates>
<devices>
<device name="" package="SOD2713X115N">
<connects>
<connect gate="G$1" pin="A" pad="2"/>
<connect gate="G$1" pin="K" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DESCRIPTION" value="Zener Diodes 5.6V Zener SOD-323"/>
<attribute name="HEIGHT" value="1.15mm"/>
<attribute name="MANUFACTURER_NAME" value="Vishay"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="BZX384C5V6-HG3-08"/>
<attribute name="MOUSER_PART_NUMBER" value="78-BZX384C5V6-HG3-08"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=78-BZX384C5V6-HG3-08"/>
<attribute name="RS_PART_NUMBER" value=""/>
<attribute name="RS_PRICE-STOCK" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="KS_DELLS1.22-JHKI-1" prefix="LED">
<description>&lt;b&gt;Standard LEDs - SMD Super Red TOPLED E 1608&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="https://www.mouser.com/ProductDetail/OSRAM-Opto-Semiconductors/KS-DELLS122-JHKI-1?qs=/ha2pyFadujNs/c2ExSW/mAgU7xSZpKq0%2BjX073j8siIKd5czqUDD5EbVTge9bPZ"&gt; Datasheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="KS_DELLS1.22-JHKI-1"/>
</gates>
<devices>
<device name="" package="KSDELLS122JHKI1">
<connects>
<connect gate="G$1" pin="A" pad="1"/>
<connect gate="G$1" pin="K" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DESCRIPTION" value="Standard LEDs - SMD Super Red TOPLED E 1608"/>
<attribute name="HEIGHT" value="mm"/>
<attribute name="MANUFACTURER_NAME" value="OSRAM"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="KS DELLS1.22-JHKI-1"/>
<attribute name="MOUSER_PART_NUMBER" value="720-KSDELLS122A4852"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=720-KSDELLS122A4852"/>
<attribute name="RS_PART_NUMBER" value=""/>
<attribute name="RS_PRICE-STOCK" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="OPT3004DNPR" prefix="IC">
<description>&lt;b&gt;Digital ambient light sensor (ALS) with increased angular IR rejection&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="http://www.ti.com/lit/ds/symlink/opt3004.pdf"&gt; Datasheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="OPT3004DNPR"/>
</gates>
<devices>
<device name="" package="SON65P200X200X65-7N">
<connects>
<connect gate="G$1" pin="ADDR" pad="2"/>
<connect gate="G$1" pin="EP" pad="7"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="INT" pad="5"/>
<connect gate="G$1" pin="SCL" pad="4"/>
<connect gate="G$1" pin="SDA" pad="6"/>
<connect gate="G$1" pin="VDD" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DESCRIPTION" value="Digital ambient light sensor (ALS) with increased angular IR rejection"/>
<attribute name="HEIGHT" value="0.65mm"/>
<attribute name="MANUFACTURER_NAME" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="OPT3004DNPR"/>
<attribute name="MOUSER_PART_NUMBER" value="595-OPT3004DNPR"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=595-OPT3004DNPR"/>
<attribute name="RS_PART_NUMBER" value=""/>
<attribute name="RS_PRICE-STOCK" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="EDC334Z5R5V" prefix="C">
<description>&lt;b&gt;Supercapacitors / Ultracapacitors 0.33F 5.5V 70C&lt;/b&gt;&lt;p&gt;
Source: &lt;a href="https://componentsearchengine.com/Datasheets/1/EDC334Z5R5V.pdf"&gt; Datasheet &lt;/a&gt;</description>
<gates>
<gate name="G$1" symbol="EDC334Z5R5V"/>
</gates>
<devices>
<device name="" package="EDC334Z5R5V">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="ALLIED_NUMBER" value="71822702"/>
<attribute name="ALLIED_PRICE-STOCK" value="https://www.alliedelec.com/cornell-dubilier-edc334z5r5v/71822702/"/>
<attribute name="DESCRIPTION" value="Supercapacitors / Ultracapacitors 0.33F 5.5V 70C"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="MANUFACTURER_NAME" value="Cornell Dubilier"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="EDC334Z5R5V"/>
<attribute name="MOUSER_PART_NUMBER" value="598-EDC334Z5R5V"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=598-EDC334Z5R5V"/>
<attribute name="RS_PART_NUMBER" value=""/>
<attribute name="RS_PRICE-STOCK" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="MF_Passives">
<packages>
<package name="C0402">
<description>&lt;b&gt;Description:&lt;/b&gt; Standard 0402 Package for Capacitors&lt;br/&gt;</description>
</package>
<package name="C0603">
<description>&lt;b&gt;Description:&lt;/b&gt; Standard 0603 Package for Capacitors&lt;br/&gt;</description>
</package>
<package name="C0805">
<description>&lt;b&gt;Description:&lt;/b&gt; Standard 0805 Package for Capacitors&lt;br/&gt;</description>
</package>
<package name="C1206">
<description>&lt;b&gt;Description:&lt;/b&gt; Standard 1206 Package for Capacitors&lt;br/&gt;</description>
</package>
<package name="C1210">
<description>&lt;b&gt;Description:&lt;/b&gt; Standard 1210 Package for Capacitors&lt;br/&gt;</description>
</package>
<package name="R0402">
<description>&lt;b&gt;Description:&lt;/b&gt; Standard 0402 Package for Resistors&lt;br/&gt;</description>
</package>
<package name="R0603">
<description>&lt;b&gt;Description:&lt;/b&gt; Standard 0603 Package for Resistors&lt;br/&gt;</description>
</package>
<package name="R0805">
<description>&lt;b&gt;Description:&lt;/b&gt; Standard 0805 Package for Resistors&lt;br/&gt;</description>
</package>
<package name="R1206">
<description>&lt;b&gt;Description:&lt;/b&gt; Standard 1206 Package for Resistors&lt;br/&gt;</description>
</package>
<package name="R1210">
<description>&lt;b&gt;Description:&lt;/b&gt; Standard 1210 Package for Resistors&lt;br/&gt;</description>
</package>
<package name="L0402">
<description>&lt;b&gt;Description:&lt;/b&gt; Standard 0402 Package for Inductors&lt;br/&gt;</description>
</package>
<package name="L0603">
<description>&lt;b&gt;Description:&lt;/b&gt; Standard 0603 Package for Inductors&lt;br/&gt;</description>
</package>
<package name="L1210">
<description>&lt;b&gt;Description:&lt;/b&gt; Standard 1210 Package for Inductors&lt;br/&gt;</description>
</package>
</packages>
<symbols>
<symbol name="CAPACITOR_NP">
<description>&lt;b&gt;Library:&lt;/b&gt;  MF_Passives&lt;br/&gt;
&lt;b&gt;Description:&lt;/b&gt; Symbol for Non-Polarized Capacitors&lt;br/&gt;</description>
<pin name="P$1" direction="pas"/>
<pin name="P$2" direction="pas"/>
</symbol>
<symbol name="RESISTOR">
<description>&lt;b&gt;Library:&lt;/b&gt;  MF_Passives&lt;br/&gt;
&lt;b&gt;Description:&lt;/b&gt; Symbol for Resistors&lt;br/&gt;</description>
<pin name="P$1" direction="pas"/>
<pin name="P$2" direction="pas"/>
</symbol>
<symbol name="INDUCTOR">
<description>&lt;b&gt;Library:&lt;/b&gt;  MF_Passives&lt;br/&gt;
&lt;b&gt;Description:&lt;/b&gt; Symbol for Inductors&lt;br/&gt;</description>
<pin name="P$1" direction="pas"/>
<pin name="P$2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="CAPACITOR_NP" prefix="C" uservalue="yes">
<description>&lt;b&gt;Library:&lt;/b&gt;  MF_Passives&lt;br/&gt;
&lt;b&gt;Description:&lt;/b&gt; Device for Non-Polarized Capacitors. Manufacture part number (MPN) can be added via Attributes. Check https://factory.macrofab.com/parts for the house parts list.&lt;br/&gt;</description>
<gates>
<gate name="G$1" symbol="CAPACITOR_NP"/>
</gates>
<devices>
<device name="_0402" package="C0402">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value=""/>
<attribute name="HOUSEPART" value=""/>
<attribute name="MPN" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="TOLERANCE" value=""/>
<attribute name="URL" value=""/>
<attribute name="VOLTAGE" value=""/>
</technology>
</technologies>
</device>
<device name="_0603" package="C0603">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value=""/>
<attribute name="HOUSEPART" value=""/>
<attribute name="MPN" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="TOLERANCE" value=""/>
<attribute name="URL" value=""/>
<attribute name="VOLTAGE" value=""/>
</technology>
</technologies>
</device>
<device name="_0805" package="C0805">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value=""/>
<attribute name="HOUSEPART" value=""/>
<attribute name="MPN" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="TOLERANCE" value=""/>
<attribute name="URL" value=""/>
<attribute name="VOLTAGE" value=""/>
</technology>
</technologies>
</device>
<device name="_1206" package="C1206">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value=""/>
<attribute name="HOUSEPART" value=""/>
<attribute name="MPN" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="TOLERANCE" value=""/>
<attribute name="URL" value=""/>
<attribute name="VOLTAGE" value=""/>
</technology>
</technologies>
</device>
<device name="_1210" package="C1210">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DIELECTRIC" value=""/>
<attribute name="HOUSEPART" value=""/>
<attribute name="MPN" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="TOLERANCE" value=""/>
<attribute name="URL" value=""/>
<attribute name="VOLTAGE" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="RESISTOR" prefix="R" uservalue="yes">
<description>&lt;b&gt;Library:&lt;/b&gt;  MF_Passives&lt;br/&gt;
&lt;b&gt;Description:&lt;/b&gt; Device for Resistors. Manufacture part number (MPN), Voltage, Tolerance, and Wattage Rating can be added via Attributes.  Check https://factory.macrofab.com/parts for the house parts list.&lt;br/&gt;</description>
<gates>
<gate name="G$1" symbol="RESISTOR"/>
</gates>
<devices>
<device name="_0402" package="R0402">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="HOUSEPART" value=""/>
<attribute name="MPN" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="TOLERANCE" value=""/>
<attribute name="URL" value=""/>
<attribute name="VOLTAGE" value=""/>
<attribute name="WATTAGE" value=""/>
</technology>
</technologies>
</device>
<device name="_0603" package="R0603">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="HOUSEPART" value=""/>
<attribute name="MPN" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="TOLERANCE" value=""/>
<attribute name="URL" value=""/>
<attribute name="VOLTAGE" value=""/>
<attribute name="WATTAGE" value=""/>
</technology>
</technologies>
</device>
<device name="_0805" package="R0805">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="HOUSEPART" value=""/>
<attribute name="MPN" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="TOLERANCE" value=""/>
<attribute name="URL" value=""/>
<attribute name="VOLTAGE" value=""/>
<attribute name="WATTAGE" value=""/>
</technology>
</technologies>
</device>
<device name="_1206" package="R1206">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="HOUSEPART" value=""/>
<attribute name="MPN" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="TOLERANCE" value=""/>
<attribute name="URL" value=""/>
<attribute name="VOLTAGE" value=""/>
<attribute name="WATTAGE" value=""/>
</technology>
</technologies>
</device>
<device name="_1210" package="R1210">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="HOUSEPART" value=""/>
<attribute name="MPN" value=""/>
<attribute name="POPULATE" value=""/>
<attribute name="TOLERANCE" value=""/>
<attribute name="URL" value=""/>
<attribute name="VOLTAGE" value=""/>
<attribute name="WATTAGE" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="INDUCTOR" prefix="L" uservalue="yes">
<description>&lt;b&gt;Library:&lt;/b&gt;  MF_Passives&lt;br/&gt;
&lt;b&gt;Description:&lt;/b&gt; Device for Inductors. Manufacture part number (MPN) can be added via Attributes. Check https://factory.macrofab.com/parts for the house parts list.&lt;br/&gt;</description>
<gates>
<gate name="G$1" symbol="INDUCTOR"/>
</gates>
<devices>
<device name="_0402" package="L0402">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="HOUSEPART" value=""/>
<attribute name="MPN" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value=""/>
</technology>
</technologies>
</device>
<device name="_0603" package="L0603">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="HOUSEPART" value=""/>
<attribute name="MPN" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value=""/>
</technology>
</technologies>
</device>
<device name="_1210" package="L1210">
<connects>
<connect gate="G$1" pin="P$1" pad="P$1"/>
<connect gate="G$1" pin="P$2" pad="P$2"/>
</connects>
<technologies>
<technology name="">
<attribute name="HOUSEPART" value=""/>
<attribute name="MPN" value=""/>
<attribute name="POPULATE" value=""/>
<attribute name="URL" value=""/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SAMTECH_FTSH-105-01">
<description>&lt;h3&gt;ARM Cortex Debug Connector (10-pin)&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.05"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.samtec.com/ftppub/cpdf/FTSH-1XX-XX-XXX-DV-XXX-MKT.pdf"&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CORTEX_DEBUG&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X5-PTH-1.27MM">
<description>&lt;h3&gt;Plated Through Hole - 2x5 ARM Cortex Debug Connector (10-pin)&lt;/h3&gt;
&lt;p&gt;tDoc (51) layer border represents maximum dimensions of plastic housing.&lt;/p&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:1.27mm&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;a href=”http://portal.fciconnect.com/Comergent//fci/drawing/20021111.pdf”&gt;Datasheet referenced for footprint&lt;/a&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_05x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
<symbols>
<symbol name="CORTEX_DEBUG">
<description>&lt;h3&gt;Cortex Debug Connector&lt;/h3&gt;
&lt;p&gt;&lt;a href="http://infocenter.arm.com/help/topic/com.arm.doc.faqs/attached/13634/cortex_debug_connectors.pdf"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;</description>
<pin name="VCC"/>
<pin name="GND@3"/>
<pin name="GND@5"/>
<pin name="KEY"/>
<pin name="GNDDTCT"/>
<pin name="!RESET"/>
<pin name="NC/TDI"/>
<pin name="SWO/TDO"/>
<pin name="SWDCLK/TCK"/>
<pin name="SWDIO/TMS"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="CORTEX_DEBUG" prefix="J">
<description>&lt;h3&gt;Cortex Debug Connector - 10 pin&lt;/h3&gt;
&lt;p&gt;Supports JTAG debug, Serial Wire debug, and Serial Wire Viewer.
PTH and SMD connector options available.&lt;/p&gt;
&lt;p&gt; &lt;ul&gt;&lt;a href=”http://infocenter.arm.com/help/topic/com.arm.doc.faqs/attached/13634/cortex_debug_connectors.pdf”&gt;General Connector Information&lt;/a&gt;
&lt;p&gt;&lt;b&gt; Products:&lt;/b&gt;
&lt;ul&gt;&lt;li&gt;&lt;a href=”http://www.digikey.com/product-detail/en/cnc-tech/3220-10-0100-00/1175-1627-ND/3883661”&gt;PTH Connector&lt;/a&gt; -via Digi-Key&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13229”&gt;SparkFun PSoc&lt;/a&gt;&lt;/li&gt;
&lt;li&gt;&lt;a href=”https://www.sparkfun.com/products/13810”&gt;SparkFun T&lt;/a&gt;&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="CORTEX_DEBUG"/>
</gates>
<devices>
<device name="_SMD" package="SAMTECH_FTSH-105-01">
<connects>
<connect gate="G$1" pin="!RESET" pad="10"/>
<connect gate="G$1" pin="GND@3" pad="3"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="GNDDTCT" pad="9"/>
<connect gate="G$1" pin="KEY" pad="7"/>
<connect gate="G$1" pin="NC/TDI" pad="8"/>
<connect gate="G$1" pin="SWDCLK/TCK" pad="4"/>
<connect gate="G$1" pin="SWDIO/TMS" pad="2"/>
<connect gate="G$1" pin="SWO/TDO" pad="6"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_PTH" package="2X5-PTH-1.27MM">
<connects>
<connect gate="G$1" pin="!RESET" pad="10"/>
<connect gate="G$1" pin="GND@3" pad="3"/>
<connect gate="G$1" pin="GND@5" pad="5"/>
<connect gate="G$1" pin="GNDDTCT" pad="9"/>
<connect gate="G$1" pin="KEY" pad="7"/>
<connect gate="G$1" pin="NC/TDI" pad="8"/>
<connect gate="G$1" pin="SWDCLK/TCK" pad="4"/>
<connect gate="G$1" pin="SWDIO/TMS" pad="2"/>
<connect gate="G$1" pin="SWO/TDO" pad="6"/>
<connect gate="G$1" pin="VCC" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="MF_Connectors">
<packages>
<package name="MICROUSB-RIGHT">
<description>&lt;b&gt;Description:&lt;/b&gt; Package for Micro USB Type B connector. Based on FCI 10118193-0001LF.&lt;br&gt;</description>
</package>
<package name="MINIUSB-RIGHT">
<description>&lt;b&gt;Description:&lt;/b&gt; Package for Mini USB Type B connector. Based on 4UCON 20236.&lt;br&gt;</description>
</package>
</packages>
<symbols>
<symbol name="USB_5PIN">
<description>&lt;b&gt;Description:&lt;/b&gt; Symbol for 5-Pin USB connectors.&lt;br&gt;</description>
<pin name="5V" direction="pwr"/>
<pin name="D-"/>
<pin name="D+"/>
<pin name="GND" direction="pwr"/>
<pin name="ID"/>
<pin name="SLD" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="USB" prefix="J" uservalue="yes">
<description>&lt;b&gt;Library:&lt;/b&gt;  MF_Connectors&lt;br/&gt;
&lt;b&gt;Description:&lt;/b&gt; 5 Pin USB Connectors. SLD is the shield connection. Usually tied to ground through a small ferrite bead.&lt;br/&gt;</description>
<gates>
<gate name="G$1" symbol="USB_5PIN"/>
</gates>
<devices>
<device name="_MICRO_RIGHT" package="MICROUSB-RIGHT">
<connects>
<connect gate="G$1" pin="5V" pad="1"/>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="SLD" pad="S1 S2 S3 S4 S5 S6"/>
</connects>
<technologies>
<technology name="">
<attribute name="HOUSEPART" value="YES"/>
<attribute name="MPN" value="MF-CON-MICROUSB-RIGHT"/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value="https://factory.macrofab.com/part/MF-CON-MICROUSB-RIGHT"/>
<attribute name="VALUE" value="MF-CON-MICROUSB-RIGHT"/>
</technology>
</technologies>
</device>
<device name="_MINI_RIGHT" package="MINIUSB-RIGHT">
<connects>
<connect gate="G$1" pin="5V" pad="1"/>
<connect gate="G$1" pin="D+" pad="3"/>
<connect gate="G$1" pin="D-" pad="2"/>
<connect gate="G$1" pin="GND" pad="5"/>
<connect gate="G$1" pin="ID" pad="4"/>
<connect gate="G$1" pin="SLD" pad="S1 S2 S3 S4"/>
</connects>
<technologies>
<technology name="">
<attribute name="HUOSEPART" value="NO"/>
<attribute name="MPN" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value="http://www.4uconnector.com/online/object/4udrawing/20236.pdf"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="adafruit">
<packages>
<package name="FEATHERWING">
</package>
<package name="FEATHERWING_DIM">
</package>
<package name="JST-PH-2-SMT-RA">
<description>2-Pin JST PH Series Right-Angle Connector (+/- for batteries)</description>
</package>
<package name="JST-PH-2-THM">
<description>4UCon #01528
http://www.4uconnector.com/online/object/4udrawing/01528.pdf</description>
</package>
<package name="JST-PH-2-THM-RA">
<description>&lt;b&gt;S2B-PH-K-S&lt;/b&gt; 
&lt;p&gt;
JST PH 2-pin thru-home side entry</description>
</package>
<package name="JST-PH-2-SMT">
</package>
</packages>
<symbols>
<symbol name="MICROSHIELD">
<pin name="!RESET" direction="in"/>
<pin name="3V" direction="sup"/>
<pin name="AREF" direction="pas"/>
<pin name="GND" direction="pwr"/>
<pin name="GPIOA0"/>
<pin name="GPIOA1"/>
<pin name="GPIOA2"/>
<pin name="GPIOA3"/>
<pin name="GPIOA4"/>
<pin name="GPIOA5"/>
<pin name="GPIOSCK"/>
<pin name="GPIOMOSI"/>
<pin name="GPIOMISO"/>
<pin name="GPIORX"/>
<pin name="GPIOTX"/>
<pin name="NC" direction="pas"/>
<pin name="GPIOSDA"/>
<pin name="GPIOSCL"/>
<pin name="GPIO5"/>
<pin name="GPIO9"/>
<pin name="GPIO6"/>
<pin name="GPIO10"/>
<pin name="GPIO11"/>
<pin name="GPIO12"/>
<pin name="GPIO13"/>
<pin name="EN" direction="pas"/>
<pin name="USB" direction="sup"/>
<pin name="VBAT" direction="sup"/>
</symbol>
<symbol name="PINHD2">
<pin name="1" direction="pas" function="dot"/>
<pin name="2" direction="pas" function="dot"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="FEATHERWING" prefix="MS">
<gates>
<gate name="G$1" symbol="MICROSHIELD"/>
</gates>
<devices>
<device name="" package="FEATHERWING">
<connects>
<connect gate="G$1" pin="!RESET" pad="1"/>
<connect gate="G$1" pin="3V" pad="2"/>
<connect gate="G$1" pin="AREF" pad="3"/>
<connect gate="G$1" pin="EN" pad="27"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GPIO10" pad="22"/>
<connect gate="G$1" pin="GPIO11" pad="23"/>
<connect gate="G$1" pin="GPIO12" pad="24"/>
<connect gate="G$1" pin="GPIO13" pad="25"/>
<connect gate="G$1" pin="GPIO5" pad="19"/>
<connect gate="G$1" pin="GPIO6" pad="20"/>
<connect gate="G$1" pin="GPIO9" pad="21"/>
<connect gate="G$1" pin="GPIOA0" pad="5"/>
<connect gate="G$1" pin="GPIOA1" pad="6"/>
<connect gate="G$1" pin="GPIOA2" pad="7"/>
<connect gate="G$1" pin="GPIOA3" pad="8"/>
<connect gate="G$1" pin="GPIOA4" pad="9"/>
<connect gate="G$1" pin="GPIOA5" pad="10"/>
<connect gate="G$1" pin="GPIOMISO" pad="13"/>
<connect gate="G$1" pin="GPIOMOSI" pad="12"/>
<connect gate="G$1" pin="GPIORX" pad="14"/>
<connect gate="G$1" pin="GPIOSCK" pad="11"/>
<connect gate="G$1" pin="GPIOSCL" pad="18"/>
<connect gate="G$1" pin="GPIOSDA" pad="17"/>
<connect gate="G$1" pin="GPIOTX" pad="15"/>
<connect gate="G$1" pin="NC" pad="16"/>
<connect gate="G$1" pin="USB" pad="26"/>
<connect gate="G$1" pin="VBAT" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_NODIM" package="FEATHERWING_DIM">
<connects>
<connect gate="G$1" pin="!RESET" pad="1"/>
<connect gate="G$1" pin="3V" pad="2"/>
<connect gate="G$1" pin="AREF" pad="3"/>
<connect gate="G$1" pin="EN" pad="27"/>
<connect gate="G$1" pin="GND" pad="4"/>
<connect gate="G$1" pin="GPIO10" pad="22"/>
<connect gate="G$1" pin="GPIO11" pad="23"/>
<connect gate="G$1" pin="GPIO12" pad="24"/>
<connect gate="G$1" pin="GPIO13" pad="25"/>
<connect gate="G$1" pin="GPIO5" pad="19"/>
<connect gate="G$1" pin="GPIO6" pad="20"/>
<connect gate="G$1" pin="GPIO9" pad="21"/>
<connect gate="G$1" pin="GPIOA0" pad="5"/>
<connect gate="G$1" pin="GPIOA1" pad="6"/>
<connect gate="G$1" pin="GPIOA2" pad="7"/>
<connect gate="G$1" pin="GPIOA3" pad="8"/>
<connect gate="G$1" pin="GPIOA4" pad="9"/>
<connect gate="G$1" pin="GPIOA5" pad="10"/>
<connect gate="G$1" pin="GPIOMISO" pad="13"/>
<connect gate="G$1" pin="GPIOMOSI" pad="12"/>
<connect gate="G$1" pin="GPIORX" pad="14"/>
<connect gate="G$1" pin="GPIOSCK" pad="11"/>
<connect gate="G$1" pin="GPIOSCL" pad="18"/>
<connect gate="G$1" pin="GPIOSDA" pad="17"/>
<connect gate="G$1" pin="GPIOTX" pad="15"/>
<connect gate="G$1" pin="NC" pad="16"/>
<connect gate="G$1" pin="USB" pad="26"/>
<connect gate="G$1" pin="VBAT" pad="28"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="JST_2PIN" prefix="CN" uservalue="yes">
<description>&lt;b&gt;JST 2-Pin Connectors of various flavors&lt;/b&gt;

&lt;ul&gt;
&lt;li&gt;SMT-RA (S2B-PH-SM4) 4UConnector #17311&lt;/li&gt;
&lt;li&gt;SMT  (B2B-PH-SM4)&lt;/li&gt;
&lt;li&gt;THM-RA (S2B-PH)&lt;/li&gt;
&lt;li&gt;THM  (B2B-PH)&lt;/li&gt;
&lt;/ul&gt;</description>
<gates>
<gate name="G$1" symbol="PINHD2"/>
</gates>
<devices>
<device name="-SMT-RA" package="JST-PH-2-SMT-RA">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-THM" package="JST-PH-2-THM">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-THM-RA" package="JST-PH-2-THM-RA">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="-SMT" package="JST-PH-2-SMT">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="torex">
<packages>
<package name="XC6206">
</package>
</packages>
<symbols>
<symbol name="XC6206">
<pin name="VSS"/>
<pin name="VOUT"/>
<pin name="VIN"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="XC6206">
<gates>
<gate name="G$1" symbol="XC6206"/>
</gates>
<devices>
<device name="" package="XC6206">
<connects>
<connect gate="G$1" pin="VIN" pad="P$3"/>
<connect gate="G$1" pin="VOUT" pad="P$2"/>
<connect gate="G$1" pin="VSS" pad="P$1"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="MF_Discrete_Semiconductor">
<packages>
<package name="SMA">
<description>&lt;b&gt;Description:&lt;/b&gt; Footprint for Diodes in SMA Standard.&lt;br/&gt;</description>
</package>
<package name="SOD-123">
<description>&lt;b&gt;Description:&lt;/b&gt; Footprint for Diodes in SOD-123 Standard.&lt;br/&gt;</description>
</package>
</packages>
<symbols>
<symbol name="DIODE">
<description>&lt;b&gt;Description:&lt;/b&gt; Symbol for Single Diodes.&lt;br/&gt;</description>
<pin name="ANODE"/>
<pin name="CATHODE"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="DIODES" prefix="D">
<description>&lt;b&gt;Library:&lt;/b&gt;  MF_Discrete_Semiconductor&lt;br/&gt;
&lt;b&gt;Description:&lt;/b&gt; Device for Single Packaged Diodes.&lt;br/&gt;</description>
<gates>
<gate name="G$1" symbol="DIODE"/>
</gates>
<devices>
<device name="_SMA" package="SMA">
<connects>
<connect gate="G$1" pin="ANODE" pad="ANODE"/>
<connect gate="G$1" pin="CATHODE" pad="CATHODE"/>
</connects>
<technologies>
<technology name="">
<attribute name="HOUSEPART" value="NO"/>
<attribute name="MPN" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value=""/>
</technology>
<technology name="_B140">
<attribute name="HOUSEPART" value="YES"/>
<attribute name="MPN" value="MF-DIO-SMA-B140"/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value="https://factory.macrofab.com/part/MF-DIO-SMA-B140"/>
<attribute name="VALUE" value="MF-DIO-SMA-B140"/>
</technology>
</technologies>
</device>
<device name="_SOD-123" package="SOD-123">
<connects>
<connect gate="G$1" pin="ANODE" pad="ANODE"/>
<connect gate="G$1" pin="CATHODE" pad="CATHODE"/>
</connects>
<technologies>
<technology name="">
<attribute name="HOUSEPART" value="NO"/>
<attribute name="MPN" value=""/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value=""/>
</technology>
<technology name="_1N4148">
<attribute name="HOUSEPART" value="YES"/>
<attribute name="MPN" value="MF-DIO-SOD123-1N4148"/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value="https://factory.macrofab.com/part/MF-DIO-SOD123-1N4148"/>
<attribute name="VALUE" value="MF-DIO-SOD123-1N4148"/>
</technology>
<technology name="_BAT42">
<attribute name="HOUSEPART" value="YES"/>
<attribute name="MPN" value="MF-DIO-SOD123-BAT42"/>
<attribute name="POPULATE" value="1"/>
<attribute name="URL" value="https://factory.macrofab.com/part/MF-DIO-SOD123-BAT42"/>
<attribute name="VALUE" value="MF-DIO-SOD123-BAT42"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
<library name="SparkFun-Jumpers">
<description>&lt;h3&gt;SparkFun Jumpers&lt;/h3&gt;
In this library you'll find jumpers, or other semipermanent means of changing current paths. The least permanent form is the solder jumper. These can be changed by adding, removing, or moving solder. In cases that are less likely to be changed we have jumpers that are connected with traces. These can be cut with a razor, or reconnected with solder. Reference designator JP.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMT-JUMPER_2_NC_PASTE_NO-SILK">
</package>
<package name="SMT-JUMPER_2_NC_PASTE_SILK">
</package>
</packages>
<symbols>
<symbol name="SMT-JUMPER_2_NC_PASTE">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="JUMPER-SMT_2_NC_PASTE" prefix="JP">
<description>&lt;h3&gt;Normally closed solder jumper&lt;/h3&gt;
&lt;p&gt;This jumper has an aperture in the stencil to allow solder paste to bridge the split in the wire so it's normally closed (NC). Wick off the solder to open the connection. Reapply solder to reclose the connection.&lt;/p&gt;</description>
<gates>
<gate name="G$1" symbol="SMT-JUMPER_2_NC_PASTE"/>
</gates>
<devices>
<device name="_NO-SILK" package="SMT-JUMPER_2_NC_PASTE_NO-SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="_SILK" package="SMT-JUMPER_2_NC_PASTE_SILK">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<parts>
<part name="FRAME1" library="frames" deviceset="A4L-LOC" device=""/>
<part name="U$1" library="ixys" deviceset="KXOB25-01X8F" device=""/>
<part name="GND1" library="supply1" deviceset="GND" device=""/>
<part name="C3" library="MF_Passives" deviceset="CAPACITOR_NP" device="_0402" value="1uF"/>
<part name="GND2" library="supply1" deviceset="GND" device=""/>
<part name="+3V2" library="supply1" deviceset="+3V3" device=""/>
<part name="C4" library="MF_Passives" deviceset="CAPACITOR_NP" device="_0402" value="0.1uF"/>
<part name="C5" library="MF_Passives" deviceset="CAPACITOR_NP" device="_0402" value="1uF"/>
<part name="GND3" library="supply1" deviceset="GND" device=""/>
<part name="+3V3" library="supply1" deviceset="+3V3" device=""/>
<part name="GND4" library="supply1" deviceset="GND" device=""/>
<part name="GND5" library="supply1" deviceset="GND" device=""/>
<part name="J1" library="SparkFun-Connectors" deviceset="CORTEX_DEBUG" device="_PTH"/>
<part name="+3V4" library="supply1" deviceset="+3V3" device=""/>
<part name="GND6" library="supply1" deviceset="GND" device=""/>
<part name="R1" library="MF_Passives" deviceset="RESISTOR" device="_0402" value="1k"/>
<part name="+3V5" library="supply1" deviceset="+3V3" device=""/>
<part name="R2" library="MF_Passives" deviceset="RESISTOR" device="_0402" value="1M"/>
<part name="C8" library="MF_Passives" deviceset="CAPACITOR_NP" device="_0402" value="4.7nF"/>
<part name="J2" library="MF_Connectors" deviceset="USB" device="_MICRO_RIGHT" value="MF-CON-MICROUSB-RIGHT"/>
<part name="GND7" library="supply1" deviceset="GND" device=""/>
<part name="P+1" library="supply1" deviceset="+5V" device=""/>
<part name="MS1" library="adafruit" deviceset="FEATHERWING" device=""/>
<part name="+3V7" library="supply1" deviceset="+3V3" device=""/>
<part name="GND8" library="supply1" deviceset="GND" device=""/>
<part name="P+2" library="supply1" deviceset="+5V" device=""/>
<part name="U$2" library="ixys" deviceset="KXOB25-01X8F" device=""/>
<part name="P+3" library="supply1" deviceset="V+" device=""/>
<part name="IC1" library="samacsys" deviceset="ATSAML21J18B-AUT" device=""/>
<part name="L1" library="MF_Passives" deviceset="INDUCTOR" device="_0603" value="10uH"/>
<part name="C1" library="MF_Passives" deviceset="CAPACITOR_NP" device="_0402" value="1uF"/>
<part name="C9" library="MF_Passives" deviceset="CAPACITOR_NP" device="_0402" value="1uF"/>
<part name="C10" library="MF_Passives" deviceset="CAPACITOR_NP" device="_0402" value="1uF"/>
<part name="+3V1" library="supply1" deviceset="+3V3" device=""/>
<part name="+3V8" library="supply1" deviceset="+3V3" device=""/>
<part name="+3V9" library="supply1" deviceset="+3V3" device=""/>
<part name="GND9" library="supply1" deviceset="GND" device=""/>
<part name="GND10" library="supply1" deviceset="GND" device=""/>
<part name="GND11" library="supply1" deviceset="GND" device=""/>
<part name="L2" library="MF_Passives" deviceset="INDUCTOR" device="_0603" value="10uH"/>
<part name="Y1" library="samacsys" deviceset="ECS-.327-7-16-C-TR" device=""/>
<part name="C2" library="MF_Passives" deviceset="CAPACITOR_NP" device="_0402" value="1uF"/>
<part name="PS1" library="samacsys" deviceset="MCP1810T-33I_J8A" device=""/>
<part name="C6" library="MF_Passives" deviceset="CAPACITOR_NP" device="_0402" value="1uF"/>
<part name="C7" library="MF_Passives" deviceset="CAPACITOR_NP" device="_0402" value="1uF"/>
<part name="GND12" library="supply1" deviceset="GND" device=""/>
<part name="+3V6" library="supply1" deviceset="+3V3" device=""/>
<part name="GND13" library="supply1" deviceset="GND" device=""/>
<part name="R3" library="MF_Passives" deviceset="RESISTOR" device="_0402" value="5.6k"/>
<part name="GND14" library="supply1" deviceset="GND" device=""/>
<part name="FRAME2" library="frames" deviceset="A4L-LOC" device=""/>
<part name="+3V10" library="supply1" deviceset="+3V3" device=""/>
<part name="GND15" library="supply1" deviceset="GND" device=""/>
<part name="AC1" library="samacsys" deviceset="LIS3DHTR" device=""/>
<part name="R4" library="MF_Passives" deviceset="RESISTOR" device="_0402" value="5.6k"/>
<part name="C11" library="MF_Passives" deviceset="CAPACITOR_NP" device="_0402" value="1uF"/>
<part name="C12" library="MF_Passives" deviceset="CAPACITOR_NP" device="_0402" value="1uF"/>
<part name="GND16" library="supply1" deviceset="GND" device=""/>
<part name="+3V11" library="supply1" deviceset="+3V3" device=""/>
<part name="GND17" library="supply1" deviceset="GND" device=""/>
<part name="+3V12" library="supply1" deviceset="+3V3" device=""/>
<part name="R5" library="MF_Passives" deviceset="RESISTOR" device="_0402" value="5.6k"/>
<part name="+3V13" library="supply1" deviceset="+3V3" device=""/>
<part name="IC2" library="samacsys" deviceset="BMP280" device=""/>
<part name="GND18" library="supply1" deviceset="GND" device=""/>
<part name="+3V14" library="supply1" deviceset="+3V3" device=""/>
<part name="C13" library="MF_Passives" deviceset="CAPACITOR_NP" device="_0402" value="1uF"/>
<part name="+3V15" library="supply1" deviceset="+3V3" device=""/>
<part name="C14" library="MF_Passives" deviceset="CAPACITOR_NP" device="_0402" value="1uF"/>
<part name="GND19" library="supply1" deviceset="GND" device=""/>
<part name="P+4" library="supply1" deviceset="V+" device=""/>
<part name="GND22" library="supply1" deviceset="GND" device=""/>
<part name="U$3" library="torex" deviceset="XC6206" device="" value="XC6206P422MR-G"/>
<part name="C15" library="MF_Passives" deviceset="CAPACITOR_NP" device="_0402" value="1uF"/>
<part name="C16" library="MF_Passives" deviceset="CAPACITOR_NP" device="_0402" value="1uF"/>
<part name="D1" library="MF_Discrete_Semiconductor" deviceset="DIODES" device="_SOD-123" technology="_BAT42" value="MF-DIO-SOD123-BAT42"/>
<part name="BATT" library="adafruit" deviceset="JST_2PIN" device="-SMT-RA" value="S2B-PH-SM4-TB(LF)(SN)"/>
<part name="GND20" library="supply1" deviceset="GND" device=""/>
<part name="R6" library="MF_Passives" deviceset="RESISTOR" device="_0402" value="825K"/>
<part name="R7" library="MF_Passives" deviceset="RESISTOR" device="_0402" value="825K"/>
<part name="GND21" library="supply1" deviceset="GND" device=""/>
<part name="JP1" library="SparkFun-Jumpers" deviceset="JUMPER-SMT_2_NC_PASTE" device="_NO-SILK" value="JUMPER"/>
<part name="Z1" library="samacsys" deviceset="BZX384C5V6-HG3-08" device=""/>
<part name="LED1" library="samacsys" deviceset="KS_DELLS1.22-JHKI-1" device=""/>
<part name="R8" library="MF_Passives" deviceset="RESISTOR" device="_0402" value="750"/>
<part name="GND23" library="supply1" deviceset="GND" device=""/>
<part name="IC3" library="samacsys" deviceset="OPT3004DNPR" device=""/>
<part name="C17" library="MF_Passives" deviceset="CAPACITOR_NP" device="_0402" value="1uF"/>
<part name="GND24" library="supply1" deviceset="GND" device=""/>
<part name="+3V16" library="supply1" deviceset="+3V3" device=""/>
<part name="C18" library="MF_Passives" deviceset="CAPACITOR_NP" device="_0402" value="8.2pF"/>
<part name="C19" library="MF_Passives" deviceset="CAPACITOR_NP" device="_0402" value="8.2pF"/>
<part name="GND25" library="supply1" deviceset="GND" device=""/>
<part name="GND26" library="supply1" deviceset="GND" device=""/>
<part name="C20" library="samacsys" deviceset="EDC334Z5R5V" device=""/>
</parts>
<sheets>
<sheet>
<plain>
</plain>
<busses>
</busses>
<nets>
<net name="GND">
<segment>
<pinref part="GND1" gate="1" pin="GND"/>
<pinref part="U$1" gate="G$1" pin="-"/>
<pinref part="Z1" gate="G$1" pin="A"/>
</segment>
<segment>
<pinref part="GND2" gate="1" pin="GND"/>
<pinref part="C3" gate="G$1" pin="P$2"/>
</segment>
<segment>
<pinref part="GND3" gate="1" pin="GND"/>
<pinref part="C4" gate="G$1" pin="P$2"/>
<pinref part="C5" gate="G$1" pin="P$2"/>
</segment>
<segment>
<pinref part="GND4" gate="1" pin="GND"/>
<pinref part="IC1" gate="G$1" pin="GND_1"/>
<pinref part="C2" gate="G$1" pin="P$2"/>
</segment>
<segment>
<pinref part="GND5" gate="1" pin="GND"/>
<pinref part="IC1" gate="G$1" pin="GND_4"/>
</segment>
<segment>
<pinref part="J1" gate="G$1" pin="GND@3"/>
<pinref part="GND6" gate="1" pin="GND"/>
<pinref part="J1" gate="G$1" pin="GND@5"/>
</segment>
<segment>
<pinref part="J2" gate="G$1" pin="GND"/>
<pinref part="GND7" gate="1" pin="GND"/>
<pinref part="C8" gate="G$1" pin="P$2"/>
<pinref part="R2" gate="G$1" pin="P$2"/>
</segment>
<segment>
<pinref part="MS1" gate="G$1" pin="GND"/>
<pinref part="GND8" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="GND_3"/>
<pinref part="C9" gate="G$1" pin="P$2"/>
<pinref part="GND9" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="GND_2"/>
<pinref part="C1" gate="G$1" pin="P$2"/>
<pinref part="GND10" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="GND11" gate="1" pin="GND"/>
<pinref part="IC1" gate="G$1" pin="GNDANA"/>
<pinref part="C10" gate="G$1" pin="P$1"/>
</segment>
<segment>
<pinref part="C6" gate="G$1" pin="P$1"/>
<pinref part="GND12" gate="1" pin="GND"/>
<pinref part="PS1" gate="G$1" pin="GND"/>
</segment>
<segment>
<pinref part="GND13" gate="1" pin="GND"/>
<pinref part="C7" gate="G$1" pin="P$2"/>
</segment>
<segment>
<pinref part="GND14" gate="1" pin="GND"/>
<pinref part="PS1" gate="G$1" pin="EP"/>
</segment>
<segment>
<pinref part="R7" gate="G$1" pin="P$2"/>
<pinref part="GND21" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="LED1" gate="G$1" pin="K"/>
<pinref part="GND23" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="C19" gate="G$1" pin="P$2"/>
<pinref part="C18" gate="G$1" pin="P$2"/>
<pinref part="GND25" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="GND26" gate="1" pin="GND"/>
<pinref part="C20" gate="G$1" pin="-"/>
</segment>
</net>
<net name="+3V3">
<segment>
<pinref part="C3" gate="G$1" pin="P$1"/>
<pinref part="+3V2" gate="G$1" pin="+3V3"/>
<pinref part="IC1" gate="G$1" pin="VDDIN"/>
</segment>
<segment>
<pinref part="+3V3" gate="G$1" pin="+3V3"/>
<pinref part="IC1" gate="G$1" pin="VDDIO_1"/>
<pinref part="C2" gate="G$1" pin="P$1"/>
</segment>
<segment>
<pinref part="J1" gate="G$1" pin="VCC"/>
<pinref part="+3V4" gate="G$1" pin="+3V3"/>
</segment>
<segment>
<pinref part="+3V5" gate="G$1" pin="+3V3"/>
<pinref part="R1" gate="G$1" pin="P$1"/>
</segment>
<segment>
<pinref part="MS1" gate="G$1" pin="3V"/>
<pinref part="+3V7" gate="G$1" pin="+3V3"/>
</segment>
<segment>
<pinref part="+3V9" gate="G$1" pin="+3V3"/>
<pinref part="L2" gate="G$1" pin="P$2"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="VDDIO_2"/>
<pinref part="C1" gate="G$1" pin="P$1"/>
<pinref part="+3V1" gate="G$1" pin="+3V3"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="VDDIO_3"/>
<pinref part="C9" gate="G$1" pin="P$1"/>
<pinref part="+3V8" gate="G$1" pin="+3V3"/>
</segment>
<segment>
<pinref part="PS1" gate="G$1" pin="VOUT"/>
<pinref part="+3V6" gate="G$1" pin="+3V3"/>
<pinref part="C6" gate="G$1" pin="P$2"/>
<pinref part="PS1" gate="G$1" pin="FB"/>
</segment>
</net>
<net name="N$1">
<segment>
<pinref part="C5" gate="G$1" pin="P$1"/>
<pinref part="C4" gate="G$1" pin="P$1"/>
<pinref part="L1" gate="G$1" pin="P$2"/>
<pinref part="IC1" gate="G$1" pin="VDDCORE"/>
</segment>
</net>
<net name="RST">
<segment>
<pinref part="J1" gate="G$1" pin="!RESET"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="!RESET"/>
</segment>
<segment>
<pinref part="MS1" gate="G$1" pin="!RESET"/>
</segment>
</net>
<net name="SWDIO">
<segment>
<pinref part="J1" gate="G$1" pin="SWDIO/TMS"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PA31"/>
</segment>
</net>
<net name="SWDCLK">
<segment>
<pinref part="J1" gate="G$1" pin="SWDCLK/TCK"/>
<pinref part="R1" gate="G$1" pin="P$2"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PA30"/>
</segment>
</net>
<net name="DP">
<segment>
<pinref part="J2" gate="G$1" pin="D+"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PA25"/>
</segment>
</net>
<net name="DM">
<segment>
<pinref part="J2" gate="G$1" pin="D-"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PA24"/>
</segment>
</net>
<net name="N$5">
<segment>
<pinref part="J2" gate="G$1" pin="SLD"/>
<pinref part="R2" gate="G$1" pin="P$1"/>
<pinref part="C8" gate="G$1" pin="P$1"/>
</segment>
</net>
<net name="+5V">
<segment>
<pinref part="J2" gate="G$1" pin="5V"/>
<pinref part="P+1" gate="1" pin="+5V"/>
</segment>
<segment>
<pinref part="MS1" gate="G$1" pin="USB"/>
<pinref part="P+2" gate="1" pin="+5V"/>
</segment>
</net>
<net name="SCL">
<segment>
<pinref part="MS1" gate="G$1" pin="GPIOSCL"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PA23"/>
</segment>
</net>
<net name="SDA">
<segment>
<pinref part="MS1" gate="G$1" pin="GPIOSDA"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PA22"/>
</segment>
</net>
<net name="RX">
<segment>
<pinref part="MS1" gate="G$1" pin="GPIORX"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PB23"/>
</segment>
</net>
<net name="TX">
<segment>
<pinref part="MS1" gate="G$1" pin="GPIOTX"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PB22"/>
</segment>
</net>
<net name="MISO">
<segment>
<pinref part="MS1" gate="G$1" pin="GPIOMISO"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PA12"/>
</segment>
</net>
<net name="MOSI">
<segment>
<pinref part="MS1" gate="G$1" pin="GPIOMOSI"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PB10"/>
</segment>
</net>
<net name="SCK">
<segment>
<pinref part="MS1" gate="G$1" pin="GPIOSCK"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PB11"/>
</segment>
</net>
<net name="A0">
<segment>
<pinref part="MS1" gate="G$1" pin="GPIOA0"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PA02"/>
</segment>
<segment>
<pinref part="JP1" gate="G$1" pin="2"/>
</segment>
</net>
<net name="A1">
<segment>
<pinref part="MS1" gate="G$1" pin="GPIOA1"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PB08"/>
</segment>
</net>
<net name="A2">
<segment>
<pinref part="MS1" gate="G$1" pin="GPIOA2"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PB09"/>
</segment>
</net>
<net name="A3">
<segment>
<pinref part="MS1" gate="G$1" pin="GPIOA3"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PA04"/>
</segment>
</net>
<net name="A4">
<segment>
<pinref part="MS1" gate="G$1" pin="GPIOA4"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PA05"/>
</segment>
</net>
<net name="A5">
<segment>
<pinref part="MS1" gate="G$1" pin="GPIOA5"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PB02"/>
</segment>
</net>
<net name="N$2">
<segment>
<pinref part="IC1" gate="G$1" pin="PA00"/>
<pinref part="Y1" gate="G$1" pin="OUT/IN"/>
<pinref part="C19" gate="G$1" pin="P$1"/>
</segment>
</net>
<net name="N$3">
<segment>
<pinref part="IC1" gate="G$1" pin="PA01"/>
<pinref part="Y1" gate="G$1" pin="IN/OUT"/>
<pinref part="C18" gate="G$1" pin="P$1"/>
</segment>
</net>
<net name="N$6">
<segment>
<pinref part="IC1" gate="G$1" pin="VSW"/>
<pinref part="L1" gate="G$1" pin="P$1"/>
</segment>
</net>
<net name="N$4">
<segment>
<pinref part="IC1" gate="G$1" pin="VDDANA"/>
<pinref part="C10" gate="G$1" pin="P$2"/>
<pinref part="L2" gate="G$1" pin="P$1"/>
</segment>
</net>
<net name="AREF">
<segment>
<pinref part="IC1" gate="G$1" pin="PA03"/>
</segment>
<segment>
<pinref part="MS1" gate="G$1" pin="AREF"/>
</segment>
</net>
<net name="D9">
<segment>
<pinref part="MS1" gate="G$1" pin="GPIO9"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PB00"/>
</segment>
</net>
<net name="D5">
<segment>
<pinref part="MS1" gate="G$1" pin="GPIO5"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PB03"/>
</segment>
</net>
<net name="D11">
<segment>
<pinref part="MS1" gate="G$1" pin="GPIO11"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PB30"/>
</segment>
</net>
<net name="D13">
<segment>
<pinref part="IC1" gate="G$1" pin="PA17"/>
</segment>
<segment>
<pinref part="MS1" gate="G$1" pin="GPIO13"/>
</segment>
</net>
<net name="D10">
<segment>
<pinref part="MS1" gate="G$1" pin="GPIO10"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PB31"/>
</segment>
</net>
<net name="D12">
<segment>
<pinref part="IC1" gate="G$1" pin="PA19"/>
</segment>
<segment>
<pinref part="MS1" gate="G$1" pin="GPIO12"/>
</segment>
</net>
<net name="D6">
<segment>
<pinref part="MS1" gate="G$1" pin="GPIO6"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PB01"/>
</segment>
</net>
<net name="P_EN">
<segment>
<pinref part="MS1" gate="G$1" pin="EN"/>
</segment>
<segment>
<pinref part="PS1" gate="G$1" pin="!SHDN"/>
<pinref part="R3" gate="G$1" pin="P$1"/>
</segment>
</net>
<net name="VBAT">
<segment>
<pinref part="MS1" gate="G$1" pin="VBAT"/>
</segment>
<segment>
<pinref part="PS1" gate="G$1" pin="VIN"/>
<pinref part="C7" gate="G$1" pin="P$1"/>
<pinref part="R3" gate="G$1" pin="P$2"/>
</segment>
<segment>
<pinref part="R6" gate="G$1" pin="P$1"/>
</segment>
<segment>
<pinref part="C20" gate="G$1" pin="+"/>
</segment>
</net>
<net name="VB_SNS">
<segment>
<pinref part="R6" gate="G$1" pin="P$2"/>
<pinref part="R7" gate="G$1" pin="P$1"/>
<pinref part="JP1" gate="G$1" pin="1"/>
</segment>
</net>
<net name="ACCEL_INT">
<segment>
<pinref part="IC1" gate="G$1" pin="PB04"/>
</segment>
</net>
<net name="V+">
<segment>
<pinref part="U$2" gate="G$1" pin="+"/>
<pinref part="P+3" gate="1" pin="V+"/>
<pinref part="Z1" gate="G$1" pin="K"/>
</segment>
</net>
<net name="N$7">
<segment>
<pinref part="U$1" gate="G$1" pin="+"/>
<pinref part="U$2" gate="G$1" pin="-"/>
</segment>
</net>
<net name="N$8">
<segment>
<pinref part="R8" gate="G$1" pin="P$2"/>
<pinref part="LED1" gate="G$1" pin="A"/>
</segment>
</net>
<net name="LED">
<segment>
<pinref part="R8" gate="G$1" pin="P$1"/>
</segment>
<segment>
<pinref part="IC1" gate="G$1" pin="PA20"/>
</segment>
</net>
</nets>
</sheet>
<sheet>
<plain>
</plain>
<busses>
</busses>
<nets>
<net name="GND">
<segment>
<pinref part="AC1" gate="G$1" pin="GND_1"/>
<pinref part="C11" gate="G$1" pin="P$2"/>
<pinref part="GND15" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="GND16" gate="1" pin="GND"/>
<pinref part="C12" gate="G$1" pin="P$2"/>
</segment>
<segment>
<pinref part="AC1" gate="G$1" pin="GND_2"/>
<pinref part="GND17" gate="1" pin="GND"/>
<pinref part="AC1" gate="G$1" pin="RES"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="GND_2"/>
<pinref part="C13" gate="G$1" pin="P$2"/>
<pinref part="GND18" gate="1" pin="GND"/>
<pinref part="C14" gate="G$1" pin="P$1"/>
<pinref part="IC2" gate="G$1" pin="SDO"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="GND_1"/>
<pinref part="GND19" gate="1" pin="GND"/>
</segment>
<segment>
<pinref part="GND22" gate="1" pin="GND"/>
<pinref part="C15" gate="G$1" pin="P$2"/>
<pinref part="U$3" gate="G$1" pin="VSS"/>
<pinref part="C16" gate="G$1" pin="P$2"/>
</segment>
<segment>
<pinref part="GND20" gate="1" pin="GND"/>
<pinref part="BATT" gate="G$1" pin="1"/>
</segment>
<segment>
<pinref part="GND24" gate="1" pin="GND"/>
<pinref part="C17" gate="G$1" pin="P$2"/>
<pinref part="IC3" gate="G$1" pin="GND"/>
<pinref part="IC3" gate="G$1" pin="ADDR"/>
</segment>
</net>
<net name="+3V3">
<segment>
<pinref part="AC1" gate="G$1" pin="VDDIO"/>
<pinref part="+3V10" gate="G$1" pin="+3V3"/>
<pinref part="C11" gate="G$1" pin="P$1"/>
<pinref part="R4" gate="G$1" pin="P$1"/>
</segment>
<segment>
<pinref part="+3V11" gate="G$1" pin="+3V3"/>
<pinref part="C12" gate="G$1" pin="P$1"/>
<pinref part="AC1" gate="G$1" pin="VDD"/>
</segment>
<segment>
<pinref part="+3V12" gate="G$1" pin="+3V3"/>
<pinref part="R5" gate="G$1" pin="P$1"/>
</segment>
<segment>
<pinref part="AC1" gate="G$1" pin="SDO/SA0"/>
<pinref part="+3V13" gate="G$1" pin="+3V3"/>
<pinref part="AC1" gate="G$1" pin="CS"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="CSB"/>
<pinref part="+3V15" gate="G$1" pin="+3V3"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="VDDIO_2"/>
<pinref part="+3V14" gate="G$1" pin="+3V3"/>
<pinref part="C13" gate="G$1" pin="P$1"/>
<pinref part="IC2" gate="G$1" pin="VDDIO_1"/>
<pinref part="C14" gate="G$1" pin="P$2"/>
</segment>
<segment>
<pinref part="+3V16" gate="G$1" pin="+3V3"/>
<pinref part="C17" gate="G$1" pin="P$1"/>
<pinref part="IC3" gate="G$1" pin="VDD"/>
</segment>
</net>
<net name="SCL">
<segment>
<pinref part="AC1" gate="G$1" pin="SCL/SPC"/>
<pinref part="R4" gate="G$1" pin="P$2"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="SCK"/>
</segment>
<segment>
<pinref part="IC3" gate="G$1" pin="SCL"/>
</segment>
</net>
<net name="ACCEL_INT">
<segment>
<pinref part="AC1" gate="G$1" pin="INT1"/>
</segment>
</net>
<net name="SDA">
<segment>
<pinref part="AC1" gate="G$1" pin="SDA/SDI/SDO"/>
<pinref part="R5" gate="G$1" pin="P$2"/>
</segment>
<segment>
<pinref part="IC2" gate="G$1" pin="SDI"/>
</segment>
<segment>
<pinref part="IC3" gate="G$1" pin="SDA"/>
</segment>
</net>
<net name="VBAT">
<segment>
<pinref part="D1" gate="G$1" pin="CATHODE"/>
<pinref part="BATT" gate="G$1" pin="2"/>
</segment>
</net>
<net name="V+">
<segment>
<pinref part="U$3" gate="G$1" pin="VIN"/>
<pinref part="P+4" gate="1" pin="V+"/>
<pinref part="C15" gate="G$1" pin="P$1"/>
</segment>
</net>
<net name="N$10">
<segment>
<pinref part="U$3" gate="G$1" pin="VOUT"/>
<pinref part="C16" gate="G$1" pin="P$1"/>
<pinref part="D1" gate="G$1" pin="ANODE"/>
</segment>
</net>
</nets>
</sheet>
</sheets>
</schematic>
</drawing>
</eagle>
