<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.1.3">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="68.05" y2="0" width="0" layer="20"/>
<wire x1="68.05" y1="0" x2="68" y2="50.5" width="0" layer="20"/>
<wire x1="68" y1="50.5" x2="0.05" y2="50.5" width="0" layer="20"/>
<wire x1="0.05" y1="50.5" x2="0" y2="0" width="0" layer="20"/>
<text>Bluebird Labs - BattLab One Production Rev A  4/15/2020</text>
<text>GND</text>
<text>RST</text>
<text>TEST</text>
<text>+3V3</text>
<text>+5V</text>
<text>NC</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="USB-B-PTH">
<description>&lt;b&gt;USB Series B Hole Mounted&lt;/b&gt;</description>
</package>
<package name="BNC">
<description>Fits Mouser Part#5227161</description>
</package>
<package name="BANANA_CONN">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1206">
</package>
</packages>
</library>
<library name="ftdichip-6">
<description>&lt;b&gt;USB-Controller from Future Technology Devices International Ltd.&lt;/b&gt; 
&lt;br&gt;&lt;br&gt;
Based on the source of the libraries ftdichip-4.lbr and ftdichip-2.lbr.&lt;br&gt;
With new Vinculum-II Chips.&lt;br&gt;

Includes the following controller:&lt;br&gt;
&lt;ul&gt;
&lt;li&gt;FT232BL , FT245BL (2nd generation)
&lt;li&gt;FT2232L (3rd generation)
&lt;li&gt;FT232RL , FT245RL (4th generation)
&lt;li&gt;FT4232HL (5th generation)
&lt;li&gt;VNC1L
&lt;li&gt;VNC2-32
&lt;li&gt;VNC2-48 (symbol compatible&lt;sup&gt;*&lt;/sup&gt; with VNC1L)
&lt;li&gt;VNC2-64
&lt;/ul&gt;
http://www.ftdichip.com

&lt;br&gt;&lt;br&gt;

Originally by:
&lt;ul&gt;
&lt;li&gt;B.Redemann, 4232 by R.Pearce (ftdichip-4.lbr)
&lt;li&gt;Paul Carpenter, PC Services www.pcserviceselectronics.co.uk (ftdichip-2.lbr)
&lt;/ul&gt;
Updated with Vinculum-II by Marcin Zakaszewski.</description>
<packages>
<package name="SSOP28DB">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="PANASONIC_F">
<description>&lt;b&gt;Panasonic Aluminium Electrolytic Capacitor VS-Serie Package F&lt;/b&gt;</description>
</package>
<package name="1X06">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;</description>
</package>
<package name="SOD-123">
</package>
</packages>
</library>
<library name="BluebirdLabs">
<packages>
<package name="SOIC-8">
</package>
<package name="VSSOP-10">
</package>
<package name="MSOP-10">
</package>
</packages>
</library>
<library name="TI_MSP430_v16">
<packages>
<package name="PW20">
<description>*** TI: PW *** JEDEC: R-PDSO-G20 *** 20 PINS ***</description>
</package>
</packages>
</library>
<library name="750315371">
<packages>
<package name="TOR-6P-HT4_SMT_6PIN_(1201)">
<description>Package Style: TOR-6P-HT4&lt;br&gt;Mounting: SMT&lt;br&gt;Pins: 6&lt;br&gt;Bobbin: 250-1201</description>
</package>
</packages>
</library>
<library name="SN6505">
<packages>
<package name="SOT95P280X145-6N">
</package>
</packages>
</library>
<library name="SOIC127P600X175-8N">
<packages>
<package name="SOIC127P600X175-8N">
</package>
</packages>
</library>
<library name="MBR0520LT1G">
<packages>
<package name="SOD3716X117(SOD-123)">
</package>
</packages>
</library>
<library name="GeekAmmo">
<description>&lt;h3&gt;GeekAmmo  Library&lt;/h3&gt;

These are parts used by the GeekAmmo company (now part of SparkFun Electronics)!

 If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt;Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-3">
</package>
</packages>
</library>
<library name="ISO7742DBQ">
<packages>
<package name="SOP63P599X175-16N">
</package>
</packages>
</library>
<library name="TPD2E2U06DRLR">
<packages>
<package name="SOT50P160X60-5N">
<description>SOT-553 layout for TPD1E001. Pads are extra wide to facilitate hand soldering</description>
</package>
</packages>
</library>
<library name="SparkFun-LED">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete LEDs for illumination or indication, but no displays.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="LED-1206">
</package>
</packages>
</library>
<library name="MIC5225-5.0YM5-TR">
<packages>
<package name="SOT95P280X130-5N">
<description>&lt;b&gt;5-Pin SOT23 (M5)&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C2" library="SparkFun-Capacitors" package="1206" value="2.2uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R2" library="SparkFun-Passives" package="1206" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Passives" package="1206" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RSENSE" library="SparkFun-Resistors" package="1206" value="0.1">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="FTDI232RL" library="ftdichip-6" package="SSOP28DB" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="AP2318" library="BluebirdLabs" package="SOIC-8" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="INA233" library="BluebirdLabs" package="VSSOP-10" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="AD5248" library="BluebirdLabs" package="MSOP-10" value="100K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="1206" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="adafruit" package="PANASONIC_F" value="1000uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="1206" value=".1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R4" library="SparkFun-Passives" package="1206" value="47K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C9" library="SparkFun-Capacitors" package="1206" value="1nF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R5" library="SparkFun-Passives" package="1206" value="47K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="MSP430" library="TI_MSP430_v16" package="PW20" value="MSP430">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RLIMIT" library="SparkFun-Resistors" package="1206" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C11" library="SparkFun-Capacitors" package="1206" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="JP1" library="adafruit" package="1X06" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="T1" library="750315371" package="TOR-6P-HT4_SMT_6PIN_(1201)" value="750315371">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" Xfrmr Fwd p-p Dc/Dc Conv Smd "/>
<attribute name="MF" value="Wurth Electronics"/>
<attribute name="MP" value="750315371"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value=" Wurth Electronics"/>
<attribute name="PRICE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="SN6505" library="SN6505" package="SOT95P280X145-6N" value="SN6505">
<attribute name="VALUE"/>
</element>
<element name="ISO1540" library="SOIC127P600X175-8N" package="SOIC127P600X175-8N" value="ISO1540">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C12" library="SparkFun-Capacitors" package="1206" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D2" library="MBR0520LT1G" package="SOD3716X117(SOD-123)" value="MBR0520LT1G">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" sod, pin, process, Schottky Diodes, repetitive, voltage, polarity, reflow, leaded, diode, Diodes, plastic, current, s... "/>
<attribute name="MF" value="ON Semiconductor"/>
<attribute name="MP" value="MBR0520LT1G"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOD-123 Motorola"/>
<attribute name="PRICE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="D3" library="MBR0520LT1G" package="SOD3716X117(SOD-123)" value="MBR0520LT1G">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" sod, pin, process, Schottky Diodes, repetitive, voltage, polarity, reflow, leaded, diode, Diodes, plastic, current, s... "/>
<attribute name="MF" value="ON Semiconductor"/>
<attribute name="MP" value="MBR0520LT1G"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOD-123 Motorola"/>
<attribute name="PRICE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="C13" library="SparkFun-Capacitors" package="1206" value="10uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C14" library="SparkFun-Capacitors" package="1206" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R6" library="SparkFun-Passives" package="1206" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R7" library="SparkFun-Passives" package="1206" value="10K">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="1206" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RSENSE1" library="SparkFun-Resistors" package="1206" value="1000">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="P-MOS" library="GeekAmmo" package="SOT23-3" value="P-MOSFET">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RLIMIT4" library="SparkFun-Resistors" package="1206" value="220">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="ISO7742" library="ISO7742DBQ" package="SOP63P599X175-16N" value="ISO7742DBQ">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" ISO7742DBQ "/>
<attribute name="MF" value="Texas Instruments"/>
<attribute name="MP" value="ISO7742DBQ"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SSOP-16 Texas Instruments"/>
<attribute name="PRICE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="USBPROT" library="TPD2E2U06DRLR" package="SOT50P160X60-5N" value="TPD2E2U06DRLR">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" Dual-Channel High-Speed ESD Protection 5-SOT -40 to 125 "/>
<attribute name="MF" value="Texas Instruments"/>
<attribute name="MP" value="TPD2E2U06DRLR"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOT-553 Texas Instruments"/>
<attribute name="PRICE" value="None"/>
<attribute name="VALUE"/>
</element>
<element name="R8" library="SparkFun-Passives" package="1206" value="100">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="1206" value="2.2uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="SparkFun-Connectors" package="USB-B-PTH" value="USB-B">
<attribute name="PROD_ID" value="CONN-08278"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="1206" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="1206" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="D4" library="SparkFun-LED" package="LED-1206" value="BLUE">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-09911"/>
<attribute name="VALUE"/>
</element>
<element name="R3" library="SparkFun-Passives" package="1206" value="470">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C10" library="SparkFun-Capacitors" package="1206" value="1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C15" library="SparkFun-Capacitors" package="1206" value="2.2uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="MIC5225-5.0YM5-TR" package="SOT95P280X130-5N" value="MIC5225-5.0YM5-TR">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" Linear Voltage Regulator IC 1 Output 150mA SOT-23-5 "/>
<attribute name="MF" value="Microchip"/>
<attribute name="MP" value="MIC5225-5.0YM5-TR"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOT-23-5 Microchip"/>
<attribute name="PRICE" value="None"/>
</element>
<element name="C16" library="SparkFun-Capacitors" package="1206" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C17" library="SparkFun-Capacitors" package="1206" value="0.1uF">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="TRIG" library="SparkFun-Connectors" package="BNC" value="BNCPTH">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J1" library="SparkFun-Connectors" package="BANANA_CONN" value=""/>
<element name="J3" library="SparkFun-Connectors" package="BANANA_CONN" value=""/>
<element name="D1" library="adafruit" package="SOD-123" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="RBLD" library="SparkFun-Passives" package="1206" value="100k"/>
</elements>
<signals>
<signal name="GND">
<contactref element="FTDI232RL" pad="25"/>
<contactref element="FTDI232RL" pad="7"/>
<contactref element="FTDI232RL" pad="18"/>
<contactref element="FTDI232RL" pad="21"/>
<contactref element="FTDI232RL" pad="26"/>
<contactref element="SN6505" pad="4"/>
<contactref element="C12" pad="2"/>
<contactref element="ISO1540" pad="4"/>
<contactref element="C5" pad="1"/>
<contactref element="JP1" pad="6"/>
<contactref element="C9" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="ISO7742" pad="2"/>
<contactref element="ISO7742" pad="8"/>
<contactref element="USBPROT" pad="4"/>
<contactref element="MSP430" pad="20"/>
<contactref element="C7" pad="1"/>
<contactref element="J2" pad="GND"/>
<contactref element="C16" pad="2"/>
</signal>
<signal name="N$17">
</signal>
<signal name="N$18">
</signal>
<signal name="VBUS+5V">
<contactref element="FTDI232RL" pad="20"/>
<contactref element="SN6505" pad="5"/>
<contactref element="SN6505" pad="2"/>
<contactref element="C12" pad="1"/>
<contactref element="T1" pad="2"/>
<contactref element="JP1" pad="3"/>
<contactref element="J2" pad="VBUS"/>
</signal>
<signal name="VREF">
<contactref element="MSP430" pad="5"/>
<contactref element="C5" pad="2"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="TRANS1">
<contactref element="SN6505" pad="3"/>
<contactref element="T1" pad="1"/>
</signal>
<signal name="TRANS3">
<contactref element="SN6505" pad="1"/>
<contactref element="T1" pad="3"/>
</signal>
<signal name="N$12">
<contactref element="T1" pad="6"/>
<contactref element="D2" pad="2"/>
</signal>
<signal name="GND1">
<contactref element="C14" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="AD5248" pad="2"/>
<contactref element="AD5248" pad="4"/>
<contactref element="AD5248" pad="10"/>
<contactref element="AD5248" pad="8"/>
<contactref element="INA233" pad="1"/>
<contactref element="INA233" pad="2"/>
<contactref element="INA233" pad="7"/>
<contactref element="ISO1540" pad="5"/>
<contactref element="C2" pad="2"/>
<contactref element="ISO7742" pad="9"/>
<contactref element="ISO7742" pad="15"/>
<contactref element="T1" pad="5"/>
<contactref element="C6" pad="2"/>
<contactref element="C8" pad="2"/>
<contactref element="C11" pad="1"/>
<contactref element="C3" pad="-"/>
<contactref element="AP2318" pad="8"/>
<contactref element="R3" pad="1"/>
<contactref element="C10" pad="2"/>
<contactref element="C15" pad="2"/>
<contactref element="IC2" pad="2"/>
<contactref element="C17" pad="2"/>
<contactref element="TRIG" pad="GND"/>
<contactref element="J3" pad="P$1"/>
<contactref element="D1" pad="A"/>
<contactref element="RBLD" pad="2"/>
</signal>
<signal name="SDA1">
<contactref element="MSP430" pad="15"/>
<contactref element="ISO1540" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
<signal name="SCL1">
<contactref element="MSP430" pad="14"/>
<contactref element="ISO1540" pad="3"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="LDO_EN1">
<contactref element="MSP430" pad="8"/>
<contactref element="RLIMIT" pad="1"/>
</signal>
<signal name="LDO_EN2">
<contactref element="AP2318" pad="2"/>
<contactref element="ISO7742" pad="13"/>
</signal>
<signal name="N$21">
<contactref element="AP2318" pad="7"/>
<contactref element="AD5248" pad="1"/>
<contactref element="AD5248" pad="3"/>
</signal>
<signal name="SDA2">
<contactref element="AD5248" pad="7"/>
<contactref element="INA233" pad="4"/>
<contactref element="ISO1540" pad="7"/>
<contactref element="R7" pad="2"/>
</signal>
<signal name="SCL2">
<contactref element="AD5248" pad="6"/>
<contactref element="INA233" pad="5"/>
<contactref element="ISO1540" pad="6"/>
<contactref element="R6" pad="2"/>
</signal>
<signal name="V_OUT">
<contactref element="INA233" pad="10"/>
<contactref element="RSENSE1" pad="1"/>
<contactref element="P-MOS" pad="2"/>
<contactref element="AP2318" pad="6"/>
<contactref element="C6" pad="1"/>
<contactref element="AD5248" pad="9"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="VOUT">
<contactref element="INA233" pad="9"/>
<contactref element="C3" pad="+"/>
<contactref element="C11" pad="2"/>
<contactref element="RSENSE" pad="2"/>
<contactref element="J1" pad="P$1"/>
<contactref element="RBLD" pad="1"/>
</signal>
<signal name="TRIGGER_MSP2">
<contactref element="R8" pad="2"/>
<contactref element="ISO7742" pad="12"/>
<contactref element="D1" pad="C"/>
</signal>
<signal name="TRIGGER_MSP1">
<contactref element="MSP430" pad="9"/>
<contactref element="ISO7742" pad="5"/>
</signal>
<signal name="RESET">
<contactref element="MSP430" pad="16"/>
<contactref element="C9" pad="2"/>
<contactref element="JP1" pad="5"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="TEST">
<contactref element="MSP430" pad="17"/>
<contactref element="JP1" pad="4"/>
</signal>
<signal name="N$4">
<contactref element="RSENSE1" pad="2"/>
<contactref element="RSENSE" pad="1"/>
<contactref element="P-MOS" pad="3"/>
</signal>
<signal name="RS_EN">
<contactref element="MSP430" pad="10"/>
<contactref element="RLIMIT4" pad="1"/>
</signal>
<signal name="RS_EN1">
<contactref element="RLIMIT4" pad="2"/>
<contactref element="ISO7742" pad="3"/>
</signal>
<signal name="LDO_EN">
<contactref element="ISO7742" pad="4"/>
<contactref element="RLIMIT" pad="2"/>
</signal>
<signal name="RS_EN2">
<contactref element="P-MOS" pad="1"/>
<contactref element="ISO7742" pad="14"/>
</signal>
<signal name="NC">
<contactref element="USBPROT" pad="1"/>
</signal>
<signal name="N$38">
<contactref element="R8" pad="1"/>
<contactref element="TRIG" pad="S"/>
</signal>
<signal name="N$10">
<contactref element="T1" pad="4"/>
<contactref element="D3" pad="2"/>
</signal>
<signal name="USB-">
<contactref element="FTDI232RL" pad="16"/>
<contactref element="J2" pad="D-"/>
<contactref element="USBPROT" pad="3"/>
</signal>
<signal name="USB+">
<contactref element="USBPROT" pad="5"/>
<contactref element="FTDI232RL" pad="15"/>
<contactref element="J2" pad="D+"/>
</signal>
<signal name="3.3V">
<contactref element="ISO7742" pad="7"/>
<contactref element="ISO7742" pad="1"/>
<contactref element="C7" pad="2"/>
<contactref element="MSP430" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="R4" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="ISO1540" pad="1"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="2"/>
<contactref element="C16" pad="1"/>
<contactref element="JP1" pad="2"/>
<contactref element="FTDI232RL" pad="17"/>
<contactref element="FTDI232RL" pad="4"/>
</signal>
<signal name="UART_TX">
<contactref element="FTDI232RL" pad="1"/>
<contactref element="MSP430" pad="3"/>
</signal>
<signal name="UART_RX">
<contactref element="MSP430" pad="4"/>
<contactref element="FTDI232RL" pad="5"/>
</signal>
<signal name="N$29">
<contactref element="D4" pad="C"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="N$8">
<contactref element="D2" pad="1"/>
<contactref element="D3" pad="1"/>
<contactref element="C13" pad="1"/>
<contactref element="C10" pad="1"/>
<contactref element="AP2318" pad="3"/>
<contactref element="C1" pad="2"/>
<contactref element="AP2318" pad="4"/>
<contactref element="C14" pad="1"/>
<contactref element="IC2" pad="1"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="+5V_LDO">
<contactref element="IC2" pad="5"/>
<contactref element="C15" pad="1"/>
<contactref element="ISO7742" pad="10"/>
<contactref element="R6" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="ISO1540" pad="8"/>
<contactref element="AD5248" pad="5"/>
<contactref element="INA233" pad="6"/>
<contactref element="ISO7742" pad="16"/>
<contactref element="C8" pad="1"/>
<contactref element="D4" pad="A"/>
<contactref element="C17" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
