<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="57.13" y1="0" x2="57.15" y2="25.4" width="0" layer="20"/>
<wire x1="57.15" y1="25.4" x2="0" y2="25.4" width="0" layer="20"/>
<wire x1="0" y1="25.4" x2="0" y2="0" width="0" layer="20"/>
<text>USB isolated
null modem
v2.2</text>
<wire x1="0" y1="0" x2="57.13" y2="0" width="0" layer="20"/>
</plain>
<libraries>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="USBC">
<packages>
<package name="USB4110-GF-A">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CHIPLED_0805">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_R971.pdf</description>
</package>
</packages>
</library>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SSOP28DB">
<description>&lt;b&gt;Small Shrink Outline Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="AD5680">
<packages>
<package name="TSSOP-16">
<description>&lt;b&gt;16-Lead Thin Shrink Small Outline Package&lt;/b&gt; [TSSOP] (RU-16)&lt;p&gt;
Source: 8x ADG1408_1409.pdf</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="R5" library="SparkFun-Resistors" package="0805" value="330Ω">
<attribute name="NAME"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0805" value="330Ω">
<attribute name="NAME"/>
</element>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="J2" library="USBC" package="USB4110-GF-A" value="USB4110-GF-A">
<attribute name="NAME"/>
</element>
<element name="J1" library="USBC" package="USB4110-GF-A" value="USB4110-GF-A">
<attribute name="NAME"/>
</element>
<element name="LED1" library="adafruit" package="CHIPLED_0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LED2" library="adafruit" package="CHIPLED_0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="5.1kΩ">
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="5.1kΩ">
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="5.1kΩ">
<attribute name="NAME"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="5.1kΩ">
<attribute name="NAME"/>
</element>
<element name="IC1" library="SparkFun-DigitalIC" package="SSOP28DB" value="CY7C65213">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="IC-12487"/>
</element>
<element name="IC2" library="SparkFun-DigitalIC" package="SSOP28DB" value="CY7C65213">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="IC-12487"/>
</element>
<element name="IC3" library="AD5680" package="TSSOP-16" value="SI8035">
<attribute name="NAME"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC4" library="AD5680" package="TSSOP-16" value="SI8035">
<attribute name="NAME"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="0805" value="">
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="J2" pad="A6"/>
<contactref element="J2" pad="B6"/>
<contactref element="IC2" pad="15"/>
</signal>
<signal name="N$2">
<contactref element="J2" pad="A7"/>
<contactref element="J2" pad="B7"/>
<contactref element="IC2" pad="16"/>
</signal>
<signal name="N$5">
<contactref element="IC2" pad="17"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="J2" pad="B5"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="N$10">
<contactref element="J2" pad="A5"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="J1" pad="A6"/>
<contactref element="J1" pad="B6"/>
<contactref element="IC1" pad="15"/>
</signal>
<signal name="N$11">
<contactref element="J1" pad="A7"/>
<contactref element="J1" pad="B7"/>
<contactref element="IC1" pad="16"/>
</signal>
<signal name="N$13">
<contactref element="IC1" pad="17"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="J1" pad="B5"/>
<contactref element="R4" pad="2"/>
</signal>
<signal name="N$16">
<contactref element="J1" pad="A5"/>
<contactref element="R3" pad="2"/>
</signal>
<signal name="GND">
<contactref element="R3" pad="1"/>
<contactref element="J1" pad="B1A12"/>
<contactref element="R4" pad="1"/>
<contactref element="C4" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="IC1" pad="21"/>
<contactref element="IC1" pad="7"/>
<contactref element="IC1" pad="18"/>
<contactref element="IC3" pad="8"/>
<contactref element="IC3" pad="2"/>
<contactref element="C5" pad="2"/>
<contactref element="IC4" pad="9"/>
<contactref element="IC4" pad="15"/>
<contactref element="C8" pad="2"/>
<contactref element="J1" pad="A1B12"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="23"/>
<contactref element="LED2" pad="C"/>
</signal>
<signal name="N$14">
<contactref element="IC2" pad="23"/>
<contactref element="LED1" pad="C"/>
</signal>
<signal name="N$20">
<contactref element="LED2" pad="A"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="R5">
<contactref element="LED1" pad="A"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="J2" pad="B4A9"/>
<contactref element="J2" pad="A4B9"/>
<contactref element="IC2" pad="20"/>
<contactref element="IC2" pad="4"/>
<contactref element="C3" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="IC3" pad="16"/>
<contactref element="C6" pad="1"/>
<contactref element="IC4" pad="1"/>
<contactref element="C7" pad="1"/>
</signal>
<signal name="GNDA">
<contactref element="R1" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="IC2" pad="21"/>
<contactref element="IC2" pad="7"/>
<contactref element="IC2" pad="18"/>
<contactref element="R2" pad="1"/>
<contactref element="J2" pad="B1A12"/>
<contactref element="IC3" pad="9"/>
<contactref element="IC3" pad="15"/>
<contactref element="C6" pad="2"/>
<contactref element="IC4" pad="8"/>
<contactref element="IC4" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="J2" pad="A1B12"/>
</signal>
<signal name="VDD">
<contactref element="J1" pad="B4A9"/>
<contactref element="J1" pad="A4B9"/>
<contactref element="IC1" pad="20"/>
<contactref element="IC1" pad="4"/>
<contactref element="C4" pad="1"/>
<contactref element="R6" pad="2"/>
<contactref element="IC3" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="IC4" pad="16"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="RXDA">
<contactref element="IC1" pad="5"/>
<contactref element="IC4" pad="14"/>
</signal>
<signal name="RTSA">
<contactref element="IC1" pad="3"/>
<contactref element="IC4" pad="13"/>
</signal>
<signal name="TXDB">
<contactref element="IC2" pad="1"/>
<contactref element="IC4" pad="3"/>
</signal>
<signal name="RXDB">
<contactref element="IC2" pad="5"/>
<contactref element="IC3" pad="14"/>
</signal>
<signal name="CTSB">
<contactref element="IC2" pad="11"/>
<contactref element="IC4" pad="4"/>
</signal>
<signal name="RTSB">
<contactref element="IC2" pad="3"/>
<contactref element="IC3" pad="13"/>
</signal>
<signal name="DTRB">
<contactref element="IC2" pad="2"/>
<contactref element="IC4" pad="5"/>
</signal>
<signal name="DSRB">
<contactref element="IC2" pad="9"/>
<contactref element="IC2" pad="10"/>
<contactref element="IC3" pad="12"/>
</signal>
<signal name="DSRA">
<contactref element="IC1" pad="9"/>
<contactref element="IC1" pad="10"/>
<contactref element="IC4" pad="12"/>
</signal>
<signal name="DTRA">
<contactref element="IC1" pad="2"/>
<contactref element="IC3" pad="5"/>
</signal>
<signal name="CTSA">
<contactref element="IC1" pad="11"/>
<contactref element="IC3" pad="4"/>
</signal>
<signal name="TXDA">
<contactref element="IC1" pad="1"/>
<contactref element="IC3" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
