Reference, Quantity, Value, Footprint, Datasheet
BZ1 ,1,"Buzzer","Buzzer_Beeper:Buzzer_12x9.5RM7.6","~"
C1 C5 ,2,"4u7","Capacitor_SMD:C_0805_2012Metric","~"
C11 C13 C10 C15 C12 C3 C4 ,7,"10n","Capacitor_SMD:C_0805_2012Metric","~"
C18 C17 ,2,"DNP","Capacitor_SMD:C_0805_2012Metric","~"
C6 C8 C2 C14 C16 ,5,"100n","Capacitor_SMD:C_0805_2012Metric","~"
C7 C9 ,2,"10u","Capacitor_SMD:C_0805_2012Metric","~"
D1 ,1,"7V","Diode_SMD:D_SMA","~"
D2 ,1,"RED","Diode_SMD:D_1206_3216Metric","~"
D7 D4 D8 D5 D6 D3 ,6,"S1G","Diode_SMD:D_SMA","~"
J1 ,1,"USB_B_Micro","Connector_USB:USB_Micro-B_Molex_47346-0001","~"
J2 ,1,"Battery terminal","Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical","~"
J3 ,1,"Display","Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical","~"
J4 ,1,"SWD","Connector_PinHeader_2.54mm:PinHeader_1x04_P2.54mm_Vertical","~"
J5 ,1,"DUT","Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical","~"
Q1 ,1,"DMP3098L","Package_TO_SOT_SMD:SOT-23","http://www.farnell.com/datasheets/1915664.pdf"
R1 R23 R35 ,3,"0R","Resistor_SMD:R_0805_2012Metric","~"
R10 R11 ,2,"2K2","Resistor_SMD:R_0805_2012Metric","~"
R14 R9 R13 R8 R12 R37 ,6,"300R","Resistor_SMD:R_0805_2012Metric","~"
R15 R28 R22 ,3,"100R","Resistor_SMD:R_0805_2012Metric","~"
R2 R17 R16 R4 ,4,"1K","Resistor_SMD:R_0805_2012Metric","~"
R24 ,1,"33K","Resistor_SMD:R_0805_2012Metric","~"
R25 R18 R19 R20 R21 ,5,"150R","Resistor_SMD:R_0805_2012Metric","~"
R26 R32 R33 ,3,"330K/.1%","Resistor_SMD:R_0805_2012Metric","~"
R29 R31 R36 ,3,"33K/.1%","Resistor_SMD:R_0805_2012Metric","~"
R30 ,1,"150R/.1%","Resistor_SMD:R_0805_2012Metric","~"
R34 ,1,"50R","Resistor_SMD:R_0805_2012Metric","~"
R6 ,1,"4K","Resistor_SMD:R_0805_2012Metric","~"
R7 R5 R27 R3 ,4,"10K","Resistor_SMD:R_0805_2012Metric","~"
SW2 SW1 ,2,"SW_Push","Button_Switch_THT:SW_PUSH_6mm","~"
U1 ,1,"MCP73831-2-OT","Package_TO_SOT_SMD:SOT-23-5","http://ww1.microchip.com/downloads/en/DeviceDoc/20001984g.pdf"
U2 ,1,"STM32F030F4Px","Package_SO:TSSOP-20_4.4x6.5mm_P0.65mm","http://www.st.com/st-web-ui/static/active/en/resource/technical/document/datasheet/DM00088500.pdf"
U3 ,1,"LM1117-3.3","Package_TO_SOT_SMD:SOT-223-3_TabPin2","http://www.ti.com/lit/ds/symlink/lm1117.pdf"
U4 U5 ,2,"MCP6022-I_SN","Package_SO:SOIC-8_3.9x4.9mm_P1.27mm","https://www.tme.eu/Document/e53df4b1836c376b19d8bc3b9f170709/mcp6021.pdf"
Y1 ,1,"8MHz","Crystal:Crystal_SMD_HC49-SD","~"