(export (version D)
  (design
    (source C:\Users\Standa\Desktop\Projects\CurrentSensor\HW\Dev\CurSens.sch)
    (date "27-Aug-20 7:24:23 PM")
    (tool "Eeschema (5.1.6)-1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title "Isolated current sensor 50 A, 1.5 MHz")
        (company "Stanislav Subrt")
        (rev AA)
        (date 2020-08-27)
        (source CurSens.sch)
        (comment (number 1) (value "Frydek-Mistek, Czech Republic"))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref R1)
      (value 10K)
      (footprint Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F3D2623))
    (comp (ref C5)
      (value 10n)
      (footprint Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F3D3058))
    (comp (ref C4)
      (value 100n)
      (footprint Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F3D58FA))
    (comp (ref R2)
      (value 1K)
      (footprint Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F3D8D8C))
    (comp (ref J3)
      (value Conn_01x01)
      (footprint TestPoint:TestPoint_Pad_4.0x4.0mm)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x01) (description "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F3DC4DF))
    (comp (ref J4)
      (value Conn_01x01)
      (footprint TestPoint:TestPoint_Pad_4.0x4.0mm)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x01) (description "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F3DCB59))
    (comp (ref J7)
      (value Conn_01x01)
      (footprint TestPoint:TestPoint_Pad_4.0x4.0mm)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x01) (description "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F3DE284))
    (comp (ref J8)
      (value Conn_01x01)
      (footprint TestPoint:TestPoint_Pad_4.0x4.0mm)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x01) (description "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F3DEC1A))
    (comp (ref J9)
      (value Conn_01x01)
      (footprint TestPoint:TestPoint_Pad_4.0x4.0mm)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x01) (description "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F3DEF09))
    (comp (ref J10)
      (value Conn_01x01)
      (footprint TestPoint:TestPoint_Pad_4.0x4.0mm)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x01) (description "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F3ED2AF))
    (comp (ref R4)
      (value 100R)
      (footprint Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F3E33CF))
    (comp (ref C6)
      (value 100p)
      (footprint Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F3E2AA5))
    (comp (ref R3)
      (value 100R)
      (footprint Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F3E22FA))
    (comp (ref RV1)
      (value 14VDC)
      (footprint Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part Varistor) (description "Voltage dependent resistor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F4AACBB))
    (comp (ref C7)
      (value 100p)
      (footprint Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F3E31A5))
    (comp (ref C8)
      (value 100p)
      (footprint Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F3F01D6))
    (comp (ref C9)
      (value 100p)
      (footprint Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F3F047F))
    (comp (ref RV2)
      (value 14VDC)
      (footprint Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part Varistor) (description "Voltage dependent resistor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F4BC405))
    (comp (ref RV3)
      (value 14VDC)
      (footprint Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part Varistor) (description "Voltage dependent resistor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F4BF887))
    (comp (ref RV4)
      (value 14VDC)
      (footprint Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part Varistor) (description "Voltage dependent resistor"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F4BFCC8))
    (comp (ref C1)
      (value 4u7)
      (footprint Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F4CBDFD))
    (comp (ref C2)
      (value 4u7)
      (footprint Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F4CCB11))
    (comp (ref C3)
      (value 4u7)
      (footprint Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F4CCF64))
    (comp (ref F1)
      (value 500mA)
      (footprint Resistor_SMD:R_1206_3216Metric_Pad1.42x1.75mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part Fuse_Small) (description "Fuse, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F4DF026))
    (comp (ref D1)
      (value "16V TVS")
      (footprint Diode_SMD:D_SMA-SMB_Universal_Handsoldering)
      (datasheet ~)
      (libsource (lib Device) (part D_TVS) (description "Bidirectional transient-voltage-suppression diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F4DF7C1))
    (comp (ref J1)
      (value Conn_01x01)
      (footprint TestPoint:TestPoint_Pad_4.0x4.0mm)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x01) (description "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F4E8012))
    (comp (ref J2)
      (value Conn_01x01)
      (footprint TestPoint:TestPoint_Pad_4.0x4.0mm)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x01) (description "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F4E892A))
    (comp (ref U1)
      (value LM1117-3.3)
      (footprint Package_TO_SOT_SMD:SOT-223-3_TabPin2)
      (datasheet http://www.ti.com/lit/ds/symlink/lm1117.pdf)
      (libsource (lib Regulator_Linear) (part LM1117-3.3) (description "800mA Low-Dropout Linear Regulator, 3.3V fixed output, TO-220/TO-252/TO-263/SOT-223"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F50CB69))
    (comp (ref U2)
      (value MCA1101-50-3)
      (footprint Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm)
      (datasheet https://navview.blob.core.windows.net/web-resources/6020-1104-01_B%20Datasheet%2C%20Current%20Sensor%20Fix%20Gain%203.3V_20190627.pdf)
      (libsource (lib Aceinna) (part MCA1101-50-3) (description "High Accuracy Current Sensor IC with 1.5MHz 3dB Bandwidth and Isolation  ±5A, ±20A, ±50A, 3.3V, Fixed Gain"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F53A233))
    (comp (ref J5)
      (value Conn_01x01)
      (footprint TestPoint:TestPoint_Pad_4.0x4.0mm)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x01) (description "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F5436A9))
    (comp (ref J6)
      (value Conn_01x01)
      (footprint TestPoint:TestPoint_Pad_4.0x4.0mm)
      (datasheet ~)
      (libsource (lib Connector_Generic) (part Conn_01x01) (description "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F546F72)))
  (libparts
    (libpart (lib Aceinna) (part MCA1101-50-3)
      (description "High Accuracy Current Sensor IC with 1.5MHz 3dB Bandwidth and Isolation  ±5A, ±20A, ±50A, 3.3V, Fixed Gain")
      (docs https://navview.blob.core.windows.net/web-resources/6020-1104-01_B%20Datasheet%2C%20Current%20Sensor%20Fix%20Gain%203.3V_20190627.pdf)
      (footprints
        (fp SOIC*7.5x10.3mm*P1.27mm*))
      (fields
        (field (name Reference) U)
        (field (name Value) MCA1101-50-3)
        (field (name Footprint) Package_SO:SOIC-16W_7.5x10.3mm_P1.27mm))
      (pins
        (pin (num 1) (name IP+) (type passive))
        (pin (num 2) (name IP+) (type passive))
        (pin (num 3) (name IP+) (type passive))
        (pin (num 4) (name IP+) (type passive))
        (pin (num 5) (name IP-) (type passive))
        (pin (num 6) (name IP-) (type passive))
        (pin (num 7) (name IP-) (type passive))
        (pin (num 8) (name IP-) (type passive))
        (pin (num 9) (name ~FAULT) (type openCol))
        (pin (num 10) (name VCC) (type power_in))
        (pin (num 11) (name GND) (type power_in))
        (pin (num 12) (name VOUT) (type output))
        (pin (num 13) (name VREF) (type output))
        (pin (num 14) (name GND) (type power_in))
        (pin (num 15) (name GND) (type power_in))
        (pin (num 16) (name VOC) (type input))))
    (libpart (lib Connector_Generic) (part Conn_01x01)
      (description "Generic connector, single row, 01x01, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x01))
      (pins
        (pin (num 1) (name Pin_1) (type passive))))
    (libpart (lib Device) (part C_Small)
      (description "Unpolarized capacitor, small symbol")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part D_TVS)
      (description "Bidirectional transient-voltage-suppression diode")
      (docs ~)
      (footprints
        (fp TO-???*)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_TVS))
      (pins
        (pin (num 1) (name A1) (type passive))
        (pin (num 2) (name A2) (type passive))))
    (libpart (lib Device) (part Fuse_Small)
      (description "Fuse, small symbol")
      (docs ~)
      (footprints
        (fp SM*))
      (fields
        (field (name Reference) F)
        (field (name Value) Fuse_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part R_Small)
      (description "Resistor, small symbol")
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part Varistor)
      (description "Voltage dependent resistor")
      (docs ~)
      (footprints
        (fp RV_*)
        (fp Varistor*))
      (fields
        (field (name Reference) RV)
        (field (name Value) Varistor))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Regulator_Linear) (part LM1117-1.8)
      (aliases
        (alias LM1117-2.5)
        (alias LM1117-3.3)
        (alias LM1117-5.0)
        (alias TLV1117-15)
        (alias TLV1117-18)
        (alias TLV1117-25)
        (alias TLV1117-33)
        (alias TLV1117-50))
      (description "800mA Low-Dropout Linear Regulator, 1.8V fixed output, TO-220/TO-252/TO-263/SOT-223")
      (docs http://www.ti.com/lit/ds/symlink/lm1117.pdf)
      (footprints
        (fp SOT?223*)
        (fp TO?263*)
        (fp TO?252*)
        (fp TO?220*))
      (fields
        (field (name Reference) U)
        (field (name Value) LM1117-1.8))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name VO) (type power_out))
        (pin (num 3) (name VI) (type power_in)))))
  (libraries
    (library (logical Aceinna)
      (uri C:\Users\Standa\Desktop\Projects\CurrentSensor\HW\Dev/Aceinna.lib))
    (library (logical Connector_Generic)
      (uri C:\Programs\KiCad\share\kicad\library/Connector_Generic.lib))
    (library (logical Device)
      (uri C:\Programs\KiCad\share\kicad\library/Device.lib))
    (library (logical Regulator_Linear)
      (uri C:\Programs\KiCad\share\kicad\library/Regulator_Linear.lib)))
  (nets
    (net (code 1) (name "Net-(C8-Pad1)")
      (node (ref C8) (pin 1))
      (node (ref J9) (pin 1))
      (node (ref RV3) (pin 1))
      (node (ref R4) (pin 1)))
    (net (code 2) (name "Net-(C9-Pad1)")
      (node (ref U2) (pin 9))
      (node (ref RV4) (pin 1))
      (node (ref C9) (pin 1))
      (node (ref J10) (pin 1)))
    (net (code 3) (name "Net-(C7-Pad1)")
      (node (ref J8) (pin 1))
      (node (ref RV2) (pin 1))
      (node (ref R3) (pin 1))
      (node (ref C7) (pin 1)))
    (net (code 4) (name "Net-(R4-Pad2)")
      (node (ref R4) (pin 2))
      (node (ref U2) (pin 12)))
    (net (code 5) (name "Net-(R3-Pad2)")
      (node (ref U2) (pin 13))
      (node (ref R3) (pin 2)))
    (net (code 6) (name "Net-(C1-Pad1)")
      (node (ref U1) (pin 3))
      (node (ref D1) (pin 1))
      (node (ref F1) (pin 2))
      (node (ref C1) (pin 1)))
    (net (code 7) (name "Net-(F1-Pad1)")
      (node (ref J1) (pin 1))
      (node (ref F1) (pin 1)))
    (net (code 8) (name GND)
      (node (ref C9) (pin 2))
      (node (ref U1) (pin 1))
      (node (ref J2) (pin 1))
      (node (ref C4) (pin 1))
      (node (ref C5) (pin 1))
      (node (ref R2) (pin 1))
      (node (ref C3) (pin 2))
      (node (ref RV1) (pin 2))
      (node (ref C7) (pin 2))
      (node (ref C8) (pin 2))
      (node (ref C1) (pin 2))
      (node (ref U2) (pin 15))
      (node (ref U2) (pin 14))
      (node (ref U2) (pin 11))
      (node (ref C6) (pin 2))
      (node (ref RV2) (pin 2))
      (node (ref RV4) (pin 2))
      (node (ref RV3) (pin 2))
      (node (ref D1) (pin 2))
      (node (ref J6) (pin 1))
      (node (ref C2) (pin 2)))
    (net (code 9) (name +3V3)
      (node (ref C3) (pin 1))
      (node (ref C2) (pin 1))
      (node (ref J5) (pin 1))
      (node (ref U1) (pin 2))
      (node (ref R1) (pin 2))
      (node (ref U2) (pin 10))
      (node (ref C5) (pin 2))
      (node (ref C4) (pin 2)))
    (net (code 10) (name "Net-(C6-Pad1)")
      (node (ref J7) (pin 1))
      (node (ref C6) (pin 1))
      (node (ref R2) (pin 2))
      (node (ref R1) (pin 1))
      (node (ref RV1) (pin 1))
      (node (ref U2) (pin 16)))
    (net (code 11) (name /IPM)
      (node (ref U2) (pin 5))
      (node (ref U2) (pin 8))
      (node (ref U2) (pin 7))
      (node (ref U2) (pin 6))
      (node (ref J4) (pin 1)))
    (net (code 12) (name /IPP)
      (node (ref U2) (pin 2))
      (node (ref U2) (pin 3))
      (node (ref J3) (pin 1))
      (node (ref U2) (pin 1))
      (node (ref U2) (pin 4)))))