<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<text>BAT</text>
<text>GND</text>
<text>5V</text>
<text>3V3</text>
<text>4</text>
<text>14</text>
<text>15</text>
<text>27</text>
<text>26</text>
<text>25</text>
<text>21</text>
<text>33</text>
<text>22</text>
<text>5</text>
<text>18</text>
<text>19</text>
<text>23</text>
<text>32</text>
<text>26</text>
<text>3V3</text>
<text>4</text>
<text>27</text>
<text>14</text>
<text>GND</text>
<text>21</text>
<text>RST</text>
<text>33</text>
<text>22</text>
<text>5</text>
<text>18</text>
<text>RST</text>
<text>GND</text>
<text>25</text>
<text>15</text>
<text>BAT</text>
<text>5V</text>
<text>19</text>
<text>23</text>
<text>GND</text>
<text>32</text>
<text>MTR1+</text>
<text>MTR1-</text>
<text>MTR5-</text>
<text>MTR5+</text>
<text>GND</text>
<text>BTN1</text>
<text>Menique</text>
<text>Anular</text>
<text>Medio</text>
<text>Indice</text>
<text>n/c</text>
<text>Menique</text>
<text>Anular</text>
<text>Medio</text>
<text>Indice</text>
<text>Desogned in GT by </text>
<text>FLATBOX, S.A</text>
<text>Use with TinyPico</text>
<text>haptic gloves shield</text>
<text>may this open your eyes to a new world.</text>
<wire x1="-19.152" y1="19.78" x2="-19.152" y2="-16" width="0" layer="20"/>
<wire x1="-19.152" y1="-16" x2="26.3516" y2="-16" width="0" layer="20"/>
<wire x1="26.3516" y1="-16" x2="26.3516" y2="19.78" width="0" layer="20"/>
<wire x1="26.3516" y1="19.78" x2="-19.152" y2="19.78" width="0" layer="20"/>
</plain>
<libraries>
<library name="UnexpectedMaker">
<description>Generated from &lt;b&gt;WattsSegment_Display.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="1X10_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole -10 Pin No Silk&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:10&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_10&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Aesthetics">
<description>&lt;h3&gt;SparkFun Aesthetics&lt;/h3&gt;
This library contiains non-functional items such as logos, build/ordering notes, frame blocks, etc. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="OSHW-LOGO-S">
<description>&lt;h3&gt;Open-Source Hardware (OSHW) Logo - Small - Silkscreen&lt;/h3&gt;
&lt;p&gt;Silkscreen logo for open-source hardware designs.&lt;/p&gt;
&lt;p&gt;Devices using:
&lt;ul&gt;&lt;li&gt;OSHW_LOGO&lt;/li&gt;&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Wurth_Connectors_WR-PHD">
<description>&lt;BR&gt;Wurth Elektronik - Connectors - Board-to-Board Connectors - WR-PHD &lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2019a, 2019-10-16&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="61301021821">
<description>&lt;B&gt;WR-PHD &lt;/B&gt;&lt;BR&gt;2.54 mm Dual Socket Header,10 Pins</description>
</package>
</packages>
</library>
<library name="SamacSys_Parts">
<description>&lt;b&gt;https://componentsearchengine.com&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by SamacSys&lt;/author&gt;</description>
<packages>
<package name="SOT95P280X145-6N">
<description>&lt;b&gt; 6 SOT23-6&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="CAPC1608X87N">
<description>&lt;b&gt;0603B104K160CT&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="QFN50P200X200X80-10N">
<description>&lt;b&gt;RUN(S-PWQFN-N10)&lt;/b&gt;&lt;br&gt;
</description>
</package>
<package name="CAPC1608X90N">
<description>&lt;b&gt;0603-1&lt;/b&gt;&lt;br&gt;
</description>
</package>
</packages>
</library>
<library name="Wurth_Connectors_WR-WST">
<description>&lt;BR&gt;Wurth Elektronik - Connectors - Wire-to-Board Connectors - WR-WST &lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2019b, 2019-11-04&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="490107671812">
<description>&lt;b&gt;WR-WST REDFIT IDC SKEDD&lt;br&gt;&lt;br&gt;&lt;/b&gt;For permanent application up to 10g vibration stable</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="LEFT" library="UnexpectedMaker" package="1X10_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-11563"/>
<attribute name="VALUE"/>
</element>
<element name="RIGHT" library="UnexpectedMaker" package="1X10_NO_SILK" value="">
<attribute name="PROD_ID" value="CONN-11563"/>
<attribute name="VALUE"/>
</element>
<element name="LOGO1" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value="OSHW-LOGOS"/>
<element name="MOTORES" library="Wurth_Connectors_WR-PHD" package="61301021821" value="MTR 10 PIN">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/61301021821.pdf"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MATES" value="WR-PHD 2.54mm SMT Dual Pin Header/THT Angled Dual Pin Header/THT Dual Board Stacker/THT Dual Pin Header"/>
<attribute name="NAME"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61301021821 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE"/>
</element>
<element name="BOTONES" library="Wurth_Connectors_WR-PHD" package="61301021821" value="BTN 10 PIN">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/61301021821.pdf"/>
<attribute name="GENDER" value="Socket Header"/>
<attribute name="IR" value="3A"/>
<attribute name="MATES" value="WR-PHD 2.54mm SMT Dual Pin Header/THT Angled Dual Pin Header/THT Dual Board Stacker/THT Dual Pin Header"/>
<attribute name="NAME"/>
<attribute name="PACKAGING" value="Tray"/>
<attribute name="PART-NUMBER" value=" 61301021821 "/>
<attribute name="PINS" value=" 10 "/>
<attribute name="ROWS" value="Dual"/>
<attribute name="TYPE" value="Straight"/>
<attribute name="VALUE"/>
</element>
<element name="IC1" library="SamacSys_Parts" package="SOT95P280X145-6N" value="MAX6817EUT+T">
<attribute name="DESCRIPTION" value="Supervisory Circuits Dual Switch Debouncer"/>
<attribute name="HEIGHT" value="1.45mm"/>
<attribute name="MANUFACTURER_NAME" value="Maxim Integrated"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="MAX6817EUT+T"/>
<attribute name="MOUSER_PART_NUMBER" value="700-MAX6817EUTT"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Maxim-Integrated/MAX6817EUT%2bT?qs=1THa7WoU59HkU%2FfQtsyW%252BA%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C1" library="SamacSys_Parts" package="CAPC1608X87N" value="0603B104K160CT">
<attribute name="DESCRIPTION" value="WALSIN - 0603B104K160CT - CAP, 0.1F, 16V, 10%, X7R, 0603"/>
<attribute name="HEIGHT" value="0.87mm"/>
<attribute name="MANUFACTURER_NAME" value="Walsin Technology Corporation"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="0603B104K160CT"/>
<attribute name="MOUSER_PART_NUMBER" value="791-0603B104K160CT"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=791-0603B104K160CT"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C2" library="SamacSys_Parts" package="CAPC1608X87N" value="0603B104K160CT">
<attribute name="DESCRIPTION" value="WALSIN - 0603B104K160CT - CAP, 0.1F, 16V, 10%, X7R, 0603"/>
<attribute name="HEIGHT" value="0.87mm"/>
<attribute name="MANUFACTURER_NAME" value="Walsin Technology Corporation"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="0603B104K160CT"/>
<attribute name="MOUSER_PART_NUMBER" value="791-0603B104K160CT"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.com/Search/Refine.aspx?Keyword=791-0603B104K160CT"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC2" library="SamacSys_Parts" package="SOT95P280X145-6N" value="MAX6817EUT+T">
<attribute name="DESCRIPTION" value="Supervisory Circuits Dual Switch Debouncer"/>
<attribute name="HEIGHT" value="1.45mm"/>
<attribute name="MANUFACTURER_NAME" value="Maxim Integrated"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="MAX6817EUT+T"/>
<attribute name="MOUSER_PART_NUMBER" value="700-MAX6817EUTT"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Maxim-Integrated/MAX6817EUT%2bT?qs=1THa7WoU59HkU%2FfQtsyW%252BA%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC5" library="SamacSys_Parts" package="QFN50P200X200X80-10N" value="DRV2603RUNR">
<attribute name="DESCRIPTION" value="Haptic Driver with Auto Resonance Tracking for LRA and Optimized Drive for ERM"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="MANUFACTURER_NAME" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="DRV2603RUNR"/>
<attribute name="MOUSER_PART_NUMBER" value="595-DRV2603RUNR"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Texas-Instruments/DRV2603RUNR?qs=l6ZoeTYLMwNhoGl8Q31%2FaA%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC6" library="SamacSys_Parts" package="QFN50P200X200X80-10N" value="DRV2603RUNR">
<attribute name="DESCRIPTION" value="Haptic Driver with Auto Resonance Tracking for LRA and Optimized Drive for ERM"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="MANUFACTURER_NAME" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="DRV2603RUNR"/>
<attribute name="MOUSER_PART_NUMBER" value="595-DRV2603RUNR"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Texas-Instruments/DRV2603RUNR?qs=l6ZoeTYLMwNhoGl8Q31%2FaA%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC7" library="SamacSys_Parts" package="QFN50P200X200X80-10N" value="DRV2603RUNR">
<attribute name="DESCRIPTION" value="Haptic Driver with Auto Resonance Tracking for LRA and Optimized Drive for ERM"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="MANUFACTURER_NAME" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="DRV2603RUNR"/>
<attribute name="MOUSER_PART_NUMBER" value="595-DRV2603RUNR"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Texas-Instruments/DRV2603RUNR?qs=l6ZoeTYLMwNhoGl8Q31%2FaA%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC8" library="SamacSys_Parts" package="QFN50P200X200X80-10N" value="DRV2603RUNR">
<attribute name="DESCRIPTION" value="Haptic Driver with Auto Resonance Tracking for LRA and Optimized Drive for ERM"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="MANUFACTURER_NAME" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="DRV2603RUNR"/>
<attribute name="MOUSER_PART_NUMBER" value="595-DRV2603RUNR"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Texas-Instruments/DRV2603RUNR?qs=l6ZoeTYLMwNhoGl8Q31%2FaA%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C3" library="SamacSys_Parts" package="CAPC1608X90N" value="06031C104KAT2A">
<attribute name="DESCRIPTION" value="AVX - 06031C104KAT2A - CAP, MLCC, X7R, 0.1UF, 100V, 0603"/>
<attribute name="HEIGHT" value="0.9mm"/>
<attribute name="MANUFACTURER_NAME" value="AVX"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="06031C104KAT2A"/>
<attribute name="MOUSER_PART_NUMBER" value="581-06031C104KAT2A"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/AVX/06031C104KAT2A?qs=oF%2FSscNnLpBUv12UcNAw2A%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C4" library="SamacSys_Parts" package="CAPC1608X90N" value="06031C104KAT2A">
<attribute name="DESCRIPTION" value="AVX - 06031C104KAT2A - CAP, MLCC, X7R, 0.1UF, 100V, 0603"/>
<attribute name="HEIGHT" value="0.9mm"/>
<attribute name="MANUFACTURER_NAME" value="AVX"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="06031C104KAT2A"/>
<attribute name="MOUSER_PART_NUMBER" value="581-06031C104KAT2A"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/AVX/06031C104KAT2A?qs=oF%2FSscNnLpBUv12UcNAw2A%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C5" library="SamacSys_Parts" package="CAPC1608X90N" value="06031C104KAT2A">
<attribute name="DESCRIPTION" value="AVX - 06031C104KAT2A - CAP, MLCC, X7R, 0.1UF, 100V, 0603"/>
<attribute name="HEIGHT" value="0.9mm"/>
<attribute name="MANUFACTURER_NAME" value="AVX"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="06031C104KAT2A"/>
<attribute name="MOUSER_PART_NUMBER" value="581-06031C104KAT2A"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/AVX/06031C104KAT2A?qs=oF%2FSscNnLpBUv12UcNAw2A%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="IC3" library="SamacSys_Parts" package="QFN50P200X200X80-10N" value="DRV2603RUNR">
<attribute name="DESCRIPTION" value="Haptic Driver with Auto Resonance Tracking for LRA and Optimized Drive for ERM"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="MANUFACTURER_NAME" value="Texas Instruments"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="DRV2603RUNR"/>
<attribute name="MOUSER_PART_NUMBER" value="595-DRV2603RUNR"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/Texas-Instruments/DRV2603RUNR?qs=l6ZoeTYLMwNhoGl8Q31%2FaA%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C6" library="SamacSys_Parts" package="CAPC1608X90N" value="06031C104KAT2A">
<attribute name="DESCRIPTION" value="AVX - 06031C104KAT2A - CAP, MLCC, X7R, 0.1UF, 100V, 0603"/>
<attribute name="HEIGHT" value="0.9mm"/>
<attribute name="MANUFACTURER_NAME" value="AVX"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="06031C104KAT2A"/>
<attribute name="MOUSER_PART_NUMBER" value="581-06031C104KAT2A"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/AVX/06031C104KAT2A?qs=oF%2FSscNnLpBUv12UcNAw2A%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="C7" library="SamacSys_Parts" package="CAPC1608X90N" value="06031C104KAT2A">
<attribute name="DESCRIPTION" value="AVX - 06031C104KAT2A - CAP, MLCC, X7R, 0.1UF, 100V, 0603"/>
<attribute name="HEIGHT" value="0.9mm"/>
<attribute name="MANUFACTURER_NAME" value="AVX"/>
<attribute name="MANUFACTURER_PART_NUMBER" value="06031C104KAT2A"/>
<attribute name="MOUSER_PART_NUMBER" value="581-06031C104KAT2A"/>
<attribute name="MOUSER_PRICE-STOCK" value="https://www.mouser.co.uk/ProductDetail/AVX/06031C104KAT2A?qs=oF%2FSscNnLpBUv12UcNAw2A%3D%3D"/>
<attribute name="NAME"/>
<attribute name="VALUE"/>
</element>
<element name="LOGO2" library="SparkFun-Aesthetics" package="OSHW-LOGO-S" value="OSHW-LOGOS"/>
<element name="J1" library="Wurth_Connectors_WR-WST" package="490107671812" value="">
<attribute name="CONTACT-RESISTANCE" value="10mOhm"/>
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/em/datasheet/490107671812.pdf"/>
<attribute name="GENDER" value="Transition"/>
<attribute name="IR" value="1A"/>
<attribute name="L" value="30.45mm"/>
<attribute name="NAME"/>
<attribute name="PACKAGING" value="Tube"/>
<attribute name="PART-NUMBER" value="490107671812"/>
<attribute name="PINS" value=" 18 "/>
<attribute name="PITCH" value="2.54mm"/>
<attribute name="TOL-R" value="max."/>
<attribute name="USE-WITH" value="WR-CAB 1.27 mm Ribbon Flat Cable/WR-CAB 1.27 mm Ribbon Flat Cable 1 m pieces"/>
<attribute name="VALUE"/>
<attribute name="WE-NUMBER" value="490107671812"/>
<attribute name="WORKING-VOLTAGE" value="100V(AC)"/>
</element>
</elements>
<signals>
<signal name="GND">
<contactref element="RIGHT" pad="10"/>
<contactref element="LEFT" pad="2"/>
<contactref element="BOTONES" pad="1"/>
<contactref element="BOTONES" pad="3"/>
<contactref element="BOTONES" pad="5"/>
<contactref element="BOTONES" pad="7"/>
<contactref element="IC1" pad="2"/>
<contactref element="C1" pad="2"/>
<contactref element="C2" pad="2"/>
<contactref element="IC2" pad="2"/>
<contactref element="IC8" pad="10"/>
<contactref element="IC8" pad="8"/>
<contactref element="IC8" pad="5"/>
<contactref element="IC7" pad="10"/>
<contactref element="IC7" pad="5"/>
<contactref element="C3" pad="2"/>
<contactref element="IC7" pad="8"/>
<contactref element="C4" pad="2"/>
<contactref element="IC6" pad="10"/>
<contactref element="IC6" pad="5"/>
<contactref element="IC6" pad="8"/>
<contactref element="C5" pad="2"/>
<contactref element="IC5" pad="8"/>
<contactref element="C6" pad="2"/>
<contactref element="IC5" pad="5"/>
<contactref element="IC5" pad="10"/>
<contactref element="IC3" pad="10"/>
<contactref element="IC3" pad="5"/>
<contactref element="IC3" pad="8"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="3.3V">
<contactref element="LEFT" pad="4"/>
<contactref element="IC1" pad="5"/>
<contactref element="C1" pad="1"/>
<contactref element="IC2" pad="5"/>
<contactref element="IC8" pad="7"/>
<contactref element="IC8" pad="3"/>
<contactref element="IC7" pad="3"/>
<contactref element="C3" pad="1"/>
<contactref element="IC7" pad="7"/>
<contactref element="C4" pad="1"/>
<contactref element="IC6" pad="3"/>
<contactref element="IC6" pad="7"/>
<contactref element="C5" pad="1"/>
<contactref element="IC5" pad="7"/>
<contactref element="C6" pad="1"/>
<contactref element="IC5" pad="3"/>
<contactref element="IC3" pad="7"/>
<contactref element="IC3" pad="3"/>
<contactref element="C7" pad="1"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="RESET">
<contactref element="RIGHT" pad="9"/>
</signal>
<signal name="GND1">
</signal>
<signal name="DATA_OUT">
</signal>
<signal name="GPIO32">
<contactref element="RIGHT" pad="7"/>
<contactref element="IC3" pad="2"/>
</signal>
<signal name="GPIO33">
<contactref element="RIGHT" pad="8"/>
<contactref element="IC8" pad="1"/>
<contactref element="IC7" pad="1"/>
<contactref element="IC6" pad="1"/>
<contactref element="IC5" pad="1"/>
<contactref element="IC3" pad="1"/>
</signal>
<signal name="GPIO25">
<contactref element="LEFT" pad="10"/>
</signal>
<signal name="GPIO26">
<contactref element="LEFT" pad="9"/>
</signal>
<signal name="GPIO27">
<contactref element="LEFT" pad="8"/>
<contactref element="IC2" pad="4"/>
</signal>
<signal name="GPIO14">
<contactref element="LEFT" pad="6"/>
<contactref element="IC1" pad="4"/>
</signal>
<signal name="GPIO15">
<contactref element="LEFT" pad="7"/>
<contactref element="IC2" pad="6"/>
</signal>
<signal name="GPIO4">
<contactref element="LEFT" pad="5"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="GPIO5">
<contactref element="RIGHT" pad="4"/>
<contactref element="IC5" pad="2"/>
</signal>
<signal name="GPIO18">
<contactref element="RIGHT" pad="3"/>
<contactref element="IC6" pad="2"/>
</signal>
<signal name="GPIO23">
<contactref element="RIGHT" pad="1"/>
<contactref element="IC8" pad="2"/>
</signal>
<signal name="GPIO22">
<contactref element="RIGHT" pad="5"/>
</signal>
<signal name="GPIO19">
<contactref element="RIGHT" pad="2"/>
<contactref element="IC7" pad="2"/>
</signal>
<signal name="GPIO21">
<contactref element="RIGHT" pad="6"/>
</signal>
<signal name="VBAT">
<contactref element="LEFT" pad="1"/>
</signal>
<signal name="USB">
<contactref element="LEFT" pad="3"/>
</signal>
<signal name="SW_PUSH_MENIQUE">
<contactref element="BOTONES" pad="2"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="SW_PUSH_INDICE">
<contactref element="BOTONES" pad="8"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="SW_PUSH_MEDIO">
<contactref element="BOTONES" pad="6"/>
<contactref element="IC1" pad="3"/>
</signal>
<signal name="SW_PUSH_ANULAR">
<contactref element="BOTONES" pad="4"/>
<contactref element="IC2" pad="1"/>
</signal>
<signal name="MTR1+">
<contactref element="MOTORES" pad="1"/>
<contactref element="IC3" pad="9"/>
</signal>
<signal name="MTR2+">
<contactref element="MOTORES" pad="3"/>
<contactref element="IC5" pad="9"/>
</signal>
<signal name="MTR3+">
<contactref element="MOTORES" pad="5"/>
<contactref element="IC6" pad="9"/>
</signal>
<signal name="MTR4+">
<contactref element="MOTORES" pad="7"/>
<contactref element="IC7" pad="9"/>
</signal>
<signal name="MTR5+">
<contactref element="MOTORES" pad="9"/>
<contactref element="IC8" pad="9"/>
</signal>
<signal name="MTR1-">
<contactref element="MOTORES" pad="2"/>
<contactref element="IC3" pad="6"/>
</signal>
<signal name="MTR2-">
<contactref element="MOTORES" pad="4"/>
<contactref element="IC5" pad="6"/>
</signal>
<signal name="MTR3-">
<contactref element="MOTORES" pad="6"/>
<contactref element="IC6" pad="6"/>
</signal>
<signal name="MTR4-">
<contactref element="MOTORES" pad="8"/>
<contactref element="IC7" pad="6"/>
</signal>
<signal name="MTR5-">
<contactref element="MOTORES" pad="10"/>
<contactref element="IC8" pad="6"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
