(footprint "C_0201_0603Metric_mod" (version 20221018) (generator pcbnew)
  (layer "F.Cu")
  (descr "Resistor SMD 0201 (0603 Metric), square (rectangular) end terminal, IPC_7351 nominal, (Body size source: https://www.vishay.com/docs/20052/crcw0201e3.pdf), generated with kicad-footprint-generator")
  (tags "resistor")
  (attr smd)
  (fp_text reference "REF**" (at 0 -1.05) (layer "F.SilkS"))
  (fp_text value "RC_0201_0603Metric" (at 0 1.05) (layer "F.Fab"))
  (fp_text user "${REFERENCE}" (at 0 -0.68) (layer "F.Fab"))
  (pad "1" smd roundrect (at -0.3 0) (size 0.3 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (pad "2" smd roundrect (at 0.3 0) (size 0.3 0.4) (layers "F.Cu" "F.Paste" "F.Mask") (roundrect_rratio 0.25))
  (model "${KICAD6_3DMODEL_DIR}/Capacitor_SMD.3dshapes/C_0201_0603Metric.wrl"
    (offset (xyz 0 0 0))
    (scale (xyz 1 1 1))
    (rotate (xyz 0 0 0))
  )
)
