<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.1">
<drawing>
<board>
<plain>
<wire x1="2" y1="0" x2="48" y2="0" width="0.001" layer="20"/>
<wire x1="48" y1="25" x2="2" y2="25" width="0.001" layer="20"/>
<wire x1="50" y1="2" x2="50" y2="23" width="0.001" layer="20"/>
<wire x1="0" y1="23" x2="0" y2="2" width="0.001" layer="20"/>
<wire x1="0" y1="2" x2="2" y2="0" width="0.001" layer="20" curve="90"/>
<wire x1="2" y1="25" x2="0" y2="23" width="0.001" layer="20" curve="90"/>
<wire x1="50" y1="23" x2="48" y2="25" width="0.001" layer="20" curve="90"/>
<wire x1="48" y1="0" x2="50" y2="2" width="0.001" layer="20" curve="90"/>
<text>GemaLight V3 r2 
29/6/2020 gemalight.net</text>
<circle x="2.5" y="2.5" radius="1.5" width="0.001" layer="20"/>
<circle x="2.5" y="22.5" radius="1.5" width="0.001" layer="20"/>
<circle x="42" y="3" radius="1.1" width="0.001" layer="20"/>
<circle x="42" y="22" radius="1.1" width="0.001" layer="20"/>
<text>Attiny85</text>
<text>3-3.7V 
CR2032,LIR2032</text>
<text>ON</text>
<text>NeoStrip</text>
<text>+</text>
<text>GND</text>
<text>DATA</text>
<text>OFF</text>
</plain>
<libraries>
<library name="SparkFun-Switches">
<description>&lt;h3&gt;SparkFun Switches, Buttons, Encoders&lt;/h3&gt;
In this library you'll find switches, buttons, joysticks, and anything that moves to create or disrupt an electrical connection.
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE_SWITCH_PTH_6.0MM">
<description>&lt;h3&gt;Momentary Switch (Pushbutton) - SPST - PTH, 6.0mm Square&lt;/h3&gt;
&lt;p&gt;Normally-open (NO) SPST momentary switches (buttons, pushbuttons).&lt;/p&gt;
&lt;p&gt;&lt;a href="https://www.omron.com/ecb/products/pdf/en-b3f.pdf"&gt;Datasheet&lt;/a&gt; (B3F-1000)&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="NeoPixel attiny 85">
<description>Generated from &lt;b&gt;GemaLight 2.1.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="ATTINY85_DIP254P762X533-8">
</package>
</packages>
</library>
<library name="MAX1551EZK_T">
<packages>
<package name="SOT95P275X110-5N">
</package>
</packages>
</library>
<library name="zx62d-b-5pa8">
<description>&lt;b&gt;Hirose ZX62D-B-5PA8 Connector&lt;/b&gt;&lt;br&gt;
( OSH Park compatible library)&lt;br&gt;
&lt;br&gt;
&amp;copy; 2015 Samuel Lourenço</description>
<packages>
<package name="ZX62D-B-5PA8">
<description>&lt;b&gt;Micro USB Type B Connector&lt;/b&gt; - Standard, Shell Through Hole&lt;br&gt;
&lt;br&gt;
Source: &lt;a href="http://www.hirose.co.jp/cataloge_hp/ed_ZX_20140804.pdf"&gt;http://www.hirose.co.jp/cataloge_hp/ed_ZX_20140804.pdf&lt;/a&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Batteries 20mm">
<description>&lt;h3&gt;SparkFun Batteries&lt;/h3&gt;
This library contains battery clips, connectors, and appropriately sized silk outlines for LiPo batteries. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="BATTCON_20MM_4LEGS">
<description>&lt;h3&gt;20mm Coin Cell Battery (CR2032) Holder - SMD (Dual Pad)&lt;/h3&gt;
&lt;p&gt;This holder fits 20mm Lithium coin cell batteries and holds the battery in place with friction. The metal housing connects to the positive (+) side of the battery and the PCB pad underneath is connected to the negative (-) side.&lt;/p&gt;
&lt;p&gt;&lt;a href="http://cdn.sparkfun.com/datasheets/Prototyping/BAT-BLH-001.jpg"&gt;Datasheet&lt;/a&gt;&lt;/p&gt;
&lt;h4&gt;Devices Using&lt;/h4&gt;
&lt;ul&gt;&lt;li&gt;BATTERY&lt;/li&gt;&lt;/ul&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Resistors&lt;/h3&gt;
This library contains resistors. Reference designator:R. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Small led LTST-S270KRKT">
<packages>
<package name="0603">
</package>
</packages>
</library>
<library name="CUS-12B">
<packages>
<package name="CUS-12B">
</package>
</packages>
</library>
<library name="NeoPixel strip connector">
<packages>
<package name="NEOSTRIPCONNECTORSMD">
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Connectors&lt;/h3&gt;
This library contains electrically-functional connectors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="PAD.03X.03">
<description>&lt;h3&gt;Electrically Conductive Pad 0.03" Circle&lt;/h3&gt;
Used as a test point connection for pogo pins or other debugging tools. 
&lt;p&gt;Specifications:
&lt;li&gt;Area: 0.03" x 0.03"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;TEST_POINT&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Capacitors&lt;/h3&gt;
This library contains capacitors. 
&lt;br&gt;
&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is &lt;b&gt; the end user's responsibility&lt;/b&gt; to ensure correctness and suitablity for a given componet or application. 
&lt;br&gt;
&lt;br&gt;If you enjoy using this library, please buy one of our products at &lt;a href=" www.sparkfun.com"&gt;SparkFun.com&lt;/a&gt;.
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;
&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0603">
<description>&lt;p&gt;&lt;b&gt;Generic 1608 (0603) package&lt;/b&gt;&lt;/p&gt;
&lt;p&gt;0.2mm courtyard excess rounded to nearest 0.05mm.&lt;/p&gt;</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="S1" library="SparkFun-Switches" package="TACTILE_SWITCH_PTH_6.0MM" value="MOMENTARY-SWITCH-SPST-PTH-6.0MM">
<attribute name="NAME"/>
<attribute name="PROD_ID" value=" SWCH-08441"/>
<attribute name="SF_SKU" value="COM-00097"/>
</element>
<element name="U1" library="NeoPixel attiny 85" package="ATTINY85_DIP254P762X533-8" value="ATTINY85_ATTINY85-20PU">
<attribute name="MPN" value="ATTINY85-20PU"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="1455162"/>
<attribute name="OC_NEWARK" value="68T3808"/>
<attribute name="PACKAGE" value="PDIP-8"/>
<attribute name="SUPPLIER" value="Atmel"/>
</element>
<element name="U2" library="MAX1551EZK_T" package="SOT95P275X110-5N" value="MAX1551EZK+T">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" Charger IC Lithium-Ion TSOT-23-5 "/>
<attribute name="MF" value="Maxim Integrated"/>
<attribute name="MP" value="MAX1551EZK+"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="SOT-23-5 Maxim"/>
<attribute name="PRICE" value="None"/>
</element>
<element name="X1" library="zx62d-b-5pa8" package="ZX62D-B-5PA8" value="ZX62D-B-5PA8">
<attribute name="MF" value="Hirose"/>
<attribute name="MPN" value="ZX62D-B-5PA8"/>
<attribute name="NAME"/>
<attribute name="OC_FARNELL" value="2300438"/>
<attribute name="OC_NEWARK" value="69W0712"/>
</element>
<element name="BT1" library="SparkFun-Batteries 20mm" package="BATTCON_20MM_4LEGS" value="">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="BATT-10373"/>
<attribute name="SF_SKU" value="PRT-11892"/>
<attribute name="VALUE"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0603" value="100">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="RES-07863"/>
<attribute name="VALUE"/>
</element>
<element name="D1" library="Small led LTST-S270KRKT" package="0603" value="LTST-S270KRKT">
<attribute name="DESCRIPTION" value=" Red 631nm LED Indication - Discrete 2V 0603 (1608 Metric) "/>
<attribute name="DIGI-KEY_PART_NUMBER" value="160-1479-1-ND"/>
<attribute name="MF" value="Lite-On Inc."/>
<attribute name="MP" value="LTST-S270KRKT"/>
<attribute name="NAME"/>
<attribute name="PACKAGE" value="0603 Lite-On Inc."/>
<attribute name="VALUE"/>
</element>
<element name="SW1" library="CUS-12B" package="CUS-12B" value="CUS-12B">
<attribute name="AVAILABILITY" value="Unavailable"/>
<attribute name="DESCRIPTION" value=" Switch, Slide, Smd "/>
<attribute name="MF" value="Copal"/>
<attribute name="MP" value="CUS-12B"/>
<attribute name="PACKAGE" value="None"/>
<attribute name="PRICE" value="None"/>
</element>
<element name="U$1" library="NeoPixel strip connector" package="NEOSTRIPCONNECTORSMD" value=""/>
<element name="TP1" library="SparkFun-Connectors" package="PAD.03X.03" value="TEST-POINT3"/>
<element name="TP2" library="SparkFun-Connectors" package="PAD.03X.03" value="TEST-POINT3"/>
<element name="TP3" library="SparkFun-Connectors" package="PAD.03X.03" value="TEST-POINT3"/>
<element name="C1" library="SparkFun-Capacitors" package="0603" value="0.1uF">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="CAP-08604"/>
<attribute name="VALUE"/>
</element>
</elements>
<signals>
<signal name="BAT+">
<contactref element="U2" pad="5"/>
<contactref element="BT1" pad="POSITIVE@4"/>
<contactref element="BT1" pad="POSITIVE@2"/>
<contactref element="BT1" pad="POSITIVE@1"/>
<contactref element="BT1" pad="POSITIVE@3"/>
<contactref element="SW1" pad="P$2"/>
</signal>
<signal name="GND">
<contactref element="U1" pad="4"/>
<contactref element="X1" pad="5"/>
<contactref element="X1" pad="4"/>
<contactref element="U2" pad="2"/>
<contactref element="S1" pad="1"/>
<contactref element="BT1" pad="GND"/>
<contactref element="U$1" pad="GND0"/>
<contactref element="U$1" pad="GND1"/>
<contactref element="TP3" pad="P$1"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="NEOPIXELDATA">
<contactref element="U1" pad="5"/>
<contactref element="U$1" pad="DATA"/>
<contactref element="TP2" pad="P$1"/>
</signal>
<signal name="PUSHBUTTON">
<contactref element="U1" pad="6"/>
<contactref element="S1" pad="3"/>
</signal>
<signal name="VCC">
<contactref element="X1" pad="1"/>
<contactref element="U2" pad="1"/>
<contactref element="D1" pad="2"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="ON">
<contactref element="U1" pad="8"/>
<contactref element="U$1" pad="VCC"/>
<contactref element="SW1" pad="P$1"/>
<contactref element="TP1" pad="P$1"/>
</signal>
<signal name="N$1">
<contactref element="D1" pad="1"/>
<contactref element="R1" pad="2"/>
</signal>
<signal name="POK">
<contactref element="U2" pad="3"/>
<contactref element="R1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
