<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.1">
<drawing>
<library>
<description>Generated from &lt;b&gt;GemaLight neo strip1.2.sch&lt;/b&gt;&lt;p&gt;
by exp-lbrs.ulp</description>
<packages>
<package name="NANO-NEOPIXEL-MANUAL-SOLDER_NEOPIXEL-NANO-2427_SK6805-2427">
<description>&lt;b&gt;Adafruit NeoPixel Nano 2427&lt;/b&gt;

&lt;br&gt;

This is the EAGLE footprint of the NeoPixel Nano 2427 by Adafruit (2.4x2.7mm).

&lt;br&gt;&lt;br&gt;

MPN: SK6805-2427
&lt;br&gt;
https://www.adafruit.com/product/3484
&lt;br&gt;&lt;br&gt;
Designed by AKstudios
&lt;br&gt;
github.com/akstudios</description>
</package>
<package name="NEOPIXEL-STRIP-CONNECTOR_NEOSTRIPCONNECTORHOLES">
</package>
<package name="NEOPIXEL-STRIP-CONNECTOR_NEOSTRIPCONNECTORSMD">
</package>
</packages>
<symbols>
<symbol name="NANO-NEOPIXEL-MANUAL-SOLDER_NEOPIXEL-NANO-2427_NEOPIXEL_NANO_2427">
<pin name="DIN"/>
<pin name="DOUT"/>
<pin name="VDD"/>
<pin name="VSS"/>
</symbol>
<symbol name="NEOPIXEL-STRIP-CONNECTOR_NEOSTRIPCONNECTOR">
<pin name="DATA"/>
<pin name="GND0"/>
<pin name="GND1"/>
<pin name="VCC"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="NANO-NEOPIXEL-MANUAL-SOLDER_NEOPIXEL-NANO-2427_NEOPIXEL_NANO_2427">
<gates>
<gate name="G$1" symbol="NANO-NEOPIXEL-MANUAL-SOLDER_NEOPIXEL-NANO-2427_NEOPIXEL_NANO_2427"/>
</gates>
<devices>
<device name="" package="NANO-NEOPIXEL-MANUAL-SOLDER_NEOPIXEL-NANO-2427_SK6805-2427">
<connects>
<connect gate="G$1" pin="DIN" pad="DIN"/>
<connect gate="G$1" pin="DOUT" pad="DOUT"/>
<connect gate="G$1" pin="VDD" pad="VCC"/>
<connect gate="G$1" pin="VSS" pad="GND"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="NEOPIXEL-STRIP-CONNECTOR_NEOSTRIPCONNECTOR" uservalue="yes">
<description>Neo pixel solder connector for strip</description>
<gates>
<gate name="G$1" symbol="NEOPIXEL-STRIP-CONNECTOR_NEOSTRIPCONNECTOR"/>
</gates>
<devices>
<device name="" package="NEOPIXEL-STRIP-CONNECTOR_NEOSTRIPCONNECTORHOLES">
<connects>
<connect gate="G$1" pin="DATA" pad="DATA"/>
<connect gate="G$1" pin="GND0" pad="GND0"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
<device name="NEOSTRIPCONNECTORSMD" package="NEOPIXEL-STRIP-CONNECTOR_NEOSTRIPCONNECTORSMD">
<connects>
<connect gate="G$1" pin="DATA" pad="DATA"/>
<connect gate="G$1" pin="GND0" pad="GND0"/>
<connect gate="G$1" pin="GND1" pad="GND1"/>
<connect gate="G$1" pin="VCC" pad="VCC"/>
</connects>
<technologies>
<technology name=""/>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
