<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<wire x1="6.6675" y1="4.445" x2="7.9375" y2="3.175" width="0" layer="20"/>
<wire x1="7.9375" y1="3.175" x2="96.2025" y2="3.175" width="0" layer="20"/>
<wire x1="96.2025" y1="3.175" x2="97.4725" y2="4.445" width="0" layer="20"/>
<text>Q</text>
<text>W</text>
<text>E</text>
<text>R</text>
<text>T</text>
<text>Y</text>
<text>U</text>
<text>I</text>
<text>O</text>
<text>P</text>
<text>A</text>
<text>S</text>
<text>D</text>
<text>F</text>
<text>G</text>
<text>H</text>
<text>J</text>
<text>K</text>
<text>L</text>
<text>DEL</text>
<text>Z</text>
<text>X</text>
<text>C</text>
<text>V</text>
<text>B</text>
<text>N</text>
<text>M</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>4</text>
<text>5</text>
<text>6</text>
<text>7</text>
<text>8</text>
<text>9</text>
<text>0</text>
<text>ALT</text>
<text>SPC</text>
<text>ENT</text>
<text>.,</text>
<text>!</text>
<text>@</text>
<text>#</text>
<text>$</text>
<text>%</text>
<text>+</text>
<text>&amp;</text>
<text>*</text>
<text>(</text>
<text>)</text>
<text>-</text>
<text>:</text>
<text>;</text>
<text>"'</text>
<text>/</text>
<text>?</text>
<text>4K7</text>
<text>4017</text>
<wire x1="63.1825" y1="79.6925" x2="68.2625" y2="79.6925" width="0" layer="20"/>
<wire x1="68.2625" y1="79.6925" x2="68.8975" y2="79.0575" width="0" layer="20"/>
<wire x1="68.8975" y1="79.0575" x2="68.8975" y2="56.515" width="0" layer="20"/>
<wire x1="68.8975" y1="52.705" x2="68.8975" y2="44.45" width="0" layer="20"/>
<wire x1="68.8975" y1="44.45" x2="68.2625" y2="43.815" width="0" layer="20"/>
<wire x1="68.2625" y1="43.815" x2="63.8175" y2="43.815" width="0" layer="20"/>
<wire x1="63.8175" y1="43.815" x2="62.5475" y2="45.085" width="0" layer="20"/>
<wire x1="62.5475" y1="45.085" x2="62.5475" y2="51.435" width="0" layer="20"/>
<wire x1="62.5475" y1="51.435" x2="59.3725" y2="54.61" width="0" layer="20"/>
<wire x1="59.3725" y1="54.61" x2="59.3725" y2="71.12" width="0" layer="20"/>
<wire x1="59.3725" y1="71.12" x2="62.5475" y2="74.295" width="0" layer="20"/>
<wire x1="62.5475" y1="74.295" x2="62.5475" y2="79.0575" width="0" layer="20"/>
<wire x1="62.5475" y1="79.0575" x2="63.1825" y2="79.6925" width="0" layer="20"/>
<wire x1="68.8975" y1="56.515" x2="70.1675" y2="56.515" width="0" layer="20"/>
<wire x1="70.1675" y1="56.515" x2="70.8025" y2="55.88" width="0" layer="20"/>
<wire x1="70.8025" y1="55.88" x2="70.8025" y2="53.34" width="0" layer="20"/>
<wire x1="70.8025" y1="53.34" x2="70.1675" y2="52.705" width="0" layer="20"/>
<wire x1="70.1675" y1="52.705" x2="68.8975" y2="52.705" width="0" layer="20"/>
<wire x1="72.0725" y1="38.1" x2="72.0725" y2="46.99" width="0" layer="20"/>
<wire x1="72.0725" y1="46.99" x2="82.2325" y2="46.99" width="0" layer="20"/>
<wire x1="82.2325" y1="46.99" x2="82.2325" y2="38.1" width="0" layer="20"/>
<wire x1="56.8325" y1="81.28" x2="58.1025" y2="82.55" width="0" layer="20"/>
<wire x1="58.1025" y1="82.55" x2="96.2025" y2="82.55" width="0" layer="20"/>
<wire x1="96.2025" y1="82.55" x2="97.4725" y2="81.28" width="0" layer="20"/>
<wire x1="55.5625" y1="76.835" x2="56.8325" y2="78.105" width="0" layer="20"/>
<wire x1="56.8325" y1="78.105" x2="56.8325" y2="81.28" width="0" layer="20"/>
<wire x1="7.9375" y1="76.835" x2="55.5625" y2="76.835" width="0" layer="20"/>
<wire x1="72.0725" y1="38.1" x2="82.2325" y2="38.1" width="0" layer="20"/>
<wire x1="6.6675" y1="4.445" x2="6.6675" y2="75.565" width="0" layer="20"/>
<wire x1="6.6675" y1="75.565" x2="7.9375" y2="76.835" width="0" layer="20"/>
<wire x1="97.4725" y1="4.445" x2="97.4725" y2="81.28" width="0" layer="20"/>
</plain>
<libraries>
<library name="microbuilder">
<packages>
<package name="MOUNTINGHOLE_2.0_PLATED">
</package>
<package name="0603-NO">
</package>
<package name="0805-NO">
</package>
<package name="_0805">
<description>&lt;b&gt;0805&lt;/b&gt;</description>
</package>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt; - 5 Pin</description>
</package>
<package name="CHIPLED_0805_NOOUTLINE">
</package>
</packages>
</library>
<library name="SparkFun-Electromechanical">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find anything that moves- switches, relays, buttons, potentiometers. Also, anything that goes on a board but isn't electrical in nature- screws, standoffs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="TACTILE-PTH">
<description>&lt;b&gt;OMRON SWITCH&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="40xx">
<description>&lt;b&gt;CMOS Logic Devices, 4000 Series&lt;/b&gt;&lt;p&gt;
Based on the following sources:
&lt;ul&gt;
&lt;li&gt;Motorola &lt;i&gt;CMOS LOGIC DATA&lt;/i&gt;; book, 02/88, DL131 REV 1
&lt;li&gt;http://www.elexp.com
&lt;li&gt;http://www.intersil.com
&lt;li&gt;http://www.ls3c.com.tw/product/1/COMOS.html
&lt;/ul&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO16">
<description>&lt;b&gt;Small Outline package&lt;/b&gt; 150 mil</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X06_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X06_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole - 6 Pin with Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_06&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="1X02_NO_SILK">
<description>&lt;h3&gt;Plated Through Hole - No Silk Outline&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:2&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_02&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
<package name="2X3">
<description>&lt;h3&gt;Plated Through Hole - 2x3&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:6&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_03x2&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="Other">
<packages>
<package name="MICRO_B">
</package>
</packages>
</library>
<library name="v-reg">
<packages>
<package name="SOT223">
<description>&lt;b&gt;Small Outline Transistor 223&lt;/b&gt;&lt;p&gt;
PLASTIC PACKAGE CASE 318E-04&lt;br&gt;
Source: http://www.onsemi.co.jp .. LM137M-D.PDF</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$4" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$13" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="S2" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S3" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S4" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S5" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S6" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S7" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S8" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S9" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S10" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S11" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S12" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S13" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S14" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S15" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S16" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S17" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S18" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S19" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S21" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S22" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S23" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S24" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S26" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S27" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S28" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S29" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S31" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S32" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S33" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="S34" library="SparkFun-Electromechanical" package="TACTILE-PTH" value="">
<attribute name="PROD_ID" value=" SWCH-08441"/>
</element>
<element name="IC4" library="40xx" package="SO16" value="4017D"/>
<element name="R11" library="microbuilder" package="0603-NO" value="4k7"/>
<element name="R12" library="microbuilder" package="0603-NO" value="4k7"/>
<element name="R13" library="microbuilder" package="0603-NO" value="4k7"/>
<element name="U$1" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$2" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="J3" library="SparkFun-Connectors" package="1X06_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J5" library="SparkFun-Connectors" package="1X06_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
<element name="U$7" library="Other" package="MICRO_B" value="MICROUSB"/>
<element name="C5" library="microbuilder" package="0805-NO" value="10µF"/>
<element name="C7" library="microbuilder" package="_0805" value="1uF"/>
<element name="C9" library="microbuilder" package="_0805" value="10µF"/>
<element name="U3" library="microbuilder" package="SOT23-5" value="MCP73831T-2ACI/OT"/>
<element name="CHG" library="microbuilder" package="CHIPLED_0805_NOOUTLINE" value="ORANGE"/>
<element name="R5" library="microbuilder" package="0603-NO" value="1K"/>
<element name="C13" library="microbuilder" package="0805-NO" value="10µF"/>
<element name="R6" library="microbuilder" package="0603-NO" value="10K\"/>
<element name="J8" library="SparkFun-Connectors" package="1X02_NO_SILK" value="">
<attribute name="VALUE"/>
</element>
<element name="J9" library="SparkFun-Connectors" package="2X3" value="FEMALE 2x3">
<attribute name="PROD_ID" value="CONN-11566"/>
</element>
<element name="IC3" library="v-reg" package="SOT223" value="LD117AS12TR"/>
</elements>
<signals>
<signal name="GND">
<contactref element="IC4" pad="13"/>
<contactref element="IC4" pad="8"/>
<contactref element="R13" pad="2"/>
<contactref element="R12" pad="2"/>
<contactref element="R11" pad="2"/>
<contactref element="J3" pad="3"/>
<contactref element="J5" pad="6"/>
<contactref element="U$7" pad="GND1"/>
<contactref element="U$7" pad="GND3"/>
<contactref element="U$7" pad="GND2"/>
<contactref element="U$7" pad="GND4"/>
<contactref element="U$7" pad="GND7"/>
<contactref element="U$7" pad="GND8"/>
<contactref element="U$7" pad="P5"/>
<contactref element="C5" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="U3" pad="2"/>
<contactref element="C13" pad="2"/>
<contactref element="IC3" pad="1"/>
<contactref element="C9" pad="2"/>
<contactref element="C7" pad="2"/>
<contactref element="J8" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="IC4" pad="16"/>
<contactref element="J3" pad="2"/>
</signal>
<signal name="N$4">
</signal>
<signal name="RES">
<contactref element="IC4" pad="15"/>
<contactref element="J5" pad="4"/>
</signal>
<signal name="CLK">
<contactref element="IC4" pad="14"/>
<contactref element="J5" pad="5"/>
</signal>
<signal name="R2">
<contactref element="S23" pad="3"/>
<contactref element="S24" pad="3"/>
<contactref element="S26" pad="3"/>
<contactref element="S27" pad="3"/>
<contactref element="S28" pad="3"/>
<contactref element="S11" pad="3"/>
<contactref element="S10" pad="3"/>
<contactref element="S9" pad="3"/>
<contactref element="S8" pad="3"/>
<contactref element="S7" pad="3"/>
<contactref element="R12" pad="1"/>
<contactref element="J5" pad="2"/>
</signal>
<signal name="R3">
<contactref element="S29" pad="3"/>
<contactref element="S31" pad="3"/>
<contactref element="S32" pad="3"/>
<contactref element="S33" pad="3"/>
<contactref element="S34" pad="3"/>
<contactref element="S16" pad="3"/>
<contactref element="S15" pad="3"/>
<contactref element="S14" pad="3"/>
<contactref element="S13" pad="3"/>
<contactref element="S12" pad="3"/>
<contactref element="R13" pad="1"/>
<contactref element="J5" pad="3"/>
</signal>
<signal name="R1">
<contactref element="S17" pad="3"/>
<contactref element="S18" pad="3"/>
<contactref element="S19" pad="3"/>
<contactref element="S21" pad="3"/>
<contactref element="S22" pad="3"/>
<contactref element="S6" pad="3"/>
<contactref element="S5" pad="3"/>
<contactref element="S4" pad="3"/>
<contactref element="S3" pad="3"/>
<contactref element="S2" pad="3"/>
<contactref element="R11" pad="1"/>
<contactref element="J5" pad="1"/>
</signal>
<signal name="K3">
<contactref element="IC4" pad="3"/>
<contactref element="S14" pad="1"/>
<contactref element="S4" pad="1"/>
<contactref element="S9" pad="1"/>
</signal>
<signal name="K2">
<contactref element="IC4" pad="2"/>
<contactref element="S13" pad="1"/>
<contactref element="S3" pad="1"/>
<contactref element="S8" pad="1"/>
</signal>
<signal name="K4">
<contactref element="IC4" pad="4"/>
<contactref element="S15" pad="1"/>
<contactref element="S5" pad="1"/>
<contactref element="S10" pad="1"/>
</signal>
<signal name="K7">
<contactref element="IC4" pad="7"/>
<contactref element="S18" pad="1"/>
<contactref element="S24" pad="1"/>
<contactref element="S31" pad="1"/>
</signal>
<signal name="K9">
<contactref element="IC4" pad="10"/>
<contactref element="S21" pad="1"/>
<contactref element="S27" pad="1"/>
<contactref element="S33" pad="1"/>
</signal>
<signal name="K1">
<contactref element="IC4" pad="1"/>
<contactref element="S12" pad="1"/>
<contactref element="S2" pad="1"/>
<contactref element="S7" pad="1"/>
</signal>
<signal name="K5">
<contactref element="IC4" pad="5"/>
<contactref element="S16" pad="1"/>
<contactref element="S11" pad="1"/>
<contactref element="S6" pad="1"/>
</signal>
<signal name="K6">
<contactref element="IC4" pad="6"/>
<contactref element="S17" pad="1"/>
<contactref element="S23" pad="1"/>
<contactref element="S29" pad="1"/>
</signal>
<signal name="K8">
<contactref element="IC4" pad="9"/>
<contactref element="S19" pad="1"/>
<contactref element="S26" pad="1"/>
<contactref element="S32" pad="1"/>
</signal>
<signal name="K10">
<contactref element="IC4" pad="11"/>
<contactref element="S22" pad="1"/>
<contactref element="S28" pad="1"/>
<contactref element="S34" pad="1"/>
</signal>
<signal name="N$3">
</signal>
<signal name="DP">
<contactref element="J3" pad="6"/>
<contactref element="U$7" pad="P3"/>
</signal>
<signal name="DM">
<contactref element="J3" pad="5"/>
<contactref element="U$7" pad="P2"/>
</signal>
<signal name="VIN">
<contactref element="J3" pad="4"/>
<contactref element="U$7" pad="P1"/>
<contactref element="J9" pad="2"/>
<contactref element="J9" pad="1"/>
<contactref element="U3" pad="4"/>
<contactref element="CHG" pad="A"/>
</signal>
<signal name="RESR">
<contactref element="J3" pad="1"/>
</signal>
<signal name="VBAT">
<contactref element="U3" pad="3"/>
<contactref element="C13" pad="1"/>
<contactref element="J9" pad="6"/>
<contactref element="J9" pad="5"/>
<contactref element="J8" pad="2"/>
</signal>
<signal name="VCC2">
<contactref element="C7" pad="1"/>
<contactref element="C9" pad="1"/>
<contactref element="IC3" pad="4"/>
</signal>
<signal name="N$20">
<contactref element="CHG" pad="C"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$21">
<contactref element="R5" pad="2"/>
<contactref element="U3" pad="1"/>
</signal>
<signal name="N$22">
<contactref element="U3" pad="5"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$23">
<contactref element="J9" pad="4"/>
<contactref element="J9" pad="3"/>
<contactref element="C5" pad="1"/>
<contactref element="IC3" pad="3"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
