<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="7.6.0">
<drawing>
<board>
<plain>
<text>BOBRICIUS www.pemi.technology</text>
<text>CS1</text>
<text>CS2</text>
<text>DC</text>
<text>RST</text>
<text>DAT</text>
<text>GND</text>
<text>VCC</text>
<text>SCK</text>
<text>Display</text>
<text>ST7789
HD IPS
Display
240x240</text>
<wire x1="102.489" y1="70.358" x2="188.214" y2="70.358" width="0" layer="20"/>
<wire x1="100.584" y1="72.263" x2="102.489" y2="70.358" width="0" layer="20" curve="90"/>
<wire x1="100.584" y1="72.263" x2="100.584" y2="104.267" width="0" layer="20"/>
<wire x1="100.584" y1="104.267" x2="102.489" y2="106.172" width="0" layer="20" curve="-90"/>
<wire x1="102.489" y1="106.172" x2="188.214" y2="106.172" width="0" layer="20"/>
<wire x1="188.214" y1="106.172" x2="190.119" y2="104.267" width="0" layer="20" curve="-90"/>
<wire x1="190.119" y1="104.267" x2="190.119" y2="72.263" width="0" layer="20"/>
<wire x1="190.119" y1="72.263" x2="188.214" y2="70.358" width="0" layer="20" curve="-90"/>
<wire x1="131.7625" y1="74.93" x2="131.7625" y2="72.0725" width="0" layer="20" curve="-167.319617"/>
<wire x1="131.7625" y1="72.0725" x2="108.9025" y2="72.0725" width="0" layer="20"/>
<wire x1="108.9025" y1="72.0725" x2="108.9025" y2="74.93" width="0" layer="20" curve="-167.319617"/>
<wire x1="108.9025" y1="74.93" x2="131.7625" y2="74.93" width="0" layer="20"/>
<wire x1="181.9275" y1="74.93" x2="181.9275" y2="72.0725" width="0" layer="20" curve="-167.319617"/>
<wire x1="181.9275" y1="72.0725" x2="159.0675" y2="72.0725" width="0" layer="20"/>
<wire x1="159.0675" y1="72.0725" x2="159.0675" y2="74.93" width="0" layer="20" curve="-167.319617"/>
<wire x1="159.0675" y1="74.93" x2="181.9275" y2="74.93" width="0" layer="20"/>
<text>ST7789
HD IPS
Display
240x240</text>
<text>AR/VR SPI IPS GOGGLES</text>
<text>10R</text>
<text>10R</text>
<text>100n</text>
<text>100n</text>
</plain>
<libraries>
<library name="microbuilder">
<packages>
<package name="MOUNTINGHOLE_2.0_PLATED">
</package>
<package name="_0805MP">
<description>&lt;b&gt;0805 MicroPitch&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; Creative Commons ShareAlike 4.0 International - https://creativecommons.org/licenses/by-sa/4.0/ 
&lt;br&gt;&lt;br&gt;
You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X08_LONGPADS">
<description>&lt;h3&gt;Plated Through Hole -8 Pin Long Pads&lt;/h3&gt;
&lt;p&gt;Specifications:
&lt;ul&gt;&lt;li&gt;Pin count:8&lt;/li&gt;
&lt;li&gt;Pin pitch:0.1"&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;Example device(s):
&lt;ul&gt;&lt;li&gt;CONN_08&lt;/li&gt;
&lt;/ul&gt;&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="ips096">
<packages>
<package name="TFT_0.96IN_160X80">
</package>
</packages>
</library>
<library name="SparkFun">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
We've spent an enormous amount of time creating and checking these footprints and parts. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SJ_2S-NOTRACE">
</package>
</packages>
</library>
<library name="rc-master-smd">
<packages>
<package name="C0805">
<description>&lt;b&gt;SMD CHIP CAP&lt;/b&gt; - 0805</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$3" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$10" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$4" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$2" library="microbuilder" package="MOUNTINGHOLE_2.0_PLATED" value="MOUNTINGHOLE2.0">
<attribute name="BOM" value="EXCLUDE"/>
</element>
<element name="U$39" library="ips096" package="TFT_0.96IN_160X80" value="DISP_LCD_0.9IN_160X80"/>
<element name="U$1" library="ips096" package="TFT_0.96IN_160X80" value="DISP_LCD_0.9IN_160X80"/>
<element name="J4" library="SparkFun-Connectors" package="1X08_LONGPADS" value="">
<attribute name="VALUE"/>
</element>
<element name="JUMPER1" library="SparkFun" package="SJ_2S-NOTRACE" value="SOLDERJUMPERNC2"/>
<element name="R4" library="microbuilder" package="_0805MP" value="10"/>
<element name="R1" library="microbuilder" package="_0805MP" value="10"/>
<element name="C3" library="rc-master-smd" package="C0805" value="100n"/>
<element name="C1" library="rc-master-smd" package="C0805" value="100n"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U$39" pad="6"/>
<contactref element="U$39" pad="5"/>
<contactref element="U$39" pad="1"/>
<contactref element="U$39" pad="12"/>
<contactref element="U$1" pad="6"/>
<contactref element="U$1" pad="5"/>
<contactref element="U$1" pad="1"/>
<contactref element="U$1" pad="12"/>
<contactref element="J4" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="R1" pad="2"/>
<contactref element="C3" pad="1"/>
<contactref element="C1" pad="1"/>
</signal>
<signal name="N$4">
</signal>
<signal name="N$164">
</signal>
<signal name="VCC1">
</signal>
<signal name="VCC">
<contactref element="U$39" pad="4"/>
<contactref element="U$39" pad="3"/>
<contactref element="U$1" pad="4"/>
<contactref element="U$1" pad="3"/>
<contactref element="J4" pad="2"/>
<contactref element="C3" pad="2"/>
<contactref element="C1" pad="2"/>
</signal>
<signal name="PA27">
<contactref element="U$39" pad="11"/>
<contactref element="U$1" pad="11"/>
<contactref element="J4" pad="5"/>
</signal>
<signal name="SCK1">
<contactref element="U$39" pad="9"/>
<contactref element="U$1" pad="9"/>
<contactref element="J4" pad="3"/>
</signal>
<signal name="MOSI1">
<contactref element="U$39" pad="10"/>
<contactref element="U$1" pad="10"/>
<contactref element="J4" pad="4"/>
</signal>
<signal name="SWC">
<contactref element="U$39" pad="7"/>
<contactref element="U$1" pad="7"/>
<contactref element="J4" pad="6"/>
</signal>
<signal name="PA0">
<contactref element="U$1" pad="8"/>
<contactref element="J4" pad="7"/>
<contactref element="JUMPER1" pad="2"/>
</signal>
<signal name="PA1">
<contactref element="U$39" pad="8"/>
<contactref element="JUMPER1" pad="1"/>
<contactref element="J4" pad="8"/>
</signal>
<signal name="N$1">
</signal>
<signal name="N$2">
<contactref element="U$39" pad="2"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="2"/>
<contactref element="R1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
