<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="8.255" y2="0" width="0" layer="20"/>
<wire x1="12.065" y1="5.08" x2="12.065" y2="7.62" width="0" layer="20"/>
<wire x1="12.065" y1="7.62" x2="8.255" y2="7.61" width="0" layer="20"/>
<wire x1="8.255" y1="7.61" x2="8.255" y2="12.7" width="0" layer="20"/>
<wire x1="8.255" y1="12.7" x2="0" y2="12.69" width="0" layer="20"/>
<wire x1="0" y1="12.69" x2="0" y2="0" width="0" layer="20"/>
<wire x1="8.255" y1="0" x2="8.255" y2="5.08" width="0" layer="20"/>
<wire x1="8.255" y1="5.08" x2="12.065" y2="5.08" width="0" layer="20"/>
<text>B to Micro</text>
<text>JLCJLCJLCJLC</text>
<text>063021</text>
</plain>
<libraries>
<library name="sjm4306-custom">
<packages>
<package name="MICRO_USB_4PTH">
</package>
</packages>
</library>
<library name="con-cypressindustries">
<description>&lt;b&gt;Connectors from Cypress Industries&lt;/b&gt;&lt;p&gt;
www.cypressindustries.com&lt;br&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="85-32004-10X">
<description>&lt;b&gt;USB B TYPE SINGLE R/A DIP&lt;/b&gt; With Rear Shell, Without Rear Shell&lt;p&gt;
Source: http://www.cypressindustries.com/pdf/85-32004-10x.pdf</description>
</package>
</packages>
</library>
<library name="sjm4306_LOGO">
<packages>
<package name="SJM4306_LOGO_SMALL">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U$1" library="sjm4306-custom" package="MICRO_USB_4PTH" value="MICRO_USB_4PTH"/>
<element name="X1" library="con-cypressindustries" package="85-32004-10X" value="MINI-USB_4P-85-32004-10X">
<attribute name="MF" value=""/>
<attribute name="MPN" value=""/>
<attribute name="OC_FARNELL" value="unknown"/>
<attribute name="OC_NEWARK" value="unknown"/>
<attribute name="POPULARITY" value="0"/>
</element>
<element name="U$2" library="sjm4306_LOGO" package="SJM4306_LOGO_SMALL" value=""/>
</elements>
<signals>
<signal name="N$2">
<contactref element="X1" pad="1"/>
<contactref element="U$1" pad="P$1"/>
</signal>
<signal name="N$3">
<contactref element="U$1" pad="P$2"/>
<contactref element="X1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="X1" pad="3"/>
<contactref element="U$1" pad="P$3"/>
</signal>
<signal name="GND">
<contactref element="X1" pad="4"/>
<contactref element="U$1" pad="P$5"/>
<contactref element="U$1" pad="P$6"/>
<contactref element="U$1" pad="P$7"/>
<contactref element="U$1" pad="P$9"/>
<contactref element="U$1" pad="P$8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
