<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="2.54" x2="35.54" y2="2.54" width="0" layer="20"/>
<wire x1="35.54" y1="2.54" x2="35.56" y2="40.005" width="0" layer="20"/>
<wire x1="35.56" y1="40.005" x2="0" y2="40.005" width="0" layer="20"/>
<wire x1="0" y1="40.005" x2="0" y2="2.54" width="0" layer="20"/>
<text>PILOT</text>
<text>GND</text>
<text>+12V</text>
<text>DUTY</text>
<text>PROG</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
<package name="1210">
</package>
</packages>
</library>
<library name="SparkFun-DiscreteSemi">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find discrete semiconductors- transistors, diodes, TRIACs, optoisolators, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SMA-DIODE">
<description>&lt;B&gt;Diode&lt;/B&gt;&lt;p&gt;
Basic SMA packaged diode. Good for reverse polarization protection. Common part #: MBRA140</description>
</package>
</packages>
</library>
<library name="TC1044S">
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package&lt;/b&gt; Fits JEDEC packages (narrow SOIC-8)</description>
</package>
</packages>
</library>
<library name="SparkFun-Connectors-new">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find connectors and sockets- basically anything that can be plugged into or onto.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="1X03">
</package>
<package name="SCREWTERMINAL-3.5MM-2">
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="DCJACK_2MM_SMT">
<description>2.0/2.1mm DC Jack - SMT
&lt;p&gt;4UConnector: 03267&lt;/p&gt;
&lt;p&gt;Note: Small tRestrict polygon's were added to the ground pads to improve solderability when this part is used in combination with a ground pour.  By default, Eagle will product four large bridges to the ground pour significantly increasing the heat distribution on the pads and preventing lead-free solder from reflowing in certain situations.  For more details, see: http://www.microbuilder.eu/Blog/09-12-14/Reducing_Thermals_for_Large_Pads_in_Eagle.aspx&lt;/p&gt;</description>
</package>
</packages>
</library>
<library name="dcx(xxxx)u">
<packages>
<package name="SOT23-6">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="SparkFun-PowerIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find drivers, regulators, and amplifiers.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SOT23-5">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="avr-7">
<description>&lt;b&gt;AVR Devices&lt;/b&gt;&lt;p&gt;
Version 7 - August 1, 2011.&lt;br&gt;&lt;br&gt;
Added ATmega164P/324P/644P devices for DIP and TQFP.
&lt;p&gt;
Version 4 - March 11, 2008.&lt;br&gt;&lt;br&gt;
This library now includes ONLY ATMEL AVR microcontrollers.  It is the result of merging all other available device libraries available at http://www.cadsoft.de/download as of the time it was made.  In addition to the legacy AT90* devices, it includes most ATMEGA devices including the new 48/88/168, most ATTiny devices and a set of ISP and JTAG pin headers.&lt;p&gt;
Based on the following sources:&lt;p&gt;
&lt;ul&gt;
&lt;li&gt;www.atmel.com
&lt;li&gt; file at90smcu_v400.zip
&lt;li&gt;avr.lbr and atmel.lbr as provided by CadSoft
&lt;li&gt;avr-1.lbr by David Blundell
&lt;li&gt;avr-2.lbr by Boris Zalokar
&lt;li&gt;avr-3.lbr by Carson Reynolds
&lt;li&gt;attiny24_44_84.lbr by Pawel Szramowski (ATTiny24/44/84 devices)
&lt;li&gt;atmel.lbr by Bob Starr (ISP headers)
&lt;li&gt;moates_custom_parts.lbr (edge ISP)
&lt;li&gt;other misc sources
&lt;/ul&gt;
&lt;author&gt;Revised by David Blundell (blundar at gmail dot com) and others.&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added Mega162, Tiny2313 John Lussmyer (cougar at casadelgato.com)&lt;/author&gt;
&lt;p&gt;
&lt;author&gt;Added XMega A1,A3,A4,D3,D4 John Lussmyer Aug 1, 2011(cougar at casadelgato.com)&lt;/author&gt;</description>
<packages>
<package name="AVR-ISP-6">
<description>&lt;b&gt;PIN HEADER&lt;/b&gt;&lt;p&gt; JTAG 6 Pin, 0.1" Straight</description>
</package>
<package name="SOT23/6">
<description>&lt;b&gt;Small Outline Transistor&lt;/b&gt;, 5 lead</description>
</package>
</packages>
</library>
<library name="IQD-Frequency-Products">
<description>&lt;b&gt;Crystals and Oscillators&lt;/b&gt;&lt;p&gt;
&lt;author&gt;Created by IQD Frequency Products&lt;/author&gt;</description>
<packages>
<package name="7.2X5.2-4-PAD">
<description>&lt;b&gt;IQD Frequency Products SMD Package&lt;/b&gt;</description>
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SJ_2S-NO">
<description>Small solder jumper with no paste layer so it will open after reflow.</description>
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="0.1µF">
<attribute name="NAME"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="1210" value="10µF">
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="1210" value="10µF">
<attribute name="NAME"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="1µF">
<attribute name="NAME"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="1µF">
<attribute name="NAME"/>
</element>
<element name="D1" library="SparkFun-DiscreteSemi" package="SMA-DIODE" value="P6KE16CA">
<attribute name="NAME"/>
<attribute name="PROD_ID" value="DIO-08053"/>
</element>
<element name="IC3" library="TC1044S" package="SO08" value="TC1044S_OA">
<attribute name="NAME"/>
</element>
<element name="R2" library="SparkFun-Connectors-new" package="1X03" value="20kΩ Pot.">
<attribute name="NAME"/>
</element>
<element name="JP1" library="adafruit" package="DCJACK_2MM_SMT" value="2.1MMJACKSMT"/>
<element name="JP3" library="SparkFun-Connectors-new" package="SCREWTERMINAL-3.5MM-2" value="PILOT">
<attribute name="NAME"/>
</element>
<element name="Q1" library="dcx(xxxx)u" package="SOT23-6" value="DMG6602SVTQ">
<attribute name="NAME"/>
</element>
<element name="Q2" library="dcx(xxxx)u" package="SOT23-6" value="DMG6602SVTQ">
<attribute name="NAME"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="10kΩ">
<attribute name="NAME"/>
</element>
<element name="R7" library="SparkFun-Resistors" package="0805" value="4.7kΩ">
<attribute name="NAME"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0805" value="4.7kΩ">
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="1kΩ 1%">
<attribute name="NAME"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="10kΩ">
<attribute name="NAME"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0805" value="1kΩ">
<attribute name="NAME"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0805" value="1kΩ">
<attribute name="NAME"/>
</element>
<element name="IC2" library="SparkFun-PowerIC" package="SOT23-5" value="V_REG_LDOSMD">
<attribute name="NAME"/>
</element>
<element name="JP2" library="avr-7" package="AVR-ISP-6" value="AVR-TPIVERT">
<attribute name="NAME"/>
</element>
<element name="IC1" library="avr-7" package="SOT23/6" value="ATTiny10">
<attribute name="NAME"/>
</element>
<element name="X1" library="IQD-Frequency-Products" package="7.2X5.2-4-PAD" value="12 MHz">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="0"/>
</element>
<element name="SJ1" library="SparkFun-Passives" package="SJ_2S-NO" value="SOLDERJUMPERNO"/>
</elements>
<signals>
<signal name="GND">
<contactref element="D1" pad="A"/>
<contactref element="Q2" pad="5"/>
<contactref element="C1" pad="2"/>
<contactref element="R2" pad="3"/>
<contactref element="JP3" pad="2"/>
<contactref element="IC3" pad="3"/>
<contactref element="C3" pad="1"/>
<contactref element="IC2" pad="2"/>
<contactref element="C4" pad="2"/>
<contactref element="JP1" pad="GNDBREAK"/>
<contactref element="JP1" pad="GND"/>
<contactref element="C5" pad="2"/>
<contactref element="JP2" pad="6"/>
<contactref element="IC1" pad="2"/>
<contactref element="X1" pad="2"/>
<contactref element="SJ1" pad="2"/>
</signal>
<signal name="+5V">
<contactref element="R4" pad="2"/>
<contactref element="Q2" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="R1" pad="1"/>
<contactref element="R2" pad="1"/>
<contactref element="C4" pad="1"/>
<contactref element="IC2" pad="5"/>
<contactref element="JP2" pad="2"/>
<contactref element="IC1" pad="5"/>
<contactref element="X1" pad="4"/>
</signal>
<signal name="PILOT_B">
<contactref element="R3" pad="2"/>
<contactref element="D1" pad="C"/>
<contactref element="JP3" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="R8" pad="2"/>
<contactref element="Q2" pad="4"/>
</signal>
<signal name="N$5">
<contactref element="R7" pad="2"/>
<contactref element="Q2" pad="6"/>
</signal>
<signal name="N$10">
<contactref element="R3" pad="1"/>
<contactref element="Q1" pad="4"/>
<contactref element="Q1" pad="6"/>
</signal>
<signal name="-12V">
<contactref element="R6" pad="1"/>
<contactref element="Q1" pad="5"/>
<contactref element="IC3" pad="5"/>
<contactref element="C3" pad="2"/>
</signal>
<signal name="+12V">
<contactref element="R5" pad="2"/>
<contactref element="Q1" pad="2"/>
<contactref element="IC3" pad="8"/>
<contactref element="IC3" pad="1"/>
<contactref element="JP1" pad="PWR1"/>
<contactref element="JP1" pad="PWR2"/>
<contactref element="IC2" pad="1"/>
<contactref element="C5" pad="1"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="N$1">
<contactref element="R5" pad="1"/>
<contactref element="R7" pad="1"/>
<contactref element="Q1" pad="3"/>
</signal>
<signal name="N$15">
<contactref element="R6" pad="2"/>
<contactref element="R8" pad="1"/>
<contactref element="Q1" pad="1"/>
</signal>
<signal name="!RESET">
<contactref element="R1" pad="2"/>
<contactref element="JP2" pad="5"/>
<contactref element="IC1" pad="6"/>
</signal>
<signal name="B2">
<contactref element="IC1" pad="4"/>
<contactref element="R2" pad="2"/>
</signal>
<signal name="N$11">
<contactref element="C2" pad="1"/>
<contactref element="IC3" pad="2"/>
</signal>
<signal name="N$12">
<contactref element="C2" pad="2"/>
<contactref element="IC3" pad="4"/>
</signal>
<signal name="B0/TPID">
<contactref element="JP2" pad="1"/>
<contactref element="R4" pad="1"/>
<contactref element="Q2" pad="3"/>
<contactref element="Q2" pad="1"/>
<contactref element="IC1" pad="1"/>
</signal>
<signal name="B1/TPIC">
<contactref element="JP2" pad="3"/>
<contactref element="IC1" pad="3"/>
<contactref element="X1" pad="3"/>
</signal>
<signal name="N$3">
<contactref element="X1" pad="1"/>
<contactref element="SJ1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
