(export (version D)
  (design
    (source D:\DIY\GPS_module_mini\gps-v1.1\gps.sch)
    (date "08/03/21 22:11:27")
    (tool "Eeschema (5.1.10)-1")
    (sheet (number 1) (name /) (tstamps /)
      (title_block
        (title)
        (company)
        (rev)
        (date)
        (source gps.sch)
        (comment (number 1) (value ""))
        (comment (number 2) (value ""))
        (comment (number 3) (value ""))
        (comment (number 4) (value "")))))
  (components
    (comp (ref C1)
      (value "2.2 uF")
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ED2C7C2))
    (comp (ref R2)
      (value 200R)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ED4CDB9))
    (comp (ref J3)
      (value Conn_Coaxial)
      (footprint Connector_Coaxial:U.FL_Molex_MCRF_73412-0110_Vertical)
      (datasheet " ~")
      (libsource (lib Connector) (part Conn_Coaxial) (description "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, ...)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ED59AAE))
    (comp (ref U2)
      (value NEO-M8N)
      (footprint RF_GPS:ublox_NEO)
      (datasheet https://www.u-blox.com/sites/default/files/NEO-M8-FW3_DataSheet_%28UBX-15031086%29.pdf)
      (libsource (lib RF_GPS) (part NEO-M8N) (description "GNSS Module NEO M8, VCC 2.7V to 3.6V"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ED35493))
    (comp (ref U3)
      (value BLUETOOTH-SERIAL-HC-06)
      (footprint gps:BLUETOOTH-SERIAL-HC-06_2)
      (datasheet "Manufacturer Recommendations")
      (fields
        (field (name Feld4) Olimex)
        (field (name Feld5) 2.2)
        (field (name Feld6) 2.0mm))
      (libsource (lib HC-06) (part BLUETOOTH-SERIAL-HC-06) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ED86CDB))
    (comp (ref C4)
      (value "0.1 uF")
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5ED89CF1))
    (comp (ref L1)
      (value 27mH)
      (footprint Inductor_SMD:L_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part L_Small) (description "Inductor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5EDA86C0))
    (comp (ref R1)
      (value 10R)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5EDA9BDD))
    (comp (ref C6)
      (value 1nF)
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5EDAB00C))
    (comp (ref C3)
      (value 1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5EEA719A))
    (comp (ref JP3)
      (value JP_SAFEBOOT)
      (footprint Jumper:SolderJumper-2_P1.3mm_Open_TrianglePad1.0x1.5mm)
      (datasheet ~)
      (libsource (lib Jumper) (part SolderJumper_2_Open) (description "Solder Jumper, 2-pole, open"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5EEB15D2))
    (comp (ref R3)
      (value 200R)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5EEB9835))
    (comp (ref FB1)
      (value Ferrite_Bead_1k)
      (footprint Inductor_SMD:L_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part Ferrite_Bead_Small) (description "Ferrite bead, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5EECDE85))
    (comp (ref FB2)
      (value Ferrite_Bead_1k)
      (footprint Inductor_SMD:L_0805_2012Metric_Pad1.15x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part Ferrite_Bead_Small) (description "Ferrite bead, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5EED13FE))
    (comp (ref C5)
      (value "2.2 uF")
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F02AC13))
    (comp (ref R7)
      (value 100k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F07FD2A))
    (comp (ref C2)
      (value "0.033 uF")
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F0AE10B))
    (comp (ref U1)
      (value LP3981IMM-2.8)
      (footprint gps:LP3981VSSOP)
      (datasheet LP3981IMM-2.8)
      (fields
        (field (name Field4) MSOP-8)
        (field (name Field5) "National Semiconductor")
        (field (name Field6) -)
        (field (name Field7) 41K7895))
      (libsource (lib LP3981) (part LP3981IMM-2.8) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F0FB993))
    (comp (ref D4)
      (value B0540WS)
      (footprint Diode_SMD:D_SOD-323_HandSoldering)
      (datasheet ~)
      (libsource (lib Device) (part D_Schottky) (description "Schottky diode"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C7E082B))
    (comp (ref Q6)
      (value IRLML6402)
      (footprint Package_TO_SOT_SMD:SOT-23_Handsoldering)
      (datasheet https://www.infineon.com/dgdl/irlml6402pbf.pdf?fileId=5546d462533600a401535668d5c2263c)
      (libsource (lib Transistor_FET) (part IRLML6402) (description "-3.7A Id, -20V Vds, 65mOhm Rds, P-Channel HEXFET Power MOSFET, SOT-23"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5C82B320))
    (comp (ref J4)
      (value Lipo)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61053041))
    (comp (ref J2)
      (value Lipo_charger)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 610576E9))
    (comp (ref J5)
      (value LED_fix)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Female) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6107D46F))
    (comp (ref J6)
      (value LED_pwr)
      (footprint Connector_PinHeader_2.54mm:PinHeader_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Female) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61084CF2))
    (comp (ref C7)
      (value 10uF)
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6109C136))
    (comp (ref J1)
      (value USB_B_Micro)
      (footprint Connector_USB:USB_Micro-B_GCT_USB3076-30-A)
      (datasheet ~)
      (libsource (lib gps-rescue) (part USB_B_Micro-Connector) (description ""))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F0578D1))
    (comp (ref U4)
      (value USBLC6-2SC6)
      (footprint Package_TO_SOT_SMD:SOT-23-6)
      (datasheet https://www.st.com/resource/en/datasheet/usblc6-2.pdf)
      (libsource (lib Power_Protection) (part USBLC6-2SC6) (description "Very low capacitance ESD protection diode, 2 data-line, SOT-23-6"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F0618BE))
    (comp (ref C8)
      (value 0.1uF)
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F06DB35))
    (comp (ref R5)
      (value 27R)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F07206B))
    (comp (ref R6)
      (value 27R)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F0756BE))
    (comp (ref C9)
      (value "1 uF")
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F04F133))
    (comp (ref C10)
      (value "1 uF")
      (footprint Capacitor_SMD:C_0805_2012Metric_Pad1.18x1.45mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part C_Small) (description "Unpolarized capacitor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F054D45))
    (comp (ref U5)
      (value MCP1700T-3302E_TT)
      (footprint Package_TO_SOT_SMD:SOT-89-5_Handsoldering)
      (datasheet http://www.microchip.com/mymicrochip/filehandler.aspx?ddocname=en011779)
      (fields
        (field (name Category) "Integrated Circuits (ICs)")
        (field (name DK_Datasheet_Link) http://www.microchip.com/mymicrochip/filehandler.aspx?ddocname=en011779)
        (field (name DK_Detail_Page) /product-detail/en/microchip-technology/MCP1700T-3302E-TT/MCP1700T3302ETTCT-ND/652677)
        (field (name Description) "IC REG LINEAR 3.3V 250MA SOT23-3")
        (field (name Digi-Key_PN) MCP1700T3302ETTCT-ND)
        (field (name Family) "PMIC - Voltage Regulators - Linear")
        (field (name MPN) MCP1700T-3302E/TT)
        (field (name Manufacturer) "Microchip Technology")
        (field (name Status) Active))
      (libsource (lib dk_PMIC-Voltage-Regulators-Linear) (part MCP1700T-3302E_TT) (description "IC REG LINEAR 3.3V 250MA SOT23-3"))
      (sheetpath (names /) (tstamps /))
      (tstamp 6106DE72))
    (comp (ref R4)
      (value 100k)
      (footprint Resistor_SMD:R_0805_2012Metric_Pad1.20x1.40mm_HandSolder)
      (datasheet ~)
      (libsource (lib Device) (part R_Small) (description "Resistor, small symbol"))
      (sheetpath (names /) (tstamps /))
      (tstamp 61045ECC))
    (comp (ref J12)
      (value pwr_sw)
      (footprint Connector_PinSocket_2.54mm:PinSocket_1x02_P2.54mm_Vertical)
      (datasheet ~)
      (libsource (lib Connector) (part Conn_01x02_Male) (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)"))
      (sheetpath (names /) (tstamps /))
      (tstamp 5F8FA227)))
  (libparts
    (libpart (lib Connector) (part Conn_01x02_Female)
      (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02_Female))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib Connector) (part Conn_01x02_Male)
      (description "Generic connector, single row, 01x02, script generated (kicad-library-utils/schlib/autogen/connector/)")
      (docs ~)
      (footprints
        (fp Connector*:*_1x??_*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_01x02_Male))
      (pins
        (pin (num 1) (name Pin_1) (type passive))
        (pin (num 2) (name Pin_2) (type passive))))
    (libpart (lib Connector) (part Conn_Coaxial)
      (description "coaxial connector (BNC, SMA, SMB, SMC, Cinch/RCA, ...)")
      (docs " ~")
      (footprints
        (fp *BNC*)
        (fp *SMA*)
        (fp *SMB*)
        (fp *SMC*)
        (fp *Cinch*))
      (fields
        (field (name Reference) J)
        (field (name Value) Conn_Coaxial))
      (pins
        (pin (num 1) (name In) (type passive))
        (pin (num 2) (name Ext) (type passive))))
    (libpart (lib Device) (part C_Small)
      (description "Unpolarized capacitor, small symbol")
      (docs ~)
      (footprints
        (fp C_*))
      (fields
        (field (name Reference) C)
        (field (name Value) C_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part D_Schottky)
      (description "Schottky diode")
      (docs ~)
      (footprints
        (fp TO-???*)
        (fp *_Diode_*)
        (fp *SingleDiode*)
        (fp D_*))
      (fields
        (field (name Reference) D)
        (field (name Value) D_Schottky))
      (pins
        (pin (num 1) (name K) (type passive))
        (pin (num 2) (name A) (type passive))))
    (libpart (lib Device) (part Ferrite_Bead_Small)
      (description "Ferrite bead, small symbol")
      (docs ~)
      (footprints
        (fp Inductor_*)
        (fp L_*)
        (fp *Ferrite*))
      (fields
        (field (name Reference) FB)
        (field (name Value) Ferrite_Bead_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part L_Small)
      (description "Inductor, small symbol")
      (docs ~)
      (footprints
        (fp Choke_*)
        (fp *Coil*)
        (fp Inductor_*)
        (fp L_*))
      (fields
        (field (name Reference) L)
        (field (name Value) L_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib Device) (part R_Small)
      (description "Resistor, small symbol")
      (docs ~)
      (footprints
        (fp R_*))
      (fields
        (field (name Reference) R)
        (field (name Value) R_Small))
      (pins
        (pin (num 1) (name ~) (type passive))
        (pin (num 2) (name ~) (type passive))))
    (libpart (lib HC-06) (part BLUETOOTH-SERIAL-HC-06)
      (fields
        (field (name Reference) U)
        (field (name Value) BLUETOOTH-SERIAL-HC-06)
        (field (name Footprint) XCVR_BLUETOOTH-SERIAL-HC-06)
        (field (name Datasheet) "Manufacturer Recommendations")
        (field (name Field4) Olimex)
        (field (name Field5) 2.2)
        (field (name Field6) 2.0mm))
      (pins
        (pin (num 1) (name TX) (type output))
        (pin (num 2) (name RX) (type input))
        (pin (num 3) (name ~CTS~) (type input))
        (pin (num 4) (name ~RTS~) (type output))
        (pin (num 5) (name PCM_CLK) (type BiDi))
        (pin (num 6) (name PCM_OUT) (type output))
        (pin (num 7) (name PCM_IN) (type input))
        (pin (num 8) (name PCM_SYNC) (type BiDi))
        (pin (num 9) (name AIO0) (type BiDi))
        (pin (num 10) (name AIO1) (type BiDi))
        (pin (num 11) (name ~RESET~) (type input))
        (pin (num 12) (name 3V3) (type power_in))
        (pin (num 13) (name GND) (type power_in))
        (pin (num 15) (name USB_D-) (type BiDi))
        (pin (num 16) (name ~CSB~) (type input))
        (pin (num 17) (name MOSI) (type input))
        (pin (num 18) (name MISO) (type output))
        (pin (num 19) (name CLK) (type input))
        (pin (num 20) (name USB_D+) (type BiDi))
        (pin (num 21) (name GND) (type power_in))
        (pin (num 22) (name GND) (type power_in))
        (pin (num 23) (name PIO0) (type BiDi))
        (pin (num 24) (name PIO1) (type BiDi))
        (pin (num 25) (name PIO2) (type BiDi))
        (pin (num 26) (name PIO3) (type BiDi))
        (pin (num 27) (name PIO4) (type BiDi))
        (pin (num 28) (name PIO5) (type BiDi))
        (pin (num 29) (name PIO6) (type BiDi))
        (pin (num 30) (name PIO7) (type BiDi))
        (pin (num 31) (name PIO8) (type BiDi))
        (pin (num 32) (name PIO9) (type BiDi))
        (pin (num 33) (name PIO10) (type BiDi))
        (pin (num 34) (name PIO11) (type BiDi))))
    (libpart (lib Jumper) (part SolderJumper_2_Open)
      (description "Solder Jumper, 2-pole, open")
      (docs ~)
      (footprints
        (fp SolderJumper*Open*))
      (fields
        (field (name Reference) JP)
        (field (name Value) SolderJumper_2_Open))
      (pins
        (pin (num 1) (name A) (type passive))
        (pin (num 2) (name B) (type passive))))
    (libpart (lib LP3981) (part LP3981IMM-2.8)
      (fields
        (field (name Reference) U)
        (field (name Value) LP3981IMM-2.8)
        (field (name Footprint) SOP65P490X110-8N)
        (field (name Datasheet) LP3981IMM-2.8)
        (field (name Field4) MSOP-8)
        (field (name Field5) "National Semiconductor")
        (field (name Field6) -)
        (field (name Field7) 41K7895))
      (pins
        (pin (num 1) (name VOUT) (type output))
        (pin (num 2) (name VIN) (type input))
        (pin (num 3) (name NC_2) (type NotConnected))
        (pin (num 4) (name VOUT-SENSE) (type output))
        (pin (num 5) (name GND) (type passive))
        (pin (num 6) (name BYPASS) (type input))
        (pin (num 7) (name VEN) (type input))
        (pin (num 8) (name NC) (type NotConnected))))
    (libpart (lib Power_Protection) (part USBLC6-2SC6)
      (description "Very low capacitance ESD protection diode, 2 data-line, SOT-23-6")
      (docs https://www.st.com/resource/en/datasheet/usblc6-2.pdf)
      (footprints
        (fp SOT?23*))
      (fields
        (field (name Reference) U)
        (field (name Value) USBLC6-2SC6)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-23-6))
      (pins
        (pin (num 1) (name I/O1) (type passive))
        (pin (num 2) (name GND) (type passive))
        (pin (num 3) (name I/O2) (type passive))
        (pin (num 4) (name I/O2) (type passive))
        (pin (num 5) (name VBUS) (type passive))
        (pin (num 6) (name I/O1) (type passive))))
    (libpart (lib RF_GPS) (part NEO-M8N)
      (aliases
        (alias NEO-8Q)
        (alias NEO-M8Q))
      (description "GNSS Module NEO M8, VCC 2.7V to 3.6V")
      (docs https://www.u-blox.com/sites/default/files/NEO-M8-FW3_DataSheet_%28UBX-15031086%29.pdf)
      (footprints
        (fp ublox*NEO*))
      (fields
        (field (name Reference) U)
        (field (name Value) NEO-M8N)
        (field (name Footprint) RF_GPS:ublox_NEO))
      (pins
        (pin (num 1) (name ~SAFEBOOT) (type input))
        (pin (num 2) (name D_SEL) (type input))
        (pin (num 3) (name TIMEPULSE) (type output))
        (pin (num 4) (name EXTINT) (type input))
        (pin (num 5) (name USB_DM) (type BiDi))
        (pin (num 6) (name USB_DP) (type BiDi))
        (pin (num 7) (name VDD_USB) (type power_in))
        (pin (num 8) (name ~RESET) (type input))
        (pin (num 9) (name VCC_RF) (type power_out))
        (pin (num 10) (name GND) (type power_in))
        (pin (num 11) (name RF_IN) (type input))
        (pin (num 12) (name GND) (type passive))
        (pin (num 13) (name GND) (type passive))
        (pin (num 14) (name LNA_EN) (type output))
        (pin (num 15) (name RESERVED) (type NotConnected))
        (pin (num 16) (name RESERVED) (type NotConnected))
        (pin (num 17) (name RESERVED) (type NotConnected))
        (pin (num 18) (name SDA/~SPI_CS) (type BiDi))
        (pin (num 19) (name SCL/SPI_CLK) (type input))
        (pin (num 20) (name TXD/SPI_MISO) (type output))
        (pin (num 21) (name RXD/SPI_MOSI) (type input))
        (pin (num 22) (name V_BCKP) (type power_in))
        (pin (num 23) (name VCC) (type power_in))
        (pin (num 24) (name GND) (type passive))))
    (libpart (lib Transistor_FET) (part TP0610T)
      (aliases
        (alias VP0610T)
        (alias BSS84)
        (alias NTR2101P)
        (alias BSS83P)
        (alias Si2319CDS)
        (alias IRLML6401)
        (alias IRLML6402)
        (alias DMG2301L)
        (alias AO3401A)
        (alias IRLML9301)
        (alias IRLML5203)
        (alias Si2371EDS)
        (alias TSM2301ACX)
        (alias FDN340P))
      (description "-0.18A Id, -60V Vds, P-Channel MOSFET, SOT-23")
      (docs http://www.vishay.com/docs/70209/70209.pdf)
      (footprints
        (fp SOT?23*))
      (fields
        (field (name Reference) Q)
        (field (name Value) TP0610T)
        (field (name Footprint) Package_TO_SOT_SMD:SOT-23))
      (pins
        (pin (num 1) (name G) (type input))
        (pin (num 2) (name S) (type passive))
        (pin (num 3) (name D) (type passive))))
    (libpart (lib dk_PMIC-Voltage-Regulators-Linear) (part MCP1700T-3302E_TT)
      (description "IC REG LINEAR 3.3V 250MA SOT23-3")
      (docs http://www.microchip.com/mymicrochip/filehandler.aspx?ddocname=en011779)
      (fields
        (field (name Reference) U)
        (field (name Value) MCP1700T-3302E_TT)
        (field (name Footprint) digikey-footprints:SOT-23-3)
        (field (name Datasheet) http://www.microchip.com/mymicrochip/filehandler.aspx?ddocname=en011779)
        (field (name Digi-Key_PN) MCP1700T3302ETTCT-ND)
        (field (name MPN) MCP1700T-3302E/TT)
        (field (name Category) "Integrated Circuits (ICs)")
        (field (name Family) "PMIC - Voltage Regulators - Linear")
        (field (name DK_Datasheet_Link) http://www.microchip.com/mymicrochip/filehandler.aspx?ddocname=en011779)
        (field (name DK_Detail_Page) /product-detail/en/microchip-technology/MCP1700T-3302E-TT/MCP1700T3302ETTCT-ND/652677)
        (field (name Description) "IC REG LINEAR 3.3V 250MA SOT23-3")
        (field (name Manufacturer) "Microchip Technology")
        (field (name Status) Active))
      (pins
        (pin (num 1) (name GND) (type power_in))
        (pin (num 2) (name OUT) (type power_out))
        (pin (num 3) (name IN) (type power_in))))
    (libpart (lib gps-rescue) (part USB_B_Micro-Connector)
      (footprints
        (fp USB*))
      (fields
        (field (name Reference) J)
        (field (name Value) USB_B_Micro-Connector))
      (pins
        (pin (num 1) (name VBUS) (type power_out))
        (pin (num 2) (name D-) (type passive))
        (pin (num 3) (name D+) (type passive))
        (pin (num 4) (name ID) (type passive))
        (pin (num 5) (name GND) (type power_out))
        (pin (num 6) (name Shield) (type passive)))))
  (libraries
    (library (logical Connector)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Connector.lib"))
    (library (logical Device)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Device.lib"))
    (library (logical HC-06)
      (uri D:/DIY/NEO8N/BLUETOOTH-SERIAL-HC-06.lib))
    (library (logical Jumper)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Jumper.lib"))
    (library (logical LP3981)
      (uri D:/DIY/NEO8N/LP3981IMM-2.8.lib))
    (library (logical Power_Protection)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Power_Protection.lib"))
    (library (logical RF_GPS)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/RF_GPS.lib"))
    (library (logical Transistor_FET)
      (uri "C:\\Program Files\\KiCad\\share\\kicad\\library/Transistor_FET.lib"))
    (library (logical dk_PMIC-Voltage-Regulators-Linear)
      (uri D:/KiCAD/digikey-kicad-library-master/digikey-symbols/dk_PMIC-Voltage-Regulators-Linear.lib))
    (library (logical gps-rescue)
      (uri D:\DIY\GPS_module_mini\gps-v1.1/gps-rescue.lib)))
  (nets
    (net (code 1) (name GND)
      (node (ref C9) (pin 2))
      (node (ref C8) (pin 2))
      (node (ref U1) (pin 5))
      (node (ref C6) (pin 1))
      (node (ref C10) (pin 2))
      (node (ref C2) (pin 2))
      (node (ref U3) (pin 22))
      (node (ref U5) (pin 1))
      (node (ref R4) (pin 2))
      (node (ref U4) (pin 2))
      (node (ref R3) (pin 1))
      (node (ref J3) (pin 2))
      (node (ref J4) (pin 1))
      (node (ref J2) (pin 2))
      (node (ref R2) (pin 1))
      (node (ref U2) (pin 10))
      (node (ref U2) (pin 12))
      (node (ref U2) (pin 13))
      (node (ref C1) (pin 2))
      (node (ref U2) (pin 24))
      (node (ref U3) (pin 21))
      (node (ref U3) (pin 13))
      (node (ref C5) (pin 2))
      (node (ref C7) (pin 2))
      (node (ref C4) (pin 1))
      (node (ref R7) (pin 1))
      (node (ref C3) (pin 2))
      (node (ref J1) (pin 5))
      (node (ref JP3) (pin 1)))
    (net (code 2) (name "Net-(J6-Pad2)")
      (node (ref R3) (pin 2))
      (node (ref J6) (pin 2)))
    (net (code 3) (name "Net-(J5-Pad1)")
      (node (ref U2) (pin 3))
      (node (ref J5) (pin 1)))
    (net (code 4) (name "Net-(J5-Pad2)")
      (node (ref J5) (pin 2))
      (node (ref R2) (pin 2)))
    (net (code 5) (name "Net-(J4-Pad2)")
      (node (ref Q6) (pin 3))
      (node (ref J4) (pin 2)))
    (net (code 6) (name "Net-(J1-Pad6)")
      (node (ref J1) (pin 6)))
    (net (code 7) (name "Net-(J1-Pad2)")
      (node (ref U4) (pin 1))
      (node (ref J1) (pin 2)))
    (net (code 8) (name "Net-(J1-Pad4)")
      (node (ref J1) (pin 4)))
    (net (code 9) (name VCC_USB_IN)
      (node (ref C8) (pin 1))
      (node (ref C9) (pin 1))
      (node (ref J1) (pin 1))
      (node (ref D4) (pin 2))
      (node (ref U4) (pin 5))
      (node (ref Q6) (pin 1))
      (node (ref J2) (pin 1))
      (node (ref U5) (pin 3))
      (node (ref R4) (pin 1)))
    (net (code 10) (name +3V3)
      (node (ref C5) (pin 1))
      (node (ref U3) (pin 12))
      (node (ref J6) (pin 1))
      (node (ref U2) (pin 22))
      (node (ref C4) (pin 2))
      (node (ref C3) (pin 1))
      (node (ref C7) (pin 1))
      (node (ref U2) (pin 23))
      (node (ref U1) (pin 1))
      (node (ref U1) (pin 4)))
    (net (code 11) (name "Net-(C2-Pad1)")
      (node (ref C2) (pin 1))
      (node (ref U1) (pin 6)))
    (net (code 12) (name "Net-(U1-Pad8)")
      (node (ref U1) (pin 8)))
    (net (code 13) (name "Net-(U1-Pad3)")
      (node (ref U1) (pin 3)))
    (net (code 14) (name VDD_USB)
      (node (ref R7) (pin 2))
      (node (ref U5) (pin 2))
      (node (ref U2) (pin 7))
      (node (ref C10) (pin 1)))
    (net (code 15) (name "Net-(C6-Pad2)")
      (node (ref R1) (pin 1))
      (node (ref C6) (pin 2))
      (node (ref U2) (pin 9)))
    (net (code 16) (name "Net-(L1-Pad1)")
      (node (ref R1) (pin 2))
      (node (ref L1) (pin 1)))
    (net (code 17) (name "Net-(D4-Pad1)")
      (node (ref J12) (pin 1))
      (node (ref Q6) (pin 2))
      (node (ref D4) (pin 1)))
    (net (code 18) (name "Net-(J1-Pad3)")
      (node (ref U4) (pin 3))
      (node (ref J1) (pin 3)))
    (net (code 19) (name USB_DP)
      (node (ref U2) (pin 6))
      (node (ref R5) (pin 2)))
    (net (code 20) (name "Net-(R5-Pad1)")
      (node (ref U4) (pin 4))
      (node (ref R5) (pin 1)))
    (net (code 21) (name "Net-(R6-Pad1)")
      (node (ref R6) (pin 1))
      (node (ref U4) (pin 6)))
    (net (code 22) (name USB_DM)
      (node (ref U2) (pin 5))
      (node (ref R6) (pin 2)))
    (net (code 23) (name "Net-(U3-Pad5)")
      (node (ref U3) (pin 5)))
    (net (code 24) (name "Net-(U3-Pad15)")
      (node (ref U3) (pin 15)))
    (net (code 25) (name "Net-(U3-Pad11)")
      (node (ref U3) (pin 11)))
    (net (code 26) (name "Net-(U3-Pad10)")
      (node (ref U3) (pin 10)))
    (net (code 27) (name "Net-(U3-Pad9)")
      (node (ref U3) (pin 9)))
    (net (code 28) (name "Net-(U3-Pad8)")
      (node (ref U3) (pin 8)))
    (net (code 29) (name "Net-(U3-Pad7)")
      (node (ref U3) (pin 7)))
    (net (code 30) (name "Net-(U3-Pad6)")
      (node (ref U3) (pin 6)))
    (net (code 31) (name "Net-(U3-Pad16)")
      (node (ref U3) (pin 16)))
    (net (code 32) (name "Net-(U3-Pad4)")
      (node (ref U3) (pin 4)))
    (net (code 33) (name "Net-(U3-Pad3)")
      (node (ref U3) (pin 3)))
    (net (code 34) (name "Net-(U2-Pad8)")
      (node (ref U2) (pin 8)))
    (net (code 35) (name "Net-(U3-Pad29)")
      (node (ref U3) (pin 29)))
    (net (code 36) (name "Net-(U3-Pad34)")
      (node (ref U3) (pin 34)))
    (net (code 37) (name "Net-(U3-Pad33)")
      (node (ref U3) (pin 33)))
    (net (code 38) (name "Net-(U3-Pad32)")
      (node (ref U3) (pin 32)))
    (net (code 39) (name "Net-(U3-Pad31)")
      (node (ref U3) (pin 31)))
    (net (code 40) (name "Net-(U3-Pad30)")
      (node (ref U3) (pin 30)))
    (net (code 41) (name "Net-(U2-Pad4)")
      (node (ref U2) (pin 4)))
    (net (code 42) (name "Net-(U3-Pad28)")
      (node (ref U3) (pin 28)))
    (net (code 43) (name "Net-(U3-Pad27)")
      (node (ref U3) (pin 27)))
    (net (code 44) (name "Net-(U3-Pad26)")
      (node (ref U3) (pin 26)))
    (net (code 45) (name "Net-(U3-Pad25)")
      (node (ref U3) (pin 25)))
    (net (code 46) (name "Net-(U3-Pad24)")
      (node (ref U3) (pin 24)))
    (net (code 47) (name "Net-(U3-Pad23)")
      (node (ref U3) (pin 23)))
    (net (code 48) (name "Net-(U3-Pad20)")
      (node (ref U3) (pin 20)))
    (net (code 49) (name "Net-(U3-Pad19)")
      (node (ref U3) (pin 19)))
    (net (code 50) (name "Net-(U3-Pad18)")
      (node (ref U3) (pin 18)))
    (net (code 51) (name "Net-(U3-Pad17)")
      (node (ref U3) (pin 17)))
    (net (code 52) (name "Net-(U2-Pad14)")
      (node (ref U2) (pin 14)))
    (net (code 53) (name "Net-(J3-Pad1)")
      (node (ref J3) (pin 1))
      (node (ref U2) (pin 11))
      (node (ref L1) (pin 2)))
    (net (code 54) (name "Net-(U2-Pad19)")
      (node (ref U2) (pin 19)))
    (net (code 55) (name "Net-(U2-Pad18)")
      (node (ref U2) (pin 18)))
    (net (code 56) (name V_IN)
      (node (ref U1) (pin 7))
      (node (ref U1) (pin 2))
      (node (ref J12) (pin 2))
      (node (ref C1) (pin 1)))
    (net (code 57) (name "Net-(U2-Pad16)")
      (node (ref U2) (pin 16)))
    (net (code 58) (name "Net-(FB1-Pad1)")
      (node (ref FB1) (pin 1))
      (node (ref U2) (pin 20)))
    (net (code 59) (name "Net-(U2-Pad2)")
      (node (ref U2) (pin 2)))
    (net (code 60) (name "Net-(U2-Pad17)")
      (node (ref U2) (pin 17)))
    (net (code 61) (name "Net-(U2-Pad15)")
      (node (ref U2) (pin 15)))
    (net (code 62) (name "Net-(JP3-Pad2)")
      (node (ref U2) (pin 1))
      (node (ref JP3) (pin 2)))
    (net (code 63) (name "Net-(FB2-Pad1)")
      (node (ref U2) (pin 21))
      (node (ref FB2) (pin 1)))
    (net (code 64) (name RX)
      (node (ref U3) (pin 1))
      (node (ref FB2) (pin 2)))
    (net (code 65) (name TX)
      (node (ref FB1) (pin 2))
      (node (ref U3) (pin 2)))))