<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<board>
<plain>
<wire x1="0" y1="0" x2="30.46" y2="0" width="0" layer="20"/>
<wire x1="30.46" y1="0" x2="30.47" y2="28.575" width="0" layer="20"/>
<wire x1="30.47" y1="28.575" x2="0.01" y2="28.575" width="0" layer="20"/>
<wire x1="0.01" y1="28.575" x2="0" y2="0" width="0" layer="20"/>
<text>IN</text>
<text>OUT</text>
</plain>
<libraries>
<library name="SparkFun-Capacitors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="linear">
<description>&lt;b&gt;Linear Devices&lt;/b&gt;&lt;p&gt;
Operational amplifiers,  comparators, voltage regulators, ADCs, DACs, etc.&lt;p&gt;
&lt;author&gt;Created by librarian@cadsoft.de&lt;/author&gt;</description>
<packages>
<package name="SO08">
<description>&lt;b&gt;Small Outline Package 8&lt;/b&gt;&lt;br&gt;
NS Package M08A</description>
</package>
</packages>
</library>
<library name="AP2331">
<packages>
<package name="SOT23-6">
</package>
</packages>
</library>
<library name="SJ2-35853A-SMT-TR">
<packages>
<package name="CUI_SJ2-35853A-SMT-TR">
</package>
</packages>
</library>
<library name="SparkFun-Resistors">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
<library name="USBC">
<packages>
<package name="UJC-HP-3">
</package>
</packages>
</library>
<library name="SparkFun-Passives">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find resistors, capacitors, inductors, test points, jumper pads, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="0805">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="C1" library="SparkFun-Capacitors" package="0805" value="10µF">
<attribute name="NAME"/>
</element>
<element name="C2" library="SparkFun-Capacitors" package="0805" value="10µF">
<attribute name="NAME"/>
</element>
<element name="C3" library="SparkFun-Capacitors" package="0805" value="10µF">
<attribute name="NAME"/>
</element>
<element name="IC1" library="linear" package="SO08" value="LM358D">
<attribute name="NAME"/>
<attribute name="POPULARITY" value="12"/>
</element>
<element name="IC2" library="AP2331" package="SOT23-6" value="MAX1720EUTG">
<attribute name="NAME"/>
</element>
<element name="J1" library="SJ2-35853A-SMT-TR" package="CUI_SJ2-35853A-SMT-TR" value="SJ2-35853A-SMT-TR">
<attribute name="MANUFACTURER" value="CUI"/>
<attribute name="MPN" value="SJ2-35853A-SMT-TR"/>
<attribute name="PART_REV" value="1.01"/>
<attribute name="STANDARD" value="Manufacturer recommendation"/>
</element>
<element name="J2" library="SJ2-35853A-SMT-TR" package="CUI_SJ2-35853A-SMT-TR" value="SJ2-35853A-SMT-TR">
<attribute name="MANUFACTURER" value="CUI"/>
<attribute name="MPN" value="SJ2-35853A-SMT-TR"/>
<attribute name="PART_REV" value="1.01"/>
<attribute name="STANDARD" value="Manufacturer recommendation"/>
</element>
<element name="R2" library="SparkFun-Resistors" package="0805" value="100kΩ">
<attribute name="NAME"/>
</element>
<element name="R1" library="SparkFun-Resistors" package="0805" value="20kΩ">
<attribute name="NAME"/>
</element>
<element name="R3" library="SparkFun-Resistors" package="0805" value="20kΩ">
<attribute name="NAME"/>
</element>
<element name="R4" library="SparkFun-Resistors" package="0805" value="100kΩ">
<attribute name="NAME"/>
</element>
<element name="C4" library="SparkFun-Capacitors" package="0805" value="10µF">
<attribute name="NAME"/>
</element>
<element name="C5" library="SparkFun-Capacitors" package="0805" value="10µF">
<attribute name="NAME"/>
</element>
<element name="C6" library="SparkFun-Capacitors" package="0805" value="1µF">
<attribute name="NAME"/>
</element>
<element name="C7" library="SparkFun-Capacitors" package="0805" value="1µF">
<attribute name="NAME"/>
</element>
<element name="R5" library="SparkFun-Resistors" package="0805" value="10kΩ">
<attribute name="NAME"/>
</element>
<element name="R6" library="SparkFun-Resistors" package="0805" value="10kΩ">
<attribute name="NAME"/>
</element>
<element name="J3" library="USBC" package="UJC-HP-3" value="UJC-HP-3"/>
<element name="R7" library="SparkFun-Resistors" package="0805" value="5.1kΩ">
<attribute name="NAME"/>
</element>
<element name="R8" library="SparkFun-Resistors" package="0805" value="5.1kΩ">
<attribute name="NAME"/>
</element>
<element name="R9" library="SparkFun-Resistors" package="0805" value="1MΩ">
<attribute name="NAME"/>
</element>
<element name="L1" library="SparkFun-Passives" package="0805" value="400Ω">
<attribute name="NAME"/>
</element>
<element name="C8" library="SparkFun-Capacitors" package="0805" value="6800pF">
<attribute name="NAME"/>
</element>
</elements>
<signals>
<signal name="N$1">
<contactref element="J1" pad="3"/>
<contactref element="C5" pad="1"/>
</signal>
<signal name="N$2">
<contactref element="J1" pad="2"/>
<contactref element="C4" pad="1"/>
</signal>
<signal name="N$3">
<contactref element="IC1" pad="1"/>
<contactref element="R4" pad="2"/>
<contactref element="J2" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="IC1" pad="7"/>
<contactref element="R2" pad="2"/>
<contactref element="J2" pad="3"/>
</signal>
<signal name="N$5">
<contactref element="IC1" pad="2"/>
<contactref element="R3" pad="1"/>
<contactref element="R4" pad="1"/>
</signal>
<signal name="N$7">
<contactref element="IC1" pad="6"/>
<contactref element="R1" pad="2"/>
<contactref element="R2" pad="1"/>
</signal>
<signal name="+5V">
<contactref element="IC1" pad="8"/>
<contactref element="IC2" pad="5"/>
<contactref element="IC2" pad="2"/>
<contactref element="C1" pad="1"/>
<contactref element="C6" pad="1"/>
<contactref element="L1" pad="2"/>
</signal>
<signal name="-5V">
<contactref element="IC1" pad="4"/>
<contactref element="IC2" pad="1"/>
<contactref element="C3" pad="2"/>
<contactref element="C7" pad="2"/>
</signal>
<signal name="GND">
<contactref element="R3" pad="2"/>
<contactref element="R1" pad="1"/>
<contactref element="C1" pad="2"/>
<contactref element="IC2" pad="4"/>
<contactref element="C3" pad="1"/>
<contactref element="J1" pad="1"/>
<contactref element="J2" pad="1"/>
<contactref element="C6" pad="2"/>
<contactref element="C7" pad="1"/>
<contactref element="R5" pad="2"/>
<contactref element="R6" pad="2"/>
<contactref element="J3" pad="B12"/>
<contactref element="R8" pad="2"/>
<contactref element="J3" pad="A12"/>
<contactref element="R9" pad="2"/>
<contactref element="R7" pad="2"/>
<contactref element="C8" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="IC2" pad="6"/>
<contactref element="C2" pad="1"/>
</signal>
<signal name="N$15">
<contactref element="C2" pad="2"/>
<contactref element="IC2" pad="3"/>
</signal>
<signal name="N$6">
<contactref element="IC1" pad="3"/>
<contactref element="C4" pad="2"/>
<contactref element="R5" pad="1"/>
</signal>
<signal name="N$8">
<contactref element="IC1" pad="5"/>
<contactref element="C5" pad="2"/>
<contactref element="R6" pad="1"/>
</signal>
<signal name="N$9">
<contactref element="J3" pad="P$1"/>
<contactref element="J3" pad="P$3"/>
<contactref element="J3" pad="P$4"/>
<contactref element="J3" pad="P$2"/>
<contactref element="R9" pad="1"/>
<contactref element="C8" pad="1"/>
</signal>
<signal name="N$11">
<contactref element="J3" pad="B5"/>
<contactref element="R7" pad="1"/>
</signal>
<signal name="N$12">
<contactref element="J3" pad="A5"/>
<contactref element="R8" pad="1"/>
</signal>
<signal name="N$17">
<contactref element="J3" pad="B9"/>
<contactref element="J3" pad="A9"/>
<contactref element="L1" pad="1"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
